<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="48.26" y2="0" width="0" layer="20"/>
<wire x1="48.26" y1="0" x2="48.26" y2="25.4" width="0" layer="20"/>
<wire x1="48.26" y1="25.4" x2="0" y2="25.4" width="0" layer="20"/>
<wire x1="0" y1="25.4" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="2X12">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02">
</package>
<package name="1X04">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="LED5MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
5 mm, round</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-1206">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="pinhead" package="2X12" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="1X02" value="PWR_BTN">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP3" library="SparkFun-Connectors" package="1X02" value="RESET_BTN">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP4" library="SparkFun-Connectors" package="1X02" value="PWR_LED">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP5" library="SparkFun-Connectors" package="1X02" value="HDD_LED">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP6" library="SparkFun-Connectors" package="1X02" value="ID_BTN">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP7" library="SparkFun-Connectors" package="1X04" value="SMBUS">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP8" library="SparkFun-Connectors" package="1X02" value="S1_LED">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP9" library="SparkFun-Connectors" package="1X02" value="S2_LED">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="NIC1_LED" library="adafruit" package="LED5MM" value="YELLOW">
<attribute name="NAME"/>
</element>
<element name="NIC2_LED" library="adafruit" package="LED5MM" value="YELLOW">
<attribute name="NAME"/>
</element>
<element name="ID_LED" library="adafruit" package="LED5MM" value="BLUE">
<attribute name="NAME"/>
</element>
<element name="3V3_LED" library="SparkFun-LED" package="LED-1206" value="GREEN">
<attribute name="PROD_ID" value="DIO-09910"/>
<attribute name="VALUE" value="GREEN"/>
<attribute name="NAME"/>
</element>
<element name="R1" library="SparkFun-Passives" package="0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Passives" package="0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun-Passives" package="0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun-Passives" package="0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="SparkFun-Passives" package="0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="SparkFun-Passives" package="0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="SparkFun-Passives" package="0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="SparkFun-Passives" package="0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="PWR_LED_CATH">
<contactref element="JP1" pad="5"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="HDD_LED_CATH">
<contactref element="JP1" pad="9"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="PWR_SW">
<contactref element="JP1" pad="11"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="RST_SW">
<contactref element="JP1" pad="15"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="GND">
<contactref element="JP1" pad="13"/>
<contactref element="JP1" pad="17"/>
<contactref element="JP6" pad="1"/>
<contactref element="JP3" pad="1"/>
<contactref element="JP2" pad="1"/>
<contactref element="JP7" pad="1"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="ID_SW">
<contactref element="JP1" pad="19"/>
<contactref element="JP6" pad="2"/>
</signal>
<signal name="TMP_SNS">
<contactref element="JP1" pad="21"/>
</signal>
<signal name="NMI_SW">
<contactref element="JP1" pad="23"/>
</signal>
<signal name="3V3_STB">
<contactref element="JP1" pad="2"/>
<contactref element="JP1" pad="1"/>
<contactref element="JP1" pad="7"/>
<contactref element="ID_LED" pad="A"/>
<contactref element="3V3_LED" pad="A"/>
<contactref element="JP7" pad="4"/>
<contactref element="JP4" pad="2"/>
<contactref element="JP5" pad="2"/>
<contactref element="JP8" pad="2"/>
<contactref element="JP9" pad="2"/>
</signal>
<signal name="5V_STB">
<contactref element="JP1" pad="4"/>
</signal>
<signal name="ID_LED_CATH">
<contactref element="JP1" pad="6"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="STATUS1_LED_CATH">
<contactref element="JP1" pad="8"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="STATUS2_LED_CATH">
<contactref element="JP1" pad="10"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="NIC1_LED_AN">
<contactref element="JP1" pad="12"/>
<contactref element="NIC1_LED" pad="A"/>
</signal>
<signal name="NIC1_LED_CATH">
<contactref element="JP1" pad="14"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="SMBUS_SDA">
<contactref element="JP1" pad="16"/>
<contactref element="JP7" pad="2"/>
</signal>
<signal name="SMBUS_SCL">
<contactref element="JP1" pad="18"/>
<contactref element="JP7" pad="3"/>
</signal>
<signal name="CHA_INT">
<contactref element="JP1" pad="20"/>
</signal>
<signal name="NIC2_LED_AN">
<contactref element="JP1" pad="22"/>
<contactref element="NIC2_LED" pad="A"/>
</signal>
<signal name="NIC2_LED_CATH">
<contactref element="JP1" pad="24"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="JP5" pad="1"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="JP4" pad="1"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$17">
<contactref element="ID_LED" pad="K"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$18">
<contactref element="NIC2_LED" pad="K"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$19">
<contactref element="NIC1_LED" pad="K"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="3V3_LED" pad="C"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="JP9" pad="1"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="JP8" pad="1"/>
<contactref element="R7" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
