(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
	)
	(setup
		(pad_to_mask_clearance 0.0508)
		(solder_mask_min_width 0.101)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions yes)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 6)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "gerbers")
		)
	)
	(net 0 "")
	(net 1 "GNDREF")
	(net 2 "VCC")
	(net 3 "/rst")
	(net 4 "Net-(ATTINY85-XTAL1{slash}PB3)")
	(net 5 "Net-(ATTINY85-XTAL2{slash}PB4)")
	(net 6 "Net-(ATTINY85-AREF{slash}PB0)")
	(net 7 "Net-(ATTINY85-PB1)")
	(net 8 "Net-(ATTINY85-PB2)")
	(net 9 "Net-(BT1--)")
	(net 10 "Net-(J3-Pin_1)")
	(footprint "Connector_PinSocket_2.00mm:PinSocket_1x02_P2.00mm_Vertical"
		(layer "F.Cu")
		(at 126.7 146.075 90)
		(descr "Through hole straight socket strip, 1x02, 2.00mm pitch, single row (from Kicad 4.0.7), script generated")
		(tags "Through hole socket strip THT 1x02 2.00mm single row")
		(property "Reference" "J3"
			(at -2.8 -2.3 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x02"
			(at 0 4.5 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinSocket_2.00mm:PinSocket_1x02_P2.00mm_Vertical"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "attiny85musicboxmini.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.35 1.35)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "Net-(J3-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2 90)
			(size 1.35 1.35)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDREF")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.00mm.3dshapes/PinSocket_1x02_P2.00mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-8_W7.62mm_Socket"
		(layer "F.Cu")
		(at 119.175 133.4)
		(descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), Socket")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil Socket")
		(property "Reference" "ATTINY85"
			(at 3.9 4.02 -90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "ATtiny85-20PU"
			(at 3.81 9.95 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm_Socket"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "attiny85musicboxmini.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 4.4 4.3 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/rst")
			(pinfunction "~{RESET}/PB5")
			(pintype "bidirectional")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(ATTINY85-XTAL1{slash}PB3)")
			(pinfunction "XTAL1/PB3")
			(pintype "bidirectional")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(ATTINY85-XTAL2{slash}PB4)")
			(pinfunction "XTAL2/PB4")
			(pintype "bidirectional")
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDREF")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "5" thru_hole oval
			(at 7.62 7.62)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Net-(ATTINY85-AREF{slash}PB0)")
			(pinfunction "AREF/PB0")
			(pintype "bidirectional")
		)
		(pad "6" thru_hole oval
			(at 7.62 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(ATTINY85-PB1)")
			(pinfunction "PB1")
			(pintype "bidirectional")
		)
		(pad "7" thru_hole oval
			(at 7.62 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "Net-(ATTINY85-PB2)")
			(pinfunction "PB2")
			(pintype "bidirectional")
		)
		(pad "8" thru_hole oval
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-8_W7.62mm_Socket.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal"
		(layer "F.Cu")
		(at 125.75 143.6 180)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "Rfilter"
			(at 2.54 0.1 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "68"
			(at 2.74 -1.2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "attiny85musicboxmini.kicad_sch")
		(attr through_hole)
		(fp_text user "Rfilt"
			(at 2.54 -0.15 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at -0.15 0 180)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "Net-(J3-Pin_1)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 5.2 0 180)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(ATTINY85-XTAL2{slash}PB4)")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D3.4mm_W2.1mm_P2.50mm"
		(layer "F.Cu")
		(at 123.7 145.925 180)
		(descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.4*2.1mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
		(tags "C Disc series Radial pin pitch 2.50mm  diameter 3.4mm width 2.1mm Capacitor")
		(property "Reference" "C2"
			(at 3.95 0 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ".1"
			(at 1.25 2.3 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_THT:C_Disc_D3.4mm_W2.1mm_P2.50mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "attiny85musicboxmini.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.52 1.52)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "Net-(J3-Pin_1)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 0 180)
			(size 1.52 1.52)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDREF")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.4mm_W2.1mm_P2.50mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "attinyspeaker:ag13by2"
		(layer "F.Cu")
		(at 110.85 136.875)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "BT1"
			(at 0.075 -0.7 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Battery"
			(at -6 4.87 0)
			(layer "F.Fab")
		)
		(property "Footprint" "attinyspeaker:ag13by2"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Multiple-cell battery"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "attiny85musicboxmini.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -5.3 0.85 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 7.35)
			(size 2.2 1.7)
			(drill oval 1.4 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VCC")
			(pinfunction "+")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 -7.35)
			(size 2.05 1.7)
			(drill oval 1.25 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "Net-(BT1--)")
			(pinfunction "-")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D3.4mm_W2.1mm_P2.50mm"
		(layer "F.Cu")
		(at 129.55 131.8 90)
		(descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.4*2.1mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
		(tags "C Disc series Radial pin pitch 2.50mm  diameter 3.4mm width 2.1mm Capacitor")
		(property "Reference" "C1"
			(at 1.2 1.875 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ".1"
			(at 1.38 0.264 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_THT:C_Disc_D3.4mm_W2.1mm_P2.50mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "attiny85musicboxmini.kicad_sch")
		(attr through_hole)
		(fp_text user "1uF"
			(at 1.25 -0.9 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.52 1.52)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VCC")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 0 90)
			(size 1.52 1.52)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDREF")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.4mm_W2.1mm_P2.50mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.00mm:PinHeader_1x02_P2.00mm_Vertical"
		(layer "F.Cu")
		(at 118.575 146.125 -90)
		(descr "Through hole straight pin header, 1x02, 2.00mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.00mm single row")
		(property "Reference" "J1"
			(at 0 -2.06 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x02"
			(at 0 4.06 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.00mm:PinHeader_1x02_P2.00mm_Vertical"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "attiny85musicboxmini.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 270)
			(size 1.3 1.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 1 "GNDREF")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2 270)
			(size 1.3 1.3)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(ATTINY85-XTAL1{slash}PB3)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_1x02_P2.00mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.2mm_M2"
		(layer "F.Cu")
		(at 133.13 144.9)
		(descr "Mounting Hole 2.2mm, no annular, M2")
		(tags "mounting hole 2.2mm no annular m2")
		(property "Reference" "H1"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole"
			(at 0 3.2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "MountingHole:MountingHole_2.2mm_M2"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "attinyspeakersimple.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0.3 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.2 2.2)
			(drill 2.2)
			(layers "F&B.Cu" "*.Mask")
		)
	)
	(footprint "Connector_PinHeader_2.00mm:PinHeader_1x01_P2.00mm_Vertical"
		(layer "F.Cu")
		(at 118.225 144.1)
		(descr "Through hole straight pin header, 1x01, 2.00mm pitch, single row")
		(tags "Through hole pin header THT 1x01 2.00mm single row")
		(property "Reference" "J2"
			(at 0 -2.06 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x01"
			(at 0 2.06 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.00mm:PinHeader_1x01_P2.00mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "attiny85musicboxmini.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.15 1.15)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.00mm.3dshapes/PinHeader_1x01_P2.00mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 130.875 134.975)
		(descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
		(tags "Through hole pin header THT 2x03 2.54mm double row")
		(property "Reference" "J5"
			(at 1.075 -2.175 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_02x03_Odd_Even"
			(at 1.27 7.41 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, double row, 02x03, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "attiny85musicboxmini.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 2.54 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.67 1.67)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(ATTINY85-PB1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.54 0)
			(size 1.68 1.68)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VCC")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54)
			(size 1.68 1.68)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "Net-(ATTINY85-PB2)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 2.54 2.54)
			(size 1.68 1.68)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Net-(ATTINY85-AREF{slash}PB0)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 5.08)
			(size 1.68 1.68)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/rst")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 2.54 5.08)
			(size 1.68 1.68)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDREF")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x03_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.2mm_M2"
		(layer "F.Cu")
		(at 133.13 130.22)
		(descr "Mounting Hole 2.2mm, no annular, M2")
		(tags "mounting hole 2.2mm no annular m2")
		(property "Reference" "H2"
			(at 0 -3.2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole"
			(at 0 3.2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "MountingHole:MountingHole_2.2mm_M2"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "attinyspeakersimple.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0.3 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 2.2 2.2)
			(drill 2.2)
			(layers "F&B.Cu" "*.Mask")
		)
	)
	(footprint "attinyspeaker:spdt_w_hole"
		(layer "F.Cu")
		(at 122.05 129.3)
		(descr "CuK miniature slide switch, OS series, SPDT, https://www.ckswitches.com/media/1428/os.pdf")
		(tags "switch SPDT")
		(property "Reference" "SW1"
			(at 0.25 -3.15 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SW_SPDT"
			(at 2 3 0)
			(layer "F.Fab")
		)
		(property "Footprint" "attinyspeaker:spdt_w_hole"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Switch, single pole double throw"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "attiny85musicboxmini.kicad_sch")
		(attr through_hole)
		(fp_text user "NO"
			(at -3.65 -0.7 0)
			(unlocked yes)
			(layer "Dwgs.User")
		)
		(fp_text user "NC"
			(at 1.4 -0.7 0)
			(unlocked yes)
			(layer "Dwgs.User")
		)
		(fp_text user "C"
			(at -0.65 -0.7 0)
			(unlocked yes)
			(layer "Dwgs.User")
		)
		(fp_text user "${REFERENCE}"
			(at 4.75 -4.75 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 2.5 0)
			(size 1.5 1.4)
			(drill oval 0.9 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "Net-(BT1--)")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 0)
			(size 1.5 1.4)
			(drill oval 0.9 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDREF")
			(pinfunction "B")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at -2.5 0)
			(size 1.5 1.4)
			(drill oval 0.9 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/rst")
			(pinfunction "C")
			(pintype "passive")
		)
		(model "${KICAD7_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_Slide_SPDT_Straight_CK_OS102011MS2Q.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "attinyspeaker:makerlogo"
		(layer "B.Cu")
		(at 115.7 134.875 180)
		(property "Reference" "REF**"
			(at 0.15 0 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "makerlogo"
			(at 0 -1 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Footprint" "attinyspeaker:makerlogo"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 0)
			(unlocked yes)
			(layer "B.Fab")
		)
	)
	(gr_line
		(start 111.2 132.3)
		(end 111.2 140.888)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 109.475 127.888)
		(end 109.475 132.3)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 134.9588 147.3)
		(end 134.9588 127.888)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 111.2 140.888)
		(end 109.475 140.888)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 109.475 140.888)
		(end 109.475 147.3)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 134.9588 127.888)
		(end 109.475 127.888)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 109.475 147.3)
		(end 134.9588 147.3)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 109.475 132.3)
		(end 111.2 132.3)
		(layer "Edge.Cuts")
	)
	(gr_text "PB3"
		(at 115.675 146.75 0)
		(layer "B.SilkS")
	)
	(gr_text "GND"
		(at 120.275 144.65 90)
		(layer "B.SilkS")
	)
	(gr_text "-"
		(at 111.775 131.975 0)
		(layer "B.SilkS")
	)
	(gr_text "SPKR"
		(at 128.525 144.425 0)
		(layer "B.SilkS")
	)
	(gr_text "(3V)"
		(at 114.25 135.825 90)
		(layer "B.SilkS")
	)
	(gr_text "ICSP"
		(at 129.7 135.875 90)
		(layer "B.SilkS")
	)
	(gr_text "VCC"
		(at 117.225 144.675 0)
		(layer "B.SilkS")
	)
	(gr_text "attiny85\naudio\nclass"
		(at 123.025 136.925 90)
		(layer "B.SilkS")
	)
	(gr_text "+"
		(at 111.725 142.8 0)
		(layer "B.SilkS")
	)
	(gr_text "2xAG13"
		(at 112.75 134.325 90)
		(layer "B.SilkS")
	)
	(gr_text "GND"
		(at 133.65 142 0)
		(layer "F.SilkS")
	)
	(gr_text "RST"
		(at 128.95 140.1 90)
		(layer "F.SilkS")
	)
	(gr_text "battery"
		(at 112.1 134.7 270)
		(layer "F.SilkS")
	)
	(gr_text "C"
		(at 121.95 146.5 0)
		(layer "F.SilkS")
	)
	(gr_text "-"
		(at 129.55 145.075 180)
		(layer "F.SilkS")
	)
	(gr_text "0.1uF"
		(at 131.75 132.525 90)
		(layer "F.SilkS")
	)
	(gr_text "MOSI"
		(at 134.625 137.5 90)
		(layer "F.SilkS")
	)
	(gr_text "+"
		(at 125.75 144.875 0)
		(layer "F.SilkS")
	)
	(gr_text "SCK"
		(at 128.95 137.5 90)
		(layer "F.SilkS")
	)
	(gr_text "switch"
		(at 119.95 131.175 0)
		(layer "F.SilkS")
	)
	(gr_text "VCC"
		(at 133.55 133.1 0)
		(layer "F.SilkS")
	)
	(gr_text "+"
		(at 109.975 147 0)
		(layer "F.SilkS")
	)
	(gr_text "R 75"
		(at 121.35 144.175 0)
		(layer "F.SilkS")
	)
	(gr_text "-"
		(at 110.1 132 0)
		(layer "F.SilkS")
	)
	(gr_text "C"
		(at 130.175 131.1 90)
		(layer "F.SilkS")
	)
	(gr_text "MISO"
		(at 128.95 134.7 90)
		(layer "F.SilkS")
	)
	(zone
		(net 2)
		(net_name "VCC")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads
			(clearance 0.3)
		)
		(min_thickness 0.2)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.3)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 109.975 141.325) (xy 111.75 141.15) (xy 111.65 131.925) (xy 110 131.825) (xy 109.95 128.25)
				(xy 130.6 128.275) (xy 130.625 132.15) (xy 134.475 134.3) (xy 134.425 141.375) (xy 130.425 143.4)
				(xy 130.4 147.175) (xy 109.925 146.875)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GNDREF")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.3)
		)
		(min_thickness 0.2)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.3)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 110 141.425) (xy 111.825 141.275) (xy 111.675 131.975) (xy 109.925 131.775) (xy 109.95 128.25)
				(xy 134.425 128.275) (xy 134.475 146.95) (xy 109.925 146.875)
			)
		)
	)
)
