(kicad_pcb (version 20171130) (host pcbnew "(5.1.10)-1")
  (general
    (thickness 1.6)
    (drawings 50)
    (tracks 239)
    (zones 0)
    (modules 9)
    (nets 27)
  )
  (page A)
  (title_block
    (title "Beetje 32U4 Blok")
    (date 2018-08-10)
    (rev 0.0)
    (company www.MakersBox.us)
    (comment 1 648.ken@gmail.com)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.3048)
    (user_trace_width 0.3556)
    (user_trace_width 0.4064)
    (user_trace_width 0.6096)
    (trace_clearance 0.2)
    (zone_clearance 0.35)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 0.5 3.500001)
    (pad_drill 0)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers/"))
  )
  (net 0 "")
  (net 1 /10)
  (net 2 /01)
  (net 3 /02)
  (net 4 /04)
  (net 5 /05)
  (net 6 /06)
  (net 7 /07)
  (net 8 /08)
  (net 9 /09)
  (net 10 /11)
  (net 11 /12)
  (net 12 /13)
  (net 13 /14)
  (net 14 /15)
  (net 15 /16)
  (net 16 /17)
  (net 17 /18)
  (net 18 /19)
  (net 19 /20)
  (net 20 /03)
  (net 21 /D2_SDA)
  (net 22 GND)
  (net 23 /D3_SCL)
  (net 24 +5V)
  (net 25 "Net-(R1-Pad1)")
  (net 26 /A)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.254)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net /01)
    (add_net /02)
    (add_net /03)
    (add_net /04)
    (add_net /05)
    (add_net /06)
    (add_net /07)
    (add_net /08)
    (add_net /09)
    (add_net /10)
    (add_net /11)
    (add_net /12)
    (add_net /13)
    (add_net /14)
    (add_net /15)
    (add_net /16)
    (add_net /17)
    (add_net /18)
    (add_net /19)
    (add_net /20)
    (add_net /A)
    (add_net /D2_SDA)
    (add_net /D3_SCL)
    (add_net GND)
    (add_net "Net-(R1-Pad1)")
  )
  (module footprints:DFN-8-1EP_3x2mm (layer F.Cu) (tedit 638826C0)
    (at 47.9 -18.7 180)
    (descr "8-Lead Plastic Dual Flat, No Lead Package (8MA2) - 2x3x0.6 mm Body [UDFN] (see Atmel-8815-SEEPROM-AT24CS01-02-Datasheet.pdf)")
    (tags "DFN 0.5")
    (attr smd)
    (fp_text reference U1 (at 0 -2.55 180) (layer F.SilkS) hide)
    (fp_text value 24LC32 (at 0 2 180) (layer F.SilkS))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad "" smd rect (at 0.325 0.375 180) (size 0.5 0.6) (layers F.Paste))
    (pad "" smd rect (at 0.325 -0.375 180) (size 0.5 0.6) (layers F.Paste))
    (pad "" smd rect (at -0.325 0.375 180) (size 0.5 0.6) (layers F.Paste))
    (pad "" smd rect (at -0.325 -0.375 180) (size 0.5 0.6) (layers F.Paste))
    (pad 9 smd rect (at 0 0 180) (size 1.3 1.5) (layers F.Cu F.Mask))
    (pad 8 smd rect (at 1.45 -0.75 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 24 +5V))
    (pad 7 smd rect (at 1.45 -0.25 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 1.45 0.25 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 23 /D3_SCL))
    (pad 5 smd rect (at 1.45 0.75 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 21 /D2_SDA))
    (pad 4 smd rect (at -1.45 0.75 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 22 GND))
    (pad 3 smd rect (at -1.45 0.25 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 22 GND))
    (pad 2 smd rect (at -1.45 -0.25 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 22 GND))
    (pad 1 smd rect (at -1.45 -0.75 180) (size 0.75 0.3) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(R1-Pad1)"))
    (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/DFN-8-1EP_3x2mm_P0.5mm_EP1.3x1.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:MEC8-113-CARD_2 locked (layer F.Cu) (tedit 637EA67F)
    (at 0 -0.1 90)
    (fp_text reference X0 (at 4.375 -1.25 90) (layer F.Fab))
    (fp_text value "Card Edge" (at 10.9 -1 90) (layer F.Fab))
    (fp_line (start -1 47.5) (end -1 7.5) (layer Edge.Cuts) (width 0.12))
    (fp_line (start 21 7.5) (end 21 47.5) (layer Edge.Cuts) (width 0.12))
    (fp_line (start 11.5 51.5) (end 19 51.5) (layer Edge.Cuts) (width 0.12))
    (fp_line (start 8.5 51.5) (end 1 51.5) (layer Edge.Cuts) (width 0.12))
    (fp_line (start 1 6.5) (end 1.5 6.5) (layer Edge.Cuts) (width 0.12))
    (fp_line (start 18.5 6.5) (end 19 6.5) (layer Edge.Cuts) (width 0.12))
    (fp_line (start 17.5 0.5) (end 17.5 5.5) (layer Edge.Cuts) (width 0.12))
    (fp_line (start 2.5 0.5) (end 2.5 5.5) (layer Edge.Cuts) (width 0.12))
    (fp_line (start 8.4 0.5) (end 8.4 5.5) (layer Edge.Cuts) (width 0.12))
    (fp_line (start 10.8 5.5) (end 10.8 0.5) (layer Edge.Cuts) (width 0.12))
    (fp_line (start 9.4 6.5) (end 9.8 6.5) (layer Edge.Cuts) (width 0.12))
    (fp_line (start 3 0) (end 7.9 0) (layer Edge.Cuts) (width 0.12))
    (fp_line (start 17 0) (end 11.3 0) (layer Edge.Cuts) (width 0.12))
    (fp_line (start 0 6.5) (end 1 6.5) (layer Edge.Cuts) (width 0.12))
    (fp_line (start 19 6.5) (end 20 6.5) (layer Edge.Cuts) (width 0.12))
    (fp_line (start -1 50.5) (end -1 47.5) (layer Edge.Cuts) (width 0.12))
    (fp_line (start 0 51.5) (end 1 51.5) (layer Edge.Cuts) (width 0.12))
    (fp_line (start 19 51.5) (end 20 51.5) (layer Edge.Cuts) (width 0.12))
    (fp_line (start 21 50.5) (end 21 47.5) (layer Edge.Cuts) (width 0.12))
    (fp_arc (start 10 51.5) (end 11.5 51.5) (angle -180) (layer Edge.Cuts) (width 0.12))
    (fp_arc (start 20 50.5) (end 20 51.5) (angle -90) (layer Edge.Cuts) (width 0.12))
    (fp_arc (start 0 50.5) (end -1 50.5) (angle -90) (layer Edge.Cuts) (width 0.12))
    (fp_arc (start 0 7.5) (end 0 6.5) (angle -90) (layer Edge.Cuts) (width 0.12))
    (fp_arc (start 20 7.5) (end 21 7.5) (angle -90) (layer Edge.Cuts) (width 0.12))
    (fp_arc (start 18.5 5.5) (end 17.5 5.5) (angle -90) (layer Edge.Cuts) (width 0.12))
    (fp_arc (start 1.5 5.5) (end 1.5 6.5) (angle -90) (layer Edge.Cuts) (width 0.12))
    (fp_arc (start 9.4 5.5) (end 8.4 5.5) (angle -90) (layer Edge.Cuts) (width 0.12))
    (fp_arc (start 9.8 5.5) (end 9.8 6.5) (angle -90) (layer Edge.Cuts) (width 0.12))
    (fp_arc (start 7.9 0.5) (end 8.4 0.5) (angle -90) (layer Edge.Cuts) (width 0.12))
    (fp_arc (start 11.3 0.5) (end 11.3 0) (angle -90) (layer Edge.Cuts) (width 0.12))
    (fp_arc (start 17 0.5) (end 17.5 0.5) (angle -90) (layer Edge.Cuts) (width 0.12))
    (fp_arc (start 3 0.5) (end 3 0) (angle -90) (layer Edge.Cuts) (width 0.12))
    (pad 14 smd rect (at 3.6 2.25 90) (size 0.5 3.5) (layers F.Cu F.Paste F.Mask)
      (net 10 /11))
    (pad 1 smd rect (at 3.6 2.25 90) (size 0.5 3.5) (layers B.Cu B.Paste B.Mask)
      (net 2 /01))
    (pad 15 smd rect (at 4.4 2.25 90) (size 0.5 3.5) (layers F.Cu F.Paste F.Mask)
      (net 11 /12))
    (pad 2 smd rect (at 4.4 2.25 90) (size 0.5 3.5) (layers B.Cu B.Paste B.Mask)
      (net 3 /02))
    (pad 16 smd rect (at 5.2 2.25 90) (size 0.5 3.5) (layers F.Cu F.Paste F.Mask)
      (net 12 /13))
    (pad 3 smd rect (at 5.2 2.25 90) (size 0.5 3.5) (layers B.Cu B.Paste B.Mask)
      (net 20 /03))
    (pad 17 smd rect (at 6 2.25 90) (size 0.5 3.5) (layers F.Cu F.Paste F.Mask)
      (net 13 /14))
    (pad 4 smd rect (at 6 2.25 90) (size 0.5 3.5) (layers B.Cu B.Paste B.Mask)
      (net 4 /04))
    (pad 18 smd rect (at 6.8 2.25 90) (size 0.5 3.5) (layers F.Cu F.Paste F.Mask)
      (net 14 /15))
    (pad 5 smd rect (at 6.8 2.25 90) (size 0.5 3.5) (layers B.Cu B.Paste B.Mask)
      (net 5 /05))
    (pad 19 smd rect (at 7.6 2.25 90) (size 0.5 3.5) (layers F.Cu F.Paste F.Mask)
      (net 15 /16))
    (pad 6 smd rect (at 7.6 2.25 90) (size 0.5 3.5) (layers B.Cu B.Paste B.Mask)
      (net 6 /06))
    (pad 20 smd rect (at 11.6 2.25 90) (size 0.5 3.5) (layers F.Cu F.Paste F.Mask)
      (net 16 /17))
    (pad 7 smd rect (at 11.6 2.25 90) (size 0.5 3.5) (layers B.Cu B.Paste B.Mask)
      (net 7 /07))
    (pad 21 smd rect (at 12.4 2.25 90) (size 0.5 3.5) (layers F.Cu F.Paste F.Mask)
      (net 17 /18))
    (pad 8 smd rect (at 12.4 2.25 90) (size 0.5 3.5) (layers B.Cu B.Paste B.Mask)
      (net 8 /08))
    (pad 22 smd rect (at 13.2 2.25 90) (size 0.5 3.5) (layers F.Cu F.Paste F.Mask)
      (net 18 /19))
    (pad 9 smd rect (at 13.2 2.25 90) (size 0.5 3.5) (layers B.Cu B.Paste B.Mask)
      (net 9 /09))
    (pad 23 smd rect (at 14 2.25 90) (size 0.5 3.5) (layers F.Cu F.Paste F.Mask)
      (net 19 /20))
    (pad 10 smd rect (at 14 2.25 90) (size 0.5 3.5) (layers B.Cu B.Paste B.Mask)
      (net 1 /10))
    (pad 24 smd rect (at 14.8 2.25 90) (size 0.5 3.5) (layers F.Cu F.Paste F.Mask)
      (net 23 /D3_SCL))
    (pad 11 smd rect (at 14.8 2.25 90) (size 0.5 3.5) (layers B.Cu B.Paste B.Mask))
    (pad 25 smd rect (at 15.6 2.25 90) (size 0.5 3.5) (layers F.Cu F.Paste F.Mask)
      (net 21 /D2_SDA))
    (pad 12 smd rect (at 15.6 2.25 90) (size 0.5 3.5) (layers B.Cu B.Paste B.Mask)
      (net 26 /A))
    (pad 26 smd rect (at 16.4 2.25 90) (size 0.5 3.5) (layers F.Cu F.Paste F.Mask)
      (net 22 GND))
    (pad 13 smd rect (at 16.4 2.25 90) (size 0.5 3.5) (layers B.Cu B.Paste B.Mask)
      (net 24 +5V))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical (layer F.Cu) (tedit 63801DD5)
    (at 45.72 -11.43)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33) (layer F.Fab))
    (fp_text value Conn_01x04 (at 0 9.95) (layer F.Fab))
    (fp_text user %R (at 0 3.81 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 +5V))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /D3_SCL))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /D2_SDA))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:PinHeader_1x10_P2.54mm_Vertical (layer F.Cu) (tedit 637F0F76)
    (at 16.51 -3.81 90)
    (descr "Through hole straight pin header, 1x10, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x10 2.54mm single row")
    (fp_text reference J6 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x10 (at 0 25.19 90) (layer F.Fab))
    (fp_text user %R (at 0 11.43 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /01))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /02))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /03))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /04))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /05))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /06))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /07))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /08))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /09))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /10))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x10_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:PinHeader_1x10_P2.54mm_Vertical (layer F.Cu) (tedit 637F0F76)
    (at 16.51 -6.35 90)
    (descr "Through hole straight pin header, 1x10, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x10 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x10 (at 0 25.19 90) (layer F.Fab))
    (fp_text user %R (at 0 11.43 180) (layer F.Fab))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /10))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /09))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /08))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /07))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /06))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /05))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /04))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /03))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /02))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /01))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x10_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:PinHeader_1x10_P2.54mm_Vertical (layer F.Cu) (tedit 637F0F76)
    (at 16.51 -11.43 90)
    (descr "Through hole straight pin header, 1x10, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x10 2.54mm single row")
    (fp_text reference J3 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x10 (at 0 25.19 90) (layer F.Fab))
    (fp_text user %R (at 0 11.43 180) (layer F.Fab))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /20))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /19))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /18))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /17))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /16))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /15))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /14))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /13))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /12))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /11))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x10_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:PinHeader_1x10_P2.54mm_Vertical (layer F.Cu) (tedit 637F0F76)
    (at 16.51 -8.89 90)
    (descr "Through hole straight pin header, 1x10, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x10 2.54mm single row")
    (fp_text reference J4 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x10 (at 0 25.19 90) (layer F.Fab))
    (fp_text user %R (at 0 11.43 180) (layer F.Fab))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /10))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /09))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /08))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /07))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /06))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /05))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /04))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /03))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /02))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /01))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x10_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:PinHeader_1x10_P2.54mm_Vertical (layer F.Cu) (tedit 637F0F76)
    (at 16.51 -13.97 90)
    (descr "Through hole straight pin header, 1x10, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x10 2.54mm single row")
    (fp_text reference J5 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x10 (at 0 25.19 90) (layer F.Fab))
    (fp_text user %R (at 0 11.43 180) (layer F.Fab))
    (pad 10 thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /20))
    (pad 9 thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /19))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /18))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /17))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /16))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /15))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /14))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /13))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /12))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /11))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x10_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_0603 (layer F.Cu) (tedit 636E7A48)
    (at 48.018 -15.748 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 1.905 0 180) (layer Dwgs.User))
    (fp_text value 10K (at -2.274 0 180) (layer F.SilkS))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(R1-Pad1)"))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 26 /A))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "GND\n\nPWR\n\nSCL\n\nSDA" (at 43.18 -7.874) (layer B.SilkS))
  (gr_text "GND\n\nPWR\n\nSCL\n\nSDA" (at 43.18 -7.874) (layer F.SilkS))
  (dimension 38 (width 0.15) (layer Dwgs.User)
    (gr_text "38.000 mm" (at 27 4.3) (layer Dwgs.User))
    (feature1 (pts (xy 46 1) (xy 46 3.586421)))
    (feature2 (pts (xy 8 1) (xy 8 3.586421)))
    (crossbar (pts (xy 8 3) (xy 46 3)))
    (arrow1a (pts (xy 46 3) (xy 44.873496 3.586421)))
    (arrow1b (pts (xy 46 3) (xy 44.873496 2.413579)))
    (arrow2a (pts (xy 8 3) (xy 9.126504 3.586421)))
    (arrow2b (pts (xy 8 3) (xy 9.126504 2.413579)))
  )
  (gr_text "20 19 18 17 16 15 14 13 12 11" (at 27.94 -15.875) (layer B.SilkS))
  (gr_text "10 09 08 07 06 05 04 03 02 01" (at 27.94 -1.905) (layer B.SilkS))
  (gr_text "01 02 03 04 05 06 07 08 09 10" (at 27.94 -1.905) (layer F.SilkS))
  (gr_text "11 12 13 14 15 16 17 18 19 20" (at 27.94 -16.002) (layer F.SilkS))
  (dimension 22.500222 (width 0.15) (layer Dwgs.User)
    (gr_text "22.500 mm" (at 17.713112 8.249848 359.7453538) (layer Dwgs.User))
    (feature1 (pts (xy 29 0) (xy 28.966283 7.586276)))
    (feature2 (pts (xy 6.5 -0.1) (xy 6.466283 7.486276)))
    (crossbar (pts (xy 6.46889 6.899861) (xy 28.96889 6.999861)))
    (arrow1a (pts (xy 28.96889 6.999861) (xy 27.839791 7.581269)))
    (arrow1b (pts (xy 28.96889 6.999861) (xy 27.845004 6.408439)))
    (arrow2a (pts (xy 6.46889 6.899861) (xy 7.592776 7.491283)))
    (arrow2b (pts (xy 6.46889 6.899861) (xy 7.597989 6.318453)))
  )
  (dimension 22 (width 0.15) (layer F.SilkS)
    (gr_text "22.000 mm" (at 54.3 -10.1 90) (layer F.SilkS))
    (feature1 (pts (xy 50.5 -21.1) (xy 53.586421 -21.1)))
    (feature2 (pts (xy 50.5 0.9) (xy 53.586421 0.9)))
    (crossbar (pts (xy 53 0.9) (xy 53 -21.1)))
    (arrow1a (pts (xy 53 -21.1) (xy 53.586421 -19.973496)))
    (arrow1b (pts (xy 53 -21.1) (xy 52.413579 -19.973496)))
    (arrow2a (pts (xy 53 0.9) (xy 53.586421 -0.226504)))
    (arrow2b (pts (xy 53 0.9) (xy 52.413579 -0.226504)))
  )
  (dimension 45 (width 0.15) (layer F.SilkS)
    (gr_text "45.000 mm" (at 29 4.3) (layer F.SilkS))
    (feature1 (pts (xy 51.5 -0.1) (xy 51.5 3.586421)))
    (feature2 (pts (xy 6.5 -0.1) (xy 6.5 3.586421)))
    (crossbar (pts (xy 6.5 3) (xy 51.5 3)))
    (arrow1a (pts (xy 51.5 3) (xy 50.373496 3.586421)))
    (arrow1b (pts (xy 51.5 3) (xy 50.373496 2.413579)))
    (arrow2a (pts (xy 6.5 3) (xy 7.626504 3.586421)))
    (arrow2b (pts (xy 6.5 3) (xy 7.626504 2.413579)))
  )
  (gr_text "Rev 0.0\nNov 2022" (at 50.165 -1.27) (layer B.SilkS))
  (gr_text github.com/aspro648/RPB (at 29 -17.78) (layer B.SilkS))
  (gr_text "2.54mm Pitch" (at 29 -18.415) (layer F.SilkS))
  (gr_text "Rapid Prototyping Card" (at 29 -19.685) (layer B.SilkS))
)
