(kicad_pcb (version 20171130) (host pcbnew 5.1.5-52549c5~86~ubuntu18.04.1)
  (general
    (thickness 1.6)
    (drawings 51)
    (tracks 258)
    (zones 0)
    (modules 28)
    (nets 47)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.1524)
    (zone_45_only no)
    (trace_min 0.1524)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.508)
    (via_min_drill 0.254)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.1016)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(A1-Pad1)")
  (net 2 "Net-(A1-Pad17)")
  (net 3 "Net-(A1-Pad2)")
  (net 4 "Net-(A1-Pad18)")
  (net 5 "Net-(A1-Pad3)")
  (net 6 "Net-(A1-Pad19)")
  (net 7 GND)
  (net 8 "Net-(A1-Pad20)")
  (net 9 "Net-(A1-Pad5)")
  (net 10 "Net-(A1-Pad21)")
  (net 11 "Net-(A1-Pad6)")
  (net 12 "Net-(A1-Pad22)")
  (net 13 "Net-(A1-Pad7)")
  (net 14 "Net-(A1-Pad23)")
  (net 15 "Net-(A1-Pad8)")
  (net 16 "Net-(A1-Pad24)")
  (net 17 "Net-(A1-Pad9)")
  (net 18 "Net-(A1-Pad25)")
  (net 19 "Net-(A1-Pad10)")
  (net 20 "Net-(A1-Pad26)")
  (net 21 "Net-(A1-Pad11)")
  (net 22 "Net-(A1-Pad27)")
  (net 23 "Net-(A1-Pad12)")
  (net 24 "Net-(A1-Pad28)")
  (net 25 "Net-(A1-Pad13)")
  (net 26 "Net-(A1-Pad14)")
  (net 27 +5V)
  (net 28 "Net-(A1-Pad15)")
  (net 29 "Net-(A1-Pad16)")
  (net 30 "Net-(C1-Pad1)")
  (net 31 "Net-(C2-Pad1)")
  (net 32 "Net-(C3-Pad1)")
  (net 33 GNDPWR)
  (net 34 +24V)
  (net 35 "Net-(J1-Pad3)")
  (net 36 "Net-(J1-Pad5)")
  (net 37 "Net-(J1-Pad7)")
  (net 38 "Net-(Q1-Pad1)")
  (net 39 "Net-(Q2-Pad1)")
  (net 40 "Net-(Q3-Pad1)")
  (net 41 "Net-(D1-Pad1)")
  (net 42 "Net-(D1-Pad2)")
  (net 43 "Net-(D2-Pad2)")
  (net 44 "Net-(D2-Pad1)")
  (net 45 "Net-(D3-Pad2)")
  (net 46 "Net-(D3-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (diff_pair_width 0.1524)
    (diff_pair_gap 0.25)
    (add_net +24V)
    (add_net +5V)
    (add_net GND)
    (add_net GNDPWR)
    (add_net "Net-(A1-Pad1)")
    (add_net "Net-(A1-Pad10)")
    (add_net "Net-(A1-Pad11)")
    (add_net "Net-(A1-Pad12)")
    (add_net "Net-(A1-Pad13)")
    (add_net "Net-(A1-Pad14)")
    (add_net "Net-(A1-Pad15)")
    (add_net "Net-(A1-Pad16)")
    (add_net "Net-(A1-Pad17)")
    (add_net "Net-(A1-Pad18)")
    (add_net "Net-(A1-Pad19)")
    (add_net "Net-(A1-Pad2)")
    (add_net "Net-(A1-Pad20)")
    (add_net "Net-(A1-Pad21)")
    (add_net "Net-(A1-Pad22)")
    (add_net "Net-(A1-Pad23)")
    (add_net "Net-(A1-Pad24)")
    (add_net "Net-(A1-Pad25)")
    (add_net "Net-(A1-Pad26)")
    (add_net "Net-(A1-Pad27)")
    (add_net "Net-(A1-Pad28)")
    (add_net "Net-(A1-Pad3)")
    (add_net "Net-(A1-Pad5)")
    (add_net "Net-(A1-Pad6)")
    (add_net "Net-(A1-Pad7)")
    (add_net "Net-(A1-Pad8)")
    (add_net "Net-(A1-Pad9)")
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(Q2-Pad1)")
    (add_net "Net-(Q3-Pad1)")
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 106.68 81.28)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H4 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 106.68 134.62)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H3 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 160.02 134.62)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H2 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 160.02 81.28)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (attr virtual)
    (fp_text reference H1 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole (at 0 4.2) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Module:Arduino_Nano (layer F.Cu) (tedit 58ACAF70)
    (at 113.03 99.06)
    (descr "Arduino Nano, http://www.mouser.com/pdfdocs/Gravitech_Arduino_Nano3_0.pdf")
    (tags "Arduino Nano")
    (fp_text reference A1 (at 19.05 39.37) (layer F.SilkS))
    (fp_text value Arduino_Nano_v3.x (at 7.2898 15.4178 90) (layer F.Fab))
    (fp_text user %R (at 6.35 19.05 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(A1-Pad1)"))
    (pad 17 thru_hole oval (at 15.24 33.02) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(A1-Pad17)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(A1-Pad2)"))
    (pad 18 thru_hole oval (at 15.24 30.48) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(A1-Pad18)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(A1-Pad3)"))
    (pad 19 thru_hole oval (at 15.24 27.94) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(A1-Pad19)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 20 thru_hole oval (at 15.24 25.4) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(A1-Pad20)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(A1-Pad5)"))
    (pad 21 thru_hole oval (at 15.24 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(A1-Pad21)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 "Net-(A1-Pad6)"))
    (pad 22 thru_hole oval (at 15.24 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 12 "Net-(A1-Pad22)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 "Net-(A1-Pad7)"))
    (pad 23 thru_hole oval (at 15.24 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(A1-Pad23)"))
    (pad 8 thru_hole oval (at 0 17.78) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(A1-Pad8)"))
    (pad 24 thru_hole oval (at 15.24 15.24) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(A1-Pad24)"))
    (pad 9 thru_hole oval (at 0 20.32) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 17 "Net-(A1-Pad9)"))
    (pad 25 thru_hole oval (at 15.24 12.7) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(A1-Pad25)"))
    (pad 10 thru_hole oval (at 0 22.86) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 19 "Net-(A1-Pad10)"))
    (pad 26 thru_hole oval (at 15.24 10.16) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(A1-Pad26)"))
    (pad 11 thru_hole oval (at 0 25.4) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 21 "Net-(A1-Pad11)"))
    (pad 27 thru_hole oval (at 15.24 7.62) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 22 "Net-(A1-Pad27)"))
    (pad 12 thru_hole oval (at 0 27.94) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 23 "Net-(A1-Pad12)"))
    (pad 28 thru_hole oval (at 15.24 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(A1-Pad28)"))
    (pad 13 thru_hole oval (at 0 30.48) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(A1-Pad13)"))
    (pad 29 thru_hole oval (at 15.24 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 GND))
    (pad 14 thru_hole oval (at 0 33.02) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 26 "Net-(A1-Pad14)"))
    (pad 30 thru_hole oval (at 15.24 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 +5V))
    (pad 15 thru_hole oval (at 0 35.56) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 "Net-(A1-Pad15)"))
    (pad 16 thru_hole oval (at 15.24 35.56) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 29 "Net-(A1-Pad16)"))
    (model ${KISYS3DMOD}/Module.3dshapes/Arduino_Nano_WithMountingHoles.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 125.73 91.44 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C1 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 10nf (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at -0.605001 0.014999 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 30 "Net-(C1-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 7 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 125.73 86.36 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C2 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 10nf (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 7 GND))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 31 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 125.73 81.28 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C3 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 10nf (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 32 "Net-(C3-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 7 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:Term_Block_1x8_P5.08mm (layer F.Cu) (tedit 5D419A27)
    (at 158.6484 88.9 270)
    (descr http://www.on-shore.com/wp-content/uploads/2015/09/osttcxx2162.pdf)
    (fp_text reference J1 (at 18.05 -5.05 90) (layer F.SilkS))
    (fp_text value Screw_Terminal_01x08 (at 18.65 5.2 90) (layer F.Fab))
    (fp_text user %R (at 17.75 0.15 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 33 GNDPWR))
    (pad 2 thru_hole circle (at 5.08 0 270) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 34 +24V))
    (pad 3 thru_hole circle (at 10.16 0 270) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 35 "Net-(J1-Pad3)"))
    (pad 4 thru_hole circle (at 15.24 0 270) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 34 +24V))
    (pad 5 thru_hole circle (at 20.32 0 270) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 36 "Net-(J1-Pad5)"))
    (pad 6 thru_hole circle (at 25.4 0 270) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 34 +24V))
    (pad 7 thru_hole circle (at 30.48 0 270) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 37 "Net-(J1-Pad7)"))
    (pad 8 thru_hole circle (at 35.56 0 270) (size 2.5 2.5) (drill 1.3) (layers *.Cu *.Mask)
      (net 34 +24V))
  )
  (module Package_TO_SOT_THT:TO-220-3_Vertical locked (layer F.Cu) (tedit 5AC8BA0D)
    (at 147.921 101.9408 90)
    (descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference Q1 (at 0.3916 2.4978 90) (layer F.SilkS))
    (fp_text value IRF540N (at 2.54 2.5 90) (layer F.Fab))
    (fp_text user %R (at 2.54 -4.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 38 "Net-(Q1-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 35 "Net-(J1-Pad3)"))
    (pad 3 thru_hole oval (at 5.08 0 90) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 33 GNDPWR))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-220-3_Vertical locked (layer F.Cu) (tedit 5AC8BA0D)
    (at 147.921 115.824 90)
    (descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference Q2 (at 0.1524 2.6248 90) (layer F.SilkS))
    (fp_text value IRF540N (at 2.54 2.5 90) (layer F.Fab))
    (fp_text user %R (at 2.54 -4.27 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 39 "Net-(Q2-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 36 "Net-(J1-Pad5)"))
    (pad 3 thru_hole oval (at 5.08 0 90) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 33 GNDPWR))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_THT:TO-220-3_Vertical (layer F.Cu) (tedit 5AC8BA0D)
    (at 147.921 129.9408 90)
    (descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference Q3 (at 0.0452 2.9296 90) (layer F.SilkS))
    (fp_text value IRF540N (at 2.54 2.5 90) (layer F.Fab))
    (fp_text user %R (at 2.54 -4.27 90) (layer F.Fab))
    (pad 3 thru_hole oval (at 5.08 0 90) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 33 GNDPWR))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 37 "Net-(J1-Pad7)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.905 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 40 "Net-(Q3-Pad1)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 120.65 92.465 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 470 (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 30 "Net-(C1-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 23 "Net-(A1-Pad12)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 151.638 81.67254 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at -0.19166 1.778 90) (layer F.SilkS))
    (fp_text value 100 (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 41 "Net-(D1-Pad1)"))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 38 "Net-(Q1-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 147.819 106.172)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at 4.2508 -0.0254) (layer F.SilkS))
    (fp_text value 1K (at 0 -1.52) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 33 GNDPWR))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 42 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 137.7913 106.1847)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R4 (at 0.3847 1.9431) (layer F.SilkS))
    (fp_text value 10K (at -3.065 -1.49) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 38 "Net-(Q1-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 33 GNDPWR))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 120.65 87.385 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R5 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 470 (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 31 "Net-(C2-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 25 "Net-(A1-Pad13)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 147.32 83.557 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R6 (at -0.0598 1.8034 90) (layer F.SilkS))
    (fp_text value 100 (at -0.525 1.67 90) (layer F.Fab))
    (fp_text user %R (at 1.025 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 44 "Net-(D2-Pad1)"))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 39 "Net-(Q2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 147.819 120.142)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R7 (at 4.327 0.0762) (layer F.SilkS))
    (fp_text value 1K (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 43 "Net-(D2-Pad2)"))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 33 GNDPWR))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 138.421 120.142)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R8 (at 0.263 1.905) (layer F.SilkS))
    (fp_text value 10K (at -3.495 -1.09) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 39 "Net-(Q2-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 33 GNDPWR))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 120.65 82.305 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R9 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 470 (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 26 "Net-(A1-Pad14)"))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 32 "Net-(C3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 143.11122 86.75508 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R10 (at -0.08752 1.74498 90) (layer F.SilkS))
    (fp_text value 100 (at -0.525 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 40 "Net-(Q3-Pad1)"))
    (pad 2 smd roundrect (at 1.025 0 90) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 46 "Net-(D3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 148.082 134.112)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R11 (at 0.254 1.9304) (layer F.SilkS))
    (fp_text value 1K (at 0 -1.52) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 33 GNDPWR))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 45 "Net-(D3-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric_Pad1.15x1.40mm_HandSolder (layer F.Cu) (tedit 5B36C52B)
    (at 138.05408 134.26694)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R12 (at 0.29972 2.08026) (layer F.SilkS))
    (fp_text value 10K (at 0 1.65) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 33 GNDPWR))
    (pad 1 smd roundrect (at -1.025 0) (size 1.15 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.217391)
      (net 40 "Net-(Q3-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-16_4.55x10.3mm_P1.27mm (layer F.Cu) (tedit 5D9F72B1)
    (at 135.89 83.82)
    (descr "SOIC, 16 Pin (https://toshiba.semicon-storage.com/info/docget.jsp?did=12858&prodName=TLP291-4), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference U1 (at 0 -6.1) (layer F.SilkS))
    (fp_text value TLP291-4 (at 0 6.1) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -3.25 -4.445) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 "Net-(C1-Pad1)"))
    (pad 2 smd roundrect (at -3.25 -3.175) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 GND))
    (pad 3 smd roundrect (at -3.25 -1.905) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 "Net-(C2-Pad1)"))
    (pad 4 smd roundrect (at -3.25 -0.635) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 GND))
    (pad 5 smd roundrect (at -3.25 0.635) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 "Net-(C3-Pad1)"))
    (pad 6 smd roundrect (at -3.25 1.905) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 GND))
    (pad 7 smd roundrect (at -3.25 3.175) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 8 smd roundrect (at -3.25 4.445) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 9 smd roundrect (at 3.25 4.445) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 10 smd roundrect (at 3.25 3.175) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 11 smd roundrect (at 3.25 1.905) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 46 "Net-(D3-Pad1)"))
    (pad 12 smd roundrect (at 3.25 0.635) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 +24V))
    (pad 13 smd roundrect (at 3.25 -0.635) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 44 "Net-(D2-Pad1)"))
    (pad 14 smd roundrect (at 3.25 -1.905) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 +24V))
    (pad 15 smd roundrect (at 3.25 -3.175) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 41 "Net-(D1-Pad1)"))
    (pad 16 smd roundrect (at 3.25 -4.445) (size 1.6 0.55) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 +24V))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-16_4.55x10.3mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module digikey-footprints:0805 (layer F.Cu) (tedit 5D288D36)
    (at 143.036 106.172)
    (attr smd)
    (fp_text reference D1 (at -0.0086 1.6256) (layer F.SilkS))
    (fp_text value LH_R974-LP-1 (at 0 1.95) (layer F.Fab))
    (pad 1 smd rect (at -1.05 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 1.05 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(D1-Pad2)"))
  )
  (module digikey-footprints:0805 (layer F.Cu) (tedit 5D288D36)
    (at 142.968 120.142)
    (attr smd)
    (fp_text reference D2 (at -0.0422 1.8034) (layer F.SilkS))
    (fp_text value LH_R974-LP-1 (at 0 1.95) (layer F.Fab))
    (pad 2 smd rect (at 1.05 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(D2-Pad2)"))
    (pad 1 smd rect (at -1.05 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 44 "Net-(D2-Pad1)"))
  )
  (module digikey-footprints:0805 (layer F.Cu) (tedit 5D288D36)
    (at 143.036 134.112)
    (attr smd)
    (fp_text reference D3 (at 0.2454 1.7526) (layer F.SilkS))
    (fp_text value LH_R974-LP-1 (at 0 1.95) (layer F.Fab))
    (pad 2 smd rect (at 1.05 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(D3-Pad2)"))
    (pad 1 smd rect (at -1.05 0) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(D3-Pad1)"))
  )
  (gr_text D13 (at 129.667 134.6454) (layer F.SilkS))
  (gr_text 3V3 (at 129.667 132.0038) (layer F.SilkS))
  (gr_text AREF (at 129.667 129.6162) (layer F.SilkS))
  (gr_text A0 (at 129.6924 127.0254) (layer F.SilkS))
  (gr_text A1 (at 129.6924 124.5616) (layer F.SilkS))
  (gr_text A2 (at 129.7178 121.92) (layer F.SilkS))
  (gr_text A3 (at 129.6924 119.38) (layer F.SilkS))
  (gr_text A4 (at 129.7178 116.8654) (layer F.SilkS))
  (gr_text A5 (at 129.6416 114.2746) (layer F.SilkS))
  (gr_text A6 (at 129.6416 111.7854) (layer F.SilkS))
  (gr_text A7 (at 129.5908 109.2708) (layer F.SilkS))
  (gr_text 5V (at 129.6416 106.7562) (layer F.SilkS))
  (gr_text RESET (at 129.6416 104.3178) (layer F.SilkS))
  (gr_text GND (at 129.5908 101.8032) (layer F.SilkS))
  (gr_text "VIN\n" (at 129.5908 99.1108) (layer F.SilkS))
  (gr_text TX1 (at 108.4834 99.1108) (layer F.SilkS))
  (gr_text D02 (at 108.4072 109.1946) (layer F.SilkS))
  (gr_text GND (at 108.4072 106.7562) (layer F.SilkS))
  (gr_text RST (at 108.458 104.1146) (layer F.SilkS))
  (gr_text RX0 (at 108.5088 101.6254) (layer F.SilkS))
  (gr_text D03 (at 108.5088 111.76) (layer F.SilkS))
  (gr_text D04 (at 108.5088 114.3) (layer F.SilkS))
  (gr_text D05 (at 108.458 116.8654) (layer F.SilkS))
  (gr_text D07 (at 108.4834 121.9708) (layer F.SilkS))
  (gr_text D06 (at 108.4834 119.4308) (layer F.SilkS))
  (gr_text D08 (at 108.5596 124.587) (layer F.SilkS))
  (gr_text D09 (at 108.5342 126.9746) (layer F.SilkS))
  (gr_text D10 (at 108.5088 129.6162) (layer F.SilkS))
  (gr_text D11 (at 108.5342 132.08) (layer F.SilkS))
  (gr_text D12 (at 108.458 134.6962) (layer F.SilkS))
  (gr_text - (at 163.8808 88.0618 90) (layer F.SilkS))
  (gr_text + (at 163.0172 94.488) (layer F.SilkS))
  (gr_text POWER (at 163.9824 93.7514 90) (layer F.SilkS))
  (gr_text CH.3 (at 163.957 103.251 90) (layer F.SilkS))
  (gr_text CH.2 (at 163.8554 113.6396 90) (layer F.SilkS))
  (gr_text CH.1 (at 163.957 123.4694 90) (layer F.SilkS))
  (gr_text - (at 163.83 99.2378 90) (layer F.SilkS))
  (gr_text - (at 163.7284 110.0328 90) (layer F.SilkS))
  (gr_text + (at 163.2966 103.9114) (layer F.SilkS))
  (gr_text + (at 163.1696 114.3) (layer F.SilkS))
  (gr_text - (at 163.8554 119.9388 90) (layer F.SilkS))
  (gr_text + (at 163.8554 125.1458 90) (layer F.SilkS))
  (gr_text "Driver Board v02\nCopyright © 327jwolf  2020.04" (at 105.156 129.794 90) (layer F.SilkS))
  (gr_arc (start 160.02 134.62) (end 160.02 139.7) (angle -90) (layer Edge.Cuts) (width 0.635))
  (gr_arc (start 106.68 134.62) (end 101.6 134.62) (angle -90) (layer Edge.Cuts) (width 0.635))
  (gr_arc (start 160.02 81.28) (end 160.02 76.2) (angle 90) (layer Edge.Cuts) (width 0.635))
  (gr_arc (start 106.68 81.28) (end 106.68 76.2) (angle -90) (layer Edge.Cuts) (width 0.635))
  (gr_line (start 106.68 76.2) (end 160.02 76.2) (layer Edge.Cuts) (width 0.635))
  (gr_line (start 101.6 134.62) (end 101.6 81.28) (layer Edge.Cuts) (width 0.635))
  (gr_line (start 160.02 139.7) (end 106.68 139.7) (layer Edge.Cuts) (width 0.635))
  (gr_line (start 165.1 81.28) (end 165.1 134.62) (layer Edge.Cuts) (width 0.635))
  (zone (net 7) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 135.89 92.71) (xy 130.81 97.79) (xy 130.81 142.24) (xy 99.06 142.24) (xy 99.06 74.93)
        (xy 135.89 74.93)
      )
    )
  )
  (zone (net 7) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 135.89 92.71) (xy 130.81 97.79) (xy 130.81 142.24) (xy 100.33 142.24) (xy 100.33 73.66)
        (xy 135.89 73.66)
      )
    )
  )
  (zone (net 33) (net_name GNDPWR) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 166.37 142.24) (xy 132.08 142.24) (xy 132.08 99.06) (xy 137.16 93.98) (xy 137.16 74.93)
        (xy 166.37 74.93)
      )
    )
  )
  (zone (net 33) (net_name GNDPWR) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 165.1 142.24) (xy 132.08 142.24) (xy 132.08 99.06) (xy 137.16 93.98) (xy 137.16 73.66)
        (xy 165.1 73.66)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 162.56 137.16) (xy 157.48 137.16) (xy 157.48 132.08) (xy 162.56 132.08)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 162.56 137.16) (xy 157.48 137.16) (xy 157.48 132.08) (xy 162.56 132.08)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 108.712 136.652) (xy 104.648 136.652) (xy 104.648 132.588) (xy 108.712 132.588)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 108.712 83.312) (xy 104.648 83.312) (xy 104.648 79.248) (xy 108.712 79.248)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 162.052 83.312) (xy 157.988 83.312) (xy 157.988 79.248) (xy 162.052 79.248)
      )
    )
  )
)
