(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "+12V")
  (net 2 "GND")
  (net 3 "-12V")
  (net 4 "Net-(D1-COM)")
  (net 5 "Net-(D2-COM)")
  (net 6 "/FACE")
  (net 7 "Net-(J1-Pin_1)")
  (net 8 "Net-(J1-Pin_10)")
  (net 9 "Net-(C6-Pad2)")
  (net 10 "Net-(U1A--)")
  (net 11 "Net-(U2-COMPEN)")
  (net 12 "Net-(U1B--)")
  (net 13 "Net-(C8-Pad2)")
  (net 14 "Net-(Q1-E)")
  (net 15 "Net-(C7-Pad2)")
  (net 16 "Net-(C10-Pad1)")
  (net 17 "Net-(C8-Pad1)")
  (net 18 "Net-(D3-K)")
  (net 19 "/NOISE'")
  (net 20 "/SOL'")
  (net 21 "Net-(U8-OUT)")
  (net 22 "Net-(U10G-VCC)")
  (net 23 "/CLK'")
  (net 24 "Net-(Q2A-E1)")
  (net 25 "Net-(D4-K)")
  (net 26 "/B0'")
  (net 27 "Net-(D5-K)")
  (net 28 "/B1'")
  (net 29 "Net-(D6-K)")
  (net 30 "/B2'")
  (net 31 "Net-(D7-K)")
  (net 32 "/B3'")
  (net 33 "Net-(D8-K)")
  (net 34 "/B4'")
  (net 35 "Net-(D9-K)")
  (net 36 "/B5'")
  (net 37 "Net-(D10-K)")
  (net 38 "/B6'")
  (net 39 "Net-(D11-K)")
  (net 40 "/B7'")
  (net 41 "Net-(D12-K)")
  (net 42 "/_CLK_LED")
  (net 43 "Net-(D13-K)")
  (net 44 "/_PULSE")
  (net 45 "Net-(J2-PadT)")
  (net 46 "unconnected-(J2-PadTN)")
  (net 47 "Net-(J3-PadT)")
  (net 48 "unconnected-(J3-PadTN)")
  (net 49 "Net-(J4-PadT)")
  (net 50 "unconnected-(J4-PadTN)")
  (net 51 "Net-(J5-PadT)")
  (net 52 "unconnected-(J5-PadTN)")
  (net 53 "/G1")
  (net 54 "/G2")
  (net 55 "/G3")
  (net 56 "/G4")
  (net 57 "/G5")
  (net 58 "/G6")
  (net 59 "/G7")
  (net 60 "/G8")
  (net 61 "/_CLK2'")
  (net 62 "/P1")
  (net 63 "/P2")
  (net 64 "/P3")
  (net 65 "/P4")
  (net 66 "/P5")
  (net 67 "/P6")
  (net 68 "/P7")
  (net 69 "/P8")
  (net 70 "/_CLK'")
  (net 71 "unconnected-(Q1-C-Pad1)")
  (net 72 "Net-(R3-Pad1)")
  (net 73 "Net-(R4-Pad1)")
  (net 74 "/LOOP_CTRL'")
  (net 75 "Net-(R5-Pad2)")
  (net 76 "Net-(U3-K)")
  (net 77 "Net-(U2-VREF+)")
  (net 78 "Net-(U2-VREF-)")
  (net 79 "Net-(R24-Pad2)")
  (net 80 "Net-(R25-Pad2)")
  (net 81 "Net-(R26-Pad2)")
  (net 82 "Net-(R27-Pad1)")
  (net 83 "Net-(U5B--)")
  (net 84 "Net-(R29-Pad1)")
  (net 85 "/RAND'")
  (net 86 "/s12'")
  (net 87 "/s9'")
  (net 88 "/s11'")
  (net 89 "/s13'")
  (net 90 "/s16'")
  (net 91 "/EOL'")
  (net 92 "unconnected-(U7A-Q2-Pad4)")
  (net 93 "unconnected-(U7B-Q3-Pad11)")
  (net 94 "unconnected-(U7B-Q2-Pad12)")
  (net 95 "unconnected-(J8-PadTN)")
  (net 96 "Net-(U14B--)")
  (net 97 "Net-(U14A--)")
  (net 98 "Net-(Q2B-B2)")
  (net 99 "Net-(Q2A-C1)")
  (net 100 "Net-(D14-A)")
  (net 101 "Net-(Q2B-C2)")
  (footprint "Eurorack:AudioJack2_Tayda_A-2566" (layer "F.Cu")
    (at 82.804 93.005)
    (property "PartNum" "A-2566")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "Tayda")
    (property "ki_description" "Audio Jack, 2 Poles (Mono / TS), Switched T Pole (Normalling)")
    (property "ki_keywords" "audio jack receptacle mono headphones phone TS connector")
    (attr through_hole)
    (fp_text reference "J5" (at 5.8928 -5.0292 unlocked) (layer "F.SilkS"))
    (fp_text value "noise" (at 0 1 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab"))
    (pad "S" thru_hole oval (at -4.7 0.6) (size 2.25 3.75) (drill oval 1.45 2.95) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "S" thru_hole oval (at 4.7 0.6) (size 2.25 2.7) (drill oval 1.45 1.9) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "T" thru_hole oval (at 0 -4.8) (size 3.5 1.5) (drill oval 2.7 0.7) (layers "*.Cu" "*.Mask")
      (net 51 "Net-(J5-PadT)") (pintype "passive"))
    (pad "TN" thru_hole oval (at 0 3.3) (size 3.5 1.5) (drill oval 2.7 0.7) (layers "*.Cu" "*.Mask")
      (net 52 "unconnected-(J5-PadTN)") (pintype "passive+no_connect"))
    (model "./models3d/A-2566.wrl"
      (offset (xyz 0 -0.15 11.5))
      (scale (xyz 0.385 0.385 0.385))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Eurorack:Mech-Potentiometer-Hole_level_180deg" (layer "F.Cu")
    (at 76.2 136.055)
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole exclude_from_bom)
    (fp_text reference "H6" (at 0 -9.906 unlocked) (layer "F.Fab"))
    (fp_text value "change" (at -0.0254 14.745 unlocked) (layer "F.SilkS"))
    (fp_text user "0" (at -5.08 6.35 unlocked) (layer "F.SilkS"))
    (fp_text user "10" (at 6.35 6.35 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 7.62 unlocked) (layer "F.Fab"))
    (pad "" thru_hole oval (at 7.8 0) (size 1.5 3.3) (drill oval 1.3 3.1) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 0 0) (size 12 12) (drill 7.5) (layers "*.Cu" "*.Mask")
      (net 6 "/FACE") (pinfunction "1") (pintype "input"))
  )
  (footprint "Eurorack:Mech-AudioJack-Hole-Input-CV" (layer "F.Cu")
    (at 57.404 214.795)
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole exclude_from_bom)
    (fp_text reference "H5" (at 0.4 0.1 unlocked) (layer "F.Fab"))
    (fp_text value "cv" (at -0.0508 6.2866 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 7.7 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 8 8) (drill 6.4) (layers "*.Cu" "*.Mask")
      (net 6 "/FACE") (pinfunction "1") (pintype "input"))
    (model "./models3d/A-2566.wrl"
      (offset (xyz 0 0 -1.5))
      (scale (xyz 0.385 0.385 0.385))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 88.5444 47.5136 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R26" (at 0 1.524 90) (layer "F.SilkS"))
    (fp_text value "10K" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 1 "+12V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 81 "Net-(R26-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 61.3013 8.931 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R2" (at -2.7067 -2.286) (layer "F.SilkS"))
    (fp_text value "10" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 4 "Net-(D1-COM)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 7 "Net-(J1-Pin_1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 79.9515 44.2418 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C22" (at 3.1515 -0.2582) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "Net-(U10G-VCC)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D3.0mm" (layer "F.Cu")
    (at 84.455 -5.039)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr through_hole)
    (fp_text reference "D6" (at -1.143 -1.8796) (layer "F.SilkS"))
    (fp_text value "LED_GREEN" (at 1.27 2.96) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 29 "Net-(D6-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 30 "/B2'") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 53.538 66.5204 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R23" (at 0 -1.65 90) (layer "F.SilkS"))
    (fp_text value "2.2K" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 41 "Net-(D12-K)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Eurorack:Mech-LED-Hole-3mm" (layer "F.Cu")
    (at 54.3 193.6444)
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole exclude_from_bom)
    (fp_text reference "H19" (at 0 -2.3 unlocked) (layer "F.SilkS") hide)
    (fp_text value "clk_led" (at 0 1 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 3.3 3.3) (drill 3) (layers "*.Cu" "*.Mask")
      (net 6 "/FACE") (pinfunction "1") (pintype "input"))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 69.3 54.8 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R34" (at 0 1.7) (layer "F.SilkS"))
    (fp_text value "10K" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 23 "/CLK'") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Eurorack:Mech-LED-Hole-3mm" (layer "F.Cu")
    (at 64.91 195.39)
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole exclude_from_bom)
    (fp_text reference "H24" (at 0 -2.3 unlocked) (layer "F.SilkS") hide)
    (fp_text value "trim" (at 0 1 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 3.3 3.3) (drill 3) (layers "*.Cu" "*.Mask")
      (net 6 "/FACE") (pinfunction "1") (pintype "input"))
  )
  (footprint "Eurorack:Mech-1M_Switch-Hole" (layer "F.Cu")
    (at 94.5896 160.652)
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole exclude_from_bom)
    (fp_text reference "H21" (at 0 -4.445 unlocked) (layer "F.Fab"))
    (fp_text value "write" (at -0.0508 6.5024 unlocked) (layer "F.SilkS"))
    (pad "1" thru_hole circle (at 0 0) (size 9 9) (drill 6.25) (layers "*.Cu" "*.Mask")
      (net 6 "/FACE") (pinfunction "1") (pintype "input"))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 68.326 13.97 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R14" (at 0 1.524 90) (layer "F.SilkS"))
    (fp_text value "3.3K" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 1 "+12V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 76 "Net-(U3-K)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D3.0mm" (layer "F.Cu")
    (at 53.025 71.8544)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr through_hole)
    (fp_text reference "D12" (at 1.27 -2.96) (layer "F.SilkS"))
    (fp_text value "LED_GREEN" (at 1.27 2.96) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 41 "Net-(D12-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 42 "/_CLK_LED") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 88.5444 58.9436 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R6" (at 0 1.524 90) (layer "F.SilkS"))
    (fp_text value "51K" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 74 "/LOOP_CTRL'") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 45 "Net-(J2-PadT)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 76.2 1.311 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R5" (at 0 -1.65 90) (layer "F.SilkS"))
    (fp_text value "100K" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 74 "/LOOP_CTRL'") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 75 "Net-(R5-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 58.674 70.358 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R7" (at 0.254 -1.778 -90) (layer "F.SilkS"))
    (fp_text value "100K" (at 0 1.65 -270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 18 "Net-(D3-K)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 47 "Net-(J3-PadT)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D3.0mm" (layer "F.Cu")
    (at 65.405 -5.039)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr through_hole)
    (fp_text reference "D9" (at -1.143 -1.8796) (layer "F.SilkS"))
    (fp_text value "LED_GREEN" (at 1.27 2.96) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 35 "Net-(D9-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 36 "/B5'") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Eurorack:Mech-AudioJack-Hole-Output-CV" (layer "F.Cu")
    (at 94.996 214.795)
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole exclude_from_bom)
    (fp_text reference "H9" (at 0.4 0.1 unlocked) (layer "F.Fab"))
    (fp_text value "out" (at 0.0254 6.2866 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 7.7 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 8 8) (drill 6.4) (layers "*.Cu" "*.Mask")
      (net 6 "/FACE") (pinfunction "1") (pintype "input"))
    (model "./models3d/A-2566.wrl"
      (offset (xyz 0 0 -1.5))
      (scale (xyz 0.385 0.385 0.385))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 73.6092 24.8522 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C23" (at 0 1.8923 90) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+12V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D3.0mm" (layer "F.Cu")
    (at 90.8 -5.039)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr through_hole)
    (fp_text reference "D5" (at -1.143 -1.8796) (layer "F.SilkS"))
    (fp_text value "LED_GREEN" (at 1.27 2.96) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 27 "Net-(D5-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 28 "/B1'") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:TSOP-6_1.65x3.05mm_P0.95mm" (layer "F.Cu")
    (at 81.7 66.1875)
    (descr "TSOP-6 package (comparable to TSOT-23), https://www.vishay.com/docs/71200/71200.pdf")
    (tags "Jedec MO-193C TSOP-6L")
    (property "PartNum" "771-BCM847DS135")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "Mouser")
    (property "ki_description" "Dual NPN transistor, 6 pin package")
    (property "ki_keywords" "transistor NPN")
    (attr smd)
    (fp_text reference "Q2" (at -1.2 -2.9875 90) (layer "F.SilkS"))
    (fp_text value "BCM847" (at 0 2.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.16 -0.95) (size 0.7 0.51) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "Net-(Q2A-E1)") (pinfunction "E1") (pintype "passive"))
    (pad "2" smd rect (at -1.16 0) (size 0.7 0.51) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "Net-(D3-K)") (pinfunction "B1") (pintype "input"))
    (pad "3" smd rect (at -1.16 0.95) (size 0.7 0.51) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 101 "Net-(Q2B-C2)") (pinfunction "C2") (pintype "passive"))
    (pad "4" smd rect (at 1.16 0.95) (size 0.7 0.51) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "Net-(Q2A-E1)") (pinfunction "E2") (pintype "passive"))
    (pad "5" smd rect (at 1.16 0) (size 0.7 0.51) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 98 "Net-(Q2B-B2)") (pinfunction "B2") (pintype "input"))
    (pad "6" smd rect (at 1.16 -0.95) (size 0.7 0.51) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 99 "Net-(Q2A-C1)") (pinfunction "C1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/TSOP-6_1.65x3.05mm_P0.95mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:TSSOP-16_4.4x5mm_P0.65mm" (layer "F.Cu")
    (at 78.5545 40.3556 180)
    (descr "TSSOP, 16 Pin (JEDEC MO-153 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "TSSOP SO")
    (property "PartNum" "595-CD4050BPWR")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "Mouser")
    (property "ki_description" "Hex Buffer")
    (property "ki_keywords" "CMOS BUFFER")
    (attr smd)
    (fp_text reference "U10" (at -5.7955 -2.3544) (layer "F.SilkS"))
    (fp_text value "4050" (at 0 3.45) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.8625 -2.275 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "Net-(U10G-VCC)") (pinfunction "VCC") (pintype "power_in"))
    (pad "2" smd roundrect (at -2.8625 -1.625 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 42 "/_CLK_LED") (pintype "output"))
    (pad "3" smd roundrect (at -2.8625 -0.975 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "/CLK'") (pintype "input"))
    (pad "4" smd roundrect (at -2.8625 -0.325 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "/_CLK2'") (pintype "output"))
    (pad "5" smd roundrect (at -2.8625 0.325 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "/CLK'") (pintype "input"))
    (pad "6" smd roundrect (at -2.8625 0.975 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 60 "/G8") (pintype "output"))
    (pad "7" smd roundrect (at -2.8625 1.625 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "/B0'") (pintype "input"))
    (pad "8" smd roundrect (at -2.8625 2.275 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "9" smd roundrect (at 2.8625 2.275 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "/B1'") (pintype "input"))
    (pad "10" smd roundrect (at 2.8625 1.625 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 59 "/G7") (pintype "output"))
    (pad "11" smd roundrect (at 2.8625 0.975 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "/CLK'") (pintype "input"))
    (pad "12" smd roundrect (at 2.8625 0.325 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 70 "/_CLK'") (pintype "output"))
    (pad "13" smd roundrect (at 2.8625 -0.325 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "14" smd roundrect (at 2.8625 -0.975 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 62 "/P1") (pintype "input"))
    (pad "15" smd roundrect (at 2.8625 -1.625 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 44 "/_PULSE") (pintype "output"))
    (pad "16" smd roundrect (at 2.8625 -2.275 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (model "${KICAD7_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-16_4.4x5mm_P0.65mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 99.2124 53.8636 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R29" (at -0.0364 1.4876 90) (layer "F.SilkS"))
    (fp_text value "100K" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 84 "Net-(R29-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 85 "/RAND'") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 99.1616 37.719 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R24" (at 0.019 1.5384 90) (layer "F.SilkS"))
    (fp_text value "1K" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 20 "/SOL'") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 79 "Net-(R24-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (at 62.23 14.519 90)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PartNum" "863-BAT54SLT1G")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "Mouser")
    (property "ki_description" "Vr 30V, If 200mA, Dual schottky barrier diode, in series, SOT-323")
    (property "ki_keywords" "schottky diode")
    (attr smd)
    (fp_text reference "D2" (at 0 -2.4 90) (layer "F.SilkS"))
    (fp_text value "BAT54S" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 -0.95 90) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "-12V") (pinfunction "A") (pintype "passive"))
    (pad "2" smd roundrect (at -0.9375 0.95 90) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+12V") (pinfunction "K") (pintype "passive"))
    (pad "3" smd roundrect (at 0.9375 0 90) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(D2-COM)") (pinfunction "COM") (pintype "passive"))
    (model "${KICAD7_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D3.0mm" (layer "F.Cu")
    (at 52.7 -5.039)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr through_hole)
    (fp_text reference "D11" (at -0.1728 -2.7432) (layer "F.SilkS"))
    (fp_text value "LED_GREEN" (at 1.27 2.96) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 39 "Net-(D11-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 40 "/B7'") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Eurorack:Mech-MountingHole" (layer "F.Cu")
    (at 55.95 104.6)
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole exclude_from_bom)
    (fp_text reference "H1" (at 0 -2.54 unlocked) (layer "F.Fab"))
    (fp_text value "mount0" (at 0 2.54 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole oval (at 0 0 90) (size 3.5 7.8) (drill oval 3.2 7.5) (layers "*.Cu" "*.Mask")
      (net 6 "/FACE") (pinfunction "1") (pintype "output"))
  )
  (footprint "LED_THT:LED_D3.0mm" (layer "F.Cu")
    (at 97.15 -5.039)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr through_hole)
    (fp_text reference "D4" (at -1.143 -1.8796) (layer "F.SilkS"))
    (fp_text value "LED_GREEN" (at 1.27 2.96) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 25 "Net-(D4-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 26 "/B0'") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:TSSOP-16_4.4x5mm_P0.65mm" (layer "F.Cu")
    (at 71.12 59.223)
    (descr "TSSOP, 16 Pin (JEDEC MO-153 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "TSSOP SO")
    (property "PartNum" "595-CD4015BPWR")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "Mouser")
    (attr smd)
    (fp_text reference "U7" (at -5.32 -2.223) (layer "F.SilkS"))
    (fp_text value "4015" (at 0 3.45) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.8625 -2.275) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "/CLK'") (pinfunction "CP") (pintype "input"))
    (pad "2" smd roundrect (at -2.8625 -1.625) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 90 "/s16'") (pinfunction "Q4") (pintype "output"))
    (pad "3" smd roundrect (at -2.8625 -0.975) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 88 "/s11'") (pinfunction "Q3") (pintype "output"))
    (pad "4" smd roundrect (at -2.8625 -0.325) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 92 "unconnected-(U7A-Q2-Pad4)") (pinfunction "Q2") (pintype "output+no_connect"))
    (pad "5" smd roundrect (at -2.8625 0.325) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 87 "/s9'") (pinfunction "Q1") (pintype "output"))
    (pad "6" smd roundrect (at -2.8625 0.975) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "MR") (pintype "input"))
    (pad "7" smd roundrect (at -2.8625 1.625) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "/B0'") (pinfunction "D") (pintype "input"))
    (pad "8" smd roundrect (at -2.8625 2.275) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "Vss") (pintype "power_in"))
    (pad "9" smd roundrect (at 2.8625 2.275) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "/CLK'") (pinfunction "CP") (pintype "input"))
    (pad "10" smd roundrect (at 2.8625 1.625) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 86 "/s12'") (pinfunction "Q4") (pintype "output"))
    (pad "11" smd roundrect (at 2.8625 0.975) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 93 "unconnected-(U7B-Q3-Pad11)") (pinfunction "Q3") (pintype "output+no_connect"))
    (pad "12" smd roundrect (at 2.8625 0.325) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 94 "unconnected-(U7B-Q2-Pad12)") (pinfunction "Q2") (pintype "output+no_connect"))
    (pad "13" smd roundrect (at 2.8625 -0.325) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 89 "/s13'") (pinfunction "Q1") (pintype "output"))
    (pad "14" smd roundrect (at 2.8625 -0.975) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "MR") (pintype "input"))
    (pad "15" smd roundrect (at 2.8625 -1.625) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 86 "/s12'") (pinfunction "D") (pintype "input"))
    (pad "16" smd roundrect (at 2.8625 -2.275) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+12V") (pinfunction "Vdd") (pintype "power_in"))
    (model "${KICAD7_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-16_4.4x5mm_P0.65mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 73.2 54.8)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C20" (at 0.1 -1.8) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+12V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 61.3013 11.217 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R1" (at -2.7067 2.286) (layer "F.SilkS"))
    (fp_text value "10" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 5 "Net-(D2-COM)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 8 "Net-(J1-Pin_10)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (at 62.23736 5.629 90)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PartNum" "863-BAT54SLT1G")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "Mouser")
    (property "ki_description" "Vr 30V, If 200mA, Dual schottky barrier diode, in series, SOT-323")
    (property "ki_keywords" "schottky diode")
    (attr smd)
    (fp_text reference "D1" (at 0 -2.4 90) (layer "F.SilkS"))
    (fp_text value "BAT54S" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 -0.95 90) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "-12V") (pinfunction "A") (pintype "passive"))
    (pad "2" smd roundrect (at -0.9375 0.95 90) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+12V") (pinfunction "K") (pintype "passive"))
    (pad "3" smd roundrect (at 0.9375 0 90) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(D1-COM)") (pinfunction "COM") (pintype "passive"))
    (model "${KICAD7_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 80 70.3 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R9" (at -0.9 -1.6 90) (layer "F.SilkS"))
    (fp_text value "470" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 24 "Net-(Q2A-E1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D3.0mm" (layer "F.Cu")
    (at 90.617 71.8544)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr through_hole)
    (fp_text reference "D13" (at 1.27 -2.96) (layer "F.SilkS"))
    (fp_text value "LED_GREEN" (at 1.27 2.96) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 43 "Net-(D13-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 44 "/_PULSE") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Eurorack:Mech-MountingHole" (layer "F.Cu")
    (at 96.45 227.1)
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole exclude_from_bom)
    (fp_text reference "H4" (at 0 -2.54 unlocked) (layer "F.Fab"))
    (fp_text value "mount1" (at 0 2.54 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole oval (at 0 0 90) (size 3.5 7.8) (drill oval 3.2 7.5) (layers "*.Cu" "*.Mask")
      (net 6 "/FACE") (pinfunction "1") (pintype "input"))
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 93.8784 59.7056 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C13" (at -0.0216 -1.5944) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+12V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "-12V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Eurorack:Mech-AudioJack-Hole-Input-Clock" (layer "F.Cu")
    (at 57.348 201.2644)
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole exclude_from_bom)
    (fp_text reference "H7" (at 0.4 0.1 unlocked) (layer "F.Fab"))
    (fp_text value "clock" (at 0 6.35 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 7.7 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 8 8) (drill 6.4) (layers "*.Cu" "*.Mask")
      (net 6 "/FACE") (pinfunction "1") (pintype "input"))
    (model "./models3d/A-2566.wrl"
      (offset (xyz 0 0 -1.5))
      (scale (xyz 0.385 0.385 0.385))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Eurorack:Mech-LED-Hole-3mm" (layer "F.Cu")
    (at 79.38 116.751 90)
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole exclude_from_bom)
    (fp_text reference "H13" (at 0 -2.3 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "b2" (at 0 1 90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 3.3 3.3) (drill 3) (layers "*.Cu" "*.Mask")
      (net 6 "/FACE") (pinfunction "1") (pintype "input"))
  )
  (footprint "Package_SO:TSSOP-16_4.4x5mm_P0.65mm" (layer "F.Cu")
    (at 59.8424 58.0038 180)
    (descr "TSSOP, 16 Pin (JEDEC MO-153 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "TSSOP SO")
    (property "PartNum" "595-CD4015BPWR")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "Mouser")
    (attr smd)
    (fp_text reference "U6" (at -5.3576 -2.3962) (layer "F.SilkS"))
    (fp_text value "4015" (at 0 3.45) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.8625 -2.275 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "/CLK'") (pinfunction "CP") (pintype "input"))
    (pad "2" smd roundrect (at -2.8625 -1.625 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "/B0'") (pinfunction "Q4") (pintype "output"))
    (pad "3" smd roundrect (at -2.8625 -0.975 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "/B5'") (pinfunction "Q3") (pintype "output"))
    (pad "4" smd roundrect (at -2.8625 -0.325 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "/B6'") (pinfunction "Q2") (pintype "output"))
    (pad "5" smd roundrect (at -2.8625 0.325 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "/B7'") (pinfunction "Q1") (pintype "output"))
    (pad "6" smd roundrect (at -2.8625 0.975 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "MR") (pintype "input"))
    (pad "7" smd roundrect (at -2.8625 1.625 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "/SOL'") (pinfunction "D") (pintype "input"))
    (pad "8" smd roundrect (at -2.8625 2.275 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "Vss") (pintype "power_in"))
    (pad "9" smd roundrect (at 2.8625 2.275 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "/CLK'") (pinfunction "CP") (pintype "input"))
    (pad "10" smd roundrect (at 2.8625 1.625 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "/B4'") (pinfunction "Q4") (pintype "output"))
    (pad "11" smd roundrect (at 2.8625 0.975 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "/B1'") (pinfunction "Q3") (pintype "output"))
    (pad "12" smd roundrect (at 2.8625 0.325 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "/B2'") (pinfunction "Q2") (pintype "output"))
    (pad "13" smd roundrect (at 2.8625 -0.325 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "/B3'") (pinfunction "Q1") (pintype "output"))
    (pad "14" smd roundrect (at 2.8625 -0.975 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "MR") (pintype "input"))
    (pad "15" smd roundrect (at 2.8625 -1.625 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "/B4'") (pinfunction "D") (pintype "input"))
    (pad "16" smd roundrect (at 2.8625 -2.275 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+12V") (pinfunction "Vdd") (pintype "power_in"))
    (model "${KICAD7_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-16_4.4x5mm_P0.65mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Eurorack:AudioJack2_Tayda_A-2566" (layer "F.Cu")
    (at 57.348 79.4744)
    (property "PartNum" "A-2566")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "Tayda")
    (property "ki_description" "Audio Jack, 2 Poles (Mono / TS), Switched T Pole (Normalling)")
    (property "ki_keywords" "audio jack receptacle mono headphones phone TS connector")
    (attr through_hole)
    (fp_text reference "J3" (at 2.596 -5.842 unlocked) (layer "F.SilkS"))
    (fp_text value "clock" (at 0 1 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab"))
    (pad "S" thru_hole oval (at -4.7 0.6) (size 2.25 3.75) (drill oval 1.45 2.95) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "S" thru_hole oval (at 4.7 0.6) (size 2.25 2.7) (drill oval 1.45 1.9) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "T" thru_hole oval (at 0 -4.8) (size 3.5 1.5) (drill oval 2.7 0.7) (layers "*.Cu" "*.Mask")
      (net 47 "Net-(J3-PadT)") (pintype "passive"))
    (pad "TN" thru_hole oval (at 0 3.3) (size 3.5 1.5) (drill oval 2.7 0.7) (layers "*.Cu" "*.Mask")
      (net 48 "unconnected-(J3-PadTN)") (pintype "passive+no_connect"))
    (model "./models3d/A-2566.wrl"
      (offset (xyz 0 -0.15 11.5))
      (scale (xyz 0.385 0.385 0.385))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-89-3" (layer "F.Cu")
    (at 77.978 34.077 180)
    (descr "SOT-89-3, http://ww1.microchip.com/downloads/en/DeviceDoc/3L_SOT-89_MB_C04-029C.pdf")
    (tags "SOT-89-3")
    (property "PartNum" "511-L78L09ACU")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "Mouser")
    (property "ki_description" "Positive 100mA 30V Linear Regulator, Fixed Output 9V, SOT-89")
    (property "ki_keywords" "Voltage Regulator 100mA Positive")
    (attr smd)
    (fp_text reference "U8" (at -3.222 -2.723) (layer "F.SilkS"))
    (fp_text value "L78L09_SOT89" (at 0 3.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.2 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.95 -1.5 180) (size 1.3 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(U8-OUT)") (pinfunction "OUT") (pintype "power_out"))
    (pad "2" smd custom (at -1.8625 0 180) (size 1.475 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (zone_connect 2) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly
          (pts
            (xy 3.8625 0.8665)
            (xy 0.7375 0.8665)
            (xy 0.7375 -0.8665)
            (xy 3.8625 -0.8665)
          )
          (width 0) (fill yes))
      ))
    (pad "3" smd roundrect (at -1.95 1.5 180) (size 1.3 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+12V") (pinfunction "IN") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-89-3.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Eurorack:Potentiometer_RV16AF-41-15R1" (layer "F.Cu")
    (at 76.2 14.265 180)
    (descr "Alpha 16mm Potentiometer Single -- Tayda Electronics ")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Potentiometer")
    (property "ki_keywords" "resistor variable")
    (attr through_hole)
    (fp_text reference "RV1" (at -9.398 16.043 unlocked) (layer "F.SilkS"))
    (fp_text value "B50K" (at 0 4.826 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 6.604 180 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -5 16 180) (size 2.2 2.2) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 73 "Net-(R4-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 16 180) (size 2.2 2.2) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 75 "Net-(R5-Pad2)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 5 16 180) (size 2.2 2.2) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 72 "Net-(R3-Pad1)") (pinfunction "3") (pintype "passive"))
  )
  (footprint "Package_TO_SOT_SMD:SOT-89-3" (layer "F.Cu")
    (at 79.9007 48.555 -90)
    (descr "SOT-89-3, http://ww1.microchip.com/downloads/en/DeviceDoc/3L_SOT-89_MB_C04-029C.pdf")
    (tags "SOT-89-3")
    (property "PartNum" "511-L78L09ACU")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "Mouser")
    (property "ki_description" "Positive 100mA 30V Linear Regulator, Fixed Output 9V, SOT-89")
    (property "ki_keywords" "Voltage Regulator 100mA Positive")
    (attr smd)
    (fp_text reference "U11" (at -1.755 -4.0993 -180) (layer "F.SilkS"))
    (fp_text value "L78L09_SOT89" (at 0 3.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.2 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.95 -1.5 270) (size 1.3 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "Net-(U10G-VCC)") (pinfunction "OUT") (pintype "power_out"))
    (pad "2" smd custom (at -1.8625 0 270) (size 1.475 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (zone_connect 2) (thermal_bridge_angle 45)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly
          (pts
            (xy 3.8625 0.8665)
            (xy 0.7375 0.8665)
            (xy 0.7375 -0.8665)
            (xy 3.8625 -0.8665)
          )
          (width 0) (fill yes))
      ))
    (pad "3" smd roundrect (at -1.95 1.5 270) (size 1.3 0.9) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+12V") (pinfunction "IN") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-89-3.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (layer "F.Cu")
    (at 66.929 82.972 90)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "PartNum" "595-TL072CDR")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "Mouser")
    (property "ki_description" "Dual Low-Noise JFET-Input Operational Amplifiers, DIP-8/SOIC-8")
    (property "ki_keywords" "dual opamp")
    (attr smd)
    (fp_text reference "U14" (at -2.228 -3.529 90) (layer "F.SilkS"))
    (fp_text value "TL072" (at 0 3.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.475 -1.905 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 17 "Net-(C8-Pad1)") (pintype "output"))
    (pad "2" smd roundrect (at -2.475 -0.635 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 97 "Net-(U14A--)") (pinfunction "-") (pintype "input"))
    (pad "3" smd roundrect (at -2.475 0.635 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at -2.475 1.905 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "-12V") (pinfunction "V-") (pintype "power_in"))
    (pad "5" smd roundrect (at 2.475 1.905 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "+") (pintype "input"))
    (pad "6" smd roundrect (at 2.475 0.635 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 96 "Net-(U14B--)") (pinfunction "-") (pintype "input"))
    (pad "7" smd roundrect (at 2.475 -0.635 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "Net-(C10-Pad1)") (pintype "output"))
    (pad "8" smd roundrect (at 2.475 -1.905 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+12V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD7_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Eurorack:AudioJack2_Tayda_A-2566" (layer "F.Cu")
    (at 94.996 93.005)
    (property "PartNum" "A-2566")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "Tayda")
    (property "ki_description" "Audio Jack, 2 Poles (Mono / TS), Switched T Pole (Normalling)")
    (property "ki_keywords" "audio jack receptacle mono headphones phone TS connector")
    (attr through_hole)
    (fp_text reference "J4" (at 4.064 -5.842 unlocked) (layer "F.SilkS"))
    (fp_text value "out" (at 0 1 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab"))
    (pad "S" thru_hole oval (at -4.7 0.6) (size 2.25 3.75) (drill oval 1.45 2.95) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "S" thru_hole oval (at 4.7 0.6) (size 2.25 2.7) (drill oval 1.45 1.9) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "T" thru_hole oval (at 0 -4.8) (size 3.5 1.5) (drill oval 2.7 0.7) (layers "*.Cu" "*.Mask")
      (net 49 "Net-(J4-PadT)") (pintype "passive"))
    (pad "TN" thru_hole oval (at 0 3.3) (size 3.5 1.5) (drill oval 2.7 0.7) (layers "*.Cu" "*.Mask")
      (net 50 "unconnected-(J4-PadTN)") (pintype "passive+no_connect"))
    (model "./models3d/A-2566.wrl"
      (offset (xyz 0 -0.15 11.5))
      (scale (xyz 0.385 0.385 0.385))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 75.946 13.97 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C5" (at -3.048 0.254 90) (layer "F.SilkS"))
    (fp_text value "10n" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "-12V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(U2-COMPEN)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 82.4484 33.5136 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C21" (at 2.4234 -0.2667) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(U8-OUT)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Eurorack:AudioJack2_Tayda_A-2566" (layer "F.Cu")
    (at 94.94 79.4744)
    (property "PartNum" "A-2566")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "Tayda")
    (property "ki_description" "Audio Jack, 2 Poles (Mono / TS), Switched T Pole (Normalling)")
    (property "ki_keywords" "audio jack receptacle mono headphones phone TS connector")
    (attr through_hole)
    (fp_text reference "J8" (at 4.064 -5.842 unlocked) (layer "F.SilkS"))
    (fp_text value "pulse" (at 0 1 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab"))
    (pad "S" thru_hole oval (at -4.7 0.6) (size 2.25 3.75) (drill oval 1.45 2.95) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "S" thru_hole oval (at 4.7 0.6) (size 2.25 2.7) (drill oval 1.45 1.9) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "T" thru_hole oval (at 0 -4.8) (size 3.5 1.5) (drill oval 2.7 0.7) (layers "*.Cu" "*.Mask")
      (net 44 "/_PULSE") (pintype "passive"))
    (pad "TN" thru_hole oval (at 0 3.3) (size 3.5 1.5) (drill oval 2.7 0.7) (layers "*.Cu" "*.Mask")
      (net 95 "unconnected-(J8-PadTN)") (pintype "passive+no_connect"))
    (model "./models3d/A-2566.wrl"
      (offset (xyz 0 -0.15 11.5))
      (scale (xyz 0.385 0.385 0.385))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 87.3 72.1 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R31" (at -0.1 1.6) (layer "F.SilkS"))
    (fp_text value "15K" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 10 "Net-(U1A--)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 73.406 13.97 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R16" (at -3.048 1.27 270) (layer "F.SilkS"))
    (fp_text value "1.6K" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 78 "Net-(U2-VREF-)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Eurorack:Mech-LED-Hole-3mm" (layer "F.Cu")
    (at 91.892 193.6444)
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole exclude_from_bom)
    (fp_text reference "H23" (at 0 -2.3 unlocked) (layer "F.SilkS") hide)
    (fp_text value "pulse_led" (at 0 1 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 3.3 3.3) (drill 3) (layers "*.Cu" "*.Mask")
      (net 6 "/FACE") (pinfunction "1") (pintype "input"))
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 71.501 35.7996)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C24" (at 0 1.8334) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+12V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 67.564 77.13 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R20" (at 2.27 2.026 270) (layer "F.SilkS"))
    (fp_text value "1K" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 96 "Net-(U14B--)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 13 "Net-(C8-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 70.866 13.97 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R15" (at -2.794 -1.27 90) (layer "F.SilkS"))
    (fp_text value "1.6K" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 76 "Net-(U3-K)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 77 "Net-(U2-VREF+)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 59.5884 61.9662 180)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C19" (at 3.2884 -0.0338) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.68) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 180) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+12V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Eurorack:Mech-LED-Hole-3mm" (layer "F.Cu")
    (at 60.325 116.751)
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole exclude_from_bom)
    (fp_text reference "H17" (at 0 -2.3 unlocked) (layer "F.SilkS") hide)
    (fp_text value "b6" (at 0 1 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 3.3 3.3) (drill 3) (layers "*.Cu" "*.Mask")
      (net 6 "/FACE") (pinfunction "1") (pintype "input"))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 88.5444 55.1336 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R28" (at 0 -1.524 90) (layer "F.SilkS"))
    (fp_text value "47K" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 74 "/LOOP_CTRL'") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 83 "Net-(U5B--)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (layer "F.Cu")
    (at 93.8784 55.6416)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "PartNum" "595-TL072CDR")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "Mouser")
    (property "ki_description" "Dual Low-Noise JFET-Input Operational Amplifiers, DIP-8/SOIC-8")
    (property "ki_keywords" "dual opamp")
    (attr smd)
    (fp_text reference "U5" (at -2.8784 -3.5416) (layer "F.SilkS"))
    (fp_text value "TL072" (at 0 3.4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 83 "Net-(U5B--)") (pintype "output"))
    (pad "2" smd roundrect (at -2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 74 "/LOOP_CTRL'") (pinfunction "-") (pintype "input"))
    (pad "3" smd roundrect (at -2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at -2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "-12V") (pinfunction "V-") (pintype "power_in"))
    (pad "5" smd roundrect (at 2.475 1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "/NOISE'") (pinfunction "+") (pintype "input"))
    (pad "6" smd roundrect (at 2.475 0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 83 "Net-(U5B--)") (pinfunction "-") (pintype "input"))
    (pad "7" smd roundrect (at 2.475 -0.635) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 84 "Net-(R29-Pad1)") (pintype "output"))
    (pad "8" smd roundrect (at 2.475 -1.905) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+12V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD7_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 99.1616 45.3488 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C11" (at -0.0254 1.524 90) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+12V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (layer "F.Cu")
    (at 80.4672 76.164 -90)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "PartNum" "595-TL072CDR")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "Mouser")
    (property "ki_description" "Dual Low-Noise JFET-Input Operational Amplifiers, DIP-8/SOIC-8")
    (property "ki_keywords" "dual opamp")
    (attr smd)
    (fp_text reference "U1" (at -2.664 -3.9328 -180) (layer "F.SilkS"))
    (fp_text value "TL072" (at 0 3.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.475 -1.905 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 100 "Net-(D14-A)") (pintype "output"))
    (pad "2" smd roundrect (at -2.475 -0.635 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(U1A--)") (pinfunction "-") (pintype "input"))
    (pad "3" smd roundrect (at -2.475 0.635 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 101 "Net-(Q2B-C2)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at -2.475 1.905 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "-12V") (pinfunction "V-") (pintype "power_in"))
    (pad "5" smd roundrect (at 2.475 1.905 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "+") (pintype "input"))
    (pad "6" smd roundrect (at 2.475 0.635 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(U1B--)") (pinfunction "-") (pintype "input"))
    (pad "7" smd roundrect (at 2.475 -0.635 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(C6-Pad2)") (pintype "output"))
    (pad "8" smd roundrect (at 2.475 -1.905 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+12V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD7_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Eurorack:Mech-MountingHole" (layer "F.Cu")
    (at 96.45 104.6)
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole exclude_from_bom)
    (fp_text reference "H2" (at 0 -2.54 unlocked) (layer "F.Fab"))
    (fp_text value "mount1" (at 0 2.54 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole oval (at 0 0 90) (size 3.5 7.8) (drill oval 3.2 7.5) (layers "*.Cu" "*.Mask")
      (net 6 "/FACE") (pinfunction "1") (pintype "input"))
  )
  (footprint "Eurorack:Mech-Potentiometer-Hole_level" (layer "F.Cu")
    (at 81.534 191.604)
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole exclude_from_bom)
    (fp_text reference "H8" (at 0 -9.906 unlocked) (layer "F.Fab"))
    (fp_text value "scale" (at 0 11.43 unlocked) (layer "F.SilkS"))
    (fp_text user "10" (at 6.35 6.35 unlocked) (layer "F.SilkS"))
    (fp_text user "0" (at -5.08 6.35 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 7.62 unlocked) (layer "F.Fab"))
    (pad "" thru_hole oval (at -7.8 0) (size 1.5 3.3) (drill oval 1.3 3.1) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 0 0) (size 12 12) (drill 7.5) (layers "*.Cu" "*.Mask")
      (net 6 "/FACE") (pinfunction "1") (pintype "input"))
  )
  (footprint "Package_SO:TSSOP-14_4.4x5mm_P0.65mm" (layer "F.Cu")
    (at 93.8784 48.5296)
    (descr "TSSOP, 14 Pin (JEDEC MO-153 Var AB-1 https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "TSSOP SO")
    (property "PartNum" "595-CD4016BPWR")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "Mouser")
    (property "ki_description" "Quad Analog Switches")
    (property "ki_keywords" "CMOS SWITCH")
    (attr smd)
    (fp_text reference "U4" (at -3.7784 -3.4296 180) (layer "F.SilkS"))
    (fp_text value "4016" (at 0 3.45) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.8625 -1.95) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "/EOL'") (pintype "passive"))
    (pad "2" smd roundrect (at -2.8625 -1.3) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 82 "Net-(R27-Pad1)") (pintype "passive"))
    (pad "3" smd roundrect (at -2.8625 -0.65) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 82 "Net-(R27-Pad1)") (pintype "passive"))
    (pad "4" smd roundrect (at -2.8625 0) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 81 "Net-(R26-Pad2)") (pintype "passive"))
    (pad "5" smd roundrect (at -2.8625 0.65) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 80 "Net-(R25-Pad2)") (pintype "input"))
    (pad "6" smd roundrect (at -2.8625 1.3) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "/EOL'") (pintype "input"))
    (pad "7" smd roundrect (at -2.8625 1.95) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "8" smd roundrect (at 2.8625 1.95) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 81 "Net-(R26-Pad2)") (pintype "passive"))
    (pad "9" smd roundrect (at 2.8625 1.3) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "10" smd roundrect (at 2.8625 0.65) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "11" smd roundrect (at 2.8625 0) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 80 "Net-(R25-Pad2)") (pintype "passive"))
    (pad "12" smd roundrect (at 2.8625 -0.65) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 85 "/RAND'") (pintype "input"))
    (pad "13" smd roundrect (at 2.8625 -1.3) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 85 "/RAND'") (pintype "input"))
    (pad "14" smd roundrect (at 2.8625 -1.95) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+12V") (pinfunction "VDD") (pintype "power_in"))
    (model "${KICAD7_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-14_4.4x5mm_P0.65mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Eurorack:Mech-LED-Hole-3mm" (layer "F.Cu")
    (at 85.73 116.751 90)
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole exclude_from_bom)
    (fp_text reference "H14" (at 0 -2.3 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "b3" (at 0 1 90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 3.3 3.3) (drill 3) (layers "*.Cu" "*.Mask")
      (net 6 "/FACE") (pinfunction "1") (pintype "input"))
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 70.993 84.115 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C25" (at 0.365 -1.967 -90) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+12V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "-12V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 66.802 -1.778 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R3" (at 0 -1.778) (layer "F.SilkS"))
    (fp_text value "10K" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 72 "Net-(R3-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 1 "+12V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 83 63.0125)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R8" (at 0 -2.1125) (layer "F.SilkS"))
    (fp_text value "8.2K" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 1 "+12V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 99 "Net-(Q2A-C1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (at 72.136 18.288)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PartNum" "595-TL431BCDBZTG4")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "Mouser")
    (property "ki_description" "Shunt Regulator, SOT-23")
    (property "ki_keywords" "diode device shunt regulator")
    (attr smd)
    (fp_text reference "U3" (at 1.778 1.524) (layer "F.SilkS"))
    (fp_text value "TL431DBZ" (at 0 2.4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 -0.95) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "Net-(U3-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at -0.9375 0.95) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "Net-(U3-K)") (pinfunction "REF") (pintype "passive"))
    (pad "3" smd roundrect (at 0.9375 0) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "A") (pintype "passive"))
    (model "${KICAD7_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:TSSOP-16_4.4x5mm_P0.65mm" (layer "F.Cu")
    (at 86.4616 34.839 90)
    (descr "TSSOP, 16 Pin (JEDEC MO-153 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "TSSOP SO")
    (property "PartNum" "595-CD4050BPWR")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "Mouser")
    (property "ki_description" "Hex Buffer")
    (property "ki_keywords" "CMOS BUFFER")
    (attr smd)
    (fp_text reference "U9" (at -5.061 -1.7616) (layer "F.SilkS"))
    (fp_text value "4050" (at 0 3.45 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.8625 -2.275 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(U8-OUT)") (pinfunction "VCC") (pintype "power_in"))
    (pad "2" smd roundrect (at -2.8625 -1.625 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 58 "/G6") (pintype "output"))
    (pad "3" smd roundrect (at -2.8625 -0.975 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "/B2'") (pintype "input"))
    (pad "4" smd roundrect (at -2.8625 -0.325 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 56 "/G4") (pintype "output"))
    (pad "5" smd roundrect (at -2.8625 0.325 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "/B4'") (pintype "input"))
    (pad "6" smd roundrect (at -2.8625 0.975 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 54 "/G2") (pintype "output"))
    (pad "7" smd roundrect (at -2.8625 1.625 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "/B6'") (pintype "input"))
    (pad "8" smd roundrect (at -2.8625 2.275 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "9" smd roundrect (at 2.8625 2.275 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "/B7'") (pintype "input"))
    (pad "10" smd roundrect (at 2.8625 1.625 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 53 "/G1") (pintype "output"))
    (pad "11" smd roundrect (at 2.8625 0.975 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "/B5'") (pintype "input"))
    (pad "12" smd roundrect (at 2.8625 0.325 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 55 "/G3") (pintype "output"))
    (pad "13" smd roundrect (at 2.8625 -0.325 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "14" smd roundrect (at 2.8625 -0.975 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "/B3'") (pintype "input"))
    (pad "15" smd roundrect (at 2.8625 -1.625 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 57 "/G5") (pintype "output"))
    (pad "16" smd roundrect (at 2.8625 -2.275 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (model "${KICAD7_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-16_4.4x5mm_P0.65mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D3.0mm" (layer "F.Cu")
    (at 59.05 -5.039)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr through_hole)
    (fp_text reference "D10" (at -0.122 -2.6924) (layer "F.SilkS"))
    (fp_text value "LED_GREEN" (at 1.27 2.96) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 37 "Net-(D10-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 38 "/B6'") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Eurorack:Potentiometer_RV16AF-41-15R1" (layer "F.Cu")
    (at 81.534 69.814)
    (descr "Alpha 16mm Potentiometer Single -- Tayda Electronics ")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Potentiometer")
    (property "ki_keywords" "resistor variable")
    (attr through_hole)
    (fp_text reference "RV2" (at -7.234 -6.514 unlocked) (layer "F.SilkS"))
    (fp_text value "B50K" (at 0 4.826 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 6.604 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -5 16) (size 2.2 2.2) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 16) (size 2.2 2.2) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 49 "Net-(J4-PadT)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 5 16) (size 2.2 2.2) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(C6-Pad2)") (pinfunction "3") (pintype "passive"))
  )
  (footprint "Eurorack:Mech-LED-Hole-3mm" (layer "F.Cu")
    (at 53.975 116.751)
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole exclude_from_bom)
    (fp_text reference "H18" (at 0 -2.3 unlocked) (layer "F.SilkS") hide)
    (fp_text value "b7" (at 0 1 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 3.3 3.3) (drill 3) (layers "*.Cu" "*.Mask")
      (net 6 "/FACE") (pinfunction "1") (pintype "input"))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 99.2124 49.5456 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R25" (at 0.041 1.4224 90) (layer "F.SilkS"))
    (fp_text value "10K" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 1 "+12V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 80 "Net-(R25-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 96.464 70.8384 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R33" (at 0 2.136 90) (layer "F.SilkS"))
    (fp_text value "2.2K" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 43 "Net-(D13-K)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Eurorack:AudioJack2_Tayda_A-2566" (layer "F.Cu")
    (at 57.404 93.005)
    (property "PartNum" "A-2566")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "Tayda")
    (property "ki_description" "Audio Jack, 2 Poles (Mono / TS), Switched T Pole (Normalling)")
    (property "ki_keywords" "audio jack receptacle mono headphones phone TS connector")
    (attr through_hole)
    (fp_text reference "J2" (at 4.064 -5.842 unlocked) (layer "F.SilkS"))
    (fp_text value "cv" (at 0 1 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 unlocked) (layer "F.Fab"))
    (pad "S" thru_hole oval (at -4.7 0.6) (size 2.25 3.75) (drill oval 1.45 2.95) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "S" thru_hole oval (at 4.7 0.6) (size 2.25 2.7) (drill oval 1.45 1.9) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "T" thru_hole oval (at 0 -4.8) (size 3.5 1.5) (drill oval 2.7 0.7) (layers "*.Cu" "*.Mask")
      (net 45 "Net-(J2-PadT)") (pintype "passive"))
    (pad "TN" thru_hole oval (at 0 3.3) (size 3.5 1.5) (drill oval 2.7 0.7) (layers "*.Cu" "*.Mask")
      (net 46 "unconnected-(J2-PadTN)") (pintype "passive+no_connect"))
    (model "./models3d/A-2566.wrl"
      (offset (xyz 0 -0.15 11.5))
      (scale (xyz 0.385 0.385 0.385))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Eurorack:Mech-LED-Hole-3mm" (layer "F.Cu")
    (at 98.425 116.751 90)
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole exclude_from_bom)
    (fp_text reference "H16" (at 0 -2.3 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "b5" (at 0 1 90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 3.3 3.3) (drill 3) (layers "*.Cu" "*.Mask")
      (net 6 "/FACE") (pinfunction "1") (pintype "input"))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 85.1 66.6 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R10" (at 0.3 -1.8 -270) (layer "F.SilkS"))
    (fp_text value "10K" (at 0 1.65 -270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 99 "Net-(Q2A-C1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 98 "Net-(Q2B-B2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 70.358 88.941 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R18" (at 0 -1.65 90) (layer "F.SilkS"))
    (fp_text value "10K" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 97 "Net-(U14A--)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 15 "Net-(C7-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm" (layer "F.Cu")
    (at 73.66 7.62 90)
    (descr "SOIC, 16 Pin (JEDEC MS-012AC, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "PartNum" "926-DAC0800LCMX/NOPB")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "Mouser")
    (property "ki_description" "8-bit multiplying DAC")
    (property "ki_keywords" "8 bit multiplying DAC")
    (attr smd)
    (fp_text reference "U2" (at -3.08 -6.06 90) (layer "F.SilkS"))
    (fp_text value "DAC0800_SOIC" (at 0 5.9 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.475 -4.445 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+12V") (pinfunction "VCC") (pintype "power_in"))
    (pad "2" smd roundrect (at -2.475 -3.175 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "Net-(U2-VREF+)") (pinfunction "VREF+") (pintype "output"))
    (pad "3" smd roundrect (at -2.475 -1.905 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 78 "Net-(U2-VREF-)") (pinfunction "VREF-") (pintype "output"))
    (pad "4" smd roundrect (at -2.475 -0.635 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(U2-COMPEN)") (pinfunction "COMPEN") (pintype "passive"))
    (pad "5" smd roundrect (at -2.475 0.635 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "VLC") (pintype "bidirectional"))
    (pad "6" smd roundrect (at -2.475 1.905 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "7" smd roundrect (at -2.475 3.175 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "-12V") (pinfunction "VEE") (pintype "power_in"))
    (pad "8" smd roundrect (at -2.475 4.445 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(U1B--)") (pinfunction "I0") (pintype "input"))
    (pad "9" smd roundrect (at 2.475 4.445 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "/B0'") (pinfunction "A1") (pintype "input"))
    (pad "10" smd roundrect (at 2.475 3.175 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "/B1'") (pinfunction "A2") (pintype "input"))
    (pad "11" smd roundrect (at 2.475 1.905 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "/B2'") (pinfunction "A3") (pintype "input"))
    (pad "12" smd roundrect (at 2.475 0.635 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "/B3'") (pinfunction "A4") (pintype "input"))
    (pad "13" smd roundrect (at 2.475 -0.635 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "/B4'") (pinfunction "A5") (pintype "input"))
    (pad "14" smd roundrect (at 2.475 -1.905 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "/B5'") (pinfunction "A6") (pintype "input"))
    (pad "15" smd roundrect (at 2.475 -3.175 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "/B6'") (pinfunction "A7") (pintype "input"))
    (pad "16" smd roundrect (at 2.475 -4.445 90) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "/B7'") (pinfunction "A8") (pintype "input"))
    (model "${KICAD7_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-16_3.9x9.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Eurorack:Mech-LED-Hole-3mm" (layer "F.Cu")
    (at 92.075 116.751 90)
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole exclude_from_bom)
    (fp_text reference "H15" (at 0 -2.3 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "b4" (at 0 1 90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 3.3 3.3) (drill 3) (layers "*.Cu" "*.Mask")
      (net 6 "/FACE") (pinfunction "1") (pintype "input"))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 70.866 70.358 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R21" (at 1.27 2.286 90) (layer "F.SilkS"))
    (fp_text value "100K" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 19 "/NOISE'") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 82.5 70.3 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R11" (at -0.2 -1.8 90) (layer "F.SilkS"))
    (fp_text value "100K" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 98 "Net-(Q2B-B2)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Eurorack:Mech-MountingHole" (layer "F.Cu")
    (at 55.95 227.1)
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole exclude_from_bom)
    (fp_text reference "H3" (at 0 -2.54 unlocked) (layer "F.Fab"))
    (fp_text value "mount1" (at 0 2.54 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole oval (at 0 0 90) (size 3.5 7.8) (drill oval 3.2 7.5) (layers "*.Cu" "*.Mask")
      (net 6 "/FACE") (pinfunction "1") (pintype "input"))
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 84.6328 77.724 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C3" (at -0.276 1.7672 90) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+12V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "-12V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D3.0mm" (layer "F.Cu")
    (at 78.105 -5.039)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr through_hole)
    (fp_text reference "D7" (at -1.143 -1.8796) (layer "F.SilkS"))
    (fp_text value "LED_GREEN" (at 1.27 2.96) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 31 "Net-(D7-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 32 "/B3'") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 83.7692 82.006 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C6" (at -0.0508 1.6764 90) (layer "F.SilkS"))
    (fp_text value "1n" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(U1B--)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(C6-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Eurorack:Mech-AudioJack-Hole-Output-Gate" (layer "F.Cu")
    (at 94.94 201.2644)
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole exclude_from_bom)
    (fp_text reference "H22" (at 0.4 0.1 unlocked) (layer "F.Fab"))
    (fp_text value "pulse" (at 0.0254 6.2866 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 7.7 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 8 8) (drill 6.4) (layers "*.Cu" "*.Mask")
      (net 6 "/FACE") (pinfunction "1") (pintype "input"))
    (model "./models3d/A-2566.wrl"
      (offset (xyz 0 0 -1.5))
      (scale (xyz 0.385 0.385 0.385))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 78.486 13.97 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C4" (at 2.794 -0.254 90) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "-12V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+12V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 70.612 77.892 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R22" (at -2.268 -0.048 90) (layer "F.SilkS"))
    (fp_text value "1K" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 51 "Net-(J5-PadT)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 19 "/NOISE'") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 81.4832 82.006 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R13" (at 0 -1.65 90) (layer "F.SilkS"))
    (fp_text value "5.1K" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 12 "Net-(U1B--)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 9 "Net-(C6-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 65.786 88.941 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R17" (at -0.1934 1.651 90) (layer "F.SilkS"))
    (fp_text value "100K" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 1 "+12V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 14 "Net-(Q1-E)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Eurorack:Mech-LED-Hole-3mm" (layer "F.Cu")
    (at 66.68 116.751 90)
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole exclude_from_bom)
    (fp_text reference "H11" (at 0 -2.3 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "b0" (at 0 1 90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 3.3 3.3) (drill 3) (layers "*.Cu" "*.Mask")
      (net 6 "/FACE") (pinfunction "1") (pintype "input"))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 81.28 1.778 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R4" (at 0.3556 -1.6764 -270) (layer "F.SilkS"))
    (fp_text value "10K" (at 0 1.65 -270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -270) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 73 "Net-(R4-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 3 "-12V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 65.278 77.13 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C9" (at 0.086 1.4732 -90) (layer "F.SilkS"))
    (fp_text value "1n" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 96 "Net-(U14B--)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "Net-(C10-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Eurorack:Mech-LED-Hole-3mm" (layer "F.Cu")
    (at 73.03 116.751 90)
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole exclude_from_bom)
    (fp_text reference "H12" (at 0 -2.3 90 unlocked) (layer "F.SilkS") hide)
    (fp_text value "b1" (at 0 1 90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 3.3 3.3) (drill 3) (layers "*.Cu" "*.Mask")
      (net 6 "/FACE") (pinfunction "1") (pintype "input"))
  )
  (footprint "Package_SO:TSSOP-14_4.4x5mm_P0.65mm" (layer "F.Cu")
    (at 77.8002 24.776 90)
    (descr "TSSOP, 14 Pin (JEDEC MO-153 Var AB-1 https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "TSSOP SO")
    (property "PartNum" "595-CD4081BPWR")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "Mouser")
    (property "ki_description" "Quad And 2 inputs")
    (property "ki_keywords" "CMOS And2")
    (attr smd)
    (fp_text reference "U12" (at -2.936 -4.3002 180) (layer "F.SilkS"))
    (fp_text value "4081" (at 0 3.45 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.8625 -1.95 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "/B4'") (pintype "input"))
    (pad "2" smd roundrect (at -2.8625 -1.3 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "/_CLK2'") (pintype "input"))
    (pad "3" smd roundrect (at -2.8625 -0.65 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 65 "/P4") (pintype "output"))
    (pad "4" smd roundrect (at -2.8625 0 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 63 "/P2") (pintype "output"))
    (pad "5" smd roundrect (at -2.8625 0.65 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "/_CLK2'") (pintype "input"))
    (pad "6" smd roundrect (at -2.8625 1.3 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "/B6'") (pintype "input"))
    (pad "7" smd roundrect (at -2.8625 1.95 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "8" smd roundrect (at 2.8625 1.95 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 40 "/B7'") (pintype "input"))
    (pad "9" smd roundrect (at 2.8625 1.3 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "/_CLK2'") (pintype "input"))
    (pad "10" smd roundrect (at 2.8625 0.65 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 62 "/P1") (pintype "output"))
    (pad "11" smd roundrect (at 2.8625 0 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 64 "/P3") (pintype "output"))
    (pad "12" smd roundrect (at 2.8625 -0.65 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "/_CLK2'") (pintype "input"))
    (pad "13" smd roundrect (at 2.8625 -1.3 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "/B5'") (pintype "input"))
    (pad "14" smd roundrect (at 2.8625 -1.95 90) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+12V") (pinfunction "VDD") (pintype "power_in"))
    (model "${KICAD7_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-14_4.4x5mm_P0.65mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-323_HandSoldering" (layer "F.Cu")
    (at 78.1 60.7)
    (descr "SOD-323")
    (tags "SOD-323")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "Diode")
    (property "ki_keywords" "diode")
    (attr smd)
    (fp_text reference "D14" (at -0.1 -1.7) (layer "F.SilkS"))
    (fp_text value "1N4148" (at 0.1 1.9) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.85) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.25 0) (size 1 1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "/CLK'") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.25 0) (size 1 1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 100 "Net-(D14-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-323.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 87.2875 74.5)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R30" (at -2.7875 0.8) (layer "F.SilkS"))
    (fp_text value "68K" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 10 "Net-(U1A--)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 1 "+12V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 78.4 66.1 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R12" (at 3.1 1.2 90) (layer "F.SilkS"))
    (fp_text value "3.9K" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 1 "+12V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 101 "Net-(Q2B-C2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-323_HandSoldering" (layer "F.Cu")
    (at 58.674 65.786 90)
    (descr "SOD-323")
    (tags "SOD-323")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "Diode")
    (property "ki_keywords" "diode")
    (attr smd)
    (fp_text reference "D3" (at 0 1.778 90) (layer "F.SilkS"))
    (fp_text value "1N4148" (at 0.1 1.9 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.85 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.25 0 90) (size 1 1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "Net-(D3-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.25 0 90) (size 1 1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-323.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Eurorack:Switch_Rotary_NKK_MRK_112" (layer "F.Cu")
    (at 62.23 42.205)
    (property "PartNum" "633-MRK112-BA")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "Mouser")
    (property "ki_description" "rotary switch with 12 positions")
    (property "ki_keywords" "rotary switch")
    (attr through_hole)
    (fp_text reference "SW1" (at 0 -7.112 unlocked) (layer "F.SilkS"))
    (fp_text value "SW_Rotary12" (at 0 7.112 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 8.636 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -1.553 5.796) (size 1.2 1.2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 38 "/B6'") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at -3 5.196) (size 1.2 1.2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 36 "/B5'") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at -4.243 4.243) (size 1.2 1.2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 34 "/B4'") (pinfunction "3") (pintype "passive"))
    (pad "4" thru_hole circle (at -6 0) (size 1.2 1.2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 32 "/B3'") (pinfunction "4") (pintype "passive"))
    (pad "5" thru_hole circle (at -5.196 -3) (size 1.2 1.2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 30 "/B2'") (pinfunction "5") (pintype "passive"))
    (pad "6" thru_hole circle (at -4.243 -4.243) (size 1.2 1.2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 28 "/B1'") (pinfunction "6") (pintype "passive"))
    (pad "7" thru_hole circle (at 0 -6) (size 1.2 1.2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 26 "/B0'") (pinfunction "7") (pintype "passive"))
    (pad "8" thru_hole circle (at 3 -5.196) (size 1.2 1.2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 87 "/s9'") (pinfunction "8") (pintype "passive"))
    (pad "9" thru_hole circle (at 4.243 -4.243) (size 1.2 1.2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 88 "/s11'") (pinfunction "9") (pintype "passive"))
    (pad "10" thru_hole circle (at 6 0) (size 1.2 1.2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 86 "/s12'") (pinfunction "10") (pintype "passive"))
    (pad "11" thru_hole circle (at 5.196 3) (size 1.2 1.2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 89 "/s13'") (pinfunction "11") (pintype "passive"))
    (pad "12" thru_hole circle (at 4.243 4.243) (size 1.2 1.2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 90 "/s16'") (pinfunction "12") (pintype "passive"))
    (pad "13" thru_hole circle (at 0 6) (size 1.2 1.2) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 91 "/EOL'") (pinfunction "13") (pintype "passive"))
  )
  (footprint "Package_SO:TSSOP-14_4.4x5mm_P0.65mm" (layer "F.Cu")
    (at 71.247 31.9896 180)
    (descr "TSSOP, 14 Pin (JEDEC MO-153 Var AB-1 https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "TSSOP SO")
    (property "PartNum" "595-CD4081BPWR")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "Mouser")
    (property "ki_description" "Quad And 2 inputs")
    (property "ki_keywords" "CMOS And2")
    (attr smd)
    (fp_text reference "U13" (at -2.953 -4.4104 90) (layer "F.SilkS"))
    (fp_text value "4081" (at 0 3.45) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.8625 -1.95 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "/B0'") (pintype "input"))
    (pad "2" smd roundrect (at -2.8625 -1.3 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 70 "/_CLK'") (pintype "input"))
    (pad "3" smd roundrect (at -2.8625 -0.65 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 69 "/P8") (pintype "output"))
    (pad "4" smd roundrect (at -2.8625 0 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 67 "/P6") (pintype "output"))
    (pad "5" smd roundrect (at -2.8625 0.65 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 70 "/_CLK'") (pintype "input"))
    (pad "6" smd roundrect (at -2.8625 1.3 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "/B2'") (pintype "input"))
    (pad "7" smd roundrect (at -2.8625 1.95 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "VSS") (pintype "power_in"))
    (pad "8" smd roundrect (at 2.8625 1.95 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "/B3'") (pintype "input"))
    (pad "9" smd roundrect (at 2.8625 1.3 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 70 "/_CLK'") (pintype "input"))
    (pad "10" smd roundrect (at 2.8625 0.65 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "/P5") (pintype "output"))
    (pad "11" smd roundrect (at 2.8625 0 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 68 "/P7") (pintype "output"))
    (pad "12" smd roundrect (at 2.8625 -0.65 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 70 "/_CLK'") (pintype "input"))
    (pad "13" smd roundrect (at 2.8625 -1.3 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "/B1'") (pintype "input"))
    (pad "14" smd roundrect (at 2.8625 -1.95 180) (size 1.475 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+12V") (pinfunction "VDD") (pintype "power_in"))
    (model "${KICAD7_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-14_4.4x5mm_P0.65mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 88.5444 51.3236 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R27" (at 0 1.524 90) (layer "F.SilkS"))
    (fp_text value "10K" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 82 "Net-(R27-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 20 "/SOL'") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 75.8 66.1 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R32" (at 3.2 0.2 90) (layer "F.SilkS"))
    (fp_text value "470K" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 23 "/CLK'") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 101 "Net-(Q2B-C2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Eurorack:Mech-AudioJack-Hole-Output" (layer "F.Cu")
    (at 82.804 214.795)
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole exclude_from_bom)
    (fp_text reference "H10" (at 0.4 0.1 unlocked) (layer "F.Fab"))
    (fp_text value "noise" (at 0.0254 6.2866 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 7.7 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 8 8) (drill 6.4) (layers "*.Cu" "*.Mask")
      (net 6 "/FACE") (pinfunction "1") (pintype "input"))
    (model "./models3d/A-2566.wrl"
      (offset (xyz 0 0 -1.5))
      (scale (xyz 0.385 0.385 0.385))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Potentiometer_THT:Potentiometer_Bourns_3296W_Vertical" (layer "F.Cu")
    (at 66.0654 72.654 -90)
    (descr "Potentiometer, vertical, Bourns 3296W, https://www.bourns.com/pdfs/3296.pdf")
    (tags "Potentiometer vertical Bourns 3296W")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Trim-potentiometer")
    (property "ki_keywords" "resistor variable trimpot trimmer")
    (attr through_hole)
    (fp_text reference "RV3" (at -1.026 3.3274 90) (layer "F.SilkS"))
    (fp_text value "5K" (at -2.54 3.67 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -3.175 0.005 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.44 1.44) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 96 "Net-(U14B--)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at -2.54 0 270) (size 1.44 1.44) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 16 "Net-(C10-Pad1)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at -5.08 0 270) (size 1.44 1.44) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 16 "Net-(C10-Pad1)") (pinfunction "3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_3296W_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Eurorack:Switch_SPDT_1M_Solder_Lug" (layer "F.Cu")
    (at 94.5896 38.862 180)
    (property "PartNum" "A-6099")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "Tayda")
    (property "ki_description" "Switch, single pole double throw, center OFF position")
    (property "ki_keywords" "switch spdt single-pole double-throw ON-OFF-ON")
    (attr through_hole)
    (fp_text reference "SW2" (at -2.1844 7.112 unlocked) (layer "F.SilkS"))
    (fp_text value "SW_SPDT_MSM" (at 0 1 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 180 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole oval (at 0 -4.7 180) (size 3.3 2) (drill oval 2.5 1.3) (layers "*.Cu" "*.Mask")
      (net 1 "+12V") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 0 180) (size 3.3 2) (drill oval 2.5 1.3) (layers "*.Cu" "*.Mask")
      (net 79 "Net-(R24-Pad2)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 4.7 180) (size 3.3 2) (drill oval 2.5 1.3) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "3") (pintype "passive"))
  )
  (footprint "LED_THT:LED_D3.0mm" (layer "F.Cu")
    (at 71.755 -5.039)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr through_hole)
    (fp_text reference "D8" (at -1.143 -1.8796) (layer "F.SilkS"))
    (fp_text value "LED_GREEN" (at 1.27 2.96) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 33 "Net-(D8-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 34 "/B4'") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 68.072 88.941 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R19" (at -3.0832 0.2794 90) (layer "F.SilkS"))
    (fp_text value "470K" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 17 "Net-(C8-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 97 "Net-(U14A--)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Eurorack:Mech-MRK-Hole" (layer "F.Cu")
    (at 62.23 163.995)
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole exclude_from_bom)
    (fp_text reference "H20" (at 0 -4.9 unlocked) (layer "F.Fab"))
    (fp_text value "length" (at 0 12.7 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 5 unlocked) (layer "F.Fab"))
    (pad "" thru_hole oval (at 0 6.5) (size 2.6 1.5) (drill oval 2.3 1.2) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 0 0) (size 8 8) (drill 6.35) (layers "*.Cu" "*.Mask")
      (net 6 "/FACE") (pinfunction "1") (pintype "input"))
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 99.1616 41.5036 -90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C12" (at 0.0606 -1.524 90) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "/SOL'") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 270) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L7.2mm_W4.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2" (layer "B.Cu")
    (at 71.374 68.153 -90)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*4.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 4.5mm Capacitor")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C10" (at 9.7742 3.2258 90) (layer "B.SilkS"))
    (fp_text value "470n box" (at 2.5 -3.5 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 16 "Net-(C10-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 19 "/NOISE'") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L7.2mm_W4.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Eurorack:PinHeader_2x05_P2.54mm_Vertical" (layer "B.Cu")
    (at 57.404 5.121 180)
    (descr "Through hole straight pin header, 2x05, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x05 2.54mm double row")
    (property "PartNum" "A-2939")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "Tayda")
    (property "ki_description" "Generic connector, double row, 02x05, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J1" (at -4.4323 -1.524) (layer "B.SilkS"))
    (fp_text value "Conn_02x05_Odd_Even" (at 1.2446 -16.2052) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 -5.08 90) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(J1-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(J1-Pin_1)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 2.54 -2.54 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 2.54 -5.08 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 2.54 -7.62 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(J1-Pin_10)") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval (at 2.54 -10.16 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(J1-Pin_10)") (pinfunction "Pin_10") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x05_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Eurorack:PinHeader_2x08_P2.54mm_Vertical" (layer "B.Cu")
    (at 94.615 25.441)
    (descr "Through hole straight pin header, 2x08, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x08 2.54mm double row")
    (property "PartNum" "A-2956")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "Tayda")
    (property "ki_description" "Generic connector, double row, 02x08, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J6" (at -3.3401 6.081) (layer "B.SilkS"))
    (fp_text value "Conn_02x08_Odd_Even" (at 0.0078 5.9372) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 -8.89 90) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 53 "/G1") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 54 "/G2") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 55 "/G3") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 2.54 -2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 56 "/G4") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 -5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 57 "/G5") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 2.54 -5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 58 "/G6") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 -7.62) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 59 "/G7") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 2.54 -7.62) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 60 "/G8") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 -10.16) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 61 "/_CLK2'") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval (at 2.54 -10.16) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 61 "/_CLK2'") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole oval (at 0 -12.7) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "-12V") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole oval (at 2.54 -12.7) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "-12V") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole oval (at 0 -15.24) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole oval (at 2.54 -15.24) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" thru_hole oval (at 0 -17.78) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "+12V") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" thru_hole oval (at 2.54 -17.78) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "+12V") (pinfunction "Pin_16") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Array_SIP9" (layer "B.Cu")
    (at 98.059 -9.103 180)
    (descr "9-pin Resistor SIP pack")
    (tags "R")
    (property "PartNum" "652-4609X-1LF-2.2K")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "Mouser")
    (property "ki_description" "8 resistor network, star topology, bussed resistors, small symbol")
    (property "ki_keywords" "R network star-topology")
    (attr through_hole)
    (fp_text reference "RN1" (at -2.2202 -0.1016 90) (layer "B.SilkS"))
    (fp_text value "2.2K" (at 11.43 -2.4) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 10.16 0) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "common") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 25 "Net-(D4-K)") (pinfunction "R1") (pintype "passive"))
    (pad "3" thru_hole oval (at 5.08 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 27 "Net-(D5-K)") (pinfunction "R2") (pintype "passive"))
    (pad "4" thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 29 "Net-(D6-K)") (pinfunction "R3") (pintype "passive"))
    (pad "5" thru_hole oval (at 10.16 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 31 "Net-(D7-K)") (pinfunction "R4") (pintype "passive"))
    (pad "6" thru_hole oval (at 12.7 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 33 "Net-(D8-K)") (pinfunction "R5") (pintype "passive"))
    (pad "7" thru_hole oval (at 15.24 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 35 "Net-(D9-K)") (pinfunction "R6") (pintype "passive"))
    (pad "8" thru_hole oval (at 17.78 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 37 "Net-(D10-K)") (pinfunction "R7") (pintype "passive"))
    (pad "9" thru_hole oval (at 20.32 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 39 "Net-(D11-K)") (pinfunction "R8") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Array_SIP9.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D5.0mm_P2.50mm" (layer "B.Cu")
    (at 65.213112 2.581 180)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C1" (at -0.826888 -3.302 90) (layer "B.SilkS"))
    (fp_text value "22u 50V" (at 1.25 -3.75) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "+12V") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D5.0mm_P2.50mm" (layer "B.Cu")
    (at 62.738 17.821)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C2" (at 3.302 -3.302 90) (layer "B.SilkS"))
    (fp_text value "22u 50V" (at 1.25 -3.75) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "-12V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L7.2mm_W4.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2" (layer "B.Cu")
    (at 71.374 80.94 90)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*4.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 4.5mm Capacitor")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C8" (at -1.1782 -3.3528 270) (layer "B.SilkS") hide)
    (fp_text value "470n box" (at 2.5 -3.5 270) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 270) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 17 "Net-(C8-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 13 "Net-(C8-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L7.2mm_W4.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Eurorack:PinHeader_2x08_P2.54mm_Vertical" (layer "B.Cu")
    (at 83.82 25.441)
    (descr "Through hole straight pin header, 2x08, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x08 2.54mm double row")
    (property "PartNum" "A-2956")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "Tayda")
    (property "ki_description" "Generic connector, double row, 02x08, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J7" (at -2.7051 6.208) (layer "B.SilkS"))
    (fp_text value "Conn_02x08_Odd_Even" (at 0.0008 5.9372) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 -8.89 90) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 62 "/P1") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 63 "/P2") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 64 "/P3") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 2.54 -2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 65 "/P4") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 -5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 66 "/P5") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 2.54 -5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 67 "/P6") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 -7.62) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 68 "/P7") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 2.54 -7.62) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 69 "/P8") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 -10.16) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 70 "/_CLK'") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval (at 2.54 -10.16) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 70 "/_CLK'") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole oval (at 0 -12.7) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "-12V") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole oval (at 2.54 -12.7) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "-12V") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole oval (at 0 -15.24) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole oval (at 2.54 -15.24) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" thru_hole oval (at 0 -17.78) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "+12V") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" thru_hole oval (at 2.54 -17.78) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "+12V") (pinfunction "Pin_16") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x08_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-92_Inline_Wide" (layer "B.Cu")
    (at 70.866 96.8038 180)
    (descr "TO-92 leads in-line, wide, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (property "PartNum" "637-BC547C")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "Mouser")
    (property "ki_description" "0.1A Ic, 45V Vce, Small Signal NPN Transistor, TO-92")
    (property "ki_keywords" "NPN Transistor")
    (attr through_hole)
    (fp_text reference "Q1" (at -0.762 1.884) (layer "B.SilkS"))
    (fp_text value "BC547" (at 2.463 -2.907) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 2.54 0) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.5 1.5) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 71 "unconnected-(Q1-C-Pad1)") (pinfunction "C") (pintype "passive+no_connect"))
    (pad "2" thru_hole circle (at 2.54 0 180) (size 1.5 1.5) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "B") (pintype "input"))
    (pad "3" thru_hole circle (at 5.08 0 180) (size 1.5 1.5) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 14 "Net-(Q1-E)") (pinfunction "E") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline_Wide.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L7.2mm_W4.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2" (layer "B.Cu")
    (at 66.08 91.5416)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*4.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 4.5mm Capacitor")
    (property "Sheetfile" "turing-machine.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C7" (at -0.5226 -3.0734 180) (layer "B.SilkS"))
    (fp_text value "470n box" (at 2.5 -3.5 180) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 180) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 14 "Net-(Q1-E)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 15 "Net-(C7-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L7.2mm_W4.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect (start 50.95 -10.94) (end 101.45 99.06)
    (fill none) (layer "Edge.Cuts"))
  (gr_rect (start 50.95 101.6) (end 101.45 230.1)
    (fill none) (layer "Edge.Cuts"))
  (gr_text "thismatters/turing-machine/v1" (at 88.7476 1.6002) (layer "B.SilkS"))
  (gr_text "NOISE" (at 70.866 86.655) (layer "B.SilkS"))
  (gr_text "BITS->VOLTS" (at 73.7108 10.7696) (layer "B.SilkS"))
  (gr_text "EXPANSIONS" (at 85.8832 36.5185) (layer "B.SilkS"))
  (gr_text "Based on the Music Thing Modular design\ngithub.com/TomWhitwell/TuringMachine" (at 52.07 53.5432 270) (layer "B.SilkS"))
  (gr_text "GATES" (at 98.5832 32.3275) (layer "B.SilkS"))
  (gr_text "LOOP\nCTRL" (at 95.6564 50.5616) (layer "B.SilkS"))
  (gr_text "PULSES" (at 88.0422 32.3275) (layer "B.SilkS"))
  (gr_text "SHIFT REGISTERS" (at 71.3486 59.2382) (layer "B.SilkS"))
  (gr_text "POWER" (at 62.484 7.661 90) (layer "B.SilkS"))
  (gr_text "INPUT\nOUTPUT" (at 85 75.6) (layer "B.SilkS"))
  (gr_text "5" (at 52.578 163.9696) (layer "F.SilkS"))
  (gr_text "2" (at 62.2554 173.647) (layer "F.SilkS"))
  (gr_text "*" (at 62.484 74.422) (layer "F.SilkS"))
  (gr_text "8" (at 62.2554 154.3176) (layer "F.SilkS"))
  (gr_text "11" (at 71.2724 159.1436) (layer "F.SilkS"))
  (gr_text "16" (at 67.7418 172.4024) (layer "F.SilkS"))
  (gr_text "13" (at 71.3232 168.7956) (layer "F.SilkS"))
  (gr_text "turing machine" (at 76.398 228.798) (layer "F.SilkS"))
  (gr_text "7" (at 57.4548 155.613) (layer "F.SilkS"))
  (gr_text "4" (at 53.8734 168.821) (layer "F.SilkS"))
  (gr_text "9" (at 67.056 155.613) (layer "F.SilkS"))
  (gr_text "6" (at 53.8988 159.0928) (layer "F.SilkS"))
  (gr_text "thismatters/turing-machine/v1" (at 100.9852 181.3 90) (layer "F.SilkS"))
  (gr_text "12" (at 72.5932 163.995) (layer "F.SilkS"))
  (gr_text "3" (at 57.404 172.4278) (layer "F.SilkS"))
  (zone (net 2) (net_name "GND") (layers "F&B.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.6))
    (polygon
      (pts
        (xy 50.546 -11.389)
        (xy 101.854 -11.389)
        (xy 101.854 99.609)
        (xy 50.546 99.609)
      )
    )
  )
  (zone (net 6) (net_name "/FACE") (layers "F&B.Cu") (hatch edge 0.5)
    (priority 1)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 50.236 101.036)
        (xy 102.052 101.036)
        (xy 102.052 231.084)
        (xy 50.236 231.084)
      )
    )
  )
)
