<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="10.73" x2="0" y2="1.27" width="0" layer="20"/>
<wire x1="0" y1="1.27" x2="1.27" y2="0" width="0" layer="20" curve="90"/>
<wire x1="1.27" y1="0" x2="35.673" y2="0" width="0" layer="20"/>
<wire x1="35.673" y1="0" x2="36.943" y2="1.27" width="0" layer="20" curve="90"/>
<wire x1="36.943" y1="1.27" x2="36.943" y2="10.73" width="0" layer="20"/>
<wire x1="36.943" y1="10.73" x2="35.673" y2="12" width="0" layer="20" curve="90"/>
<wire x1="35.673" y1="12" x2="1.27" y2="12" width="0" layer="20"/>
<wire x1="1.27" y1="12" x2="0" y2="10.73" width="0" layer="20" curve="90"/>
<hole x="4" y="8" drill="4"/>
<hole x="32.943" y="8" drill="4"/>
</plain>
<libraries>
<library name="GLOBAL CONNECTOR TECHNOLOGY - USB3145-30-1-A">
<description>Upverter Parts Library

Created by Upverter.com</description>
<packages>
<package name="GLOBAL_CONNECTOR_TECHNOLOGY_USB3145-30-1-A_0">
<description>Micro USB 2.0 Connector</description>
</package>
</packages>
</library>
<library name="con-lsta">
<description>&lt;b&gt;Female Headers etc.&lt;/b&gt;&lt;p&gt;
Naming:&lt;p&gt;
FE = female&lt;p&gt;
# contacts - # rows&lt;p&gt;
W = angled&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="FE05-1">
<description>&lt;b&gt;FEMALE HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="USB" library="GLOBAL CONNECTOR TECHNOLOGY - USB3145-30-1-A" package="GLOBAL_CONNECTOR_TECHNOLOGY_USB3145-30-1-A_0" value="GLOBAL_CONNECTOR_TECHNOLOGY_USB3145-30-1-AGLOBAL_CONNECTOR_TECHNOLOGY_USB3145-30-1-A_0_0">
<attribute name="CENTROID_NOT_SPECIFIED" value="No"/>
<attribute name="CURRENT_RATING_POWER" value="1.8A"/>
<attribute name="CURRENT_RATING_SIGNALS" value="1A"/>
<attribute name="DATASHEET" value="http://www.farnell.com/datasheets/1841848.pdf"/>
<attribute name="IS_FEMALE" value="yes"/>
<attribute name="LEAD_FREE" value="yes"/>
<attribute name="MF" value="GLOBAL CONNECTOR TECHNOLOGY"/>
<attribute name="MPN" value="USB3145-30-1-A"/>
<attribute name="PACKAGE" value="CONN_USB_PTH_7MM80_2MM77"/>
<attribute name="PREFIX" value="J"/>
<attribute name="ROHS" value="yes"/>
<attribute name="TEMPERATURE_RANGE_HIGH" value="+85°C"/>
<attribute name="TEMPERATURE_RANGE_LOW" value="-30°C"/>
<attribute name="VOLTAGE" value="100VAC"/>
</element>
<element name="HEADER" library="con-lsta" package="FE05-1" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="POPULARITY" value="7"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="USB1">
<contactref element="USB" pad="1"/>
<contactref element="HEADER" pad="1"/>
</signal>
<signal name="USB2">
<contactref element="USB" pad="2"/>
<contactref element="HEADER" pad="2"/>
</signal>
<signal name="USB3">
<contactref element="USB" pad="3"/>
<contactref element="HEADER" pad="3"/>
</signal>
<signal name="USB4">
<contactref element="USB" pad="4"/>
<contactref element="HEADER" pad="4"/>
</signal>
<signal name="USB5">
<contactref element="USB" pad="5"/>
<contactref element="HEADER" pad="5"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
