(kicad_pcb (version 20171130) (host pcbnew "(5.0.1)-3")
  (general
    (thickness 1.6)
    (drawings 42)
    (tracks 2692)
    (zones 0)
    (modules 46)
    (nets 177)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user hide)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.127)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFF7FF)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /AD7)
  (net 3 /AD6)
  (net 4 /AD5)
  (net 5 /AD4)
  (net 6 /AD3)
  (net 7 /AD2)
  (net 8 /AD1)
  (net 9 /AD0)
  (net 10 /~RD)
  (net 11 /~WR)
  (net 12 /PI_REQ)
  (net 13 +5V)
  (net 14 /~IOR)
  (net 15 /~IOW)
  (net 16 /~MEMR)
  (net 17 /~MEMW)
  (net 18 /CON_IOW)
  (net 19 /~CON_IOR)
  (net 20 /~STS_IOR)
  (net 21 /~CON_SO)
  (net 22 /~CON_SI)
  (net 23 "Net-(U14-Pad16)")
  (net 24 /~RESET)
  (net 25 /~CON_R)
  (net 26 /CON_W)
  (net 27 /~HAK)
  (net 28 /~HRQ)
  (net 29 /A0)
  (net 30 /A1)
  (net 31 "Net-(U12-Pad19)")
  (net 32 /IO~M)
  (net 33 /A23)
  (net 34 /A22)
  (net 35 /A21)
  (net 36 /A20)
  (net 37 /A19)
  (net 38 /A18)
  (net 39 /A17)
  (net 40 /A16)
  (net 41 /A15)
  (net 42 /A14)
  (net 43 /A13)
  (net 44 /A12)
  (net 45 /A11)
  (net 46 /A10)
  (net 47 /A9)
  (net 48 /A8)
  (net 49 /A7)
  (net 50 /A6)
  (net 51 /A5)
  (net 52 /A4)
  (net 53 /A3)
  (net 54 /A2)
  (net 55 "Net-(J1-Pad34)")
  (net 56 "Net-(J1-Pad35)")
  (net 57 "Net-(J1-Pad36)")
  (net 58 "Net-(J1-Pad37)")
  (net 59 "Net-(J1-Pad38)")
  (net 60 "Net-(J1-Pad39)")
  (net 61 "Net-(J1-Pad40)")
  (net 62 "Net-(J1-Pad41)")
  (net 63 "Net-(J1-Pad42)")
  (net 64 "Net-(J1-Pad43)")
  (net 65 "Net-(J1-Pad44)")
  (net 66 "Net-(J1-Pad45)")
  (net 67 "Net-(J1-Pad46)")
  (net 68 "Net-(J1-Pad47)")
  (net 69 "Net-(J1-Pad48)")
  (net 70 "Net-(J1-Pad49)")
  (net 71 "Net-(J1-Pad50)")
  (net 72 "Net-(J1-Pad51)")
  (net 73 "Net-(J1-Pad52)")
  (net 74 "Net-(J1-Pad53)")
  (net 75 "Net-(J1-Pad54)")
  (net 76 "Net-(J1-Pad55)")
  (net 77 "Net-(J1-Pad56)")
  (net 78 +3V3)
  (net 79 /+5VSB)
  (net 80 "Net-(J1-Pad65)")
  (net 81 "Net-(J1-Pad66)")
  (net 82 "Net-(J1-Pad67)")
  (net 83 "Net-(J1-Pad68)")
  (net 84 "Net-(J1-Pad69)")
  (net 85 "Net-(J1-Pad70)")
  (net 86 "Net-(J1-Pad71)")
  (net 87 "Net-(J1-Pad72)")
  (net 88 "Net-(J1-Pad73)")
  (net 89 /D7)
  (net 90 /D6)
  (net 91 /D5)
  (net 92 /D4)
  (net 93 /D3)
  (net 94 /D2)
  (net 95 /D1)
  (net 96 /D0)
  (net 97 /~HOLD)
  (net 98 /~HLDA)
  (net 99 "Net-(J1-Pad84)")
  (net 100 /~RFSH)
  (net 101 "Net-(J1-Pad86)")
  (net 102 "Net-(J1-Pad87)")
  (net 103 "Net-(J1-Pad88)")
  (net 104 /~MASTER)
  (net 105 /~AEN)
  (net 106 /~DRQ0)
  (net 107 /~DAK0)
  (net 108 /~DRQ1)
  (net 109 /~DAK1)
  (net 110 /~DRQ2)
  (net 111 /~DAK2)
  (net 112 /~DRQ3)
  (net 113 /~DAK3)
  (net 114 "Net-(J1-Pad99)")
  (net 115 "Net-(J1-Pad100)")
  (net 116 "Net-(J1-Pad101)")
  (net 117 /~IRQ7)
  (net 118 /~IRQ6)
  (net 119 /~IRQ5)
  (net 120 /~IRQ4)
  (net 121 /~IRQ3)
  (net 122 /~IRQ2)
  (net 123 /~IRQ1)
  (net 124 /~IRQ0)
  (net 125 "Net-(J1-Pad110)")
  (net 126 "Net-(J1-Pad111)")
  (net 127 "Net-(J1-Pad112)")
  (net 128 /SDA)
  (net 129 /SCL)
  (net 130 "Net-(RN1-Pad6)")
  (net 131 "Net-(RN1-Pad5)")
  (net 132 "Net-(RN1-Pad4)")
  (net 133 "Net-(RN1-Pad3)")
  (net 134 "Net-(RN1-Pad2)")
  (net 135 "Net-(RN3-Pad9)")
  (net 136 "Net-(RN3-Pad8)")
  (net 137 "Net-(RN3-Pad7)")
  (net 138 "Net-(RN3-Pad6)")
  (net 139 "Net-(RN3-Pad5)")
  (net 140 "Net-(RN3-Pad4)")
  (net 141 "Net-(RN3-Pad3)")
  (net 142 /PD1)
  (net 143 /PU1)
  (net 144 /~pINT)
  (net 145 /~pRFSH)
  (net 146 "Net-(C1-Pad1)")
  (net 147 "Net-(J6-Pad1)")
  (net 148 "Net-(J6-Pad3)")
  (net 149 "Net-(J6-Pad5)")
  (net 150 "Net-(J5-Pad5)")
  (net 151 "Net-(J5-Pad4)")
  (net 152 /pPI_REQ)
  (net 153 "Net-(C6-Pad1)")
  (net 154 /ALE_X)
  (net 155 /~pCON_SO)
  (net 156 /ALE_H)
  (net 157 "Net-(J6-Pad27)")
  (net 158 "Net-(J6-Pad28)")
  (net 159 /ALE_L)
  (net 160 "Net-(J5-Pad6)")
  (net 161 "Net-(J5-Pad3)")
  (net 162 "Net-(J5-Pad2)")
  (net 163 "Net-(U12-Pad1)")
  (net 164 "Net-(RN3-Pad2)")
  (net 165 "Net-(J3-Pad10)")
  (net 166 /PIPWR)
  (net 167 "Net-(J2-Pad16)")
  (net 168 "Net-(J2-Pad15)")
  (net 169 "Net-(J2-Pad14)")
  (net 170 "Net-(J2-Pad13)")
  (net 171 "Net-(J2-Pad12)")
  (net 172 "Net-(J2-Pad11)")
  (net 173 "Net-(J2-Pad10)")
  (net 174 "Net-(J2-Pad9)")
  (net 175 "Net-(RN2-Pad8)")
  (net 176 "Net-(J1-Pad121)")
  (net_class Default "This is the default net class."
    (clearance 0.127)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /A0)
    (add_net /A1)
    (add_net /A10)
    (add_net /A11)
    (add_net /A12)
    (add_net /A13)
    (add_net /A14)
    (add_net /A15)
    (add_net /A16)
    (add_net /A17)
    (add_net /A18)
    (add_net /A19)
    (add_net /A2)
    (add_net /A20)
    (add_net /A21)
    (add_net /A22)
    (add_net /A23)
    (add_net /A3)
    (add_net /A4)
    (add_net /A5)
    (add_net /A6)
    (add_net /A7)
    (add_net /A8)
    (add_net /A9)
    (add_net /AD0)
    (add_net /AD1)
    (add_net /AD2)
    (add_net /AD3)
    (add_net /AD4)
    (add_net /AD5)
    (add_net /AD6)
    (add_net /AD7)
    (add_net /ALE_H)
    (add_net /ALE_L)
    (add_net /ALE_X)
    (add_net /CON_IOW)
    (add_net /CON_W)
    (add_net /D0)
    (add_net /D1)
    (add_net /D2)
    (add_net /D3)
    (add_net /D4)
    (add_net /D5)
    (add_net /D6)
    (add_net /D7)
    (add_net /IO~M)
    (add_net /PD1)
    (add_net /PI_REQ)
    (add_net /PU1)
    (add_net /SCL)
    (add_net /SDA)
    (add_net /pPI_REQ)
    (add_net /~AEN)
    (add_net /~CON_IOR)
    (add_net /~CON_R)
    (add_net /~CON_SI)
    (add_net /~CON_SO)
    (add_net /~DAK0)
    (add_net /~DAK1)
    (add_net /~DAK2)
    (add_net /~DAK3)
    (add_net /~DRQ0)
    (add_net /~DRQ1)
    (add_net /~DRQ2)
    (add_net /~DRQ3)
    (add_net /~HAK)
    (add_net /~HLDA)
    (add_net /~HOLD)
    (add_net /~HRQ)
    (add_net /~IOR)
    (add_net /~IOW)
    (add_net /~IRQ0)
    (add_net /~IRQ1)
    (add_net /~IRQ2)
    (add_net /~IRQ3)
    (add_net /~IRQ4)
    (add_net /~IRQ5)
    (add_net /~IRQ6)
    (add_net /~IRQ7)
    (add_net /~MASTER)
    (add_net /~MEMR)
    (add_net /~MEMW)
    (add_net /~RD)
    (add_net /~RESET)
    (add_net /~RFSH)
    (add_net /~STS_IOR)
    (add_net /~WR)
    (add_net /~pCON_SO)
    (add_net /~pINT)
    (add_net /~pRFSH)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C6-Pad1)")
    (add_net "Net-(J1-Pad100)")
    (add_net "Net-(J1-Pad101)")
    (add_net "Net-(J1-Pad110)")
    (add_net "Net-(J1-Pad111)")
    (add_net "Net-(J1-Pad112)")
    (add_net "Net-(J1-Pad121)")
    (add_net "Net-(J1-Pad34)")
    (add_net "Net-(J1-Pad35)")
    (add_net "Net-(J1-Pad36)")
    (add_net "Net-(J1-Pad37)")
    (add_net "Net-(J1-Pad38)")
    (add_net "Net-(J1-Pad39)")
    (add_net "Net-(J1-Pad40)")
    (add_net "Net-(J1-Pad41)")
    (add_net "Net-(J1-Pad42)")
    (add_net "Net-(J1-Pad43)")
    (add_net "Net-(J1-Pad44)")
    (add_net "Net-(J1-Pad45)")
    (add_net "Net-(J1-Pad46)")
    (add_net "Net-(J1-Pad47)")
    (add_net "Net-(J1-Pad48)")
    (add_net "Net-(J1-Pad49)")
    (add_net "Net-(J1-Pad50)")
    (add_net "Net-(J1-Pad51)")
    (add_net "Net-(J1-Pad52)")
    (add_net "Net-(J1-Pad53)")
    (add_net "Net-(J1-Pad54)")
    (add_net "Net-(J1-Pad55)")
    (add_net "Net-(J1-Pad56)")
    (add_net "Net-(J1-Pad65)")
    (add_net "Net-(J1-Pad66)")
    (add_net "Net-(J1-Pad67)")
    (add_net "Net-(J1-Pad68)")
    (add_net "Net-(J1-Pad69)")
    (add_net "Net-(J1-Pad70)")
    (add_net "Net-(J1-Pad71)")
    (add_net "Net-(J1-Pad72)")
    (add_net "Net-(J1-Pad73)")
    (add_net "Net-(J1-Pad84)")
    (add_net "Net-(J1-Pad86)")
    (add_net "Net-(J1-Pad87)")
    (add_net "Net-(J1-Pad88)")
    (add_net "Net-(J1-Pad99)")
    (add_net "Net-(J2-Pad10)")
    (add_net "Net-(J2-Pad11)")
    (add_net "Net-(J2-Pad12)")
    (add_net "Net-(J2-Pad13)")
    (add_net "Net-(J2-Pad14)")
    (add_net "Net-(J2-Pad15)")
    (add_net "Net-(J2-Pad16)")
    (add_net "Net-(J2-Pad9)")
    (add_net "Net-(J3-Pad10)")
    (add_net "Net-(J5-Pad2)")
    (add_net "Net-(J5-Pad3)")
    (add_net "Net-(J5-Pad4)")
    (add_net "Net-(J5-Pad5)")
    (add_net "Net-(J5-Pad6)")
    (add_net "Net-(J6-Pad1)")
    (add_net "Net-(J6-Pad27)")
    (add_net "Net-(J6-Pad28)")
    (add_net "Net-(J6-Pad3)")
    (add_net "Net-(J6-Pad5)")
    (add_net "Net-(RN1-Pad2)")
    (add_net "Net-(RN1-Pad3)")
    (add_net "Net-(RN1-Pad4)")
    (add_net "Net-(RN1-Pad5)")
    (add_net "Net-(RN1-Pad6)")
    (add_net "Net-(RN2-Pad8)")
    (add_net "Net-(RN3-Pad2)")
    (add_net "Net-(RN3-Pad3)")
    (add_net "Net-(RN3-Pad4)")
    (add_net "Net-(RN3-Pad5)")
    (add_net "Net-(RN3-Pad6)")
    (add_net "Net-(RN3-Pad7)")
    (add_net "Net-(RN3-Pad8)")
    (add_net "Net-(RN3-Pad9)")
    (add_net "Net-(U12-Pad1)")
    (add_net "Net-(U12-Pad19)")
    (add_net "Net-(U14-Pad16)")
  )
  (net_class Power ""
    (clearance 0.127)
    (trace_width 0.6)
    (via_dia 0.8)
    (via_drill 0.6)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net /+5VSB)
    (add_net /PIPWR)
    (add_net GND)
  )
  (module Pin_Headers:Pin_Header_Straight_2x20_Pitch2.54mm locked (layer F.Cu) (tedit 5BFE2382)
    (at 163.195 38.1 270)
    (descr "Through hole straight pin header, 2x20, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x20 2.54mm double row")
    (fp_text reference J6 (at -2.54 24.13) (layer F.SilkS))
    (fp_text value Raspberry_Pi_2_3 (at 0 26.46 270) (layer F.Fab))
    (fp_text user %R (at 1.27 24.13) (layer F.Fab))
    (pad 1 thru_hole rect (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 147 "Net-(J6-Pad1)"))
    (pad 2 thru_hole oval (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 166 /PIPWR))
    (pad 3 thru_hole oval (at 2.54 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 148 "Net-(J6-Pad3)"))
    (pad 4 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 166 /PIPWR))
    (pad 5 thru_hole oval (at 2.54 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 149 "Net-(J6-Pad5)"))
    (pad 6 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole oval (at 2.54 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /~WR))
    (pad 8 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 150 "Net-(J5-Pad5)"))
    (pad 9 thru_hole oval (at 2.54 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 10 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 151 "Net-(J5-Pad4)"))
    (pad 11 thru_hole oval (at 2.54 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /AD1))
    (pad 12 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /AD2))
    (pad 13 thru_hole oval (at 2.54 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 152 /pPI_REQ))
    (pad 14 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 15 thru_hole oval (at 2.54 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /AD6))
    (pad 16 thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /AD7))
    (pad 17 thru_hole oval (at 2.54 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 153 "Net-(C6-Pad1)"))
    (pad 18 thru_hole oval (at 0 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 154 /ALE_X))
    (pad 19 thru_hole oval (at 2.54 22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /CON_W))
    (pad 20 thru_hole oval (at 0 22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 21 thru_hole oval (at 2.54 25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 155 /~pCON_SO))
    (pad 22 thru_hole oval (at 0 25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 156 /ALE_H))
    (pad 23 thru_hole oval (at 2.54 27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /~CON_R))
    (pad 24 thru_hole oval (at 0 27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /~HAK))
    (pad 25 thru_hole oval (at 2.54 30.48 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 26 thru_hole oval (at 0 30.48 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /~HRQ))
    (pad 27 thru_hole oval (at 2.54 33.02 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 157 "Net-(J6-Pad27)"))
    (pad 28 thru_hole oval (at 0 33.02 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 158 "Net-(J6-Pad28)"))
    (pad 29 thru_hole oval (at 2.54 35.56 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /~RD))
    (pad 30 thru_hole oval (at 0 35.56 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 31 thru_hole oval (at 2.54 38.1 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /IO~M))
    (pad 32 thru_hole oval (at 0 38.1 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 144 /~pINT))
    (pad 33 thru_hole oval (at 2.54 40.64 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 145 /~pRFSH))
    (pad 34 thru_hole oval (at 0 40.64 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 35 thru_hole oval (at 2.54 43.18 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /AD3))
    (pad 36 thru_hole oval (at 0 43.18 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /AD0))
    (pad 37 thru_hole oval (at 2.54 45.72 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 159 /ALE_L))
    (pad 38 thru_hole oval (at 0 45.72 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /AD4))
    (pad 39 thru_hole oval (at 2.54 48.26 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 40 thru_hole oval (at 0 48.26 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /AD5))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x20_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x05_Pitch2.54mm (layer F.Cu) (tedit 5BFE1E03)
    (at 137.795 118.11 90)
    (descr "Through hole straight pin header, 2x05, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x05 2.54mm double row")
    (fp_text reference J4 (at 1.27 -2.33 90) (layer F.SilkS))
    (fp_text value HAK (at 1.27 12.49 90) (layer F.SilkS))
    (fp_text user %R (at 1.27 5.08 180) (layer F.Fab))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 143 /PU1))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 98 /~HLDA))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 143 /PU1))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 107 /~DAK0))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 143 /PU1))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 109 /~DAK1))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 143 /PU1))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 111 /~DAK2))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 143 /PU1))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 113 /~DAK3))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x05_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_THT:SW_DIP_x6_W7.62mm_Slide (layer F.Cu) (tedit 5BFE16F1)
    (at 136.525 98.425 90)
    (descr "6x-dip-switch, Slide, row spacing 7.62 mm (300 mils)")
    (tags "DIP Switch Slide 7.62mm 300mil")
    (fp_text reference SW1 (at 3.81 -3.48 90) (layer F.SilkS))
    (fp_text value ADDR_L (at 3.81 16.18 90) (layer F.SilkS))
    (fp_text user %R (at 3.81 6.35 90) (layer F.Fab))
    (pad 12 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 142 /PD1))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 +5V))
    (pad 11 thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 134 "Net-(RN1-Pad2)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 +5V))
    (pad 10 thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 133 "Net-(RN1-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 +5V))
    (pad 9 thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 132 "Net-(RN1-Pad4)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 +5V))
    (pad 8 thru_hole oval (at 7.62 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 131 "Net-(RN1-Pad5)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 +5V))
    (pad 7 thru_hole oval (at 7.62 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 130 "Net-(RN1-Pad6)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 +5V))
    (model ${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/SW_DIP_x6_W7.62mm_Slide.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Buttons_Switches_THT:SW_DIP_x8_W7.62mm_Slide (layer F.Cu) (tedit 5BFE16EC)
    (at 109.855 98.425 90)
    (descr "8x-dip-switch, Slide, row spacing 7.62 mm (300 mils)")
    (tags "DIP Switch Slide 7.62mm 300mil")
    (fp_text reference SW2 (at 3.81 -3.48 90) (layer F.SilkS))
    (fp_text value ADDR_H (at 3.81 21.26 90) (layer F.SilkS))
    (fp_text user %R (at 3.81 8.89 90) (layer F.Fab))
    (pad 16 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 164 "Net-(RN3-Pad2)"))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 +5V))
    (pad 15 thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 141 "Net-(RN3-Pad3)"))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 +5V))
    (pad 14 thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 140 "Net-(RN3-Pad4)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 +5V))
    (pad 13 thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 139 "Net-(RN3-Pad5)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 +5V))
    (pad 12 thru_hole oval (at 7.62 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 138 "Net-(RN3-Pad6)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 +5V))
    (pad 11 thru_hole oval (at 7.62 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 137 "Net-(RN3-Pad7)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 +5V))
    (pad 10 thru_hole oval (at 7.62 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 136 "Net-(RN3-Pad8)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 +5V))
    (pad 9 thru_hole oval (at 7.62 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 135 "Net-(RN3-Pad9)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 +5V))
    (model ${KISYS3DMOD}/Buttons_Switches_THT.3dshapes/SW_DIP_x8_W7.62mm_Slide.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 197.485 99.06 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C8 (at -3.175 0 180) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 13 +5V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 132.1 60.96 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C12 (at -3.79 0 180) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 13 +5V))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 127.655 46.99 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C13 (at -3.79 0 180) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 13 +5V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 184.17 56.515 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C14 (at 0 1.905 180) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 13 +5V))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 196.87 81.28 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C15 (at -3.79 0 180) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 13 +5V))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 148.61 60.96 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C16 (at -3.79 0 180) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 13 +5V))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 165.715 99.06 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C10 (at -3.83 0 180) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 13 +5V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 139.065 46.99 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C9 (at -3.81 0 180) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 78 +3V3))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 181.61 81.28 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at -3.175 0 180) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 78 +3V3))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 153.015 49.53)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 -1.75) (layer F.SilkS))
    (fp_text value 100pF (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.75) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 146 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 147.32 49.53 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at 0 1.905 180) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 153 "Net-(C6-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 164.485 60.96 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at -3.155 0 180) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 78 +3V3))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 181.63 99.06 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C11 (at -3.79 0 180) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 13 +5V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 164.485 46.99 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at 0 -1.75 180) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 13 +5V))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 165.1 81.28 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C17 (at -3.81 0 180) (layer F.SilkS))
    (fp_text value .1uF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 180) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 13 +5V))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:CP_Tantalum_Case-B_EIA-3528-21_Hand (layer F.Cu) (tedit 58CC8C08)
    (at 106.68 127.39 270)
    (descr "Tantalum capacitor, Case B, EIA 3528-21, 3.5x2.8x1.9mm, Hand soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference C2 (at -4.835 0 180) (layer F.SilkS))
    (fp_text value 33uF (at 0 3.15 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -2.15 0 270) (size 3.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 13 +5V))
    (pad 2 smd rect (at 2.15 0 270) (size 3.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model Capacitors_Tantalum_SMD.3dshapes/CP_Tantalum_Case-B_EIA-3528-21.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:CP_Tantalum_Case-B_EIA-3528-21_Hand (layer F.Cu) (tedit 58CC8C08)
    (at 200.66 127.39 90)
    (descr "Tantalum capacitor, Case B, EIA 3528-21, 3.5x2.8x1.9mm, Hand soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference C3 (at 4.835 0) (layer F.SilkS))
    (fp_text value 33uF (at 0 3.15 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 2.15 0 90) (size 3.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -2.15 0 90) (size 3.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 78 +3V3))
    (model Capacitors_Tantalum_SMD.3dshapes/CP_Tantalum_Case-B_EIA-3528-21.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-16_W7.62mm (layer F.Cu) (tedit 5BFE16E0)
    (at 109.22 115.57 90)
    (descr "16-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference J2 (at 3.81 -2.33 90) (layer F.SilkS))
    (fp_text value INT (at 3.81 20.11 90) (layer F.SilkS))
    (fp_text user %R (at 3.81 8.89 90) (layer F.Fab))
    (pad 16 thru_hole oval (at 7.62 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 167 "Net-(J2-Pad16)"))
    (pad 8 thru_hole oval (at 0 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 117 /~IRQ7))
    (pad 15 thru_hole oval (at 7.62 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 168 "Net-(J2-Pad15)"))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 118 /~IRQ6))
    (pad 14 thru_hole oval (at 7.62 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 169 "Net-(J2-Pad14)"))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 119 /~IRQ5))
    (pad 13 thru_hole oval (at 7.62 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 170 "Net-(J2-Pad13)"))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 120 /~IRQ4))
    (pad 12 thru_hole oval (at 7.62 10.16 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 171 "Net-(J2-Pad12)"))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 121 /~IRQ3))
    (pad 11 thru_hole oval (at 7.62 12.7 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 172 "Net-(J2-Pad11)"))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 122 /~IRQ2))
    (pad 10 thru_hole oval (at 7.62 15.24 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 173 "Net-(J2-Pad10)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 123 /~IRQ1))
    (pad 9 thru_hole oval (at 7.62 17.78 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 174 "Net-(J2-Pad9)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 124 /~IRQ0))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-16_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-14_3.9x8.7mm_Pitch1.27mm (layer F.Cu) (tedit 58CC8F64)
    (at 126.365 53.34)
    (descr "14-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at -3.175 -5.715) (layer F.SilkS))
    (fp_text value 74HCT125 (at 0 5.375) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 14 smd rect (at 2.7 -3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 +5V))
    (pad 13 smd rect (at 2.7 -2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 /~CON_SI))
    (pad 12 smd rect (at 2.7 -1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 11 smd rect (at 2.7 0) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 168 "Net-(J2-Pad15)"))
    (pad 10 smd rect (at 2.7 1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 144 /~pINT))
    (pad 9 smd rect (at 2.7 2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 8 smd rect (at 2.7 3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 167 "Net-(J2-Pad16)"))
    (pad 7 smd rect (at -2.7 3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -2.7 2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 100 /~RFSH))
    (pad 5 smd rect (at -2.7 1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 145 /~pRFSH))
    (pad 4 smd rect (at -2.7 0) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 /~HAK))
    (pad 3 smd rect (at -2.7 -1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 165 "Net-(J3-Pad10)"))
    (pad 2 smd rect (at -2.7 -2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -2.7 -3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 /~HRQ))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-14_3.9x8.7mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-14_3.9x8.7mm_Pitch1.27mm (layer F.Cu) (tedit 58CC8F64)
    (at 137.795 53.34)
    (descr "14-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U2 (at -3.175 -5.715) (layer F.SilkS))
    (fp_text value 74LVC125 (at 0 5.375) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 /~HAK))
    (pad 2 smd rect (at -2.7 -2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 3 smd rect (at -2.7 -1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 104 /~MASTER))
    (pad 4 smd rect (at -2.7 0) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 5 smd rect (at -2.7 1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 /PI_REQ))
    (pad 6 smd rect (at -2.7 2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 152 /pPI_REQ))
    (pad 7 smd rect (at -2.7 3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 8 smd rect (at 2.7 3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 155 /~pCON_SO))
    (pad 9 smd rect (at 2.7 2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 21 /~CON_SO))
    (pad 10 smd rect (at 2.7 1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 11 smd rect (at 2.7 0) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 /~HAK))
    (pad 12 smd rect (at 2.7 -1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 143 /PU1))
    (pad 13 smd rect (at 2.7 -2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 /~HRQ))
    (pad 14 smd rect (at 2.7 -3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 78 +3V3))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-14_3.9x8.7mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-14_3.9x8.7mm_Pitch1.27mm (layer F.Cu) (tedit 58CC8F64)
    (at 163.195 53.34)
    (descr "14-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U7 (at -3.175 -5.715) (layer F.SilkS))
    (fp_text value 74HCT125 (at 0 5.375) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 14 smd rect (at 2.7 -3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 +5V))
    (pad 13 smd rect (at 2.7 -2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 /~STS_IOR))
    (pad 12 smd rect (at 2.7 -1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 144 /~pINT))
    (pad 11 smd rect (at 2.7 0) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 93 /D3))
    (pad 10 smd rect (at 2.7 1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 /~STS_IOR))
    (pad 9 smd rect (at 2.7 2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 /PI_REQ))
    (pad 8 smd rect (at 2.7 3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 94 /D2))
    (pad 7 smd rect (at -2.7 3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 6 smd rect (at -2.7 2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 95 /D1))
    (pad 5 smd rect (at -2.7 1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 21 /~CON_SO))
    (pad 4 smd rect (at -2.7 0) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 /~STS_IOR))
    (pad 3 smd rect (at -2.7 -1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 96 /D0))
    (pad 2 smd rect (at -2.7 -2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 /~CON_SI))
    (pad 1 smd rect (at -2.7 -3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 /~STS_IOR))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-14_3.9x8.7mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-20W_7.5x12.8mm_Pitch1.27mm (layer F.Cu) (tedit 58CC8F64)
    (at 177.8 89.535)
    (descr "20-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U4 (at -5.08 -7.62) (layer F.SilkS))
    (fp_text value 74LVC244 (at 0 7.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 20 smd rect (at 4.7 -5.715) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 78 +3V3))
    (pad 19 smd rect (at 4.7 -4.445) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 /~RD))
    (pad 18 smd rect (at 4.7 -3.175) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 /AD0))
    (pad 17 smd rect (at 4.7 -1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 92 /D4))
    (pad 16 smd rect (at 4.7 -0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 /AD1))
    (pad 15 smd rect (at 4.7 0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 91 /D5))
    (pad 14 smd rect (at 4.7 1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 /AD2))
    (pad 13 smd rect (at 4.7 3.175) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 90 /D6))
    (pad 12 smd rect (at 4.7 4.445) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 /AD3))
    (pad 11 smd rect (at 4.7 5.715) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 89 /D7))
    (pad 10 smd rect (at -4.7 5.715) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at -4.7 4.445) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 /AD7))
    (pad 8 smd rect (at -4.7 3.175) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 93 /D3))
    (pad 7 smd rect (at -4.7 1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 /AD6))
    (pad 6 smd rect (at -4.7 0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 94 /D2))
    (pad 5 smd rect (at -4.7 -0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 /AD5))
    (pad 4 smd rect (at -4.7 -1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 95 /D1))
    (pad 3 smd rect (at -4.7 -3.175) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 /AD4))
    (pad 2 smd rect (at -4.7 -4.445) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 96 /D0))
    (pad 1 smd rect (at -4.7 -5.715) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 /~RD))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-20W_7.5x12.8mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-20W_7.5x12.8mm_Pitch1.27mm (layer F.Cu) (tedit 58CC8F64)
    (at 161.29 89.535)
    (descr "20-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U5 (at -5.08 -7.62) (layer F.SilkS))
    (fp_text value 74HCT374 (at 0 7.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -4.7 -5.715) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 19 /~CON_IOR))
    (pad 2 smd rect (at -4.7 -4.445) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 96 /D0))
    (pad 3 smd rect (at -4.7 -3.175) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 /AD0))
    (pad 4 smd rect (at -4.7 -1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 /AD1))
    (pad 5 smd rect (at -4.7 -0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 95 /D1))
    (pad 6 smd rect (at -4.7 0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 94 /D2))
    (pad 7 smd rect (at -4.7 1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 /AD2))
    (pad 8 smd rect (at -4.7 3.175) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 /AD3))
    (pad 9 smd rect (at -4.7 4.445) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 93 /D3))
    (pad 10 smd rect (at -4.7 5.715) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 11 smd rect (at 4.7 5.715) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 26 /CON_W))
    (pad 12 smd rect (at 4.7 4.445) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 92 /D4))
    (pad 13 smd rect (at 4.7 3.175) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 /AD4))
    (pad 14 smd rect (at 4.7 1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 /AD5))
    (pad 15 smd rect (at 4.7 0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 91 /D5))
    (pad 16 smd rect (at 4.7 -0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 90 /D6))
    (pad 17 smd rect (at 4.7 -1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 /AD6))
    (pad 18 smd rect (at 4.7 -3.175) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 /AD7))
    (pad 19 smd rect (at 4.7 -4.445) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 89 /D7))
    (pad 20 smd rect (at 4.7 -5.715) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 +5V))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-20W_7.5x12.8mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-20W_7.5x12.8mm_Pitch1.27mm (layer F.Cu) (tedit 58CC8F64)
    (at 161.29 69.215)
    (descr "20-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U6 (at -5.08 -7.5) (layer F.SilkS))
    (fp_text value 74LVC374 (at 0 7.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 20 smd rect (at 4.7 -5.715) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 78 +3V3))
    (pad 19 smd rect (at 4.7 -4.445) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 /AD7))
    (pad 18 smd rect (at 4.7 -3.175) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 89 /D7))
    (pad 17 smd rect (at 4.7 -1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 90 /D6))
    (pad 16 smd rect (at 4.7 -0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 /AD6))
    (pad 15 smd rect (at 4.7 0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 /AD5))
    (pad 14 smd rect (at 4.7 1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 91 /D5))
    (pad 13 smd rect (at 4.7 3.175) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 92 /D4))
    (pad 12 smd rect (at 4.7 4.445) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 /AD4))
    (pad 11 smd rect (at 4.7 5.715) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 18 /CON_IOW))
    (pad 10 smd rect (at -4.7 5.715) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at -4.7 4.445) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 /AD3))
    (pad 8 smd rect (at -4.7 3.175) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 93 /D3))
    (pad 7 smd rect (at -4.7 1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 94 /D2))
    (pad 6 smd rect (at -4.7 0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 /AD2))
    (pad 5 smd rect (at -4.7 -0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 /AD1))
    (pad 4 smd rect (at -4.7 -1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 95 /D1))
    (pad 3 smd rect (at -4.7 -3.175) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 96 /D0))
    (pad 2 smd rect (at -4.7 -4.445) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 /AD0))
    (pad 1 smd rect (at -4.7 -5.715) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 25 /~CON_R))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-20W_7.5x12.8mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-20W_7.5x12.8mm_Pitch1.27mm (layer F.Cu) (tedit 58CC8F64)
    (at 193.675 89.535)
    (descr "20-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U3 (at -5.08 -7.62) (layer F.SilkS))
    (fp_text value 74HCT244 (at 0 7.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -4.7 -5.715) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 /~WR))
    (pad 2 smd rect (at -4.7 -4.445) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 /AD0))
    (pad 3 smd rect (at -4.7 -3.175) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 92 /D4))
    (pad 4 smd rect (at -4.7 -1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 /AD1))
    (pad 5 smd rect (at -4.7 -0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 91 /D5))
    (pad 6 smd rect (at -4.7 0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 /AD2))
    (pad 7 smd rect (at -4.7 1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 90 /D6))
    (pad 8 smd rect (at -4.7 3.175) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 /AD3))
    (pad 9 smd rect (at -4.7 4.445) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 89 /D7))
    (pad 10 smd rect (at -4.7 5.715) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 11 smd rect (at 4.7 5.715) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 /AD7))
    (pad 12 smd rect (at 4.7 4.445) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 93 /D3))
    (pad 13 smd rect (at 4.7 3.175) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 /AD6))
    (pad 14 smd rect (at 4.7 1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 94 /D2))
    (pad 15 smd rect (at 4.7 0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 /AD5))
    (pad 16 smd rect (at 4.7 -0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 95 /D1))
    (pad 17 smd rect (at 4.7 -1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 /AD4))
    (pad 18 smd rect (at 4.7 -3.175) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 96 /D0))
    (pad 19 smd rect (at 4.7 -4.445) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 /~WR))
    (pad 20 smd rect (at 4.7 -5.715) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 +5V))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-20W_7.5x12.8mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-20W_7.5x12.8mm_Pitch1.27mm (layer F.Cu) (tedit 58CC8F64)
    (at 161.925 107.315)
    (descr "20-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U8 (at -5.08 -7.5) (layer F.SilkS))
    (fp_text value 74HCT374 (at 0 7.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 20 smd rect (at 4.7 -5.715) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 +5V))
    (pad 19 smd rect (at 4.7 -4.445) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 49 /A7))
    (pad 18 smd rect (at 4.7 -3.175) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 /AD7))
    (pad 17 smd rect (at 4.7 -1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 /AD6))
    (pad 16 smd rect (at 4.7 -0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 50 /A6))
    (pad 15 smd rect (at 4.7 0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 51 /A5))
    (pad 14 smd rect (at 4.7 1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 /AD5))
    (pad 13 smd rect (at 4.7 3.175) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 /AD4))
    (pad 12 smd rect (at 4.7 4.445) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 52 /A4))
    (pad 11 smd rect (at 4.7 5.715) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 159 /ALE_L))
    (pad 10 smd rect (at -4.7 5.715) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at -4.7 4.445) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 53 /A3))
    (pad 8 smd rect (at -4.7 3.175) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 /AD3))
    (pad 7 smd rect (at -4.7 1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 /AD2))
    (pad 6 smd rect (at -4.7 0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 54 /A2))
    (pad 5 smd rect (at -4.7 -0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 30 /A1))
    (pad 4 smd rect (at -4.7 -1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 /AD1))
    (pad 3 smd rect (at -4.7 -3.175) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 /AD0))
    (pad 2 smd rect (at -4.7 -4.445) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 29 /A0))
    (pad 1 smd rect (at -4.7 -5.715) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 /~HAK))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-20W_7.5x12.8mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-20W_7.5x12.8mm_Pitch1.27mm (layer F.Cu) (tedit 58CC8F64)
    (at 177.8 107.315)
    (descr "20-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U9 (at -5.08 -7.62) (layer F.SilkS))
    (fp_text value 74HCT374 (at 0 7.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -4.7 -5.715) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 /~HAK))
    (pad 2 smd rect (at -4.7 -4.445) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 48 /A8))
    (pad 3 smd rect (at -4.7 -3.175) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 /AD0))
    (pad 4 smd rect (at -4.7 -1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 /AD1))
    (pad 5 smd rect (at -4.7 -0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 47 /A9))
    (pad 6 smd rect (at -4.7 0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 46 /A10))
    (pad 7 smd rect (at -4.7 1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 /AD2))
    (pad 8 smd rect (at -4.7 3.175) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 /AD3))
    (pad 9 smd rect (at -4.7 4.445) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 45 /A11))
    (pad 10 smd rect (at -4.7 5.715) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 11 smd rect (at 4.7 5.715) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 156 /ALE_H))
    (pad 12 smd rect (at 4.7 4.445) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 44 /A12))
    (pad 13 smd rect (at 4.7 3.175) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 /AD4))
    (pad 14 smd rect (at 4.7 1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 /AD5))
    (pad 15 smd rect (at 4.7 0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 43 /A13))
    (pad 16 smd rect (at 4.7 -0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 42 /A14))
    (pad 17 smd rect (at 4.7 -1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 /AD6))
    (pad 18 smd rect (at 4.7 -3.175) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 /AD7))
    (pad 19 smd rect (at 4.7 -4.445) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 41 /A15))
    (pad 20 smd rect (at 4.7 -5.715) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 +5V))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-20W_7.5x12.8mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-20W_7.5x12.8mm_Pitch1.27mm (layer F.Cu) (tedit 58CC8F64)
    (at 193.675 107.315)
    (descr "20-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U10 (at -4.445 -7.62) (layer F.SilkS))
    (fp_text value 74HCT374 (at 0 7.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -4.7 -5.715) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 /~HAK))
    (pad 2 smd rect (at -4.7 -4.445) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 40 /A16))
    (pad 3 smd rect (at -4.7 -3.175) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 /AD0))
    (pad 4 smd rect (at -4.7 -1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 /AD1))
    (pad 5 smd rect (at -4.7 -0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 39 /A17))
    (pad 6 smd rect (at -4.7 0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 38 /A18))
    (pad 7 smd rect (at -4.7 1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 /AD2))
    (pad 8 smd rect (at -4.7 3.175) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 /AD3))
    (pad 9 smd rect (at -4.7 4.445) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 37 /A19))
    (pad 10 smd rect (at -4.7 5.715) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 11 smd rect (at 4.7 5.715) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 154 /ALE_X))
    (pad 12 smd rect (at 4.7 4.445) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 36 /A20))
    (pad 13 smd rect (at 4.7 3.175) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 /AD4))
    (pad 14 smd rect (at 4.7 1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 /AD5))
    (pad 15 smd rect (at 4.7 0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 35 /A21))
    (pad 16 smd rect (at 4.7 -0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 34 /A22))
    (pad 17 smd rect (at 4.7 -1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 /AD6))
    (pad 18 smd rect (at 4.7 -3.175) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 /AD7))
    (pad 19 smd rect (at 4.7 -4.445) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 33 /A23))
    (pad 20 smd rect (at 4.7 -5.715) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 +5V))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-20W_7.5x12.8mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-20W_7.5x12.8mm_Pitch1.27mm (layer F.Cu) (tedit 58CC8F64)
    (at 144.78 69.215)
    (descr "20-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U12 (at -4.445 -7.5) (layer F.SilkS))
    (fp_text value 74HCT688 (at 0 7.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -4.7 -5.715) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 163 "Net-(U12-Pad1)"))
    (pad 2 smd rect (at -4.7 -4.445) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 105 /~AEN))
    (pad 3 smd rect (at -4.7 -3.175) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 +5V))
    (pad 4 smd rect (at -4.7 -1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 +5V))
    (pad 5 smd rect (at -4.7 -0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 +5V))
    (pad 6 smd rect (at -4.7 0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 49 /A7))
    (pad 7 smd rect (at -4.7 1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 142 /PD1))
    (pad 8 smd rect (at -4.7 3.175) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 50 /A6))
    (pad 9 smd rect (at -4.7 4.445) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 134 "Net-(RN1-Pad2)"))
    (pad 10 smd rect (at -4.7 5.715) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 11 smd rect (at 4.7 5.715) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 51 /A5))
    (pad 12 smd rect (at 4.7 4.445) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 133 "Net-(RN1-Pad3)"))
    (pad 13 smd rect (at 4.7 3.175) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 52 /A4))
    (pad 14 smd rect (at 4.7 1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 132 "Net-(RN1-Pad4)"))
    (pad 15 smd rect (at 4.7 0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 53 /A3))
    (pad 16 smd rect (at 4.7 -0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 131 "Net-(RN1-Pad5)"))
    (pad 17 smd rect (at 4.7 -1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 54 /A2))
    (pad 18 smd rect (at 4.7 -3.175) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 130 "Net-(RN1-Pad6)"))
    (pad 19 smd rect (at 4.7 -4.445) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(U12-Pad19)"))
    (pad 20 smd rect (at 4.7 -5.715) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 +5V))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-20W_7.5x12.8mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-20W_7.5x12.8mm_Pitch1.27mm (layer F.Cu) (tedit 58CC8F64)
    (at 128.27 69.215)
    (descr "20-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U13 (at -5.08 -7.5) (layer F.SilkS))
    (fp_text value 74HCT688 (at 0 7.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 20 smd rect (at 4.7 -5.715) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 +5V))
    (pad 19 smd rect (at 4.7 -4.445) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 163 "Net-(U12-Pad1)"))
    (pad 18 smd rect (at 4.7 -3.175) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 135 "Net-(RN3-Pad9)"))
    (pad 17 smd rect (at 4.7 -1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 48 /A8))
    (pad 16 smd rect (at 4.7 -0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 136 "Net-(RN3-Pad8)"))
    (pad 15 smd rect (at 4.7 0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 47 /A9))
    (pad 14 smd rect (at 4.7 1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 137 "Net-(RN3-Pad7)"))
    (pad 13 smd rect (at 4.7 3.175) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 46 /A10))
    (pad 12 smd rect (at 4.7 4.445) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 138 "Net-(RN3-Pad6)"))
    (pad 11 smd rect (at 4.7 5.715) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 45 /A11))
    (pad 10 smd rect (at -4.7 5.715) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 9 smd rect (at -4.7 4.445) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 139 "Net-(RN3-Pad5)"))
    (pad 8 smd rect (at -4.7 3.175) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 44 /A12))
    (pad 7 smd rect (at -4.7 1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 140 "Net-(RN3-Pad4)"))
    (pad 6 smd rect (at -4.7 0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 43 /A13))
    (pad 5 smd rect (at -4.7 -0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 141 "Net-(RN3-Pad3)"))
    (pad 4 smd rect (at -4.7 -1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 42 /A14))
    (pad 3 smd rect (at -4.7 -3.175) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 164 "Net-(RN3-Pad2)"))
    (pad 2 smd rect (at -4.7 -4.445) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 41 /A15))
    (pad 1 smd rect (at -4.7 -5.715) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-20W_7.5x12.8mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm (layer F.Cu) (tedit 58CD0CDA)
    (at 150.495 55.245)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U11 (at 0 -3.5) (layer F.SilkS))
    (fp_text value PCA9306 (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 8 smd rect (at 2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 146 "Net-(C1-Pad1)"))
    (pad 7 smd rect (at 2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 146 "Net-(C1-Pad1)"))
    (pad 6 smd rect (at 2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 129 /SCL))
    (pad 5 smd rect (at 2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 128 /SDA))
    (pad 4 smd rect (at -2.7 1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 148 "Net-(J6-Pad3)"))
    (pad 3 smd rect (at -2.7 0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 149 "Net-(J6-Pad5)"))
    (pad 2 smd rect (at -2.7 -0.635) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 153 "Net-(C6-Pad1)"))
    (pad 1 smd rect (at -2.7 -1.905) (size 1.55 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_2.7mm_Pad_Via locked (layer F.Cu) (tedit 56DDBBFF)
    (at 110.099 39.2938 90)
    (descr "Mounting Hole 2.7mm")
    (tags "mounting hole 2.7mm")
    (zone_connect 2)
    (attr virtual)
    (fp_text reference J8 (at 0 -3.7 90) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 3.7 90) (layer F.Fab))
    (fp_text user %R (at 0.3 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 5.4 5.4) (drill 2.7) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 2.025 0 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 1.431891 1.431891 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 0 2.025 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at -1.431891 1.431891 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at -2.025 0 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at -1.431891 -1.431891 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 0 -2.025 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 1.431891 -1.431891 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
  )
  (module Mounting_Holes:MountingHole_2.7mm_Pad_Via locked (layer F.Cu) (tedit 56DDBBFF)
    (at 168.099 39.2938 90)
    (descr "Mounting Hole 2.7mm")
    (tags "mounting hole 2.7mm")
    (zone_connect 2)
    (attr virtual)
    (fp_text reference J9 (at 0 -3.7 90) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 3.7 90) (layer F.Fab))
    (fp_text user %R (at 0.3 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.431891 -1.431891 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 0 -2.025 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at -1.431891 -1.431891 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at -2.025 0 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at -1.431891 1.431891 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 0 2.025 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 1.431891 1.431891 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 2.025 0 90) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
    (pad 1 thru_hole circle (at 0 0 90) (size 5.4 5.4) (drill 2.7) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
  )
  (module Pin_Headers:Pin_Header_Angled_1x06_Pitch2.54mm locked (layer F.Cu) (tedit 59650532)
    (at 193.04 36.83)
    (descr "Through hole angled pin header, 1x06, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x06 2.54mm single row")
    (fp_text reference J5 (at 2.54 6.35 90) (layer F.SilkS))
    (fp_text value FTDI_3.3V (at 4.385 14.97) (layer F.Fab))
    (fp_text user %R (at 2.77 6.35 90) (layer F.Fab))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 160 "Net-(J5-Pad6)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 150 "Net-(J5-Pad5)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 151 "Net-(J5-Pad4)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 161 "Net-(J5-Pad3)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 162 "Net-(J5-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Angled_1x06_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 5BFDFF6F)
    (at 186.69 119.38 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference J7 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value "PI PWR" (at 2.54 2.54 180) (layer F.SilkS))
    (fp_text user %R (at 0 2.54 180) (layer F.Fab))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 +5V))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 166 /PIPWR))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 79 /+5VSB))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x05_Pitch2.54mm (layer F.Cu) (tedit 5BFE16D4)
    (at 137.795 109.22 90)
    (descr "Through hole straight pin header, 2x05, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x05 2.54mm double row")
    (fp_text reference J3 (at 1.27 -2.33 90) (layer F.SilkS))
    (fp_text value HRQ (at 1.27 12.49 90) (layer F.SilkS))
    (fp_text user %R (at 1.27 5.08 180) (layer F.Fab))
    (pad 10 thru_hole oval (at 2.54 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 165 "Net-(J3-Pad10)"))
    (pad 9 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 97 /~HOLD))
    (pad 8 thru_hole oval (at 2.54 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 165 "Net-(J3-Pad10)"))
    (pad 7 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 106 /~DRQ0))
    (pad 6 thru_hole oval (at 2.54 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 165 "Net-(J3-Pad10)"))
    (pad 5 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 108 /~DRQ1))
    (pad 4 thru_hole oval (at 2.54 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 165 "Net-(J3-Pad10)"))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 110 /~DRQ2))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 165 "Net-(J3-Pad10)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 112 /~DRQ3))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x05_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 153.115 45.72)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 -1.7) (layer F.SilkS))
    (fp_text value 200K (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 166 /PIPWR))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 146 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Array_SIP10 (layer F.Cu) (tedit 57FA3974)
    (at 126.365 80.645)
    (descr "10-pin Resistor SIP pack")
    (tags R)
    (fp_text reference RN2 (at 12.7 -2.4) (layer F.SilkS))
    (fp_text value 10k (at 12.7 2.4) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 78 +3V3))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 145 /~pRFSH))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 28 /~HRQ))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 144 /~pINT))
    (pad 5 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 /~RD))
    (pad 6 thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 143 /PU1))
    (pad 7 thru_hole oval (at 15.24 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 27 /~HAK))
    (pad 8 thru_hole oval (at 17.78 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 175 "Net-(RN2-Pad8)"))
    (pad 9 thru_hole oval (at 20.32 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 /~CON_R))
    (pad 10 thru_hole oval (at 22.86 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 /~WR))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Array_SIP10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Array_SIP10 (layer F.Cu) (tedit 57FA3974)
    (at 107.315 85.725)
    (descr "10-pin Resistor SIP pack")
    (tags R)
    (fp_text reference RN3 (at 12.7 -2.4) (layer F.SilkS))
    (fp_text value 10k (at 12.7 2.4) (layer F.Fab))
    (pad 10 thru_hole oval (at 22.86 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 142 /PD1))
    (pad 9 thru_hole oval (at 20.32 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 135 "Net-(RN3-Pad9)"))
    (pad 8 thru_hole oval (at 17.78 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 136 "Net-(RN3-Pad8)"))
    (pad 7 thru_hole oval (at 15.24 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 137 "Net-(RN3-Pad7)"))
    (pad 6 thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 138 "Net-(RN3-Pad6)"))
    (pad 5 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 139 "Net-(RN3-Pad5)"))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 140 "Net-(RN3-Pad4)"))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 141 "Net-(RN3-Pad3)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 164 "Net-(RN3-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Array_SIP10.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_THT:R_Array_SIP6 (layer F.Cu) (tedit 57FA3974)
    (at 136.525 85.725)
    (descr "6-pin Resistor SIP pack")
    (tags R)
    (fp_text reference RN1 (at 7.62 -2.4) (layer F.SilkS))
    (fp_text value 10k (at 7.62 2.4) (layer F.Fab))
    (pad 6 thru_hole oval (at 12.7 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 130 "Net-(RN1-Pad6)"))
    (pad 5 thru_hole oval (at 10.16 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 131 "Net-(RN1-Pad5)"))
    (pad 4 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 132 "Net-(RN1-Pad4)"))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 133 "Net-(RN1-Pad3)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 134 "Net-(RN1-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Array_SIP6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.39 0.39 0.39))
      (rotate (xyz 0 0 0))
    )
  )
  (module SamacSys_Parts:JAE_TX24-120R-LT-H1E locked (layer F.Cu) (tedit 5BE48DC8)
    (at 153.67 131.953 180)
    (descr JAE_TX24-120R-LT-H1E)
    (tags Connector)
    (fp_text reference J1 (at -5.0546 -9.017 180) (layer F.SilkS))
    (fp_text value CheapBusTX24-RA (at -5.0546 -9.017 180) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -38.1 6.858 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 2 thru_hole circle (at -36.83 4.953 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 3 thru_hole circle (at -35.56 6.858 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 4 thru_hole circle (at -34.29 4.953 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 5 thru_hole circle (at -33.02 6.858 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 6 thru_hole circle (at -31.75 4.953 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 33 /A23))
    (pad 7 thru_hole circle (at -30.48 6.858 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 34 /A22))
    (pad 8 thru_hole circle (at -29.21 4.953 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 35 /A21))
    (pad 9 thru_hole circle (at -27.94 6.858 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 36 /A20))
    (pad 10 thru_hole circle (at -26.67 4.953 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 37 /A19))
    (pad 11 thru_hole circle (at -25.4 6.858 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 38 /A18))
    (pad 12 thru_hole circle (at -24.13 4.953 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 39 /A17))
    (pad 13 thru_hole circle (at -22.86 6.858 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 40 /A16))
    (pad 14 thru_hole circle (at -21.59 4.953 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 41 /A15))
    (pad 15 thru_hole circle (at -20.32 6.858 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 42 /A14))
    (pad 16 thru_hole circle (at -19.05 4.953 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 43 /A13))
    (pad 17 thru_hole circle (at -17.78 6.858 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 44 /A12))
    (pad 18 thru_hole circle (at -16.51 4.953 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 45 /A11))
    (pad 19 thru_hole circle (at -15.24 6.858 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 46 /A10))
    (pad 20 thru_hole circle (at -13.97 4.953 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 47 /A9))
    (pad 21 thru_hole circle (at -12.7 6.858 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 48 /A8))
    (pad 22 thru_hole circle (at -11.43 4.953 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 49 /A7))
    (pad 23 thru_hole circle (at -10.16 6.858 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 50 /A6))
    (pad 24 thru_hole circle (at -8.89 4.953 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 51 /A5))
    (pad 25 thru_hole circle (at -7.62 6.858 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 52 /A4))
    (pad 26 thru_hole circle (at -6.35 4.953 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 53 /A3))
    (pad 27 thru_hole circle (at -5.08 6.858 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 54 /A2))
    (pad 28 thru_hole circle (at -3.81 4.953 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 30 /A1))
    (pad 29 thru_hole circle (at -2.54 6.858 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 29 /A0))
    (pad 30 thru_hole circle (at -1.27 4.953 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 14 /~IOR))
    (pad 31 thru_hole circle (at 0 6.858 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 15 /~IOW))
    (pad 32 thru_hole circle (at 1.27 4.953 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 16 /~MEMR))
    (pad 33 thru_hole circle (at 2.54 6.858 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 17 /~MEMW))
    (pad 34 thru_hole circle (at 3.81 4.953 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 55 "Net-(J1-Pad34)"))
    (pad 35 thru_hole circle (at 5.08 6.858 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 56 "Net-(J1-Pad35)"))
    (pad 36 thru_hole circle (at 6.35 4.953 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 57 "Net-(J1-Pad36)"))
    (pad 37 thru_hole circle (at 7.62 6.858 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 58 "Net-(J1-Pad37)"))
    (pad 38 thru_hole circle (at 8.89 4.953 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 59 "Net-(J1-Pad38)"))
    (pad 39 thru_hole circle (at 10.16 6.858 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 60 "Net-(J1-Pad39)"))
    (pad 40 thru_hole circle (at 11.43 4.953 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 61 "Net-(J1-Pad40)"))
    (pad 41 thru_hole circle (at 12.7 6.858 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 62 "Net-(J1-Pad41)"))
    (pad 42 thru_hole circle (at 13.97 4.953 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 63 "Net-(J1-Pad42)"))
    (pad 43 thru_hole circle (at 15.24 6.858 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 64 "Net-(J1-Pad43)"))
    (pad 44 thru_hole circle (at 16.51 4.953 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 65 "Net-(J1-Pad44)"))
    (pad 45 thru_hole circle (at 17.78 6.858 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 66 "Net-(J1-Pad45)"))
    (pad 46 thru_hole circle (at 19.05 4.953 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 67 "Net-(J1-Pad46)"))
    (pad 47 thru_hole circle (at 20.32 6.858 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 68 "Net-(J1-Pad47)"))
    (pad 48 thru_hole circle (at 21.59 4.953 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 69 "Net-(J1-Pad48)"))
    (pad 49 thru_hole circle (at 22.86 6.858 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 70 "Net-(J1-Pad49)"))
    (pad 50 thru_hole circle (at 24.13 4.953 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 71 "Net-(J1-Pad50)"))
    (pad 51 thru_hole circle (at 25.4 6.858 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 72 "Net-(J1-Pad51)"))
    (pad 52 thru_hole circle (at 26.67 4.953 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 73 "Net-(J1-Pad52)"))
    (pad 53 thru_hole circle (at 27.94 6.858 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 74 "Net-(J1-Pad53)"))
    (pad 54 thru_hole circle (at 29.21 4.953 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 75 "Net-(J1-Pad54)"))
    (pad 55 thru_hole circle (at 30.48 6.858 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 76 "Net-(J1-Pad55)"))
    (pad 56 thru_hole circle (at 31.75 4.953 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 77 "Net-(J1-Pad56)"))
    (pad 57 thru_hole circle (at 33.02 6.858 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 78 +3V3))
    (pad 58 thru_hole circle (at 34.29 4.953 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 13 +5V))
    (pad 59 thru_hole circle (at 35.56 6.858 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 13 +5V))
    (pad 60 thru_hole circle (at 36.83 4.953 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 13 +5V))
    (pad 61 thru_hole circle (at -38.1 3.048 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 13 +5V))
    (pad 62 thru_hole circle (at -36.83 1.143 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 13 +5V))
    (pad 63 thru_hole circle (at -35.56 3.048 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 79 /+5VSB))
    (pad 64 thru_hole circle (at -34.29 1.143 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 78 +3V3))
    (pad 65 thru_hole circle (at -33.02 3.048 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 80 "Net-(J1-Pad65)"))
    (pad 66 thru_hole circle (at -31.75 1.143 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 81 "Net-(J1-Pad66)"))
    (pad 67 thru_hole circle (at -30.48 3.048 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 82 "Net-(J1-Pad67)"))
    (pad 68 thru_hole circle (at -29.21 1.143 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 83 "Net-(J1-Pad68)"))
    (pad 69 thru_hole circle (at -27.94 3.048 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 84 "Net-(J1-Pad69)"))
    (pad 70 thru_hole circle (at -26.67 1.143 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 85 "Net-(J1-Pad70)"))
    (pad 71 thru_hole circle (at -25.4 3.048 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 86 "Net-(J1-Pad71)"))
    (pad 72 thru_hole circle (at -24.13 1.143 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 87 "Net-(J1-Pad72)"))
    (pad 73 thru_hole circle (at -22.86 3.048 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 88 "Net-(J1-Pad73)"))
    (pad 74 thru_hole circle (at -21.59 1.143 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 89 /D7))
    (pad 75 thru_hole circle (at -20.32 3.048 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 90 /D6))
    (pad 76 thru_hole circle (at -19.05 1.143 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 91 /D5))
    (pad 77 thru_hole circle (at -17.78 3.048 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 92 /D4))
    (pad 78 thru_hole circle (at -16.51 1.143 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 93 /D3))
    (pad 79 thru_hole circle (at -15.24 3.048 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 94 /D2))
    (pad 80 thru_hole circle (at -13.97 1.143 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 95 /D1))
    (pad 81 thru_hole circle (at -12.7 3.048 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 96 /D0))
    (pad 82 thru_hole circle (at -11.43 1.143 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 97 /~HOLD))
    (pad 83 thru_hole circle (at -10.16 3.048 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 98 /~HLDA))
    (pad 84 thru_hole circle (at -8.89 1.143 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 99 "Net-(J1-Pad84)"))
    (pad 85 thru_hole circle (at -7.62 3.048 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 100 /~RFSH))
    (pad 86 thru_hole circle (at -6.35 1.143 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 101 "Net-(J1-Pad86)"))
    (pad 87 thru_hole circle (at -5.08 3.048 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 102 "Net-(J1-Pad87)"))
    (pad 88 thru_hole circle (at -3.81 1.143 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 103 "Net-(J1-Pad88)"))
    (pad 89 thru_hole circle (at -2.54 3.048 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 104 /~MASTER))
    (pad 90 thru_hole circle (at -1.27 1.143 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 105 /~AEN))
    (pad 91 thru_hole circle (at 0 3.048 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 106 /~DRQ0))
    (pad 92 thru_hole circle (at 1.27 1.143 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 107 /~DAK0))
    (pad 93 thru_hole circle (at 2.54 3.048 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 108 /~DRQ1))
    (pad 94 thru_hole circle (at 3.81 1.143 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 109 /~DAK1))
    (pad 95 thru_hole circle (at 5.08 3.048 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 110 /~DRQ2))
    (pad 96 thru_hole circle (at 6.35 1.143 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 111 /~DAK2))
    (pad 97 thru_hole circle (at 7.62 3.048 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 112 /~DRQ3))
    (pad 98 thru_hole circle (at 8.89 1.143 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 113 /~DAK3))
    (pad 99 thru_hole circle (at 10.16 3.048 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 114 "Net-(J1-Pad99)"))
    (pad 100 thru_hole circle (at 11.43 1.143 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 115 "Net-(J1-Pad100)"))
    (pad 101 thru_hole circle (at 12.7 3.048 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 116 "Net-(J1-Pad101)"))
    (pad 102 thru_hole circle (at 13.97 1.143 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 117 /~IRQ7))
    (pad 103 thru_hole circle (at 15.24 3.048 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 118 /~IRQ6))
    (pad 104 thru_hole circle (at 16.51 1.143 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 119 /~IRQ5))
    (pad 105 thru_hole circle (at 17.78 3.048 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 120 /~IRQ4))
    (pad 106 thru_hole circle (at 19.05 1.143 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 121 /~IRQ3))
    (pad 107 thru_hole circle (at 20.32 3.048 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 122 /~IRQ2))
    (pad 108 thru_hole circle (at 21.59 1.143 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 123 /~IRQ1))
    (pad 109 thru_hole circle (at 22.86 3.048 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 124 /~IRQ0))
    (pad 110 thru_hole circle (at 24.13 1.143 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 125 "Net-(J1-Pad110)"))
    (pad 111 thru_hole circle (at 25.4 3.048 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 126 "Net-(J1-Pad111)"))
    (pad 112 thru_hole circle (at 26.67 1.143 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 127 "Net-(J1-Pad112)"))
    (pad 113 thru_hole circle (at 27.94 3.048 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 128 /SDA))
    (pad 114 thru_hole circle (at 29.21 1.143 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 129 /SCL))
    (pad 115 thru_hole circle (at 30.48 3.048 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 24 /~RESET))
    (pad 116 thru_hole circle (at 31.75 1.143 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 117 thru_hole circle (at 33.02 3.048 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 118 thru_hole circle (at 34.29 1.143 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 119 thru_hole circle (at 35.56 3.048 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 120 thru_hole circle (at 36.83 1.143 270) (size 1.2192 1.2192) (drill 0.8128) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
    (pad 121 thru_hole circle (at -42.545 1.143 270) (size 3.3147 3.3147) (drill 2.2098) (layers *.Cu *.Mask F.SilkS)
      (net 176 "Net-(J1-Pad121)"))
    (pad 122 thru_hole circle (at 42.545 1.143 270) (size 3.3147 3.3147) (drill 2.2098) (layers *.Cu *.Mask F.SilkS)
      (net 1 GND))
  )
  (module Sockets:PLCC28 (layer F.Cu) (tedit 0)
    (at 184.15 67.31)
    (descr "Support Plcc 28 pins, pads ronds")
    (tags PLCC)
    (fp_text reference U14 (at 1.27 10.16) (layer F.SilkS))
    (fp_text value 22V10-PLCC (at 0 0) (layer F.Fab))
    (pad 28 thru_hole circle (at 1.27 -6.35) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 13 +5V))
    (pad 27 thru_hole circle (at 3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 14 /~IOR))
    (pad 26 thru_hole circle (at 3.81 -6.35) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 15 /~IOW))
    (pad 25 thru_hole circle (at 6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 16 /~MEMR))
    (pad 24 thru_hole circle (at 3.81 -1.27) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 17 /~MEMW))
    (pad 23 thru_hole circle (at 6.35 -1.27) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 12 /PI_REQ))
    (pad 22 thru_hole circle (at 3.81 1.27) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 21 thru_hole circle (at 6.35 1.27) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 18 /CON_IOW))
    (pad 20 thru_hole circle (at 3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 19 /~CON_IOR))
    (pad 19 thru_hole circle (at 6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 20 /~STS_IOR))
    (pad 18 thru_hole circle (at 3.81 6.35) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 21 /~CON_SO))
    (pad 17 thru_hole circle (at 1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 22 /~CON_SI))
    (pad 16 thru_hole circle (at 1.27 6.35) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 23 "Net-(U14-Pad16)"))
    (pad 15 thru_hole circle (at -1.27 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 14 thru_hole circle (at -1.27 6.35) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 13 thru_hole circle (at -3.81 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 24 /~RESET))
    (pad 12 thru_hole circle (at -3.81 6.35) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 25 /~CON_R))
    (pad 11 thru_hole circle (at -6.35 3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 26 /CON_W))
    (pad 10 thru_hole circle (at -3.81 1.27) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 27 /~HAK))
    (pad 9 thru_hole circle (at -6.35 1.27) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 28 /~HRQ))
    (pad 8 thru_hole circle (at -3.81 -1.27) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole circle (at -6.35 -1.27) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 29 /A0))
    (pad 6 thru_hole circle (at -3.81 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 30 /A1))
    (pad 5 thru_hole circle (at -6.35 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 31 "Net-(U12-Pad19)"))
    (pad 4 thru_hole circle (at -3.81 -6.35) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 10 /~RD))
    (pad 3 thru_hole circle (at -1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 11 /~WR))
    (pad 2 thru_hole circle (at -1.27 -6.35) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 32 /IO~M))
    (pad 1 thru_hole rect (at 1.27 -3.81) (size 1.397 1.397) (drill 0.8128) (layers *.Cu *.Mask)
      (net 13 +5V))
  )
  (gr_text H (at 147.955 112.395 90) (layer F.SilkS))
  (gr_text 0 (at 145.415 112.395 90) (layer F.SilkS))
  (gr_text 1 (at 142.875 112.395 90) (layer F.SilkS))
  (gr_text 2 (at 140.335 112.395 90) (layer F.SilkS))
  (gr_text 3 (at 137.795 112.395 90) (layer F.SilkS))
  (gr_text CON (at 111.76 105.41 90) (layer F.SilkS))
  (gr_text PI (at 109.22 105.41 90) (layer F.SilkS))
  (gr_text IRQ7 (at 127 118.745 90) (layer F.SilkS))
  (gr_text IRQ6 (at 124.46 118.745 90) (layer F.SilkS))
  (gr_text IRQ5 (at 121.92 118.745 90) (layer F.SilkS))
  (gr_text IRQ4 (at 119.38 118.745 90) (layer F.SilkS))
  (gr_text IRQ3 (at 116.84 118.745 90) (layer F.SilkS))
  (gr_text IRQ2 (at 114.3 118.745 90) (layer F.SilkS))
  (gr_text IRQ1 (at 111.76 118.745 90) (layer F.SilkS))
  (gr_text IRQ0 (at 109.22 118.745 90) (layer F.SilkS))
  (gr_text A2 (at 149.225 100.965 90) (layer F.SilkS))
  (gr_text A3 (at 146.685 100.965 90) (layer F.SilkS))
  (gr_text A4 (at 144.145 100.965 90) (layer F.SilkS))
  (gr_text A5 (at 141.605 100.965 90) (layer F.SilkS))
  (gr_text A6 (at 139.065 100.965 90) (layer F.SilkS))
  (gr_text A7 (at 136.525 100.965 90) (layer F.SilkS))
  (gr_text A8 (at 127.635 100.965 90) (layer F.SilkS))
  (gr_text A9 (at 125.095 100.965 90) (layer F.SilkS))
  (gr_text A10 (at 122.555 101.6 90) (layer F.SilkS))
  (gr_text A11 (at 120.015 101.6 90) (layer F.SilkS))
  (gr_text A12 (at 117.475 101.6 90) (layer F.SilkS))
  (gr_text A13 (at 114.935 101.6 90) (layer F.SilkS))
  (gr_text A14 (at 112.395 101.6 90) (layer F.SilkS))
  (gr_text A15 (at 109.855 101.6 90) (layer F.SilkS))
  (gr_text NC (at 189.865 49.53) (layer F.SilkS))
  (gr_text TXD (at 189.865 46.99) (layer F.SilkS))
  (gr_text RXD (at 189.865 44.45) (layer F.SilkS))
  (gr_text NC (at 189.865 41.91) (layer F.SilkS))
  (gr_text NC (at 189.865 39.37) (layer F.SilkS))
  (gr_text GND (at 189.865 36.83) (layer F.SilkS))
  (gr_text "PI CONSOLE" (at 196.215 34.29) (layer F.SilkS))
  (gr_text "3.3V IO\nNOT 5V TOLERANT!" (at 196.215 52.705) (layer F.SilkS))
  (gr_text "5VSB  5V" (at 189.23 121.92) (layer F.SilkS))
  (gr_line (start 203.505 133.02) (end 203.505 33.02) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 103.505 133.02) (end 203.505 133.02) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 103.505 33.02) (end 203.505 33.02) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 103.505 133.02) (end 103.505 33.02) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 103.505 33.02) (xy 203.835 33.02) (xy 203.835 133.35) (xy 103.505 133.35)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.3))
    (polygon
      (pts
        (xy 103.505 33.02) (xy 203.835 33.02) (xy 203.835 133.35) (xy 103.505 133.35)
      )
    )
  )
)
