(kicad_pcb (version 4) (host pcbnew 4.0.0-rc1-stable)
  (general
    (links 1256)
    (no_connects 35)
    (area 27.404999 57.649999 143.855001 174.100001)
    (thickness 1.6)
    (drawings 27)
    (tracks 179)
    (zones 0)
    (modules 17)
    (nets 12)
  )
  (page USLetter)
  (title_block
    (title LED2GrOMato)
    (rev 1D)
    (company Air2IT)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 1.4)
    (trace_clearance 1)
    (zone_clearance 2)
    (zone_45_only no)
    (trace_min 0.635)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 2)
    (via_drill 1)
    (via_min_size 1)
    (via_min_drill 1)
    (uvia_size 1.8)
    (uvia_drill 1)
    (uvias_allowed no)
    (uvia_min_size 1.6941)
    (uvia_min_drill 0.7924)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 5 5)
    (pad_drill 2)
    (pad_to_mask_clearance 0)
    (pad_to_paste_clearance -0.003)
    (aux_axis_origin 36.1 167.945)
    (grid_origin 36.1 167.945)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_80000001)
      (usegerberextensions true)
      (excludeedgelayer false)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin true)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(D101-Pad1)")
  (net 3 "Net-(D102-Pad2)")
  (net 4 VPP)
  (net 5 "Net-(D105-Pad1)")
  (net 6 "Net-(F101-Pad1)")
  (net 7 "Net-(D106-Pad2)")
  (net 8 GNDPWR)
  (net 9 "Net-(D103-Pad1)")
  (net 10 "Net-(D104-Pad2)")
  (net 11 "Net-(D107-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 1)
    (trace_width 1.4)
    (via_dia 2)
    (via_drill 1)
    (uvia_dia 1.8)
    (uvia_drill 1)
    (add_net GND)
    (add_net GNDPWR)
    (add_net "Net-(D101-Pad1)")
    (add_net "Net-(D102-Pad2)")
    (add_net "Net-(D103-Pad1)")
    (add_net "Net-(D104-Pad2)")
    (add_net "Net-(D105-Pad1)")
    (add_net "Net-(D106-Pad2)")
    (add_net "Net-(D107-Pad1)")
    (add_net "Net-(F101-Pad1)")
    (add_net VPP)
  )
  (module switchbox:switchbox (layer F.Cu) (tedit 577E95D8)
    (at 85.63 115.875)
    (fp_text reference U101 (at 2.54 55.88) (layer F.SilkS))
    (fp_text value electricalboxhole (at 1.27 -54.61) (layer F.Fab))
    (pad 2 thru_hole circle (at 54 -35) (size 5 5) (drill 4) (layers *.Cu *.Mask F.SilkS)
      (net 8 GNDPWR))
    (pad 4 thru_hole circle (at 54 35) (size 5 5) (drill 4) (layers *.Cu *.Mask F.SilkS)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -54 35) (size 5 5) (drill 4) (layers *.Cu *.Mask F.SilkS)
      (net 8 GNDPWR))
    (pad 1 thru_hole circle (at -54 -35) (size 5 5) (drill 4) (layers *.Cu *.Mask F.SilkS)
      (net 8 GNDPWR))
  )
  (module SMD_Packages:SMD-1206_Pol (layer F.Cu) (tedit 57825ED5)
    (at 88.17 63.805)
    (attr smd)
    (fp_text reference F101 (at 0.127 2.286) (layer F.SilkS))
    (fp_text value 30A (at 0.127 -2.159) (layer F.Fab))
    (pad 1 smd rect (at -1.651 0) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(F101-Pad1)"))
    (pad 2 smd rect (at 1.651 0) (size 1.524 2.032) (layers F.Cu F.Paste F.Mask)
      (net 4 VPP))
    (model SMD_Packages.3dshapes/SMD-1206_Pol.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.17 0.16 0.16))
      (rotate (xyz 0 0 0))
    )
  )
  (module Walts_lib:3-2106431-2 (layer F.Cu) (tedit 56733AFE)
    (at 70.39 73.965)
    (attr smd)
    (fp_text reference P101 (at -5 0 90) (layer F.SilkS) hide)
    (fp_text value CONN_01X02 (at -7 0 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.1 2 90) (size 3.1 2.45) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(F101-Pad1)"))
    (pad 2 smd rect (at -2.1 -2 90) (size 3.1 2.45) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2.1 -2 90) (size 3.1 2.45) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at 2.1 2 90) (size 3.1 2.45) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(F101-Pad1)"))
  )
  (module mountgnd:mountgnd (layer F.Cu) (tedit 579ADF21)
    (at 69.12 89.205)
    (fp_text reference M101 (at 0 3.81) (layer F.SilkS))
    (fp_text value mountgnd (at 0 -3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 6 6) (drill 5) (layers *.Cu *.Mask F.SilkS)
      (net 8 GNDPWR))
  )
  (module FID:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 579AE05E)
    (at 36.1 167.945)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID101 (at 5.08 3.81) (layer F.SilkS))
    (fp_text value FIDUCIAL (at 0 -3.81) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module FID:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 579CB9D1)
    (at 36.1 62.535)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID102 (at 5.08 3.81) (layer F.SilkS))
    (fp_text value FIDUCIAL (at 11.43 0) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module FID:Fiducial_1mm_Dia_2.54mm_Outer_CopperTop (layer F.Cu) (tedit 579CB9A7)
    (at 137.7 167.945)
    (descr "Circular Fiducial, 1mm bare copper top; 2.54mm keepout")
    (tags marker)
    (attr virtual)
    (fp_text reference FID103 (at -3.81 3.81) (layer F.SilkS))
    (fp_text value FIDUCIAL (at 0 -3.81) (layer F.Fab))
    (pad ~ smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (solder_mask_margin 0.77) (clearance 0.77))
  )
  (module glass:M-B012 (layer F.Cu) (tedit 579B9048)
    (at 85.63 115.875 180)
    (fp_text reference HS101 (at 0 27.94 180) (layer F.SilkS))
    (fp_text value M-C092_HS (at 0 -27.94 180) (layer F.Fab))
    (pad 1 thru_hole circle (at -53.34 -45 180) (size 4 4) (drill 4) (layers *.Cu *.Mask F.SilkS)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -53.34 45 180) (size 4 4) (drill 4) (layers *.Cu *.Mask F.SilkS)
      (net 8 GNDPWR))
    (pad 4 thru_hole circle (at 53.34 45 180) (size 4 4) (drill 4) (layers *.Cu *.Mask F.SilkS)
      (net 8 GNDPWR))
    (pad 2 thru_hole circle (at 53.34 -45 180) (size 4 4) (drill 4) (layers *.Cu *.Mask F.SilkS)
      (net 8 GNDPWR))
  )
  (module M-B012:M-B012 (layer F.Cu) (tedit 579AEFCE)
    (at 103.41 115.875 90)
    (fp_text reference HS102 (at 0 27.94 90) (layer F.SilkS))
    (fp_text value M-C092_HS (at 0 -27.94 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -53.34 -25.4 90) (size 4 4) (drill 4) (layers *.Cu *.Mask F.SilkS)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -53.34 25.4 90) (size 4 4) (drill 4) (layers *.Cu *.Mask F.SilkS)
      (net 8 GNDPWR))
    (pad 4 thru_hole circle (at 53.34 25.4 90) (size 4 4) (drill 4) (layers *.Cu *.Mask F.SilkS)
      (net 8 GNDPWR))
    (pad 2 thru_hole circle (at 53.34 -25.4 90) (size 4 4) (drill 4) (layers *.Cu *.Mask F.SilkS)
      (net 8 GNDPWR))
  )
  (module ref:CreeXPE2 (layer F.Cu) (tedit 579CB495)
    (at 95.79 77.775 180)
    (attr smd)
    (fp_text reference D101 (at 12.7 -3.81 270) (layer F.SilkS))
    (fp_text value LED_D_RED (at 12.7 7.62 270) (layer F.Fab))
    (pad 3 thru_hole circle (at 7.62 -3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 -5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 -6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 -7.62 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 -6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 -5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 -3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 -2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 -2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 -1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 -1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 -8.89 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 -7.62 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 -6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 -5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 -3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 -2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 -1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 7.62 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 7.62 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 8.89 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 -8.89 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 -7.62 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 -7.62 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 -6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 -6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 -6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 -5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 -5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 -5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 -3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 -3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 -3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 -2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 -2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 -2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 -1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 -1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 -1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 7.62 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 7.62 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 8.89 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 -8.89 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 -7.62 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 -6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 -5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 -3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 -2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 -1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 7.62 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 8.89 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 -8.89 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 -6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 -7.62 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 -5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 -3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 -2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 -1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 7.62 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 8.89 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 8.89 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 8.89 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 7.62 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 7.62 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 -1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 -2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 -3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 -5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 -6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 -7.62 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 -8.89 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 -1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 -2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 -3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 -5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 -6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 -7.62 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 -8.89 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 2.54 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu B.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 1.27 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask F.Paste)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 0 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask F.Paste)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -1.27 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask F.Paste)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -2.54 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu B.Mask)
      (net 8 GNDPWR))
    (pad 3 smd rect (at 6.3 0 270) (size 1.3 7.3) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 smd rect (at 2.15 0 270) (size 1.3 1) (layers *.Cu B.Mask)
      (net 8 GNDPWR))
    (pad 3 smd rect (at -2.15 0 270) (size 1.3 1) (layers *.Cu B.Mask)
      (net 8 GNDPWR))
    (pad 2 smd rect (at 0 6.3 270) (size 10.3 3.3) (layers F.Cu)
      (net 4 VPP))
    (pad 1 smd rect (at 0 -6.3 270) (size 10.3 3.3) (layers F.Cu)
      (net 2 "Net-(D101-Pad1)"))
    (pad 3 smd rect (at -6.3 5.3 270) (size 9.3 7.3) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 smd rect (at -6.3 -5.3 270) (size 9.3 7.3) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 smd rect (at 6.3 5.3 270) (size 9.3 7.3) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 smd rect (at 6.3 -5.3 270) (size 9.3 7.3) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 smd rect (at -6.3 0 270) (size 1.3 7.3) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 2 smd rect (at 0 1.4 270) (size 0.5 3.3) (layers F.Cu F.Paste F.Mask)
      (net 4 VPP))
    (pad 3 smd rect (at 0 0 270) (size 1.3 3.3) (layers *.Cu *.Mask F.Paste)
      (net 8 GNDPWR))
    (pad 1 smd rect (at 0 -1.4 270) (size 0.5 3.3) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(D101-Pad1)"))
  )
  (module ref:CreeXPE2 (layer F.Cu) (tedit 579CB495)
    (at 121.19 77.775)
    (attr smd)
    (fp_text reference D102 (at 12.7 -3.81 90) (layer F.SilkS))
    (fp_text value LED_D_RED (at 12.7 7.62 90) (layer F.Fab))
    (pad 3 thru_hole circle (at 7.62 -3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 -5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 -6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 -7.62 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 -6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 -5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 -3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 -2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 -2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 -1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 -1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 -8.89 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 -7.62 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 -6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 -5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 -3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 -2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 -1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 7.62 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 7.62 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 8.89 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 -8.89 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 -7.62 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 -7.62 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 -6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 -6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 -6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 -5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 -5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 -5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 -3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 -3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 -3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 -2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 -2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 -2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 -1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 -1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 -1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 7.62 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 7.62 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 8.89 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 -8.89 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 -7.62 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 -6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 -5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 -3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 -2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 -1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 7.62 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 8.89 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 -8.89 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 -6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 -7.62 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 -5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 -3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 -2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 -1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 7.62 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 8.89 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 8.89 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 8.89 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 7.62 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 7.62 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 -1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 -2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 -3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 -5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 -6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 -7.62 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 -8.89 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 -1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 -2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 -3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 -5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 -6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 -7.62 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 -8.89 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 2.54 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu B.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 1.27 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask F.Paste)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 0 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask F.Paste)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -1.27 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask F.Paste)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -2.54 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu B.Mask)
      (net 8 GNDPWR))
    (pad 3 smd rect (at 6.3 0 90) (size 1.3 7.3) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 smd rect (at 2.15 0 90) (size 1.3 1) (layers *.Cu B.Mask)
      (net 8 GNDPWR))
    (pad 3 smd rect (at -2.15 0 90) (size 1.3 1) (layers *.Cu B.Mask)
      (net 8 GNDPWR))
    (pad 2 smd rect (at 0 6.3 90) (size 10.3 3.3) (layers F.Cu)
      (net 3 "Net-(D102-Pad2)"))
    (pad 1 smd rect (at 0 -6.3 90) (size 10.3 3.3) (layers F.Cu)
      (net 1 GND))
    (pad 3 smd rect (at -6.3 5.3 90) (size 9.3 7.3) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 smd rect (at -6.3 -5.3 90) (size 9.3 7.3) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 smd rect (at 6.3 5.3 90) (size 9.3 7.3) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 smd rect (at 6.3 -5.3 90) (size 9.3 7.3) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 smd rect (at -6.3 0 90) (size 1.3 7.3) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 2 smd rect (at 0 1.4 90) (size 0.5 3.3) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D102-Pad2)"))
    (pad 3 smd rect (at 0 0 90) (size 1.3 3.3) (layers *.Cu *.Mask F.Paste)
      (net 8 GNDPWR))
    (pad 1 smd rect (at 0 -1.4 90) (size 0.5 3.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
  )
  (module ref:CreeXPE2 (layer F.Cu) (tedit 579CB495)
    (at 95.79 103.175 180)
    (attr smd)
    (fp_text reference D103 (at 12.7 -3.81 270) (layer F.SilkS))
    (fp_text value LED_D_RED (at 12.7 7.62 270) (layer F.Fab))
    (pad 3 thru_hole circle (at 7.62 -3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 -5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 -6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 -7.62 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 -6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 -5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 -3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 -2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 -2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 -1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 -1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 -8.89 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 -7.62 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 -6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 -5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 -3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 -2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 -1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 7.62 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 7.62 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 8.89 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 -8.89 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 -7.62 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 -7.62 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 -6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 -6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 -6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 -5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 -5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 -5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 -3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 -3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 -3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 -2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 -2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 -2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 -1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 -1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 -1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 7.62 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 7.62 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 8.89 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 -8.89 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 -7.62 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 -6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 -5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 -3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 -2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 -1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 7.62 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 8.89 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 -8.89 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 -6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 -7.62 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 -5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 -3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 -2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 -1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 7.62 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 8.89 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 8.89 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 8.89 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 7.62 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 7.62 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 -1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 -2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 -3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 -5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 -6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 -7.62 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 -8.89 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 -1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 -2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 -3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 -5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 -6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 -7.62 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 -8.89 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 2.54 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu B.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 1.27 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask F.Paste)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 0 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask F.Paste)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -1.27 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask F.Paste)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -2.54 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu B.Mask)
      (net 8 GNDPWR))
    (pad 3 smd rect (at 6.3 0 270) (size 1.3 7.3) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 smd rect (at 2.15 0 270) (size 1.3 1) (layers *.Cu B.Mask)
      (net 8 GNDPWR))
    (pad 3 smd rect (at -2.15 0 270) (size 1.3 1) (layers *.Cu B.Mask)
      (net 8 GNDPWR))
    (pad 2 smd rect (at 0 6.3 270) (size 10.3 3.3) (layers F.Cu)
      (net 2 "Net-(D101-Pad1)"))
    (pad 1 smd rect (at 0 -6.3 270) (size 10.3 3.3) (layers F.Cu)
      (net 9 "Net-(D103-Pad1)"))
    (pad 3 smd rect (at -6.3 5.3 270) (size 9.3 7.3) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 smd rect (at -6.3 -5.3 270) (size 9.3 7.3) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 smd rect (at 6.3 5.3 270) (size 9.3 7.3) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 smd rect (at 6.3 -5.3 270) (size 9.3 7.3) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 smd rect (at -6.3 0 270) (size 1.3 7.3) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 2 smd rect (at 0 1.4 270) (size 0.5 3.3) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(D101-Pad1)"))
    (pad 3 smd rect (at 0 0 270) (size 1.3 3.3) (layers *.Cu *.Mask F.Paste)
      (net 8 GNDPWR))
    (pad 1 smd rect (at 0 -1.4 270) (size 0.5 3.3) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D103-Pad1)"))
  )
  (module ref:CreeXPE2 (layer F.Cu) (tedit 579CB495)
    (at 121.19 103.175)
    (attr smd)
    (fp_text reference D104 (at 12.7 -3.81 90) (layer F.SilkS))
    (fp_text value LED_D_RED (at 12.7 7.62 90) (layer F.Fab))
    (pad 3 thru_hole circle (at 7.62 -3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 -5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 -6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 -7.62 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 -6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 -5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 -3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 -2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 -2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 -1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 -1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 -8.89 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 -7.62 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 -6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 -5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 -3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 -2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 -1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 7.62 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 7.62 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 8.89 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 -8.89 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 -7.62 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 -7.62 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 -6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 -6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 -6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 -5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 -5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 -5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 -3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 -3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 -3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 -2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 -2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 -2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 -1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 -1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 -1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 7.62 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 7.62 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 8.89 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 -8.89 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 -7.62 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 -6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 -5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 -3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 -2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 -1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 7.62 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 8.89 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 -8.89 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 -6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 -7.62 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 -5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 -3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 -2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 -1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 7.62 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 8.89 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 8.89 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 8.89 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 7.62 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 7.62 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 -1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 -2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 -3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 -5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 -6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 -7.62 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 -8.89 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 -1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 -2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 -3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 -5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 -6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 -7.62 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 -8.89 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 2.54 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu B.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 1.27 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask F.Paste)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 0 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask F.Paste)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -1.27 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask F.Paste)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -2.54 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu B.Mask)
      (net 8 GNDPWR))
    (pad 3 smd rect (at 6.3 0 90) (size 1.3 7.3) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 smd rect (at 2.15 0 90) (size 1.3 1) (layers *.Cu B.Mask)
      (net 8 GNDPWR))
    (pad 3 smd rect (at -2.15 0 90) (size 1.3 1) (layers *.Cu B.Mask)
      (net 8 GNDPWR))
    (pad 2 smd rect (at 0 6.3 90) (size 10.3 3.3) (layers F.Cu)
      (net 10 "Net-(D104-Pad2)"))
    (pad 1 smd rect (at 0 -6.3 90) (size 10.3 3.3) (layers F.Cu)
      (net 3 "Net-(D102-Pad2)"))
    (pad 3 smd rect (at -6.3 5.3 90) (size 9.3 7.3) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 smd rect (at -6.3 -5.3 90) (size 9.3 7.3) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 smd rect (at 6.3 5.3 90) (size 9.3 7.3) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 smd rect (at 6.3 -5.3 90) (size 9.3 7.3) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 smd rect (at -6.3 0 90) (size 1.3 7.3) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 2 smd rect (at 0 1.4 90) (size 0.5 3.3) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D104-Pad2)"))
    (pad 3 smd rect (at 0 0 90) (size 1.3 3.3) (layers *.Cu *.Mask F.Paste)
      (net 8 GNDPWR))
    (pad 1 smd rect (at 0 -1.4 90) (size 0.5 3.3) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D102-Pad2)"))
  )
  (module ref:CreeXPE2 (layer F.Cu) (tedit 579CB495)
    (at 95.79 128.575 180)
    (attr smd)
    (fp_text reference D105 (at 12.7 -3.81 270) (layer F.SilkS))
    (fp_text value LED_D_RED (at 12.7 7.62 270) (layer F.Fab))
    (pad 3 thru_hole circle (at 7.62 -3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 -5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 -6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 -7.62 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 -6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 -5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 -3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 -2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 -2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 -1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 -1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 -8.89 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 -7.62 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 -6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 -5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 -3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 -2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 -1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 7.62 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 7.62 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 8.89 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 -8.89 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 -7.62 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 -7.62 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 -6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 -6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 -6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 -5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 -5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 -5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 -3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 -3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 -3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 -2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 -2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 -2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 -1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 -1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 -1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 7.62 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 7.62 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 8.89 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 -8.89 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 -7.62 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 -6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 -5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 -3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 -2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 -1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 7.62 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 8.89 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 -8.89 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 -6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 -7.62 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 -5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 -3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 -2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 -1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 7.62 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 8.89 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 8.89 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 8.89 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 7.62 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 7.62 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 -1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 -2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 -3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 -5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 -6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 -7.62 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 -8.89 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 -1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 -2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 -3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 -5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 -6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 -7.62 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 -8.89 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 2.54 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu B.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 1.27 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask F.Paste)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 0 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask F.Paste)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -1.27 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask F.Paste)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -2.54 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu B.Mask)
      (net 8 GNDPWR))
    (pad 3 smd rect (at 6.3 0 270) (size 1.3 7.3) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 smd rect (at 2.15 0 270) (size 1.3 1) (layers *.Cu B.Mask)
      (net 8 GNDPWR))
    (pad 3 smd rect (at -2.15 0 270) (size 1.3 1) (layers *.Cu B.Mask)
      (net 8 GNDPWR))
    (pad 2 smd rect (at 0 6.3 270) (size 10.3 3.3) (layers F.Cu)
      (net 9 "Net-(D103-Pad1)"))
    (pad 1 smd rect (at 0 -6.3 270) (size 10.3 3.3) (layers F.Cu)
      (net 5 "Net-(D105-Pad1)"))
    (pad 3 smd rect (at -6.3 5.3 270) (size 9.3 7.3) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 smd rect (at -6.3 -5.3 270) (size 9.3 7.3) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 smd rect (at 6.3 5.3 270) (size 9.3 7.3) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 smd rect (at 6.3 -5.3 270) (size 9.3 7.3) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 smd rect (at -6.3 0 270) (size 1.3 7.3) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 2 smd rect (at 0 1.4 270) (size 0.5 3.3) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D103-Pad1)"))
    (pad 3 smd rect (at 0 0 270) (size 1.3 3.3) (layers *.Cu *.Mask F.Paste)
      (net 8 GNDPWR))
    (pad 1 smd rect (at 0 -1.4 270) (size 0.5 3.3) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D105-Pad1)"))
  )
  (module ref:CreeXPE2 (layer F.Cu) (tedit 579CB495)
    (at 121.19 128.575)
    (attr smd)
    (fp_text reference D106 (at 12.7 -3.81 90) (layer F.SilkS))
    (fp_text value LED_D_RED (at 12.7 7.62 90) (layer F.Fab))
    (pad 3 thru_hole circle (at 7.62 -3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 -5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 -6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 -7.62 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 -6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 -5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 -3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 -2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 -2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 -1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 -1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 -8.89 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 -7.62 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 -6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 -5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 -3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 -2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 -1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 7.62 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 7.62 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 8.89 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 -8.89 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 -7.62 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 -7.62 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 -6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 -6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 -6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 -5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 -5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 -5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 -3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 -3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 -3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 -2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 -2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 -2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 -1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 -1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 -1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 7.62 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 7.62 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 8.89 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 -8.89 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 -7.62 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 -6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 -5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 -3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 -2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 -1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 7.62 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 8.89 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 -8.89 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 -6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 -7.62 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 -5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 -3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 -2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 -1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 7.62 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 8.89 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 8.89 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 8.89 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 7.62 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 7.62 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 -1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 -2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 -3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 -5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 -6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 -7.62 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 -8.89 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 -1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 -2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 -3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 -5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 -6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 -7.62 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 -8.89 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 2.54 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu B.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 1.27 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask F.Paste)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 0 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask F.Paste)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -1.27 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask F.Paste)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -2.54 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu B.Mask)
      (net 8 GNDPWR))
    (pad 3 smd rect (at 6.3 0 90) (size 1.3 7.3) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 smd rect (at 2.15 0 90) (size 1.3 1) (layers *.Cu B.Mask)
      (net 8 GNDPWR))
    (pad 3 smd rect (at -2.15 0 90) (size 1.3 1) (layers *.Cu B.Mask)
      (net 8 GNDPWR))
    (pad 2 smd rect (at 0 6.3 90) (size 10.3 3.3) (layers F.Cu)
      (net 7 "Net-(D106-Pad2)"))
    (pad 1 smd rect (at 0 -6.3 90) (size 10.3 3.3) (layers F.Cu)
      (net 10 "Net-(D104-Pad2)"))
    (pad 3 smd rect (at -6.3 5.3 90) (size 9.3 7.3) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 smd rect (at -6.3 -5.3 90) (size 9.3 7.3) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 smd rect (at 6.3 5.3 90) (size 9.3 7.3) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 smd rect (at 6.3 -5.3 90) (size 9.3 7.3) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 smd rect (at -6.3 0 90) (size 1.3 7.3) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 2 smd rect (at 0 1.4 90) (size 0.5 3.3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D106-Pad2)"))
    (pad 3 smd rect (at 0 0 90) (size 1.3 3.3) (layers *.Cu *.Mask F.Paste)
      (net 8 GNDPWR))
    (pad 1 smd rect (at 0 -1.4 90) (size 0.5 3.3) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(D104-Pad2)"))
  )
  (module ref:CreeXPE2 (layer F.Cu) (tedit 579CB495)
    (at 95.79 153.975 180)
    (attr smd)
    (fp_text reference D107 (at 12.7 -3.81 270) (layer F.SilkS))
    (fp_text value LED_BL (at 12.7 7.62 270) (layer F.Fab))
    (pad 3 thru_hole circle (at 7.62 -3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 -5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 -6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 -7.62 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 -6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 -5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 -3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 -2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 -2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 -1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 -1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 -8.89 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 -7.62 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 -6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 -5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 -3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 -2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 -1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 7.62 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 7.62 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 8.89 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 -8.89 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 -7.62 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 -7.62 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 -6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 -6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 -6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 -5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 -5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 -5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 -3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 -3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 -3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 -2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 -2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 -2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 -1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 -1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 -1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 7.62 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 7.62 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 8.89 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 -8.89 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 -7.62 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 -6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 -5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 -3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 -2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 -1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 7.62 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 8.89 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 -8.89 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 -6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 -7.62 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 -5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 -3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 -2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 -1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 7.62 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 8.89 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 8.89 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 8.89 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 7.62 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 7.62 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 -1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 -2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 -3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 -5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 -6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 -7.62 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 -8.89 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 -1.27 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 -2.54 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 -3.81 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 -5.08 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 -6.35 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 -7.62 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 -8.89 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 2.54 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu B.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 1.27 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask F.Paste)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 0 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask F.Paste)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -1.27 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask F.Paste)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -2.54 0 270) (size 1.2 1.2) (drill 0.7) (layers *.Cu B.Mask)
      (net 8 GNDPWR))
    (pad 3 smd rect (at 6.3 0 270) (size 1.3 7.3) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 smd rect (at 2.15 0 270) (size 1.3 1) (layers *.Cu B.Mask)
      (net 8 GNDPWR))
    (pad 3 smd rect (at -2.15 0 270) (size 1.3 1) (layers *.Cu B.Mask)
      (net 8 GNDPWR))
    (pad 2 smd rect (at 0 6.3 270) (size 10.3 3.3) (layers F.Cu)
      (net 5 "Net-(D105-Pad1)"))
    (pad 1 smd rect (at 0 -6.3 270) (size 10.3 3.3) (layers F.Cu)
      (net 11 "Net-(D107-Pad1)"))
    (pad 3 smd rect (at -6.3 5.3 270) (size 9.3 7.3) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 smd rect (at -6.3 -5.3 270) (size 9.3 7.3) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 smd rect (at 6.3 5.3 270) (size 9.3 7.3) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 smd rect (at 6.3 -5.3 270) (size 9.3 7.3) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 smd rect (at -6.3 0 270) (size 1.3 7.3) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 2 smd rect (at 0 1.4 270) (size 0.5 3.3) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D105-Pad1)"))
    (pad 3 smd rect (at 0 0 270) (size 1.3 3.3) (layers *.Cu *.Mask F.Paste)
      (net 8 GNDPWR))
    (pad 1 smd rect (at 0 -1.4 270) (size 0.5 3.3) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(D107-Pad1)"))
  )
  (module ref:CreeXPE2 (layer F.Cu) (tedit 579CB495)
    (at 121.19 153.975)
    (attr smd)
    (fp_text reference D108 (at 12.7 -3.81 90) (layer F.SilkS))
    (fp_text value LED_D_RED (at 12.7 7.62 90) (layer F.Fab))
    (pad 3 thru_hole circle (at 7.62 -3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 -5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 -6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 -7.62 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 -6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 -5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 -3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 -2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 -2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 -1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 -1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 -8.89 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 -7.62 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 -6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 -5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 -3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 -2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 -1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 8.89 6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 7.62 7.62 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 7.62 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 6.35 8.89 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 -8.89 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 -7.62 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 -7.62 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 -6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 -6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 -6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 -5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 -5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 -5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 -3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 -3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 -3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 -2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 -2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 -2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 -1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 -1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 -1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -8.89 6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 7.62 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 7.62 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -6.35 8.89 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 -8.89 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 -7.62 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 -6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 -5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 -3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 -2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 -1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 7.62 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 8.89 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 -8.89 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 -6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 -7.62 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 -5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 -3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 -2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 -1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 7.62 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 3.81 8.89 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 8.89 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 8.89 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 7.62 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 7.62 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 -1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 -2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 -3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 -5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 -6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -7.62 -7.62 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -5.08 -8.89 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 -1.27 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 -2.54 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 -3.81 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 -5.08 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 -6.35 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 -7.62 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -3.81 -8.89 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 2.54 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu B.Mask)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 1.27 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask F.Paste)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at 0 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask F.Paste)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -1.27 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu *.Mask F.Paste)
      (net 8 GNDPWR))
    (pad 3 thru_hole circle (at -2.54 0 90) (size 1.2 1.2) (drill 0.7) (layers *.Cu B.Mask)
      (net 8 GNDPWR))
    (pad 3 smd rect (at 6.3 0 90) (size 1.3 7.3) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 smd rect (at 2.15 0 90) (size 1.3 1) (layers *.Cu B.Mask)
      (net 8 GNDPWR))
    (pad 3 smd rect (at -2.15 0 90) (size 1.3 1) (layers *.Cu B.Mask)
      (net 8 GNDPWR))
    (pad 2 smd rect (at 0 6.3 90) (size 10.3 3.3) (layers F.Cu)
      (net 11 "Net-(D107-Pad1)"))
    (pad 1 smd rect (at 0 -6.3 90) (size 10.3 3.3) (layers F.Cu)
      (net 7 "Net-(D106-Pad2)"))
    (pad 3 smd rect (at -6.3 5.3 90) (size 9.3 7.3) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 smd rect (at -6.3 -5.3 90) (size 9.3 7.3) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 smd rect (at 6.3 5.3 90) (size 9.3 7.3) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 smd rect (at 6.3 -5.3 90) (size 9.3 7.3) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 3 smd rect (at -6.3 0 90) (size 1.3 7.3) (layers *.Cu *.Mask)
      (net 8 GNDPWR))
    (pad 2 smd rect (at 0 1.4 90) (size 0.5 3.3) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(D107-Pad1)"))
    (pad 3 smd rect (at 0 0 90) (size 1.3 3.3) (layers *.Cu *.Mask F.Paste)
      (net 8 GNDPWR))
    (pad 1 smd rect (at 0 -1.4 90) (size 0.5 3.3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D106-Pad2)"))
  )
  (gr_line (start 28.48 58.725) (end 29.115 58.725) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 28.48 86.03) (end 28.48 58.725) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 53.245 86.03) (end 28.48 86.03) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 53.245 101.27) (end 53.245 86.03) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 28.48 101.27) (end 53.245 101.27) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 28.48 115.875) (end 28.48 101.27) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 52.61 115.875) (end 28.48 115.875) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 52.61 120.955) (end 52.61 115.875) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 28.48 120.955) (end 52.61 120.955) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 28.48 128.575) (end 28.48 120.955) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 52.61 128.575) (end 28.48 128.575) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 52.61 140.005) (end 52.61 128.575) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 52.61 145.085) (end 52.61 140.005) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 28.48 145.085) (end 52.61 145.085) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 28.48 173.025) (end 28.48 145.085) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.78 173.025) (end 28.48 173.025) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.78 145.085) (end 142.78 173.025) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 136.43 145.085) (end 142.78 145.085) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 136.43 86.665) (end 136.43 145.085) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.78 86.665) (end 136.43 86.665) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.78 58.725) (end 142.78 86.665) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 28.48 58.725) (end 142.78 58.725) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_text "Cable AK500-OE-7-0.5" (at 69.12 101.905) (layer F.SilkS))
  (gr_text 3-2106431-2 (at 72.93 82.855) (layer F.SilkS))
  (gr_text "M-B012 HEAT SINK" (at 41.18 124.765) (layer F.SilkS))
  (gr_text "APC-12-350\nCC PSU \n29mm height \nlength 77mm \nwidth 44mm\n" (at 46.26 108.255) (layer F.SilkS))
  (gr_text "Air2IT LLC LED2GrO GrOMatO" (at 57.69 120.955 90) (layer F.SilkS))
  (zone (net 8) (net_name GNDPWR) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 1))
    (polygon
      (pts
        (xy 142.78 86.665) (xy 136.43 86.665) (xy 136.43 145.085) (xy 142.78 145.085) (xy 142.78 173.025)
        (xy 28.48 173.025) (xy 28.48 145.085) (xy 52.61 145.085) (xy 52.61 128.575) (xy 28.48 128.575)
        (xy 28.48 120.955) (xy 52.61 120.955) (xy 52.61 115.875) (xy 28.48 115.875) (xy 28.48 101.27)
        (xy 53.245 101.27) (xy 53.245 86.03) (xy 28.48 86.03) (xy 28.48 58.725) (xy 142.78 58.725)
        (xy 142.78 86.665)
      )
    )
  )
  (zone (net 8) (net_name GNDPWR) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 2))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 1))
    (polygon
      (pts
        (xy 142.78 86.665) (xy 136.43 86.665) (xy 136.43 145.085) (xy 142.78 145.085) (xy 142.78 173.025)
        (xy 28.48 173.025) (xy 28.48 145.085) (xy 52.61 145.085) (xy 52.61 128.575) (xy 28.48 129.21)
        (xy 28.48 120.955) (xy 52.61 120.955) (xy 52.61 115.875) (xy 28.48 115.875) (xy 28.48 101.27)
        (xy 53.245 101.27) (xy 53.245 86.03) (xy 28.48 86.03) (xy 28.48 58.725) (xy 142.78 58.725)
        (xy 142.78 86.665)
      )
    )
  )
)
