(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "VDD")
  (net 2 "GND")
  (net 3 "Net-(C1-Pad2)")
  (net 4 "Net-(U1-DIS)")
  (net 5 "Net-(D1-K)")
  (net 6 "Net-(D1-A)")
  (net 7 "Net-(D2-A)")
  (net 8 "Net-(D3-A)")
  (net 9 "Net-(D4-A)")
  (net 10 "Net-(D5-A)")
  (net 11 "Net-(D6-A)")
  (net 12 "Net-(D7-A)")
  (net 13 "Net-(D8-A)")
  (net 14 "Net-(D9-A)")
  (net 15 "Net-(D10-A)")
  (net 16 "Net-(Q1-C)")
  (net 17 "Net-(Q1-B)")
  (net 18 "Net-(U1-OUT)")
  (net 19 "unconnected-(U1-CV-Pad5)")
  (net 20 "unconnected-(U2-CO-Pad12)")
  (net 21 "unconnected-(U2-ENA-Pad13)")
  (footprint "LED_THT:LED_D3.0mm_Clear" (layer "F.Cu")
    (at 196.5452 65.2272)
    (descr "IR-LED, diameter 3.0mm, 2 pins, color: clear")
    (tags "IR infrared LED diameter 3.0mm 2 pins clear")
    (property "Sheetfile" "555-roulette.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr through_hole)
    (fp_text reference "D4" (at 1.27 -2.96) (layer "F.SilkS"))
    (fp_text value "LED" (at 1.27 2.96) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.47 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(D1-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(D4-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D3.0mm_Clear.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_Tantal_D6.0mm_P5.00mm" (layer "F.Cu")
    (at 155.8544 38.6588 180)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=6.0mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 6.0mm Tantal Electrolytic Capacitor")
    (property "Sheetfile" "555-roulette.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C1" (at 2.5 -4.25) (layer "F.SilkS"))
    (fp_text value "1uF" (at 2.5 4.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "VDD") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(C1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_Tantal_D6.0mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D3.0mm_Clear" (layer "F.Cu")
    (at 239.8268 114.8588)
    (descr "IR-LED, diameter 3.0mm, 2 pins, color: clear")
    (tags "IR infrared LED diameter 3.0mm 2 pins clear")
    (property "Sheetfile" "555-roulette.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr through_hole)
    (fp_text reference "D9" (at 1.27 -2.96) (layer "F.SilkS"))
    (fp_text value "LED" (at 1.27 2.96) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.47 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(D1-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 14 "Net-(D9-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D3.0mm_Clear.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 173.6852 71.374)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "555-roulette.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R5" (at 3.81 -1.92) (layer "F.SilkS"))
    (fp_text value "330" (at 3.81 1.92) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(D1-K)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D3.0mm_Clear" (layer "F.Cu")
    (at 154.681 103.2256)
    (descr "IR-LED, diameter 3.0mm, 2 pins, color: clear")
    (tags "IR infrared LED diameter 3.0mm 2 pins clear")
    (property "Field4" "")
    (property "Sheetfile" "555-roulette.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr through_hole)
    (fp_text reference "D2" (at 1.27 -2.96) (layer "F.SilkS"))
    (fp_text value "LED" (at 1.27 2.96) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.47 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(D1-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(D2-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D3.0mm_Clear.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 181.6608 59.944)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "555-roulette.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R1" (at 3.81 -1.92) (layer "F.SilkS"))
    (fp_text value "3.3M" (at 3.81 1.92) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(U1-DIS)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ICM7555:PHOTO-SFH6721" (layer "F.Cu")
    (at 176.3014 63.4746)
    (property "Sheetfile" "555-roulette.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U1" (at -3.556 -1.27 180) (layer "F.SilkS"))
    (fp_text value "7555" (at 3.556 -6.223 180) (layer "F.Fab"))
    (pad "1" smd rect (at -1.905 3.0734) (size 0.6604 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "input") (solder_mask_margin 0.102))
    (pad "2" smd rect (at -0.635 3.0734) (size 0.6604 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Net-(U1-DIS)") (pinfunction "~{TRIG}") (pintype "input") (solder_mask_margin 0.102))
    (pad "3" smd rect (at 0.635 3.0734) (size 0.6604 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "Net-(U1-OUT)") (pinfunction "OUT") (pintype "input") (solder_mask_margin 0.102))
    (pad "4" smd rect (at 1.905 3.0734) (size 0.6604 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "VDD") (pinfunction "~{RESET}") (pintype "input") (solder_mask_margin 0.102))
    (pad "5" smd rect (at 1.905 -3.0734) (size 0.6604 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 19 "unconnected-(U1-CV-Pad5)") (pinfunction "CV") (pintype "input") (solder_mask_margin 0.102))
    (pad "6" smd rect (at 0.635 -3.0734) (size 0.6604 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Net-(U1-DIS)") (pinfunction "THRESH") (pintype "input") (solder_mask_margin 0.102))
    (pad "7" smd rect (at -0.635 -3.0734) (size 0.6604 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "Net-(U1-DIS)") (pinfunction "DIS") (pintype "input") (solder_mask_margin 0.102))
    (pad "8" smd rect (at -1.905 -3.0734) (size 0.6604 2.032) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "VDD") (pinfunction "Vdd") (pintype "input") (solder_mask_margin 0.102))
  )
  (footprint "CD4017BE:DIP794W45P254L1969H508Q16" (layer "F.Cu")
    (at 161.5872 71.3232)
    (property "Sheetfile" "555-roulette.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U2" (at -1.425 -10.835) (layer "F.SilkS"))
    (fp_text value "~" (at 11.275 10.835) (layer "F.Fab"))
    (pad "1" thru_hole rect (at -3.97 -8.89) (size 1.13 1.13) (drill 0.78) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(D6-A)") (pinfunction "Q5") (pintype "input") (solder_mask_margin 0.102))
    (pad "2" thru_hole circle (at -3.97 -6.35) (size 1.13 1.13) (drill 0.78) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(D2-A)") (pinfunction "Q1") (pintype "input") (solder_mask_margin 0.102))
    (pad "3" thru_hole circle (at -3.97 -3.81) (size 1.13 1.13) (drill 0.78) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(D1-A)") (pinfunction "Q0") (pintype "input") (solder_mask_margin 0.102))
    (pad "4" thru_hole circle (at -3.97 -1.27) (size 1.13 1.13) (drill 0.78) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(D3-A)") (pinfunction "Q2") (pintype "input") (solder_mask_margin 0.102))
    (pad "5" thru_hole circle (at -3.97 1.27) (size 1.13 1.13) (drill 0.78) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(D7-A)") (pinfunction "Q6") (pintype "input") (solder_mask_margin 0.102))
    (pad "6" thru_hole circle (at -3.97 3.81) (size 1.13 1.13) (drill 0.78) (layers "*.Cu" "*.Mask")
      (net 13 "Net-(D8-A)") (pinfunction "Q7") (pintype "input") (solder_mask_margin 0.102))
    (pad "7" thru_hole circle (at -3.97 6.35) (size 1.13 1.13) (drill 0.78) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(D4-A)") (pinfunction "Q3") (pintype "input") (solder_mask_margin 0.102))
    (pad "8" thru_hole circle (at -3.97 8.89) (size 1.13 1.13) (drill 0.78) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "VSS") (pintype "input") (solder_mask_margin 0.102))
    (pad "9" thru_hole circle (at 3.97 8.89) (size 1.13 1.13) (drill 0.78) (layers "*.Cu" "*.Mask")
      (net 14 "Net-(D9-A)") (pinfunction "Q8") (pintype "input") (solder_mask_margin 0.102))
    (pad "10" thru_hole circle (at 3.97 6.35) (size 1.13 1.13) (drill 0.78) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(D5-A)") (pinfunction "Q4") (pintype "input") (solder_mask_margin 0.102))
    (pad "11" thru_hole circle (at 3.97 3.81) (size 1.13 1.13) (drill 0.78) (layers "*.Cu" "*.Mask")
      (net 15 "Net-(D10-A)") (pinfunction "Q9") (pintype "input") (solder_mask_margin 0.102))
    (pad "12" thru_hole circle (at 3.97 1.27) (size 1.13 1.13) (drill 0.78) (layers "*.Cu" "*.Mask")
      (net 20 "unconnected-(U2-CO-Pad12)") (pinfunction "CO") (pintype "input") (solder_mask_margin 0.102))
    (pad "13" thru_hole circle (at 3.97 -1.27) (size 1.13 1.13) (drill 0.78) (layers "*.Cu" "*.Mask")
      (net 21 "unconnected-(U2-ENA-Pad13)") (pinfunction "ENA") (pintype "input") (solder_mask_margin 0.102))
    (pad "14" thru_hole circle (at 3.97 -3.81) (size 1.13 1.13) (drill 0.78) (layers "*.Cu" "*.Mask")
      (net 18 "Net-(U1-OUT)") (pinfunction "CLK") (pintype "input") (solder_mask_margin 0.102))
    (pad "15" thru_hole circle (at 3.97 -6.35) (size 1.13 1.13) (drill 0.78) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "RES") (pintype "input") (solder_mask_margin 0.102))
    (pad "16" thru_hole circle (at 3.97 -8.89) (size 1.13 1.13) (drill 0.78) (layers "*.Cu" "*.Mask")
      (net 1 "VDD") (pinfunction "VDD") (pintype "input") (solder_mask_margin 0.102))
  )
  (footprint "Potentiometer_THT:Potentiometer_TT_P0915N" (layer "F.Cu")
    (at 183.4024 51.3912)
    (descr "http://www.ttelectronics.com/sites/default/files/download-files/Datasheet_PanelPot_P09xSeries.pdf")
    (tags "potentiometer vertical TT P0915N single")
    (property "Sheetfile" "555-roulette.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Variable resistor, US symbol")
    (property "ki_keywords" "R res resistor variable potentiometer rheostat")
    (attr through_hole)
    (fp_text reference "R6" (at 2.5 -13.5) (layer "F.SilkS"))
    (fp_text value "R_Variable_US" (at 2.5 2) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 -7.5) (layer "F.Fab"))
    (pad "" thru_hole oval (at -2.25 -7.5) (size 4 4) (drill 2) (layers "*.Cu" "*.Mask"))
    (pad "" thru_hole oval (at 7.25 -7.5) (size 4 4) (drill 2) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole rect (at 0 0) (size 1.8 1.8) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "VDD") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0) (size 1.8 1.8) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "3" thru_hole circle (at 5 0) (size 1.8 1.8) (drill 1) (layers "*.Cu" "*.Mask"))
    (model "${KICAD6_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_TT_P0915N.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D3.0mm_Clear" (layer "F.Cu")
    (at 230.9368 54.5592)
    (descr "IR-LED, diameter 3.0mm, 2 pins, color: clear")
    (tags "IR infrared LED diameter 3.0mm 2 pins clear")
    (property "Sheetfile" "555-roulette.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr through_hole)
    (fp_text reference "D5" (at 1.27 -2.96) (layer "F.SilkS"))
    (fp_text value "LED" (at 1.27 2.96) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.47 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(D1-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(D5-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D3.0mm_Clear.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D3.0mm_Clear" (layer "F.Cu")
    (at 203.0476 87.3252)
    (descr "IR-LED, diameter 3.0mm, 2 pins, color: clear")
    (tags "IR infrared LED diameter 3.0mm 2 pins clear")
    (property "Sheetfile" "555-roulette.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr through_hole)
    (fp_text reference "D10" (at 1.27 -2.96) (layer "F.SilkS"))
    (fp_text value "LED" (at 1.27 2.96) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.47 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(D1-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 15 "Net-(D10-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D3.0mm_Clear.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 153.8224 54.5592)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "555-roulette.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R3" (at 3.81 -1.92) (layer "F.SilkS"))
    (fp_text value "10M" (at 3.81 1.92) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(C1-Pad2)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 17 "Net-(Q1-B)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_BarrelJack:BarrelJack_CUI_PJ-063AH_Horizontal" (layer "F.Cu")
    (at 147.2396 81.138)
    (descr "Barrel Jack, 2.0mm ID, 5.5mm OD, 24V, 8A, no switch, https://www.cui.com/product/resource/pj-063ah.pdf")
    (tags "barrel jack cui dc power")
    (property "Sheetfile" "555-roulette.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Multiple-cell battery")
    (property "ki_keywords" "batt voltage-source cell")
    (attr through_hole)
    (fp_text reference "BT1" (at 0 -2.3) (layer "F.SilkS"))
    (fp_text value "Battery" (at 0 13) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 5.5) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at 0 9) (size 1.6 1.6) (drill 1.6) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole rect (at 0 0) (size 4 2) (drill oval 3 1) (layers "*.Cu" "*.Mask")
      (net 1 "VDD") (pinfunction "+") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 6) (size 3.3 2) (drill oval 2.3 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "-") (pintype "passive"))
    (pad "MP" thru_hole oval (at -4.5 7) (size 2 3.5) (drill oval 1 2.5) (layers "*.Cu" "*.Mask"))
    (pad "MP" thru_hole oval (at 4.5 7) (size 2 3.5) (drill oval 1 2.5) (layers "*.Cu" "*.Mask"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_BarrelJack.3dshapes/BarrelJack_CUI_PJ-063AH_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 166.5732 54.9148)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "555-roulette.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R4" (at 3.81 -1.92) (layer "F.SilkS"))
    (fp_text value "3.3M" (at 3.81 1.92) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 17 "Net-(Q1-B)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 1 "VDD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D3.0mm_Clear" (layer "F.Cu")
    (at 177.7492 89.916)
    (descr "IR-LED, diameter 3.0mm, 2 pins, color: clear")
    (tags "IR infrared LED diameter 3.0mm 2 pins clear")
    (property "Sheetfile" "555-roulette.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr through_hole)
    (fp_text reference "D1" (at 1.27 -2.96) (layer "F.SilkS"))
    (fp_text value "LED" (at 1.27 2.96) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.47 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(D1-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(D1-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D3.0mm_Clear.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_Tantal_D6.0mm_P5.00mm" (layer "F.Cu")
    (at 140.9484 66.548)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=5.00mm, , diameter=6.0mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
    (tags "CP Radial_Tantal series Radial pin pitch 5.00mm  diameter 6.0mm Tantal Electrolytic Capacitor")
    (property "Sheetfile" "555-roulette.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C2" (at 2.5 -4.25) (layer "F.SilkS"))
    (fp_text value "100nF" (at 2.5 4.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(U1-DIS)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_Tantal_D6.0mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D3.0mm_Clear" (layer "F.Cu")
    (at 173.8376 78.8924)
    (descr "IR-LED, diameter 3.0mm, 2 pins, color: clear")
    (tags "IR infrared LED diameter 3.0mm 2 pins clear")
    (property "Sheetfile" "555-roulette.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr through_hole)
    (fp_text reference "D3" (at 1.27 -2.96) (layer "F.SilkS"))
    (fp_text value "LED" (at 1.27 2.96) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.47 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(D1-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(D3-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D3.0mm_Clear.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 139.4968 46.228)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "555-roulette.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R2" (at 3.81 -1.92) (layer "F.SilkS"))
    (fp_text value "10K" (at 3.81 1.92) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(U1-DIS)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 16 "Net-(Q1-C)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D3.0mm_Clear" (layer "F.Cu")
    (at 250.3932 71.2724)
    (descr "IR-LED, diameter 3.0mm, 2 pins, color: clear")
    (tags "IR infrared LED diameter 3.0mm 2 pins clear")
    (property "Sheetfile" "555-roulette.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr through_hole)
    (fp_text reference "D6" (at 1.27 -2.96) (layer "F.SilkS"))
    (fp_text value "LED" (at 1.27 2.96) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.47 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(D1-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(D6-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D3.0mm_Clear.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-92_Inline" (layer "F.Cu")
    (at 161.036 46.0248)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (property "Sheetfile" "555-roulette.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "0.1A Ic, 45V Vce, PNP Small Signal Transistor, TO-92")
    (property "ki_keywords" "PNP Transistor")
    (attr through_hole)
    (fp_text reference "Q1" (at 1.27 -3.56) (layer "F.SilkS"))
    (fp_text value "BC557" (at 1.27 2.79) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 16 "Net-(Q1-C)") (pinfunction "C") (pintype "passive"))
    (pad "2" thru_hole oval (at 1.27 0) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 17 "Net-(Q1-B)") (pinfunction "B") (pintype "input"))
    (pad "3" thru_hole oval (at 2.54 0) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 1 "VDD") (pinfunction "E") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D3.0mm_Clear" (layer "F.Cu")
    (at 220.0656 71.0692)
    (descr "IR-LED, diameter 3.0mm, 2 pins, color: clear")
    (tags "IR infrared LED diameter 3.0mm 2 pins clear")
    (property "Sheetfile" "555-roulette.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr through_hole)
    (fp_text reference "D7" (at 1.27 -2.96) (layer "F.SilkS"))
    (fp_text value "LED" (at 1.27 2.96) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.47 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(D1-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(D7-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D3.0mm_Clear.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D3.0mm_Clear" (layer "F.Cu")
    (at 237.5916 91.9988)
    (descr "IR-LED, diameter 3.0mm, 2 pins, color: clear")
    (tags "IR infrared LED diameter 3.0mm 2 pins clear")
    (property "Sheetfile" "555-roulette.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr through_hole)
    (fp_text reference "D8" (at 1.27 -2.96) (layer "F.SilkS"))
    (fp_text value "LED" (at 1.27 2.96) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.47 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(D1-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 13 "Net-(D8-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D3.0mm_Clear.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect (start 137.5156 30.48) (end 258.9784 124.8664)
    (fill none) (layer "Edge.Cuts"))
  (image (at 202.5396 77.5716) (layer "F.SilkS") (scale 0.67367))
)
