(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.5318)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(4 "In1.Cu" signal)
		(6 "In2.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.0432)
			)
			(layer "dielectric 1"
				(type "prepreg")
				(thickness 0.1999)
				(material "FR4")
				(epsilon_r 3.68)
				(loss_tangent 0.02)
			)
			(layer "In1.Cu"
				(type "copper")
				(thickness 0.0175)
			)
			(layer "dielectric 2"
				(type "core")
				(thickness 0.9906)
				(material "FR4")
				(epsilon_r 3.68)
				(loss_tangent 0.02)
			)
			(layer "In2.Cu"
				(type "copper")
				(thickness 0.0175)
			)
			(layer "dielectric 3"
				(type "prepreg")
				(thickness 0.1999)
				(material "FR4")
				(epsilon_r 3.68)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.0432)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "Net-(IC1-VCC_1)")
	(net 3 "Net-(IC2-RF_IN)")
	(net 4 "Net-(FL1-OUTPUT)")
	(net 5 "Net-(C4-Pad2)")
	(net 6 "Net-(IC2-RF_OUT)")
	(net 7 "Net-(IC4-VCC_1)")
	(net 8 "Net-(IC5-IN)")
	(net 9 "Net-(FL1-INPUT)")
	(net 10 "Net-(IC1-TUNE)")
	(net 11 "unconnected-(IC1-N.C.-Pad1)")
	(net 12 "Net-(IC1-OUT)")
	(net 13 "unconnected-(IC3-OUT_2-Pad2)")
	(net 14 "Net-(IC4-TUNE)")
	(net 15 "Net-(IC4-OUT)")
	(net 16 "unconnected-(IC4-N.C.-Pad1)")
	(net 17 "unconnected-(IC5-OUT_2-Pad2)")
	(net 18 "Net-(U2-F)")
	(net 19 "Net-(J4-SLEEVE)")
	(net 20 "Net-(J1-SLEEVE)")
	(net 21 "unconnected-(J1-RING-Pad3)")
	(net 22 "unconnected-(J4-RING-Pad3)")
	(net 23 "Net-(IC3-IN)")
	(net 24 "Net-(IC1-~{SHDN})")
	(net 25 "Net-(IC4-~{SHDN})")
	(net 26 "Net-(J5-Pin_3)")
	(net 27 "Net-(S1-COM_1)")
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 137.25 48.925)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R1"
			(at 0 -1.65 0)
			(layer "F.SilkS")
		)
		(property "Value" "2.64k"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "4layer_transmit_receiver.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 24 "Net-(IC1-~{SHDN})")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 27 "Net-(S1-COM_1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_1.00mm:PinHeader_1x04_P1.00mm_Vertical"
		(layer "F.Cu")
		(at 134.15 36.225 180)
		(descr "Through hole straight pin header, 1x04, 1.00mm pitch, single row")
		(tags "Through hole pin header THT 1x04 1.00mm single row")
		(property "Reference" "J5"
			(at 0 -2.55 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 4.61 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x04, script generated"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "4layer_transmit_receiver.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.5 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 0.85 0.85)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 1 180)
			(size 0.85 0.85)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "Net-(IC1-TUNE)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 2 180)
			(size 0.85 0.85)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "Net-(J5-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 0 3 180)
			(size 0.85 0.85)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "Net-(IC3-IN)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_1.00mm.3dshapes/PinHeader_1x04_P1.00mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MAX2623EUA:SOP65P490X110-9N"
		(layer "F.Cu")
		(at 125.675 49.9 180)
		(descr "8 µMAX 1")
		(tags "Integrated Circuit")
		(property "Reference" "IC1"
			(at -4.775 -1.9 180)
			(layer "F.SilkS")
		)
		(property "Value" "MAX2623EUA+"
			(at 0 0 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX2622-MAX2624.pdf"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Voltage Controlled Oscillator 950MHz, 8-Pin uMAX"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "1.1"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "700-MAX2623EUA"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Analog-Devices-Maxim-Integrated/MAX2623EUA%2b?qs=1THa7WoU59G3eRvnxYOLFg%3D%3D"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Analog Devices"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "MAX2623EUA+"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "4layer_transmit_receiver.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -4.775 -1.9 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.212 -0.975 270)
			(size 0.45 1.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 11 "unconnected-(IC1-N.C.-Pad1)")
			(pinfunction "N.C.")
			(pintype "no_connect")
		)
		(pad "2" smd rect
			(at -2.212 -0.325 270)
			(size 0.45 1.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "Net-(IC1-TUNE)")
			(pinfunction "TUNE")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -2.212 0.325 270)
			(size 0.45 1.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_1")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -2.212 0.975 270)
			(size 0.45 1.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "Net-(IC1-~{SHDN})")
			(pinfunction "~{SHDN}")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 2.212 0.975 270)
			(size 0.45 1.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "Net-(IC1-VCC_1)")
			(pinfunction "VCC_1")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 2.212 0.325 270)
			(size 0.45 1.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "Net-(IC1-VCC_1)")
			(pinfunction "VCC_2")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 2.212 -0.325 270)
			(size 0.45 1.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "Net-(IC1-OUT)")
			(pinfunction "OUT")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at 2.212 -0.975 270)
			(size 0.45 1.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_2")
			(pintype "passive")
		)
		(pad "9" smd rect
			(at 0 0 180)
			(size 1.88 2.515)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "EP")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "MAX2623EUA+.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "SYM_63LH:TTT166_MNC"
		(layer "F.Cu")
		(at 109.175 50.35 180)
		(tags "SYM-63LH+ ")
		(property "Reference" "U1"
			(at -8.675 -4.826 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "SYM-63LH+"
			(at 0 0.0762 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "SYM-63LH+"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TTT166_MNC")
		(sheetname "/")
		(sheetfile "4layer_transmit_receiver.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -8.675 -4.826 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 5.969 0.0762 180)
			(size 1.778 1.524)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 20 "Net-(J1-SLEEVE)")
			(pinfunction "F")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at -5.969 0.0762 180)
			(size 1.778 1.524)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "Net-(IC1-OUT)")
			(pinfunction "LO")
			(pintype "unspecified")
		)
		(pad "3" smd rect
			(at 0 4.445 180)
			(size 1.524 1.778)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "Net-(FL1-INPUT)")
			(pinfunction "IF")
			(pintype "unspecified")
		)
		(pad "4" smd rect
			(at 0 -4.318 180)
			(size 1.524 1.778)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GROUND")
			(pintype "power_out")
		)
		(pad "5" smd rect
			(at -4.445 4.445 180)
			(size 1.524 1.778)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GROUND")
			(pintype "power_out")
		)
		(pad "6" smd rect
			(at 4.445 4.445 180)
			(size 1.524 1.778)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GROUND")
			(pintype "power_out")
		)
		(embedded_fonts no)
	)
	(footprint "ADP3338AKCZ-5-R7:SOT230P700X180-4N"
		(layer "F.Cu")
		(at 121.7 35.675 180)
		(descr "SOT230P700X180-4N")
		(tags "Integrated Circuit")
		(property "Reference" "IC3"
			(at -0.35 -4.8 180)
			(layer "F.SilkS")
		)
		(property "Value" "ADP3338AKCZ-5-R7"
			(at -4.8006 -3.556 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Analog Devices ADP3338AKCZ-5-R7, LDO Voltage Regulator, 1A, 5 V +/-1.6%, 2.7  8 Vin, 3-Pin SOT-223"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "584-ADP3338AKCZ-5-R7"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Analog-Devices/ADP3338AKCZ-5-R7?qs=WIvQP4zGangs6Tv%252BSE3hsA%3D%3D"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Analog Devices"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "ADP3338AKCZ-5-R7"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "4layer_transmit_receiver.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -4.8006 -3.556 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -3.2004 -2.3114 270)
			(size 0.889 1.6256)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -3.2004 0 270)
			(size 0.889 1.6256)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "unconnected-(IC3-OUT_2-Pad2)")
			(pinfunction "OUT_2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -3.2004 2.3114 270)
			(size 0.889 1.6256)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 23 "Net-(IC3-IN)")
			(pinfunction "IN")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 3.2004 0 180)
			(size 1.6256 3.175)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "Net-(IC1-VCC_1)")
			(pinfunction "OUT")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "MAX2623EUA:SOP65P490X110-9N"
		(layer "F.Cu")
		(at 124.8869 83.8685 180)
		(descr "8 µMAX 1")
		(tags "Integrated Circuit")
		(property "Reference" "IC4"
			(at -4.825 -1.94295 180)
			(layer "F.SilkS")
		)
		(property "Value" "MAX2623EUA+"
			(at 0 0 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX2622-MAX2624.pdf"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Voltage Controlled Oscillator 950MHz, 8-Pin uMAX"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "1.1"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "700-MAX2623EUA"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Analog-Devices-Maxim-Integrated/MAX2623EUA%2b?qs=1THa7WoU59G3eRvnxYOLFg%3D%3D"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Analog Devices"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "MAX2623EUA+"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "4layer_transmit_receiver.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -4.825 -1.94295 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.212 -0.975 270)
			(size 0.45 1.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 16 "unconnected-(IC4-N.C.-Pad1)")
			(pinfunction "N.C.")
			(pintype "no_connect")
		)
		(pad "2" smd rect
			(at -2.212 -0.325 270)
			(size 0.45 1.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 14 "Net-(IC4-TUNE)")
			(pinfunction "TUNE")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -2.212 0.325 270)
			(size 0.45 1.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_1")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -2.212 0.975 270)
			(size 0.45 1.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 25 "Net-(IC4-~{SHDN})")
			(pinfunction "~{SHDN}")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 2.212 0.975 270)
			(size 0.45 1.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "Net-(IC4-VCC_1)")
			(pinfunction "VCC_1")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 2.212 0.325 270)
			(size 0.45 1.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "Net-(IC4-VCC_1)")
			(pinfunction "VCC_2")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 2.212 -0.325 270)
			(size 0.45 1.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "Net-(IC4-OUT)")
			(pinfunction "OUT")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at 2.212 -0.975 270)
			(size 0.45 1.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_2")
			(pintype "passive")
		)
		(pad "9" smd rect
			(at 0 0 180)
			(size 1.88 2.515)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "EP")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "MAX2623EUA+.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "RF2-143-T-17-50-G:ADAMTECH_RF2-143-T-17-50-G"
		(layer "F.Cu")
		(at 122.2 25.5934 180)
		(property "Reference" "J2"
			(at -4.725 -2.4566 0)
			(layer "F.SilkS")
		)
		(property "Value" "RF2-143-T-17-50-G"
			(at 13.01 -5.135 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" "9/11/15"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" "Manufacturer Recommendations"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "3.57mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Adam Tech"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "4layer_transmit_receiver.kicad_sch")
		(attr smd)
		(fp_text user "PCB EDGE"
			(at 3.75 -0.25 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0 -2.0066 180)
			(size 1.1938 4.0132)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "Net-(C4-Pad2)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "G1" smd rect
			(at -2.7813 -2.0066 180)
			(size 1.1938 4.0132)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "G2" smd rect
			(at 2.7813 -2.0066 180)
			(size 1.1938 4.0132)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "G3" smd rect
			(at 2.7813 -2.0066 180)
			(size 1.1938 4.0132)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "G4" smd rect
			(at -2.7813 -2.0066 180)
			(size 1.1938 4.0132)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "ADP3338AKCZ-5-R7:SOT230P700X180-4N"
		(layer "F.Cu")
		(at 128.3325 75.7 180)
		(descr "SOT230P700X180-4N")
		(tags "Integrated Circuit")
		(property "Reference" "IC5"
			(at 0.0956 4.43855 180)
			(layer "F.SilkS")
		)
		(property "Value" "ADP3338AKCZ-5-R7"
			(at -4.8006 -3.556 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Analog Devices ADP3338AKCZ-5-R7, LDO Voltage Regulator, 1A, 5 V +/-1.6%, 2.7  8 Vin, 3-Pin SOT-223"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "584-ADP3338AKCZ-5-R7"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Analog-Devices/ADP3338AKCZ-5-R7?qs=WIvQP4zGangs6Tv%252BSE3hsA%3D%3D"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Analog Devices"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "ADP3338AKCZ-5-R7"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "4layer_transmit_receiver.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.0956 4.43855 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -3.2004 -2.3114 270)
			(size 0.889 1.6256)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -3.2004 0 270)
			(size 0.889 1.6256)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "unconnected-(IC5-OUT_2-Pad2)")
			(pinfunction "OUT_2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -3.2004 2.3114 270)
			(size 0.889 1.6256)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "Net-(IC5-IN)")
			(pinfunction "IN")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 3.2004 0 180)
			(size 1.6256 3.175)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "Net-(IC4-VCC_1)")
			(pinfunction "OUT")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Connector_PinHeader_1.00mm:PinHeader_1x04_P1.00mm_Vertical"
		(layer "F.Cu")
		(at 139.5325 76.375 180)
		(descr "Through hole straight pin header, 1x04, 1.00mm pitch, single row")
		(tags "Through hole pin header THT 1x04 1.00mm single row")
		(property "Reference" "J6"
			(at -2.1294 3.01355 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 4.61 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x04, script generated"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "4layer_transmit_receiver.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.5 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 0.85 0.85)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 1 180)
			(size 0.85 0.85)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "Net-(IC4-TUNE)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 2 180)
			(size 0.85 0.85)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "Net-(IC4-~{SHDN})")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 0 3 180)
			(size 0.85 0.85)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "Net-(IC5-IN)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_1.00mm.3dshapes/PinHeader_1x04_P1.00mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 107.675 36.075 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C3"
			(at 0 -1.68 90)
			(layer "F.SilkS")
		)
		(property "Value" "100pF"
			(at 0 1.68 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "4layer_transmit_receiver.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 90)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 4 "Net-(FL1-OUTPUT)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 90)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 3 "Net-(IC2-RF_IN)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 130.075 36.2375 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C2"
			(at 0.8625 -1.75 90)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.68 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "4layer_transmit_receiver.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 90)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 90)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 23 "Net-(IC3-IN)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 135.8825 75.9375 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C6"
			(at -0.15105 -1.6544 90)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.68 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "4layer_transmit_receiver.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 270)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 8 "Net-(IC5-IN)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 270)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "SJ3-35053A:SJ335053A"
		(layer "F.Cu")
		(at 97 50.45 90)
		(descr "SJ3-35053A-1")
		(tags "Connector")
		(property "Reference" "J1"
			(at -7.125 5.675 180)
			(layer "F.SilkS")
		)
		(property "Value" "SJ3-35053A"
			(at -0.933 -3.425 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "https://sameskydevices.com/product/resource/sj3-3505x.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Phone Connectors Audio Jack, 3.5mm, Through Hole, 3 Conductors, 0 Switches"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "17.75"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "179-SJ3-35053A"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Same-Sky/SJ3-35053A?qs=IKkN%2F947nfD3IjPRDtzsJA%3D%3D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Same Sky"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "SJ3-35053A"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "4layer_transmit_receiver.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -7.125 5.675 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 3.5 3.5)
			(drill 2.57)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "Net-(J1-SLEEVE)")
			(pinfunction "SLEEVE")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -4.9 -3.5 90)
			(size 3.93 3.93)
			(drill 2.57)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "TIP")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 3.2 -3.5 90)
			(size 3.6 3.6)
			(drill 2.62)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "unconnected-(J1-RING-Pad3)")
			(pinfunction "RING")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "SJ3-35053A.stp"
			(offset
				(xyz -0.6100000051 3.400000044 20.60000007)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "SJ3-35053A:SJ335053A"
		(layer "F.Cu")
		(at 110.5075 72.525)
		(descr "SJ3-35053A-1")
		(tags "Connector")
		(property "Reference" "J4"
			(at -9.3706 1.78645 0)
			(layer "F.SilkS")
		)
		(property "Value" "SJ3-35053A"
			(at -0.933 -3.425 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "https://sameskydevices.com/product/resource/sj3-3505x.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Phone Connectors Audio Jack, 3.5mm, Through Hole, 3 Conductors, 0 Switches"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "17.75"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "179-SJ3-35053A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Same-Sky/SJ3-35053A?qs=IKkN%2F947nfD3IjPRDtzsJA%3D%3D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Same Sky"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "SJ3-35053A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "4layer_transmit_receiver.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -9.3706 1.78645 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 3.5 3.5)
			(drill 2.57)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "Net-(J4-SLEEVE)")
			(pinfunction "SLEEVE")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -4.9 -3.5)
			(size 3.93 3.93)
			(drill 2.57)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "TIP")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 3.2 -3.5)
			(size 3.6 3.6)
			(drill 2.62)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "unconnected-(J4-RING-Pad3)")
			(pinfunction "RING")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "SJ3-35053A.stp"
			(offset
				(xyz -0.6100000051 3.400000044 20.60000007)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 114.675 37.525 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C1"
			(at 0 -1.68 90)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.68 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "4layer_transmit_receiver.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 90)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 90)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 2 "Net-(IC1-VCC_1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 114.0125 31.175)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C4"
			(at 0 -1.68 0)
			(layer "F.SilkS")
		)
		(property "Value" "100pF"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "4layer_transmit_receiver.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 6 "Net-(IC2-RF_OUT)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 5 "Net-(C4-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TS02-66-73-BK-260-SCR-D:TS026673BK260SCRD"
		(layer "F.Cu")
		(at 139.125 42.6 90)
		(descr "TS02-66-73-BK-260-SCR-D-2")
		(tags "Switch")
		(property "Reference" "S1"
			(at -3 4.75 180)
			(layer "F.SilkS")
		)
		(property "Value" "TS02-66-73-BK-260-SCR-D"
			(at 3.25 2.25 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "https://www.sameskydevices.com/product/resource/ts02.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "6 x 6 mm, 7.3 mm Actuator Height, 260 gf, Black, Short Crimped, Through Hole, SPST, Tactile Switch"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "7.5"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "179-TS026673BK260SCR"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/CUI-Devices/TS02-66-73-BK-260-SCR-D?qs=A6eO%252BMLsxmRmxUGYhOJgKw%3D%3D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Same Sky"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "TS02-66-73-BK-260-SCR-D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "4layer_transmit_receiver.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -3 4.75 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "Net-(S1-COM_1)")
			(pinfunction "NO_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 6.5 0 90)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "Net-(J5-Pin_3)")
			(pinfunction "NO_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 4.5 90)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "Net-(S1-COM_1)")
			(pinfunction "COM_1")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 6.5 4.5 90)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "Net-(J5-Pin_3)")
			(pinfunction "COM_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "TS02-66-73-BK-260-SCR-D.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "RF2-143-T-17-50-G:ADAMTECH_RF2-143-T-17-50-G"
		(layer "F.Cu")
		(at 87.8551 84.1063 -90)
		(property "Reference" "J3"
			(at -0.5019 -9.1318 180)
			(layer "F.SilkS")
		)
		(property "Value" "RF2-143-T-17-50-G"
			(at 13.01 -5.135 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" "9/11/15"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" "Manufacturer Recommendations"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "3.57mm"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Adam Tech"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "4layer_transmit_receiver.kicad_sch")
		(attr smd)
		(fp_text user "PCB EDGE"
			(at 3.75 -0.25 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0 -2.0066 270)
			(size 1.1938 4.0132)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 18 "Net-(U2-F)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "G1" smd rect
			(at -2.7813 -2.0066 270)
			(size 1.1938 4.0132)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "G2" smd rect
			(at 2.7813 -2.0066 270)
			(size 1.1938 4.0132)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "G3" smd rect
			(at 2.7813 -2.0066 270)
			(size 1.1938 4.0132)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "G4" smd rect
			(at -2.7813 -2.0066 270)
			(size 1.1938 4.0132)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 119.245 77 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C5"
			(at 0 -1.68 0)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "4layer_transmit_receiver.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 180)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 7 "Net-(IC4-VCC_1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 180)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 141.75 49.925 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R2"
			(at -2.675 -0.05 180)
			(layer "F.SilkS")
		)
		(property "Value" "2.64k"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "4layer_transmit_receiver.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 27 "Net-(S1-COM_1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 133.225 50.0625 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C7"
			(at 2.6125 0.025 180)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.68 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "4layer_transmit_receiver.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 90)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 90)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 24 "Net-(IC1-~{SHDN})")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "SF2098H:SF2098H"
		(layer "F.Cu")
		(at 108.575 40.975 90)
		(descr "SM2016-4 Case")
		(tags "Filter")
		(property "Reference" "FL1"
			(at 0.575 -3.3 90)
			(layer "F.SilkS")
		)
		(property "Value" "SF2098H"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "https://www.rfmi.co/pdf/datasheet/sf2098h.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Signal Conditioning FILTER, SAW, 915 MHZ, 4SMD"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "0.75"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "198-SF2098H"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/RFMi/SF2098H?qs=zW32dvEIR3sr0A1e2MY2bg%3D%3D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "RFMi"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "SF2098H"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "4layer_transmit_receiver.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.575 -3.3 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.7 0.6 180)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "Net-(FL1-INPUT)")
			(pinfunction "INPUT")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.7 0.6 180)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GROUND_1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 0.7 -0.6 180)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "Net-(FL1-OUTPUT)")
			(pinfunction "OUTPUT")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -0.7 -0.6 180)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GROUND_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "SF2098H.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "SYM_63LH:TTT166_MNC"
		(layer "F.Cu")
		(at 110.5369 84.2635 180)
		(tags "SYM-63LH+ ")
		(property "Reference" "U2"
			(at -8.875 -4.826 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "SYM-63LH+"
			(at 0 0.0762 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "SYM-63LH+"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TTT166_MNC")
		(sheetname "/")
		(sheetfile "4layer_transmit_receiver.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -8.875 -4.826 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 5.969 0.0762 180)
			(size 1.778 1.524)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 18 "Net-(U2-F)")
			(pinfunction "F")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at -5.969 0.0762 180)
			(size 1.778 1.524)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "Net-(IC4-OUT)")
			(pinfunction "LO")
			(pintype "unspecified")
		)
		(pad "3" smd rect
			(at 0 4.445 180)
			(size 1.524 1.778)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 19 "Net-(J4-SLEEVE)")
			(pinfunction "IF")
			(pintype "unspecified")
		)
		(pad "4" smd rect
			(at 0 -4.318 180)
			(size 1.524 1.778)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GROUND")
			(pintype "power_out")
		)
		(pad "5" smd rect
			(at -4.445 4.445 180)
			(size 1.524 1.778)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GROUND")
			(pintype "power_out")
		)
		(pad "6" smd rect
			(at 4.445 4.445 180)
			(size 1.524 1.778)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GROUND")
			(pintype "power_out")
		)
		(embedded_fonts no)
	)
	(footprint "BGA2866_115:SOT65P210X110-6N"
		(layer "F.Cu")
		(at 108.575 32.025 180)
		(descr "NXP SOT-363")
		(tags "Integrated Circuit")
		(property "Reference" "IC2"
			(at 0.1 2.4 180)
			(layer "F.SilkS")
		)
		(property "Value" "BGA2866,115"
			(at 0 0 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/BGA2866.pdf"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "NXP - BGA2866,115 - MMIC RF AMP, 2.2GHZ, 24.3DB, SOT-363-6"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "1.1"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "771-BGA2866115"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/NXP-Semiconductors/BGA2866115?qs=0kdNCY%252BdvEBuzkt9XLooaw%3D%3D"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "NXP"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "BGA2866,115"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "4layer_transmit_receiver.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.1 2.4 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.95 -0.65 270)
			(size 0.45 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "Net-(IC1-VCC_1)")
			(pinfunction "VCC")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.95 0 270)
			(size 0.45 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND2_1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -0.95 0.65 270)
			(size 0.45 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "Net-(IC2-RF_OUT)")
			(pinfunction "RF_OUT")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 0.95 0.65 270)
			(size 0.45 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND1")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 0.95 0 270)
			(size 0.45 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND2_2")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 0.95 -0.65 270)
			(size 0.45 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "Net-(IC2-RF_IN)")
			(pinfunction "RF_IN")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "BGA2866,115.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_rect
		(start 87.1 24.5493)
		(end 146.325 91.5507)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_text "Transmitter\n"
		(at 88.725 27.1 0)
		(layer "F.SilkS")
	)
	(gr_text "Receiver\n"
		(at 88.575 64.275 0)
		(layer "F.SilkS")
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 10.25 10.7) (xy 11.75 197.5) (xy 288.2 199.875) (xy 285.825 9.525)
			)
		)
	)
	(embedded_fonts no)
)
