<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<wire x1="26.34" y1="24.070075" x2="26.34" y2="69.8414625" width="0" layer="20"/>
<wire x1="26.34" y1="69.8414625" x2="23.0394625" y2="73.142" width="0" layer="20" curve="90"/>
<wire x1="23.0394625" y1="73.142" x2="10.0145375" y2="73.142" width="0" layer="20"/>
<wire x1="10.0145375" y1="73.142" x2="6.35" y2="69.9854625" width="0" layer="20" curve="90"/>
<wire x1="6.35" y1="69.9854625" x2="6.35" y2="24.701253125" width="0" layer="20"/>
<wire x1="6.35" y1="24.701253125" x2="14.541253125" y2="16.51" width="0" layer="20" curve="90"/>
<wire x1="14.541253125" y1="16.51" x2="18.779925" y2="16.51" width="0" layer="20"/>
<wire x1="18.779925" y1="16.51" x2="26.34" y2="24.070075" width="0" layer="20" curve="90"/>
<hole x="16.51" y="19.558" drill="4"/>
<text>MySensorboard V2.1</text>
<text>D13</text>
<text>3V3</text>
<text>REF</text>
<text>A0</text>
<text>A1</text>
<text>A2</text>
<text>A3</text>
<text>A4</text>
<text>A5</text>
<text>A6</text>
<text>A7</text>
<text>5V</text>
<text>RST</text>
<text>GND</text>
<text>VIN</text>
<text>TX1</text>
<text>RX0</text>
<text>RST</text>
<text>GND</text>
<text>D2</text>
<text>D3</text>
<text>D4</text>
<text>D6</text>
<text>D7</text>
<text>D8</text>
<text>D9</text>
<text>D10</text>
<text>D11</text>
<text>D12</text>
<text>Made By</text>
<text>Made By</text>
<text>Bram</text>
<text>Bram</text>
</plain>
<libraries>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CPOL-RADIAL-100UF-25V">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="1X15-CB">
</package>
<package name="2X04">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="jet-lib">
<packages>
<package name="PDIP-32">
<description>Arduino Nano footprint</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun-Passives" package="CPOL-RADIAL-100UF-25V" value="100uf">
<attribute name="NAME"/>
</element>
<element name="JP1" library="adafruit" package="1X15-CB" value="6"/>
<element name="JP2" library="adafruit" package="1X15-CB" value="4"/>
<element name="NRF24L01+" library="adafruit" package="2X04" value="2">
<attribute name="NAME"/>
</element>
<element name="U$1" library="jet-lib" package="PDIP-32" value="ARDUINONANO"/>
</elements>
<signals>
<signal name="GND">
<contactref element="U$1" pad="GND1"/>
<contactref element="JP2" pad="2"/>
<contactref element="NRF24L01+" pad="8"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="5V">
<contactref element="JP2" pad="1"/>
<contactref element="U$1" pad="VIN"/>
</signal>
<signal name="N$3">
<contactref element="JP1" pad="15"/>
<contactref element="U$1" pad="D1/TX"/>
</signal>
<signal name="N$4">
<contactref element="JP1" pad="14"/>
<contactref element="U$1" pad="D0/RX"/>
</signal>
<signal name="N$5">
<contactref element="JP1" pad="13"/>
<contactref element="U$1" pad="RESET"/>
</signal>
<signal name="N$6">
<contactref element="JP1" pad="12"/>
<contactref element="U$1" pad="GND"/>
</signal>
<signal name="D2">
<contactref element="JP1" pad="11"/>
<contactref element="U$1" pad="D2"/>
<contactref element="NRF24L01+" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="JP1" pad="10"/>
<contactref element="U$1" pad="D3"/>
</signal>
<signal name="N$9">
<contactref element="JP1" pad="9"/>
<contactref element="U$1" pad="D4"/>
</signal>
<signal name="N$10">
<contactref element="JP1" pad="8"/>
<contactref element="U$1" pad="D5"/>
</signal>
<signal name="N$11">
<contactref element="JP1" pad="7"/>
<contactref element="U$1" pad="D6"/>
</signal>
<signal name="N$12">
<contactref element="JP1" pad="6"/>
<contactref element="U$1" pad="D7"/>
</signal>
<signal name="N$13">
<contactref element="JP1" pad="5"/>
<contactref element="U$1" pad="D8"/>
</signal>
<signal name="D9">
<contactref element="JP1" pad="4"/>
<contactref element="U$1" pad="D9"/>
<contactref element="NRF24L01+" pad="6"/>
</signal>
<signal name="D10">
<contactref element="JP1" pad="3"/>
<contactref element="U$1" pad="D10"/>
<contactref element="NRF24L01+" pad="5"/>
</signal>
<signal name="D11">
<contactref element="JP1" pad="2"/>
<contactref element="U$1" pad="D11"/>
<contactref element="NRF24L01+" pad="3"/>
</signal>
<signal name="D12">
<contactref element="JP1" pad="1"/>
<contactref element="U$1" pad="D12"/>
<contactref element="NRF24L01+" pad="2"/>
</signal>
<signal name="N$20">
<contactref element="JP2" pad="3"/>
<contactref element="U$1" pad="RESET1"/>
</signal>
<signal name="N$21">
<contactref element="JP2" pad="4"/>
<contactref element="U$1" pad="+5V"/>
</signal>
<signal name="N$22">
<contactref element="JP2" pad="5"/>
<contactref element="U$1" pad="A0"/>
</signal>
<signal name="N$23">
<contactref element="JP2" pad="6"/>
<contactref element="U$1" pad="A1"/>
</signal>
<signal name="N$24">
<contactref element="JP2" pad="7"/>
<contactref element="U$1" pad="A2"/>
</signal>
<signal name="N$25">
<contactref element="JP2" pad="8"/>
<contactref element="U$1" pad="A3"/>
</signal>
<signal name="N$26">
<contactref element="JP2" pad="9"/>
<contactref element="U$1" pad="A4"/>
</signal>
<signal name="N$27">
<contactref element="JP2" pad="10"/>
<contactref element="U$1" pad="A5"/>
</signal>
<signal name="N$28">
<contactref element="JP2" pad="11"/>
<contactref element="U$1" pad="A6"/>
</signal>
<signal name="N$29">
<contactref element="JP2" pad="12"/>
<contactref element="U$1" pad="A7"/>
</signal>
<signal name="N$30">
<contactref element="JP2" pad="13"/>
<contactref element="U$1" pad="AREF"/>
</signal>
<signal name="3V3">
<contactref element="C1" pad="1"/>
<contactref element="NRF24L01+" pad="7"/>
<contactref element="U$1" pad="3V3"/>
<contactref element="JP2" pad="14"/>
</signal>
<signal name="D13">
<contactref element="JP2" pad="15"/>
<contactref element="U$1" pad="D13"/>
<contactref element="NRF24L01+" pad="4"/>
</signal>
<signal name="N$14">
</signal>
<signal name="N$16">
</signal>
<signal name="N$17">
</signal>
<signal name="N$18">
</signal>
<signal name="N$19">
</signal>
<signal name="N$31">
</signal>
<signal name="N$32">
</signal>
<signal name="N$33">
</signal>
<signal name="N$15">
</signal>
</signals>
</board>
</drawing>
</eagle>
