(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0.051)
		(solder_mask_min_width 0.25)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x0021020_7fffffff)
			(plot_on_all_layers_selection 0x0001000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes no)
			(usegerberadvancedattributes no)
			(creategerberjobfile no)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue no)
			(plotfptext yes)
			(plotinvisibletext yes)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 5)
			(mirror no)
			(drillshape 2)
			(scaleselection 1)
			(outputdirectory "board/svg/")
		)
	)
	(net 0 "")
	(net 1 "+3V3")
	(net 2 "Vh")
	(net 3 "/VHp")
	(net 4 "/LED_EN")
	(net 5 "/LED_R")
	(net 6 "/OVP/OVP_SW")
	(net 7 "/OVP/OVP_TRIG")
	(net 8 "/EN_5V")
	(net 9 "/LDO_ADJ")
	(net 10 "GND")
	(net 11 "/EN_3V")
	(net 12 "+5V")
	(net 13 "/5V/BuckIn")
	(net 14 "/5V/COMP_Z")
	(net 15 "/5V/COMP")
	(net 16 "/5V/SS")
	(net 17 "/5V/BOOT")
	(net 18 "/5V/VBsw")
	(net 19 "/5V/FB")
	(net 20 "/5VLED_R")
	(footprint "Pin_Headers:Pin_Header_Angled_2x02_Pitch2.54mm"
		(layer "F.Cu")
		(at 24.13 38.735 -90)
		(descr "Through hole angled pin header, 2x02, 2.54mm pitch, 6mm pin length, double rows")
		(tags "Through hole angled pin header THT 2x02 2.54mm double row")
		(property "Reference" "J3"
			(at 5.365 0.03 180)
			(layer "F.SilkS")
		)
		(property "Value" "V_IN"
			(at 5.655 4.81 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Pin_Headers:Pin_Header_Angled_2x02_Pitch2.54mm"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "ModPSU-5V-Buck-3V3.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.31 1.27 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Vh")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0 270)
			(size 1.73 1.73)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Vh")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
			(zone_connect 2)
		)
		(pad "4" thru_hole oval
			(at 2.54 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
			(zone_connect 2)
		)
		(model "${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x02_P2.54mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TPW-Passive:C_0603_HandSoldering-Medium"
		(layer "F.Cu")
		(at 22.65 26.1 180)
		(descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
		(tags "capacitor 0603")
		(property "Reference" "C12"
			(at -1.35 -1 180)
			(layer "F.SilkS")
		)
		(property "Value" "OPT/100n"
			(at 0 1.249999 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TPW-Passive:C_0603_HandSoldering-Medium"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "OVP")
		(sheetfile "OVP.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.7 0 180)
			(size 0.9 0.75)
			(drill
				(offset -0.1 0)
			)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "/OVP/OVP_SW")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.7 0 180)
			(size 0.9 0.75)
			(drill
				(offset 0.1 0)
			)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "GND")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TPW-Passive:C_0805_0603_HandSoldering-Medium"
		(layer "F.Cu")
		(at 40.1 27.199999 90)
		(descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
		(tags "capacitor 0805")
		(property "Reference" "C5"
			(at 3.199999 -0.3 180)
			(layer "F.SilkS")
		)
		(property "Value" "10u/OPT"
			(at 0 1.75 90)
			(layer "F.Fab")
		)
		(property "Footprint" "TPW-Passive:C_0805_0603_HandSoldering-Medium"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" "GRM188R6YA106MA73J"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Vmax" "30V+"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "5V")
		(sheetfile "Buck-5V.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.000001 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd custom
			(at -1.1 0 90)
			(size 1.2 1.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 13 "/5V/BuckIn")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0.75 0.375) (xy 0.6 0.375) (xy 0.6 -0.375) (xy 0.75 -0.375)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd custom
			(at 1.1 0 90)
			(size 1.2 1.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "GND")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_poly
					(pts
						(xy -0.6 0.375) (xy -0.75 0.375) (xy -0.75 -0.375) (xy -0.6 -0.375)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TPW-Passive:L_0805_0603_HandSoldering-Medium"
		(layer "F.Cu")
		(at 35.2 28.2 180)
		(descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
		(tags "capacitor 0805")
		(property "Reference" "L1"
			(at 2.5 -0.2 0)
			(layer "F.SilkS")
		)
		(property "Value" "L_Core_Ferrite"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TPW-Passive:L_0805_0603_HandSoldering-Medium"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor with ferrite core"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" "MFBM1V1608-150-R"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartAlt" "WLBD1608HCU121TH"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Vendor" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "5V")
		(sheetfile "Buck-5V.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd custom
			(at -1.15 0 180)
			(size 1.1 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 13 "/5V/BuckIn")
			(pinfunction "1")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0.55 -0.45) (xy 0.65 -0.45) (xy 0.65 0.45) (xy 0.55 0.45) (xy 0.55 -0.65)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd custom
			(at 1.15 0 180)
			(size 1.1 1.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "/VHp")
			(pinfunction "2")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_poly
					(pts
						(xy -0.55 0.45) (xy -0.65 0.45) (xy -0.65 -0.45) (xy -0.55 -0.45)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TPW-Passive:R_0603_HandSoldering-Medium"
		(layer "F.Cu")
		(at 29 33.2)
		(descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
		(tags "resistor 0603")
		(property "Reference" "R7"
			(at -1.8 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.3 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TPW-Passive:R_0603_HandSoldering-Medium"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" "CR0603-FX-1002ELF"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "OVP")
		(sheetfile "OVP.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.75 0)
			(size 0.75 0.9)
			(drill
				(offset -0.125 0)
			)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "Vh")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.75 0)
			(size 0.75 0.9)
			(drill
				(offset 0.125 0)
			)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "/OVP/OVP_TRIG")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm"
		(layer "F.Cu")
		(at 27.55 27.95 90)
		(descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
		(tags "SOIC 1.27")
		(property "Reference" "Q1"
			(at -2.85 -3.15 -90)
			(layer "F.SilkS")
		)
		(property "Value" "PMOS-2CH"
			(at 0 3.5 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Dual PMOS transistor, 8 pin package"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" "DMP6110SSDQ-13"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartAlt" "DMP6050SSD-13"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Vendor" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SO*")
		(sheetname "OVP")
		(sheetfile "OVP.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.7 -1.905 90)
			(size 1.55 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "Vh")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -2.7 -0.635 90)
			(size 1.55 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "/OVP/OVP_SW")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -2.7 0.635 90)
			(size 1.55 0.6)
			(drill
				(offset -0.075 0)
			)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "Vh")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at -2.7 1.905 90)
			(size 1.55 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "/OVP/OVP_TRIG")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at 2.7 1.905 90)
			(size 1.55 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "/OVP/OVP_SW")
			(pinfunction "D")
			(pintype "passive")
		)
		(pad "6" smd roundrect
			(at 2.7 0.635 90)
			(size 1.55 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "/OVP/OVP_SW")
			(pinfunction "D")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 2.7 -0.635 90)
			(size 1.55 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "/VHp")
			(pinfunction "D")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at 2.7 -1.905 90)
			(size 1.55 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "/VHp")
			(pinfunction "D")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TPW-Passive:C_0603_HandSoldering-Medium"
		(layer "F.Cu")
		(at 38.6 38.5 -90)
		(descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
		(tags "capacitor 0603")
		(property "Reference" "C7"
			(at 2 0.7 90)
			(layer "F.SilkS")
		)
		(property "Value" "47p"
			(at 0 1.25 90)
			(layer "F.Fab")
		)
		(property "Footprint" "TPW-Passive:C_0603_HandSoldering-Medium"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartAlt" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "5V")
		(sheetfile "Buck-5V.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.75 0 270)
			(size 1 0.75)
			(drill
				(offset -0.1 0)
			)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 15 "/5V/COMP")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.75 0 270)
			(size 1 0.75)
			(drill
				(offset 0.1 0)
			)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "GND")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TPW-Passive:C_0603_HandSoldering-Medium"
		(layer "F.Cu")
		(at 43.000001 33.9 90)
		(descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
		(tags "capacitor 0603")
		(property "Reference" "C9"
			(at -1.9 0.399999 180)
			(layer "F.SilkS")
		)
		(property "Value" "100n"
			(at 0 1.25 90)
			(layer "F.Fab")
		)
		(property "Footprint" "TPW-Passive:C_0603_HandSoldering-Medium"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" "CL10B105KA8NFNC"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartAlt" "CL10A105KO8NNWC"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "5V")
		(sheetfile "Buck-5V.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.75 0 90)
			(size 1 0.75)
			(drill
				(offset -0.1 0)
			)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 18 "/5V/VBsw")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.75 0 90)
			(size 1 0.75)
			(drill
				(offset 0.1 0)
			)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 17 "/5V/BOOT")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TPW-Passive:C_0603_HandSoldering-Medium"
		(layer "F.Cu")
		(at 42.000001 38.5 -90)
		(descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
		(tags "capacitor 0603")
		(property "Reference" "C6"
			(at 2.2 0.8 90)
			(layer "F.SilkS")
		)
		(property "Value" "1n"
			(at 0 1.25 90)
			(layer "F.Fab")
		)
		(property "Footprint" "TPW-Passive:C_0603_HandSoldering-Medium"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartAlt" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "5V")
		(sheetfile "Buck-5V.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.75 0 270)
			(size 1 0.75)
			(drill
				(offset -0.1 0)
			)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "/5V/COMP_Z")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.75 0 270)
			(size 1 0.75)
			(drill
				(offset 0.1 0)
			)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "GND")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TPW-Passive:R_0603_HandSoldering-Medium"
		(layer "F.Cu")
		(at 43.000001 30.8 -90)
		(descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
		(tags "resistor 0603")
		(property "Reference" "R5"
			(at 1.3 0.900001 90)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.3 90)
			(layer "F.Fab")
		)
		(property "Footprint" "TPW-Passive:R_0603_HandSoldering-Medium"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" "RC0603FR-0710KL"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "5V")
		(sheetfile "Buck-5V.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.75 0 270)
			(size 0.75 0.9)
			(drill
				(offset -0.125 0)
			)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 12 "+5V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.75 0 270)
			(size 0.75 0.9)
			(drill
				(offset 0.125 0)
			)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 19 "/5V/FB")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TPW-Passive:R_0603_HandSoldering-Medium"
		(layer "F.Cu")
		(at 36.805001 38.499999 -90)
		(descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
		(tags "resistor 0603")
		(property "Reference" "R6"
			(at 2.000001 0.8 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k8"
			(at 0 1.3 90)
			(layer "F.Fab")
		)
		(property "Footprint" "TPW-Passive:R_0603_HandSoldering-Medium"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" "RC0603FR-072K8L"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "5V")
		(sheetfile "Buck-5V.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.75 0 270)
			(size 0.75 0.9)
			(drill
				(offset -0.125 0)
			)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 19 "/5V/FB")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.75 0 270)
			(size 0.75 0.9)
			(drill
				(offset 0.125 0)
			)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "GND")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TPW-Passive:R_0603_HandSoldering-Medium"
		(layer "F.Cu")
		(at 40.3 38.5 -90)
		(descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
		(tags "resistor 0603")
		(property "Reference" "R4"
			(at 2.2 0.2 -90)
			(layer "F.SilkS")
		)
		(property "Value" "29k4"
			(at 0 1.3 90)
			(layer "F.Fab")
		)
		(property "Footprint" "TPW-Passive:R_0603_HandSoldering-Medium"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" "RC0603FR-0729K4L"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "5V")
		(sheetfile "Buck-5V.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.75 0 270)
			(size 0.75 0.9)
			(drill
				(offset -0.125 0)
			)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 15 "/5V/COMP")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.75 0 270)
			(size 0.75 0.9)
			(drill
				(offset 0.125 0)
			)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "/5V/COMP_Z")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TPW-Passive:R_0603_HandSoldering-Medium"
		(layer "F.Cu")
		(at 35 37.2 -90)
		(descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
		(tags "resistor 0603")
		(property "Reference" "R3"
			(at 2.7 0.4 0)
			(layer "F.SilkS")
		)
		(property "Value" "22k"
			(at 0 1.3 90)
			(layer "F.Fab")
		)
		(property "Footprint" "TPW-Passive:R_0603_HandSoldering-Medium"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" "RC0603FR-1022KL"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "5V")
		(sheetfile "Buck-5V.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.75 0 270)
			(size 0.75 0.9)
			(drill
				(offset -0.125 0)
			)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "/EN_5V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.75 0 270)
			(size 0.75 0.9)
			(drill
				(offset 0.125 0)
			)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "GND")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm"
		(layer "F.Cu")
		(at 39 33.2 -90)
		(descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
		(tags "SOIC 1.27")
		(property "Reference" "U2"
			(at 3.1 -2.9 90)
			(layer "F.SilkS")
		)
		(property "Value" "2A"
			(at 0 3.5 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Housings_SOIC:SOIC-8_3.9x4.9mm_Pitch1.27mm"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/gpn/tps54231"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" "TPS54231"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Texas Instruments"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartAlt" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Vendor" "https://www.mouser.com/ProductDetail/Texas-Instruments/TPS54231DR?qs=XGzIaZb%2FFYKibJTOhGUd1A%3D%3D"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOIC*3.9x4.9mm*")
		(sheetname "5V")
		(sheetfile "Buck-5V.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.7 -1.905 270)
			(size 1.55 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 17 "/5V/BOOT")
			(pinfunction "BOOT")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -2.7 -0.635 270)
			(size 1.55 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 13 "/5V/BuckIn")
			(pinfunction "VIN")
			(pintype "power_in")
		)
		(pad "3" smd rect
			(at -2.7 0.635 270)
			(size 1.55 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "/EN_5V")
			(pinfunction "EN")
			(pintype "input")
		)
		(pad "4" smd rect
			(at -2.7 1.905 270)
			(size 1.55 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 16 "/5V/SS")
			(pinfunction "SS")
			(pintype "input")
		)
		(pad "5" smd rect
			(at 2.7 1.905 270)
			(size 1.55 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 19 "/5V/FB")
			(pinfunction "FB")
			(pintype "input")
		)
		(pad "6" smd rect
			(at 2.7 0.635 270)
			(size 1.55 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 15 "/5V/COMP")
			(pinfunction "COMP")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 2.7 -0.635 270)
			(size 1.55 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "8" smd rect
			(at 2.7 -1.905 270)
			(size 1.55 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 18 "/5V/VBsw")
			(pinfunction "PH")
			(pintype "output")
		)
		(model "${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TPW-Passive:DO-214AC_V2_Handsolder"
		(layer "F.Cu")
		(at 46.400001 39.3)
		(descr "SMA/DO-214AC Diode")
		(tags "DO-214AC SMA")
		(property "Reference" "D1"
			(at 4.4 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "3A"
			(at 0 -2.159 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TPW-Passive:DO-214AC_V2_Handsolder"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Schottky diode"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" "SDT5A50SA-13"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartAlt" "SK54A-LTP,SK56A-LTP"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Vr" "30V+"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "5V")
		(sheetfile "Buck-5V.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.875 0)
			(size 2.2 2.2)
			(drill
				(offset -0.425 0)
			)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 18 "/5V/VBsw")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.875 0)
			(size 2.2 2.2)
			(drill
				(offset 0.425 0)
			)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "GND")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMA.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TPW-Passive:C_0805_0603_HandSoldering-Medium"
		(layer "F.Cu")
		(at 38.1 27.2 90)
		(descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
		(tags "capacitor 0805")
		(property "Reference" "C4"
			(at 3.2 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 1.75 90)
			(layer "F.Fab")
		)
		(property "Footprint" "TPW-Passive:C_0805_0603_HandSoldering-Medium"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" "GRM188R6YA106MA73J"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "5V")
		(sheetfile "Buck-5V.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd custom
			(at -1.1 0 90)
			(size 1.2 1.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 13 "/5V/BuckIn")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0.75 0.375) (xy 0.6 0.375) (xy 0.6 -0.375) (xy 0.75 -0.375)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd custom
			(at 1.1 0 90)
			(size 1.2 1.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "GND")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_poly
					(pts
						(xy -0.6 0.375) (xy -0.75 0.375) (xy -0.75 -0.375) (xy -0.6 -0.375)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TPW-Passive:R_0603_HandSoldering-Medium"
		(layer "F.Cu")
		(at 35.159771 34 90)
		(descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
		(tags "resistor 0603")
		(property "Reference" "R2"
			(at 1.4 -0.859771 90)
			(layer "F.SilkS")
		)
		(property "Value" "169k"
			(at 0 1.3 90)
			(layer "F.Fab")
		)
		(property "Footprint" "TPW-Passive:R_0603_HandSoldering-Medium"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" "RC0603FR-07169KL"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "5V")
		(sheetfile "Buck-5V.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.75 0 90)
			(size 0.75 0.9)
			(drill
				(offset -0.125 0)
			)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 13 "/5V/BuckIn")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.75 0 90)
			(size 0.75 0.9)
			(drill
				(offset 0.125 0)
			)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "/EN_5V")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TPW-Passive:C_0805_0603_HandSoldering-Medium"
		(layer "F.Cu")
		(at 35.2 26.275)
		(descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
		(tags "capacitor 0805")
		(property "Reference" "C3"
			(at 0 -1.375 0)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 1.75 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TPW-Passive:C_0805_0603_HandSoldering-Medium"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" "GRM188R6YA106MA73J"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "5V")
		(sheetfile "Buck-5V.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0.025 0)
			(layer "F.Fab")
		)
		(pad "1" smd custom
			(at -1.1 0)
			(size 1.2 1.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "/VHp")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0.75 0.375) (xy 0.6 0.375) (xy 0.6 -0.375) (xy 0.75 -0.375)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd custom
			(at 1.1 0)
			(size 1.2 1.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "GND")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_poly
					(pts
						(xy -0.6 0.375) (xy -0.75 0.375) (xy -0.75 -0.375) (xy -0.6 -0.375)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TPW-Connectors:TestPoint-PTH-1.0mm-Octagon"
		(layer "F.Cu")
		(at 32 25.2)
		(descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row, test point")
		(tags "Through hole pin header THT 1x01 2.54mm single row test point")
		(property "Reference" "TP2"
			(at 0 1.9 0)
			(layer "F.SilkS")
		)
		(property "Value" "Vhp"
			(at 0 1.9 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TPW-Connectors:TestPoint-PTH-1.0mm-Octagon"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "ModPSU-5V-Buck-3V3.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole custom
			(at 0 0)
			(size 1.1 1.1)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/VHp")
			(pinfunction "1")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0.8 -0.4) (xy 0.8 0.4) (xy 0.4 0.8) (xy -0.4 0.8) (xy -0.8 0.4) (xy -0.8 -0.4) (xy -0.4 -0.8)
						(xy 0.4 -0.8)
					)
					(width 0)
					(fill yes)
				)
			)
		)
	)
	(footprint "TPW-Passive:C_0603_HandSoldering-Medium"
		(layer "F.Cu")
		(at 60.3 29.6 90)
		(descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
		(tags "capacitor 0603")
		(property "Reference" "C1"
			(at -2.1 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "1u"
			(at 0 1.249999 90)
			(layer "F.Fab")
		)
		(property "Footprint" "TPW-Passive:C_0603_HandSoldering-Medium"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" "CL10B105KA8NFNC"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartAlt" "CL10A105KO8NNWC"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Vendor" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "ModPSU-5V-Buck-3V3.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.75 0 90)
			(size 1 0.75)
			(drill
				(offset -0.1 0)
			)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 12 "+5V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.75 0 90)
			(size 1 0.75)
			(drill
				(offset 0.1 0)
			)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "GND")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TPW-Passive:R_0603_HandSoldering-Medium"
		(layer "F.Cu")
		(at 72.8 25.7 180)
		(descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
		(tags "resistor 0603")
		(property "Reference" "R1"
			(at 0 0 -90)
			(layer "F.SilkS")
		)
		(property "Value" "2k?"
			(at 0 1.3 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TPW-Passive:R_0603_HandSoldering-Medium"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "ModPSU-5V-Buck-3V3.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.75 0 180)
			(size 0.75 0.9)
			(drill
				(offset -0.125 0)
			)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.75 0 180)
			(size 0.75 0.9)
			(drill
				(offset 0.125 0)
			)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "/LED_R")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TPW-Connectors:Jumper-Solder-Wedge-30V"
		(layer "F.Cu")
		(at 70.6 26.2 -90)
		(descr "Jumper Solder 1mm Wedge Shape Approx 30V 1A")
		(tags "Jumper Solder 30V")
		(property "Reference" "JP1"
			(at -0.9 1.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LED_EN"
			(at 0 -1.099999 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TPW-Connectors:Jumper-Solder-Wedge-30V"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "ModPSU-5V-Buck-3V3.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd custom
			(at -0.75 0 270)
			(size 1 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "/LED_EN")
			(pinfunction "Pin_1")
			(pintype "passive")
			(zone_connect 0)
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0.75 0) (xy 0.25 0.5) (xy 0 0.5) (xy 0 -0.5) (xy 0.25 -0.5)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd custom
			(at 0.499999 0 270)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
			(zone_connect 0)
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_arc
					(start 0 -0.25)
					(mid 0.25 0)
					(end 0 0.25)
					(width 0.5)
				)
				(gr_poly
					(pts
						(xy 0 0.5) (xy -0.75 0.5) (xy -0.25 0) (xy -0.75 -0.5) (xy 0 -0.5)
					)
					(width 0)
					(fill yes)
				)
			)
		)
	)
	(footprint "TPW-Connectors:TestPoint-PTH-1.0mm-Octagon"
		(layer "F.Cu")
		(at 59.7 25.9)
		(descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row, test point")
		(tags "Through hole pin header THT 1x01 2.54mm single row test point")
		(property "Reference" "TP3"
			(at 0 -1.9 0)
			(layer "F.SilkS")
		)
		(property "Value" "5V"
			(at 0 1.9 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TPW-Connectors:TestPoint-PTH-1.0mm-Octagon"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "ModPSU-5V-Buck-3V3.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole custom
			(at 0 0)
			(size 1.1 1.1)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "+5V")
			(pinfunction "1")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0.8 -0.4) (xy 0.8 0.4) (xy 0.4 0.8) (xy -0.4 0.8) (xy -0.8 0.4) (xy -0.8 -0.4) (xy -0.4 -0.8)
						(xy 0.4 -0.8)
					)
					(width 0)
					(fill yes)
				)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_2x05_P2.54mm_Horizontal"
		(layer "F.Cu")
		(at 72.39 38.735 -90)
		(descr "Through hole angled pin header, 2x05, 2.54mm pitch, 6mm pin length, double rows")
		(tags "Through hole angled pin header THT 2x05 2.54mm double row")
		(property "Reference" "J4"
			(at 5.265 10.19 0)
			(layer "F.SilkS")
		)
		(property "Value" "V_OUT"
			(at 5.655 12.43 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_2x05_P2.54mm_Horizontal"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x10, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Vendor" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartAlt" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "ModPSU-5V-Buck-3V3.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.31 5.08 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+3V3")
			(pinfunction "Pin_3")
			(pintype "passive")
			(zone_connect 2)
		)
		(pad "4" thru_hole oval
			(at 2.54 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+3V3")
			(pinfunction "Pin_4")
			(pintype "passive")
			(zone_connect 2)
		)
		(pad "5" thru_hole oval
			(at 0 5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/EN_3V")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 2.54 5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/EN_5V")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 0 7.62 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "+5V")
			(pinfunction "Pin_7")
			(pintype "passive")
			(zone_connect 2)
		)
		(pad "8" thru_hole oval
			(at 2.54 7.62 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "+5V")
			(pinfunction "Pin_8")
			(pintype "passive")
			(zone_connect 2)
		)
		(pad "9" thru_hole circle
			(at 0 10.16 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "GND")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" thru_hole circle
			(at 2.54 10.16 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "GND")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x05_P2.54mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TPW-Passive:C_0603_HandSoldering-Medium"
		(layer "F.Cu")
		(at 35.159771 30.9 -90)
		(descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
		(tags "capacitor 0603")
		(property "Reference" "C8"
			(at -1.1 0.859771 90)
			(layer "F.SilkS")
		)
		(property "Value" "10n"
			(at 0 1.25 90)
			(layer "F.Fab")
		)
		(property "Footprint" "TPW-Passive:C_0603_HandSoldering-Medium"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" "CL10B103KB8WPND"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "5V")
		(sheetfile "Buck-5V.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.75 0 270)
			(size 1 0.75)
			(drill
				(offset -0.1 0)
			)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 16 "/5V/SS")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.75 0 270)
			(size 1 0.75)
			(drill
				(offset 0.1 0)
			)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "GND")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TPW-Passive:DO-214AC_V2_Handsolder"
		(layer "F.Cu")
		(at 32.3 33.1 -90)
		(descr "SMA/DO-214AC Diode")
		(tags "DO-214AC SMA")
		(property "Reference" "D2"
			(at 4.4 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "3.5A+"
			(at 0 -2.159 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TPW-Passive:DO-214AC_V2_Handsolder"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Schottky diode"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" "SDT5A50SA-13"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartAlt" "SK54A-LTP;SK56A-LTP"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Vendor" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "OVP")
		(sheetfile "OVP.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.875 0 270)
			(size 2.2 2.2)
			(drill
				(offset -0.425 0)
			)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "/VHp")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.875 0 270)
			(size 2.2 2.2)
			(drill
				(offset 0.425 0)
			)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "GND")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SMA.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LEDs:LED_0603_HandSoldering"
		(layer "F.Cu")
		(at 72.3 24.3)
		(descr "LED SMD 0603, hand soldering")
		(tags "LED 0603")
		(property "Reference" "LED1"
			(at -3.5 -0.2 180)
			(layer "F.SilkS")
		)
		(property "Value" "ORG"
			(at 0 1.550001 0)
			(layer "F.Fab")
		)
		(property "Footprint" "LEDs:LED_0603_HandSoldering"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Vendor" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartAlt" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "Root")
		(sheetfile "ModPSU-5V-Buck-3V3.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.05 0)
			(size 1.1 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "/LED_EN")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.05 0)
			(size 1.1 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "/LED_R")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 180)
			)
		)
		(model "${KISYS3DMOD}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TPW-Passive:C_0805_0603_HandSoldering-Medium"
		(layer "F.Cu")
		(at 55 38.3)
		(descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
		(tags "capacitor 0805")
		(property "Reference" "C11"
			(at 2.500001 0 -90)
			(layer "F.SilkS")
		)
		(property "Value" "22u"
			(at 0 1.75 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TPW-Passive:C_0805_0603_HandSoldering-Medium"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartAlt" "GRM188R61A226ME15J"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" "GRM21BR61C226ME44K"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Vendor" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "5V")
		(sheetfile "Buck-5V.kicad_sch")
		(attr smd dnp)
		(fp_text user "${REFERENCE}"
			(at 0 -1.5 0)
			(layer "F.Fab")
		)
		(pad "1" smd custom
			(at -1.099999 0)
			(size 1.2 1.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "GND")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0.75 0.375) (xy 0.6 0.375) (xy 0.6 -0.375) (xy 0.75 -0.375)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd custom
			(at 1.099999 0)
			(size 1.2 1.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 12 "+5V")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_poly
					(pts
						(xy -0.6 0.375) (xy -0.75 0.375) (xy -0.75 -0.375) (xy -0.6 -0.375)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SOD-123"
		(layer "F.Cu")
		(at 72.6 28.8 90)
		(descr "SOD-123")
		(tags "SOD-123")
		(property "Reference" "Z1"
			(at -3 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "3V6"
			(at 0 2.1 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Diode_SMD:D_SOD-123"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Zener diode"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" "BZT52C3V6-TP"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartAlt" "BZX79-C3V6,143;KDZVTR3.6B"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Vendor" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "Root")
		(sheetfile "ModPSU-5V-Buck-3V3.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "+3V3")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.65 0 90)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "GND")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "STMicroelectronics:LF50ABPTTR"
		(layer "F.Cu")
		(at 65.5 30.8 90)
		(descr "PPAK_FFW")
		(tags "Integrated Circuit")
		(property "Reference" "U1"
			(at -0.525 -3.8 -90)
			(layer "F.SilkS")
		)
		(property "Value" "LD39150PT-R"
			(at 0.5 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "STMicroelectronics:LF50ABPTTR"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/ld39150.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "STMicroelectronics"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" "LD39150PT-R"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartAlt" "LD39150DT33-R"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Vendor" "https://www.mouser.com/ProductDetail/STMicroelectronics/LD39150PT-R?qs=VJaATVMq%252BXpRWquXeJ%252BxYA%3D%3D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO*252*")
		(sheetname "Root")
		(sheetfile "ModPSU-5V-Buck-3V3.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.5 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -3.525 -2.54 180)
			(size 0.7 2.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "/EN_3V")
			(pinfunction "EN")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -3.525 -1.27 180)
			(size 0.7 2.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 12 "+5V")
			(pinfunction "VIN")
			(pintype "power_in")
			(zone_connect 2)
		)
		(pad "3" smd rect
			(at 3.275 0 90)
			(size 5.85 6.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "4" smd rect
			(at -3.525 1.27 180)
			(size 0.7 2.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "+3V3")
			(pinfunction "VOUT")
			(pintype "power_out")
			(zone_connect 2)
		)
		(pad "5" smd rect
			(at -3.525 2.54 180)
			(size 0.7 2.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "/LDO_ADJ")
			(pinfunction "ADJ")
			(pintype "input")
		)
		(model "${KICAD_USER_3DMODEL_DIR}/ST.3dshapes/LD39150PT-R.step"
			(offset
				(xyz 2.1 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 90)
			)
		)
	)
	(footprint "TPW-Passive:R_0603_HandSoldering-Medium"
		(layer "F.Cu")
		(at 70.8 33.75 180)
		(descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
		(tags "resistor 0603")
		(property "Reference" "R10"
			(at 0.7 1.25 0)
			(layer "F.SilkS")
		)
		(property "Value" "4k7"
			(at 0 1.3 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TPW-Passive:R_0603_HandSoldering-Medium"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "ModPSU-5V-Buck-3V3.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.75 0 180)
			(size 0.75 0.9)
			(drill
				(offset -0.125 0)
			)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "GND")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.75 0 180)
			(size 0.75 0.9)
			(drill
				(offset 0.125 0)
			)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "/LDO_ADJ")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TPW-Passive:R_0603_HandSoldering-Medium"
		(layer "F.Cu")
		(at 70.8 35.15 180)
		(descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
		(tags "resistor 0603")
		(property "Reference" "R9"
			(at -2.1 -0.05 0)
			(layer "F.SilkS")
		)
		(property "Value" "8k25"
			(at 0 1.3 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TPW-Passive:R_0603_HandSoldering-Medium"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Vendor" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartAlt" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "ModPSU-5V-Buck-3V3.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.75 0 180)
			(size 0.75 0.9)
			(drill
				(offset -0.125 0)
			)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.75 0 180)
			(size 0.75 0.9)
			(drill
				(offset 0.125 0)
			)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "/LDO_ADJ")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TPW-Passive:C_0603_HandSoldering-Medium"
		(layer "F.Cu")
		(at 70.7 29.5 90)
		(descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
		(tags "capacitor 0603")
		(property "Reference" "C2"
			(at -1.949999 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "2u2"
			(at 0 1.249999 90)
			(layer "F.Fab")
		)
		(property "Footprint" "TPW-Passive:C_0603_HandSoldering-Medium"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" "CL10A225KO8NNNC"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartAlt" "CL10A225KP8NNWC;CL10A225KP8NNNC"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "ModPSU-5V-Buck-3V3.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.75 0 90)
			(size 1 0.75)
			(drill
				(offset -0.1 0)
			)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.75 0 90)
			(size 1 0.75)
			(drill
				(offset 0.1 0)
			)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "GND")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TPW-Connectors:TestPoint-PTH-1.0mm-Octagon"
		(layer "F.Cu")
		(at 21.8 28.3 180)
		(descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row, test point")
		(tags "Through hole pin header THT 1x01 2.54mm single row test point")
		(property "Reference" "TP1"
			(at -1.905 -0.254 -90)
			(layer "F.SilkS")
		)
		(property "Value" "Vh"
			(at 0 1.9 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "TPW-Connectors:TestPoint-PTH-1.0mm-Octagon"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Vendor" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartAlt" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "Root")
		(sheetfile "ModPSU-5V-Buck-3V3.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole custom
			(at 0 0 180)
			(size 1.1 1.1)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Vh")
			(pinfunction "1")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0.8 -0.4) (xy 0.8 0.4) (xy 0.4 0.8) (xy -0.4 0.8) (xy -0.8 0.4) (xy -0.8 -0.4) (xy -0.4 -0.8)
						(xy 0.4 -0.8)
					)
					(width 0)
					(fill yes)
				)
			)
		)
	)
	(footprint "TPW-Passive:D_SOD-123_HS"
		(layer "F.Cu")
		(at 29.3 37.065 -90)
		(property "Reference" "Z2"
			(at 4.135 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "24"
			(at 0 -1.6 90)
			(layer "F.Fab")
		)
		(property "Footprint" "TPW-Passive:D_SOD-123_HS"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Zener diode"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" "BZT52C22-TP"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartAlt" "BZT52C20-TP"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "OVP")
		(sheetfile "OVP.kicad_sch")
		(solder_paste_margin -0.05)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "" smd circle
			(at 0 0 270)
			(size 1.2 1.2)
			(layers "F.Adhes")
		)
		(pad "1" smd rect
			(at -1.635 0 270)
			(size 1.5 1.22)
			(drill
				(offset -0.295 0)
			)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "/OVP/OVP_TRIG")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.635 0 270)
			(size 1.5 1.22)
			(drill
				(offset 0.295 0)
			)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "GND")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductors_SMD:L_Taiyo-Yuden_NR-80xx_HandSoldering"
		(layer "F.Cu")
		(at 50.6 32 -90)
		(descr "Inductor, Taiyo Yuden, NR series, Taiyo-Yuden_NR-80xx, 8.0mmx8.0mm")
		(tags "inductor taiyo-yuden nr smd")
		(property "Reference" "L2"
			(at -4.6 -4.85 0)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 5.5 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Inductors_SMD:L_Taiyo-Yuden_NR-80xx_HandSoldering"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" "NRS8040T100MJGJ"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartAlt" "NR8040T100M;BWVS00808040100M00"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Vendor" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "5V")
		(sheetfile "Buck-5V.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -3.45 0 270)
			(size 3.1 7.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 12 "+5V")
			(pinfunction "1")
			(pintype "passive")
			(zone_connect 2)
		)
		(pad "2" smd rect
			(at 3.45 0 270)
			(size 3.1 7.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 18 "/5V/VBsw")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KICAD_USER_3DMODEL_DIR}/TaiyoYuden.3dshapes/AndreyGulyants-NRS8040.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 90)
			)
		)
	)
	(footprint "TPW-Passive:R_0603_HandSoldering-Medium"
		(layer "F.Cu")
		(at 22.6 24.7 180)
		(descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
		(tags "resistor 0603")
		(property "Reference" "R8"
			(at -1.9 0 -90)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.3 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TPW-Passive:R_0603_HandSoldering-Medium"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" "CR0603-FX-1002ELF"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "OVP")
		(sheetfile "OVP.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.75 0 180)
			(size 0.75 0.9)
			(drill
				(offset -0.125 0)
			)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "/OVP/OVP_SW")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.75 0 180)
			(size 0.75 0.9)
			(drill
				(offset 0.125 0)
			)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "GND")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TPW-Passive:C_0805_0603_HandSoldering-Medium"
		(layer "F.Cu")
		(at 43.3 27.2 -90)
		(descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
		(tags "capacitor 0805")
		(property "Reference" "C10"
			(at 0.5 -1.8 90)
			(layer "F.SilkS")
		)
		(property "Value" "22u"
			(at 0 1.75 90)
			(layer "F.Fab")
		)
		(property "Footprint" "TPW-Passive:C_0805_0603_HandSoldering-Medium"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartAlt" "GRM188R61A226ME15J"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" "GRM21BR61C226ME44K"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "5V")
		(sheetfile "Buck-5V.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -1.5 90)
			(layer "F.Fab")
		)
		(pad "1" smd custom
			(at -1.1 0 270)
			(size 1.2 1.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 10 "GND")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0.75 0.375) (xy 0.6 0.375) (xy 0.6 -0.375) (xy 0.75 -0.375)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd custom
			(at 1.1 0 270)
			(size 1.2 1.25)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 12 "+5V")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_poly
					(pts
						(xy -0.6 0.375) (xy -0.75 0.375) (xy -0.75 -0.375) (xy -0.6 -0.375)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(model "${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TPW-Passive:R_0603_HandSoldering-Medium"
		(layer "F.Cu")
		(at 41.7 26.9 90)
		(descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
		(tags "resistor 0603")
		(property "Reference" "R11"
			(at -1.9 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "2k?"
			(at 0 1.3 90)
			(layer "F.Fab")
		)
		(property "Footprint" "TPW-Passive:R_0603_HandSoldering-Medium"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "ModPSU-5V-Buck-3V3.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.75 0 90)
			(size 0.75 0.9)
			(drill
				(offset -0.125 0)
			)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 12 "+5V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.75 0 90)
			(size 0.75 0.9)
			(drill
				(offset 0.125 0)
			)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 20 "/5VLED_R")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TPW-Decorative:sig-wlx"
		(layer "F.Cu")
		(at 25.4 36.2)
		(property "Reference" "G1"
			(at 0 0.1 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "WLX"
			(at 0.75 0.1 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Footprint" "TPW-Decorative:sig-wlx"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Vendor" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartAlt" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TPW-Decorative:sig-wlx")
		(sheetname "Root")
		(sheetfile "ModPSU-5V-Buck-3V3.kicad_sch")
		(attr exclude_from_pos_files)
	)
	(footprint "TPW-Passive:R_0603_HandSoldering-Medium"
		(layer "F.Cu")
		(at 60.3 34)
		(descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
		(tags "resistor 0603")
		(property "Reference" "R12"
			(at 0 1.3 180)
			(layer "F.SilkS")
		)
		(property "Value" "100k"
			(at 0 1.3 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TPW-Passive:R_0603_HandSoldering-Medium"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "ModPSU-5V-Buck-3V3.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.75 0)
			(size 0.75 0.9)
			(drill
				(offset -0.125 0)
			)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 12 "+5V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.75 0)
			(size 0.75 0.9)
			(drill
				(offset 0.125 0)
			)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 11 "/EN_3V")
			(pintype "passive")
		)
		(model "${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SOD-123"
		(layer "F.Cu")
		(at 54.7 40.5 180)
		(descr "SOD-123")
		(tags "SOD-123")
		(property "Reference" "Z3"
			(at -3 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "5V6"
			(at 0 2.1 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Diode_SMD:D_SOD-123"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Zener diode"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" "BZT52C3V6-TP"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartAlt" "BZX79-C3V6,143;KDZVTR3.6B"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Vendor" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "Root")
		(sheetfile "ModPSU-5V-Buck-3V3.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.000001 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.65 0 180)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 12 "+5V")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.65 0 180)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "GND")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SMA"
		(layer "F.Cu")
		(at 21.7 33.3 -90)
		(descr "Diode SMA (DO-214AC)")
		(tags "Diode SMA (DO-214AC)")
		(property "Reference" "D3"
			(at 0 -2.5 -90)
			(layer "F.SilkS")
		)
		(property "Value" "3.5A+"
			(at 0 2.6 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Diode_SMD:D_SMA"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Schottky diode"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" "SDT5A50SA-13"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartAlt" "SK54A-LTP;SK56A-LTP"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Vendor" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "Root")
		(sheetfile "ModPSU-5V-Buck-3V3.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2 0 270)
			(size 2.5 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1388888889)
			(net 2 "Vh")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2 0 270)
			(size 2.5 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.1388888889)
			(net 10 "GND")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 42.6 24.4 180)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED handsolder")
		(property "Reference" "LED2"
			(at -3 -0.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "PRP"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Vendor" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartAlt" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "Root")
		(sheetfile "ModPSU-5V-Buck-3V3.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.874999 0 180)
			(size 1.05 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "GND")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.874999 0 180)
			(size 1.05 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 20 "/5VLED_R")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_Bourns_SRR1210A"
		(layer "F.Cu")
		(at 50.6 30.25 -90)
		(descr "Bourns SRR1210A series SMD inductor https://www.bourns.com/docs/Product-Datasheets/SRR1210A.pdf")
		(tags "Bourns SRR1210A SMD inductor")
		(property "Reference" "L3"
			(at -4.05 -4.85 0)
			(layer "F.SilkS")
		)
		(property "Value" "33u"
			(at 0 7.4 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Inductor_SMD:L_Bourns_SRR1210A"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.mouser.com/datasheet/2/54/srr1210-1391529.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" "SRR1210-330M"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PartAlt" "MSS1278H-333MED,7447709330"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Vendor" "https://www.mouser.com/ProductDetail/Bourns/SRR1210-330M?qs=4vvWAaIu%2Fq5hzjlBVntWJw%3D%3D"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Bourns"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "5V")
		(sheetfile "Buck-5V.kicad_sch")
		(attr smd dnp)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -5.05 0 270)
			(size 2.8 5.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 12 "+5V")
			(pinfunction "1")
			(pintype "passive")
			(zone_connect 2)
		)
		(pad "2" smd rect
			(at 5.05 0 270)
			(size 2.8 5.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 18 "/5V/VBsw")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_Bourns_SRR1210A.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KICAD8_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_Bourns_SRR1260.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TPW-Decorative:webster-face"
		(layer "B.Cu")
		(at 46.2 36.25 180)
		(property "Reference" "G2"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "WebsterFace"
			(at 0.75 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "TPW-Decorative:webster-face"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Vendor" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PartAlt" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "ModPSU-5V-Buck-3V3.kicad_sch")
		(attr through_hole)
	)
	(footprint "TPW-Decorative:sig-wlx"
		(layer "B.Cu")
		(at 47 29.85 180)
		(property "Reference" "G3"
			(at 0 -0.1 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "WLX"
			(at 0.75 -0.1 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" "TPW-Decorative:sig-wlx"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Vendor" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PartAlt" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TPW-Decorative:sig-wlx")
		(sheetname "Root")
		(sheetfile "ModPSU-5V-Buck-3V3.kicad_sch")
		(attr exclude_from_pos_files)
	)
	(footprint "TPW-Decorative:Tseaby-Flag-Silkscreen-Mask"
		(layer "B.Cu")
		(at 27 27.6 180)
		(property "Reference" "G5"
			(at 0 3.9 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Value" "~"
			(at 0 -8.45 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Footprint" "TPW-Decorative:Tseaby-Flag-Silkscreen-Mask"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Part" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Vendor" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PartAlt" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "ModPSU-5V-Buck-3V3.kicad_sch")
	)
	(gr_line
		(start 20 24.2)
		(end 20 44.896447)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 73.5 23.2)
		(end 21 23.2)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 20 24.2)
		(mid 20.292893 23.492893)
		(end 21 23.2)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 20.5 45.396447)
		(end 27 45.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 20.5 45.396447)
		(mid 20.146447 45.25)
		(end 20 44.896447)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 28 43.4)
		(mid 28.292893 42.692893)
		(end 29 42.4)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 29 42.4)
		(end 57 42.4)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 59 45.4)
		(end 73.5 45.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 57 42.4)
		(mid 57.707107 42.692893)
		(end 58 43.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 59 45.4)
		(mid 58.292893 45.107107)
		(end 58 44.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 73.5 23.2)
		(mid 74.207107 23.492893)
		(end 74.5 24.2)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 74.5 44.4)
		(end 74.5 24.2)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 74.5 44.4)
		(mid 74.207107 45.107107)
		(end 73.5 45.4)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 28 43.4)
		(end 28 44.4)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 58 43.4)
		(end 58 44.4)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 28 44.4)
		(mid 27.707107 45.107107)
		(end 27 45.4)
		(layer "Edge.Cuts")
	)
	(gr_text "2025"
		(at 55.3 29.85 0)
		(layer "B.SilkS")
	)
	(gr_text "v1"
		(at 38.7 29.85 0)
		(layer "B.SilkS")
	)
	(gr_text "Vin"
		(at 24.13 43.307 0)
		(layer "B.SilkS")
	)
	(gr_text "G"
		(at 72.39 43.434 0)
		(layer "B.SilkS")
	)
	(gr_text "3V"
		(at 69.85 43.434 0)
		(layer "B.SilkS")
	)
	(gr_text "EN"
		(at 67.31 43.434 0)
		(layer "B.SilkS")
	)
	(gr_text "G"
		(at 21.717 43.307 0)
		(layer "B.SilkS")
	)
	(gr_text "ABSOLUTE\nMAXIMUM\n6V INPUT"
		(at 59.7 27.600001 -90)
		(layer "B.SilkS")
	)
	(gr_text "G"
		(at 62.23 43.434 0)
		(layer "B.SilkS")
	)
	(gr_text "ABSOLUTE\nMAXIMUM\n28V INPUT"
		(at 32.1 27 -90)
		(layer "B.SilkS")
	)
	(gr_text "5V"
		(at 64.8 43.5 0)
		(layer "B.SilkS")
	)
	(gr_text "APCVMOD-05V3V"
		(at 55.3 27.35 0)
		(layer "B.SilkS")
	)
	(gr_text "Buck"
		(at 39 33.2 0)
		(layer "F.SilkS")
	)
	(gr_text "APCVMOD-05V3V"
		(at 57.6 30.3 90)
		(layer "F.SilkS")
	)
	(gr_text "LDO"
		(at 65.55 35.6 90)
		(layer "F.SilkS")
	)
	(gr_text "2025"
		(at 26.8 40.2 90)
		(layer "F.SilkS")
	)
	(gr_text "OVP"
		(at 27.6 27.9 0)
		(layer "F.SilkS")
	)
	(dimension
		(type aligned)
		(layer "Dwgs.User")
		(pts
			(xy 74.5 22) (xy 20 22)
		)
		(height 3)
		(gr_text "54.5000 mm"
			(at 47.25 17.85 0)
			(layer "Dwgs.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.15)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "Dwgs.User")
		(pts
			(xy 19 23.2) (xy 19 45.4)
		)
		(height 3)
		(gr_text "22.2000 mm"
			(at 14.85 34.3 90)
			(layer "Dwgs.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.15)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "Dwgs.User")
		(pts
			(xy 57 42) (xy 29 42)
		)
		(height -4.5)
		(gr_text "28.0000 mm"
			(at 43 45.35 0)
			(layer "Dwgs.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.12)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "Dwgs.User")
		(pts
			(xy 67.31 53.34) (xy 24.13 53.34)
		)
		(height -0.635)
		(gr_text "1.7000 in"
			(at 45.72 52.825 0)
			(layer "Dwgs.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 0)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.15)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0) keep_text_aligned)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 71.3 35.6) (xy 71.1 35.6) (xy 71.1 33.3) (xy 71.3 33.3)
			)
		)
	)
	(zone
		(net 12)
		(net_name "+5V")
		(layer "F.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0.25)
		)
		(min_thickness 0.2)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.2)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 54.4 26) (xy 55.1 26.7) (xy 57.7 26.7) (xy 58.9 25.5) (xy 60.5 26.3) (xy 59.5 27.3) (xy 59.5 30.8)
				(xy 59.8 31.1) (xy 64.8 31.1) (xy 65.3 31.6) (xy 65.3 35.6) (xy 62.5 35.6) (xy 63.3 36.4) (xy 65.3 36.4)
				(xy 66 37.1) (xy 66 43.5) (xy 65.7 44.1) (xy 65 44.5) (xy 59.9 44.5) (xy 59.2 44.2) (xy 59 43.6)
				(xy 59 42.7) (xy 58.6 42) (xy 57.8 41.5) (xy 56.2 41.5) (xy 55.9 41.2) (xy 55.9 39.8) (xy 55.6 39.5)
				(xy 55.6 37.5) (xy 55.1 37) (xy 55.1 33.4) (xy 54.1 32.4) (xy 49.1 32.4) (xy 46.8 30.1) (xy 46.8 23.7)
				(xy 54.4 23.7)
			)
		)
		(polygon
			(pts
				(xy 59 33.4) (xy 59.1 33.7) (xy 59.1 34.3) (xy 59 34.6) (xy 59.1 34.7) (xy 60 34.7) (xy 60 33.3)
				(xy 59.1 33.3)
			)
		)
		(polygon
			(pts
				(xy 60.5 33.3) (xy 60.5 34.7) (xy 62.6 34.7) (xy 62.6 33.3)
			)
		)
	)
	(zone
		(net 10)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.508)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.254)
		)
		(polygon
			(pts
				(xy 69.8 24.525) (xy 69.8 30.125) (xy 69.4 30.525) (xy 61.6 30.525) (xy 61.2 30.125) (xy 61.2 24.525)
				(xy 62.1 23.625) (xy 68.9 23.625)
			)
		)
	)
	(zone
		(net 10)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.508)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.254)
		)
		(polygon
			(pts
				(xy 52.000001 40.794829) (xy 50.400001 40.794829) (xy 50.200001 40.6) (xy 50.200001 38) (xy 50.400001 37.8)
				(xy 52.000001 37.8) (xy 52.200001 38.002586) (xy 52.200001 40.6)
			)
		)
	)
	(zone
		(net 3)
		(net_name "/VHp")
		(layer "F.Cu")
		(hatch edge 0.508)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.2)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 2)
		)
		(polygon
			(pts
				(xy 27.3 26.3) (xy 27.7 26.7) (xy 29.9 26.7) (xy 30.7 25.9) (xy 30.7 25.3) (xy 31.4 24.6) (xy 32.6 24.6)
				(xy 33 25) (xy 34 25) (xy 34.6 25.6) (xy 34.6 28.5) (xy 33.4 29.7) (xy 33.4 32) (xy 31.2 32) (xy 31.2 29.7)
				(xy 30.3 28.8) (xy 27.1 28.8) (xy 25.3 27) (xy 25.3 24.5) (xy 27.3 24.5)
			)
		)
	)
	(zone
		(net 10)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.508)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.254)
		)
		(polygon
			(pts
				(xy 53.1 38.900001) (xy 52.6 38.899998) (xy 52.299999 38.6) (xy 52.299999 38) (xy 52.599999 37.7)
				(xy 53.099999 37.7)
			)
		)
	)
	(zone
		(net 18)
		(net_name "/5V/VBsw")
		(layer "F.Cu")
		(hatch edge 0.508)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.254)
		)
		(polygon
			(pts
				(xy 54.4 37) (xy 54.1 37.3) (xy 44.100001 37.3) (xy 43.500001 36.670602) (xy 41.500001 36.675) (xy 41.500001 35.15)
				(xy 41.700001 35.1) (xy 42.500001 34.3) (xy 43.400001 34.3) (xy 43.8 33.9) (xy 54.4 33.9)
			)
		)
	)
	(zone
		(net 13)
		(net_name "/5V/BuckIn")
		(layer "F.Cu")
		(hatch edge 0.508)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.254)
		)
		(polygon
			(pts
				(xy 40.7 29) (xy 40.5 29.3) (xy 40.35 29.3) (xy 40.15 29.4) (xy 40.05 29.6) (xy 40.05 30.5) (xy 39.95 31.2)
				(xy 39.3 31.2) (xy 39.2 30.5) (xy 39.2 29.6) (xy 39.1 29.4) (xy 38.9 29.3) (xy 37.1 29.301909) (xy 36.8 29)
				(xy 35.9 29) (xy 35.8 28.9) (xy 35.8 27.5) (xy 35.9 27.4) (xy 37.2 27.4) (xy 37.5 27.7) (xy 40.7 27.7)
			)
		)
	)
	(zone
		(net 10)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.254)
		)
		(polygon
			(pts
				(xy 35.7 26.6) (xy 35.7 24.525) (xy 35.95 24.275) (xy 36.65 24.275) (xy 36.9 24.525) (xy 36.9 26.6)
			)
		)
	)
	(zone
		(net 2)
		(net_name "Vh")
		(layer "F.Cu")
		(hatch edge 0.508)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.2)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 2)
		)
		(polygon
			(pts
				(xy 21.4 27.5) (xy 20.8 28.1) (xy 20.8 33.9) (xy 23.2 36.3) (xy 23.2 42.2) (xy 23.7 42.7) (xy 26.8 42.7)
				(xy 28 41.5) (xy 28 34.9) (xy 27.4 34.3) (xy 27.4 32) (xy 26 30.6) (xy 26 29.8) (xy 25.2 29) (xy 23.7 29)
				(xy 22.6 27.9)
			)
		)
	)
	(zone
		(net 10)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.254)
		)
		(polygon
			(pts
				(xy 37.475 26.7) (xy 37.475 24.625) (xy 37.725 24.375) (xy 38.475 24.375) (xy 38.725 24.625) (xy 38.725 26.7)
			)
		)
	)
	(zone
		(net 10)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.254)
		)
		(polygon
			(pts
				(xy 39.5 26.7) (xy 39.5 24.7) (xy 39.8 24.4) (xy 40.4 24.4) (xy 40.7 24.7) (xy 40.7 26.7)
			)
		)
	)
	(zone
		(net 10)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.508)
		(connect_pads yes
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.254)
		)
		(polygon
			(pts
				(xy 30.805171 40) (xy 30.805171 37.2) (xy 31 37) (xy 33.6 37) (xy 33.8 37.2) (xy 33.805171 40) (xy 33.6 40.2)
				(xy 31 40.2)
			)
		)
	)
	(zone
		(net 1)
		(net_name "+3V3")
		(layer "F.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0.2)
		)
		(min_thickness 0.2)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.2)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 74.1 31.8) (xy 74.1 42.2) (xy 73.4 42.9) (xy 69.3 42.9) (xy 68.5 42.1) (xy 68.5 38.2) (xy 67.8 37.5)
				(xy 67 37.5) (xy 65.7 36.2) (xy 65.7 31.6) (xy 66.2 31.1) (xy 73.4 31.1)
			)
		)
		(polygon
			(pts
				(xy 67.6 33.1) (xy 67.4 33.3) (xy 67.4 35.4) (xy 67.6 35.6) (xy 70.2 35.6) (xy 70.5 35.3) (xy 70.5 33.4)
				(xy 70.2 33.1)
			)
		)
	)
	(zone
		(net 10)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0.2)
		)
		(min_thickness 0.2)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 76 47) (xy 19 47) (xy 19 21) (xy 76 21)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "B.Mask")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0.25)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 75 46) (xy 20 46) (xy 21 44.1) (xy 21.4 44.5) (xy 26.5 44.5) (xy 27 44) (xy 27 42.5) (xy 28 41.5)
				(xy 58 41.5) (xy 59 42.5) (xy 59 44) (xy 59.488779 44.5) (xy 73.1 44.5) (xy 73.4 44.2) (xy 73.4 42.9)
				(xy 73.9 42.4) (xy 73.9 24.7) (xy 73.3 24.1) (xy 32.9 24.1) (xy 32.6 23.8) (xy 31.4 23.8) (xy 31.1 24.1)
				(xy 21.7 24.1) (xy 21 24.8) (xy 21 26.9) (xy 20.4 27.5) (xy 20.4 29.1) (xy 21 29.7) (xy 21 37) (xy 20.4 37.6)
				(xy 20.4 42.4) (xy 21 43) (xy 21 44.1) (xy 20 46) (xy 20 22) (xy 75 22)
			)
		)
	)
)
