<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<circle x="47.3075" y="43.053" radius="9.55" width="0.001" layer="20"/>
<wire x1="23.23968125" y1="57.87293125" x2="13.8231" y2="51.943" width="0.001" layer="20" curve="23.177139"/>
<wire x1="23.23968125" y1="57.87293125" x2="46.506971875" y2="71.306309375" width="0.001" layer="20" curve="99.577271"/>
<wire x1="56.35073125" y1="76.496340625" x2="46.50696875" y2="71.306309375" width="0.001" layer="20" curve="23.177138"/>
<wire x1="72.17585" y1="56.48638125" x2="71.748665625" y2="67.60634375" width="0.001" layer="20" curve="23.177132"/>
<wire x1="72.17585" y1="56.48638125" x2="72.17585" y2="29.61961875" width="0.001" layer="20" curve="99.577298"/>
<wire x1="71.748659375" y1="18.499659375" x2="72.175840625" y2="29.61961875" width="0.001" layer="20" curve="23.177129"/>
<wire x1="46.50696875" y1="14.799690625" x2="56.35073125" y2="9.609659375" width="0.001" layer="20" curve="23.177139"/>
<wire x1="46.50696875" y1="14.799690625" x2="23.239684375" y2="28.2330625" width="0.001" layer="20" curve="99.577253"/>
<wire x1="13.8231" y1="34.163" x2="23.23968125" y2="28.233065625" width="0.001" layer="20" curve="23.17714"/>
<wire x1="56.35073125" y1="9.609659375" x2="62.139540625" y2="-0.51845" width="0.001" layer="20"/>
<wire x1="62.139540625" y1="-0.51845" x2="77.60686875" y2="8.352959375" width="0.001" layer="20"/>
<wire x1="77.60686875" y1="8.352959375" x2="71.748659375" y2="18.499659375" width="0.001" layer="20"/>
<wire x1="71.748659375" y1="67.606340625" x2="77.625459375" y2="77.68365" width="0.001" layer="20"/>
<wire x1="77.625459375" y1="77.68365" x2="62.20893125" y2="86.643040625" width="0.001" layer="20"/>
<wire x1="62.20893125" y1="86.643040625" x2="56.35073125" y2="76.496340625" width="0.001" layer="20"/>
<wire x1="13.8231" y1="51.943" x2="2.1575" y2="51.9938" width="0.001" layer="20"/>
<wire x1="2.1575" y1="51.9938" x2="2.1067" y2="34.163" width="0.001" layer="20"/>
<wire x1="2.1067" y1="34.163" x2="13.8231" y2="34.163" width="0.001" layer="20"/>
</plain>
<libraries>
<library name="minipov4">
<packages>
<package name="USB-B-PTH">
<description>&lt;b&gt;USB Series B Hole Mounted&lt;/b&gt;</description>
</package>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="M0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.10 W</description>
</package>
</packages>
</library>
<library name="Wurth_Elektronik_Optoelectronics_rev15b">
<description>&lt;BR&gt;Würth Elektronik --Signal LEDs,White LEDs&lt;br&gt;&lt;Hr&gt;
&lt;BR&gt;&lt;BR&gt; 
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-405&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/eagle"&gt;http://www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither CadSoft nor WE-eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;&lt;BR&gt;&lt;br&gt;
&lt;hr&gt;
Eagle Version 6, Library Revision 2015b, 08.04.2015&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="3528-COMMON-ANODE">
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="BATTCON_20MM">
</package>
<package name="AYZ0202">
<description>&lt;b&gt;DPDT Slide Switch SMD&lt;/b&gt;
www.SparkFun.com SKU : Comp-SMDS</description>
</package>
<package name="TACTILE_SWITCH_SMD">
</package>
</packages>
</library>
<library name="SparkFun">
<packages>
<package name="1X12">
</package>
<package name="SOD-323">
</package>
</packages>
</library>
<library name="SparkFun-Sensors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find sensors- accelerometers, gyros, compasses, magnetometers, light sensors, imagers, temp sensors, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="QRE1113-W">
</package>
</packages>
</library>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="P1-13">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="Q2" library="minipov4" package="SOT23" value="2n2222">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q3" library="minipov4" package="SOT23" value="2n2222">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q4" library="minipov4" package="SOT23" value="2n2222">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="adafruit" package="M0805" value="2.2K">
<attribute name="NAME"/>
</element>
<element name="R15" library="adafruit" package="M0805" value="2.2K">
<attribute name="NAME"/>
</element>
<element name="R16" library="adafruit" package="M0805" value="2.2K"/>
<element name="R5" library="adafruit" package="M0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="adafruit" package="M0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="adafruit" package="M0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="adafruit" package="M0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="adafruit" package="M0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="adafruit" package="M0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="adafruit" package="M0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="adafruit" package="M0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="Wurth_Elektronik_Optoelectronics_rev15b" package="3528-COMMON-ANODE" value="rgb">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BAT2" library="SparkFun-Electromechanical" package="BATTCON_20MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="Wurth_Elektronik_Optoelectronics_rev15b" package="3528-COMMON-ANODE" value="rgb">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D5" library="Wurth_Elektronik_Optoelectronics_rev15b" package="3528-COMMON-ANODE" value="rgb">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D6" library="Wurth_Elektronik_Optoelectronics_rev15b" package="3528-COMMON-ANODE" value="rgb">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D7" library="Wurth_Elektronik_Optoelectronics_rev15b" package="3528-COMMON-ANODE" value="rgb">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D8" library="Wurth_Elektronik_Optoelectronics_rev15b" package="3528-COMMON-ANODE" value="rgb">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D9" library="Wurth_Elektronik_Optoelectronics_rev15b" package="3528-COMMON-ANODE" value="rgb">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D10" library="Wurth_Elektronik_Optoelectronics_rev15b" package="3528-COMMON-ANODE" value="rgb">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP6" library="SparkFun" package="1X12" value="">
<attribute name="VALUE"/>
</element>
<element name="JP7" library="SparkFun" package="1X12" value="">
<attribute name="VALUE"/>
</element>
<element name="S1" library="SparkFun-Electromechanical" package="AYZ0202" value="">
<attribute name="PROD_ID" value="SWCH-08179"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S3" library="SparkFun-Electromechanical" package="TACTILE_SWITCH_SMD" value="!RESET">
<attribute name="PROD_ID" value="SWCH-08247"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="SparkFun-Sensors" package="QRE1113-W" value=""/>
<element name="R1" library="adafruit" package="M0805" value="100ohm">
<attribute name="VALUE"/>
</element>
<element name="R2" library="adafruit" package="M0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D3" library="SparkFun" package="SOD-323" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JUMPER" library="adafruit" package="M0805" value="Jumper">
<attribute name="VALUE"/>
</element>
<element name="BAT1" library="SparkFun-Electromechanical" package="BATTCON_20MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP1" library="testpad" package="P1-13" value="TPPAD1-13">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
<element name="GND" library="testpad" package="P1-13" value="TPPAD1-13">
<attribute name="TP_SIGNAL_NAME" value=""/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="Q4" pad="2"/>
<contactref element="Q3" pad="2"/>
<contactref element="Q2" pad="2"/>
<contactref element="BAT2" pad="2"/>
<contactref element="JP7" pad="9"/>
<contactref element="JP6" pad="2"/>
<contactref element="JP7" pad="10"/>
<contactref element="S3" pad="1"/>
<contactref element="U1" pad="4"/>
<contactref element="U1" pad="2"/>
<contactref element="BAT1" pad="2"/>
<contactref element="GND" pad="TP"/>
</signal>
<signal name="N$5">
<contactref element="R6" pad="1"/>
<contactref element="D2" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="R5" pad="1"/>
<contactref element="D1" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="R12" pad="1"/>
<contactref element="D10" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="R11" pad="1"/>
<contactref element="D9" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="R10" pad="1"/>
<contactref element="D8" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="R9" pad="1"/>
<contactref element="D7" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="R8" pad="1"/>
<contactref element="D6" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="R7" pad="1"/>
<contactref element="D5" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="Q4" pad="3"/>
<contactref element="D1" pad="2"/>
<contactref element="D2" pad="2"/>
<contactref element="D5" pad="2"/>
<contactref element="D6" pad="2"/>
<contactref element="D7" pad="2"/>
<contactref element="D8" pad="2"/>
<contactref element="D9" pad="2"/>
<contactref element="D10" pad="2"/>
</signal>
<signal name="N$17">
<contactref element="Q3" pad="3"/>
<contactref element="D1" pad="3"/>
<contactref element="D2" pad="3"/>
<contactref element="D5" pad="3"/>
<contactref element="D6" pad="3"/>
<contactref element="D7" pad="3"/>
<contactref element="D8" pad="3"/>
<contactref element="D9" pad="3"/>
<contactref element="D10" pad="3"/>
</signal>
<signal name="N$18">
<contactref element="Q2" pad="3"/>
<contactref element="D1" pad="4"/>
<contactref element="D2" pad="4"/>
<contactref element="D5" pad="4"/>
<contactref element="D6" pad="4"/>
<contactref element="D7" pad="4"/>
<contactref element="D8" pad="4"/>
<contactref element="D9" pad="4"/>
<contactref element="D10" pad="4"/>
</signal>
<signal name="N$19">
<contactref element="R14" pad="1"/>
<contactref element="Q2" pad="1"/>
</signal>
<signal name="N$20">
<contactref element="R15" pad="1"/>
<contactref element="Q3" pad="1"/>
</signal>
<signal name="N$21">
<contactref element="R16" pad="1"/>
<contactref element="Q4" pad="1"/>
</signal>
<signal name="LED-C-RED">
<contactref element="R14" pad="2"/>
<contactref element="JP6" pad="8"/>
</signal>
<signal name="LED-C-BLUE">
<contactref element="R15" pad="2"/>
<contactref element="JP6" pad="7"/>
</signal>
<signal name="LED-C-GREEN">
<contactref element="R16" pad="2"/>
<contactref element="JP6" pad="6"/>
</signal>
<signal name="LED-A-1">
<contactref element="R5" pad="2"/>
<contactref element="JP7" pad="1"/>
</signal>
<signal name="LED-A-2">
<contactref element="R6" pad="2"/>
<contactref element="JP7" pad="2"/>
</signal>
<signal name="LED-A-6">
<contactref element="R10" pad="2"/>
<contactref element="JP7" pad="6"/>
</signal>
<signal name="LED-A-5">
<contactref element="R9" pad="2"/>
<contactref element="JP7" pad="5"/>
</signal>
<signal name="LED-A-7">
<contactref element="R11" pad="2"/>
<contactref element="JP7" pad="7"/>
</signal>
<signal name="LED-A-4">
<contactref element="R8" pad="2"/>
<contactref element="JP7" pad="4"/>
</signal>
<signal name="LED-A-8">
<contactref element="R12" pad="2"/>
<contactref element="JP7" pad="8"/>
</signal>
<signal name="LED-A-3">
<contactref element="R7" pad="2"/>
<contactref element="JP7" pad="3"/>
</signal>
<signal name="S$1">
</signal>
<signal name="LIPO">
<contactref element="S1" pad="2"/>
<contactref element="D3" pad="1"/>
<contactref element="JUMPER" pad="1"/>
</signal>
<signal name="RESET">
<contactref element="JP6" pad="3"/>
<contactref element="S3" pad="3"/>
</signal>
<signal name="SCK">
<contactref element="JP6" pad="9"/>
</signal>
<signal name="MISO">
<contactref element="JP6" pad="10"/>
</signal>
<signal name="MOSI">
<contactref element="JP6" pad="11"/>
</signal>
<signal name="TXO">
<contactref element="JP7" pad="12"/>
</signal>
<signal name="VCC">
<contactref element="JP6" pad="4"/>
<contactref element="R2" pad="1"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="RAW">
<contactref element="JP6" pad="1"/>
<contactref element="S1" pad="1"/>
</signal>
<signal name="A3">
<contactref element="JP6" pad="5"/>
</signal>
<signal name="RXI">
<contactref element="JP7" pad="11"/>
</signal>
<signal name="SENSOR">
<contactref element="U1" pad="3"/>
<contactref element="R2" pad="2"/>
<contactref element="JP6" pad="12"/>
</signal>
<signal name="N$3">
<contactref element="U1" pad="1"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="BAT2" pad="1"/>
<contactref element="D3" pad="2"/>
<contactref element="JUMPER" pad="2"/>
<contactref element="BAT1" pad="1"/>
<contactref element="TP1" pad="TP"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
