(kicad_pcb (version 20171130) (host pcbnew 5.1.10-88a1d61d58~88~ubuntu20.10.1)
  (general
    (thickness 1.6)
    (drawings 23)
    (tracks 214)
    (zones 0)
    (modules 13)
    (nets 28)
  )
  (page A4)
  (title_block
    (title "LPT Capture")
    (date 2021-06-29)
    (rev 009)
    (company b.kenyon.w@gmail.com)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.2)
    (user_trace_width 0.4)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.5)
    (via_drill 0.3)
    (via_min_size 0.5)
    (via_min_drill 0.3)
    (user_via 0.8 0.5)
    (uvia_size 0.5)
    (uvia_drill 0.3)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (solder_mask_min_width 0.22)
    (aux_axis_origin 0 0)
    (grid_origin 150 100)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "GERBER_LPT_Capture_009"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /3v3)
  (net 3 /USB+)
  (net 4 /USB-)
  (net 5 /D1)
  (net 6 /D2)
  (net 7 /D0)
  (net 8 /D3)
  (net 9 /D5)
  (net 10 /D6)
  (net 11 /D4)
  (net 12 /D7)
  (net 13 /WR)
  (net 14 /~TXE)
  (net 15 VCC)
  (net 16 /RST_ERR)
  (net 17 /PD7)
  (net 18 /PD6)
  (net 19 /PD5)
  (net 20 /PD4)
  (net 21 /PD3)
  (net 22 /PD2)
  (net 23 /PD1)
  (net 24 /PD0)
  (net 25 /~STROBE)
  (net 26 VBUS)
  (net 27 /BUSY)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.5)
    (via_drill 0.3)
    (uvia_dia 0.5)
    (uvia_drill 0.3)
    (add_net /3v3)
    (add_net /BUSY)
    (add_net /D0)
    (add_net /D1)
    (add_net /D2)
    (add_net /D3)
    (add_net /D4)
    (add_net /D5)
    (add_net /D6)
    (add_net /D7)
    (add_net /PD0)
    (add_net /PD1)
    (add_net /PD2)
    (add_net /PD3)
    (add_net /PD4)
    (add_net /PD5)
    (add_net /PD6)
    (add_net /PD7)
    (add_net /RST_ERR)
    (add_net /WR)
    (add_net /~STROBE)
    (add_net /~TXE)
    (add_net GND)
    (add_net VBUS)
    (add_net VCC)
  )
  (net_class "USB Data" ""
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.5)
    (via_drill 0.3)
    (uvia_dia 0.5)
    (uvia_drill 0.3)
    (diff_pair_width 0.2)
    (diff_pair_gap 0.2)
    (add_net /USB+)
    (add_net /USB-)
  )
  (module 000_LOCAL:SolderJumper-2_P1.3mm_Open_TrianglePad1.0x1.5mm (layer F.Cu) (tedit 60DBCF64)
    (at 146.7 98.2)
    (descr "SMD Solder Jumper, 1x1.5mm Triangular Pads, 0.3mm gap, open")
    (tags "solder jumper open")
    (attr virtual)
    (fp_text reference JP1 (at 2.6 0.55) (layer F.SilkS) hide)
    (fp_text value SolderJumper_2_Open (at 0 1.9) (layer F.Fab))
    (pad 1 smd custom (at -0.725 0) (size 0.3 0.3) (layers F.Cu F.Mask)
      (net 26 VBUS) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy -0.5 -0.75) (xy 0.5 -0.75) (xy 1 0) (xy 0.5 0.75) (xy -0.5 0.75)
) (width 0))
      ))
    (pad 2 smd custom (at 0.725 0) (size 0.3 0.3) (layers F.Cu F.Mask)
      (net 15 VCC) (zone_connect 2)
      (options (clearance outline) (anchor rect))
      (primitives
        (gr_poly (pts
           (xy -0.65 -0.75) (xy 0.5 -0.75) (xy 0.5 0.75) (xy -0.65 0.75) (xy -0.15 0)
) (width 0))
      ))
  )
  (module 000_LOCAL:GCT_USB3155-XX-X_REVA (layer F.Cu) (tedit 60DAAE92)
    (at 141 100 270)
    (fp_text reference J1 (at -4.9 -2.4 270 unlocked) (layer F.SilkS) hide)
    (fp_text value USB3155-XX-X_REVA (at 6.72209 -11.89754 270) (layer F.Fab))
    (fp_text user PCB~Edge (at -4.80007 2.50003 90) (layer F.Fab))
    (pad S thru_hole oval (at 4.94 0 270) (size 1.2 2.5) (drill oval 0.6 1.9) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad S thru_hole oval (at -4.94 0 270) (size 1.2 2.5) (drill oval 0.6 1.9) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 smd rect (at 1.3 -3.475 270) (size 0.43 0.95) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0.65 -3.475 270) (size 0.43 0.95) (layers F.Cu F.Paste F.Mask))
    (pad 3 smd rect (at 0 -3.475 270) (size 0.43 0.95) (layers F.Cu F.Paste F.Mask)
      (net 3 /USB+))
    (pad 2 smd rect (at -0.65 -3.475 270) (size 0.43 0.95) (layers F.Cu F.Paste F.Mask)
      (net 4 /USB-))
    (pad 1 smd rect (at -1.3 -3.475 270) (size 0.43 0.95) (layers F.Cu F.Paste F.Mask)
      (net 26 VBUS))
    (model ${KIPRJMOD}/000_LOCAL.pretty/3d/USB3155-30-A.stp
      (offset (xyz 0 -2.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module 000_LOCAL:R_Array_Convex_4x0603 (layer F.Cu) (tedit 60C9CA25)
    (at 153 91.65)
    (descr "Chip Resistor Network, ROHM MNR14 (see mnr_g.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN1 (at 0 -2.25) (layer F.SilkS))
    (fp_text value 100 (at -0.05 2.35 unlocked) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 5 smd roundrect (at 0.9 1.2) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 17 /PD7))
    (pad 6 smd roundrect (at 0.9 0.4) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 25 /~STROBE))
    (pad 8 smd roundrect (at 0.9 -1.2) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 27 /BUSY))
    (pad 7 smd roundrect (at 0.9 -0.4) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 1 GND))
    (pad 4 smd roundrect (at -0.9 1.2) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 12 /D7))
    (pad 2 smd roundrect (at -0.9 -0.4) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 1 GND))
    (pad 3 smd roundrect (at -0.9 0.4) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2))
    (pad 1 smd roundrect (at -0.9 -1.2) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 14 /~TXE))
    (model ${KIPRJMOD}/000_LOCAL.pretty/3d/R_Array_Convex_4x0603.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000_LOCAL:R_Array_Convex_4x0603 (layer F.Cu) (tedit 60C9CA25)
    (at 153 101.4)
    (descr "Chip Resistor Network, ROHM MNR14 (see mnr_g.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN2 (at 0 -2.2) (layer F.SilkS))
    (fp_text value 100 (at 0 2.3) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 5 smd roundrect (at 0.9 1.2) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 21 /PD3))
    (pad 6 smd roundrect (at 0.9 0.4) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 20 /PD4))
    (pad 8 smd roundrect (at 0.9 -1.2) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 18 /PD6))
    (pad 7 smd roundrect (at 0.9 -0.4) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 19 /PD5))
    (pad 4 smd roundrect (at -0.9 1.2) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 8 /D3))
    (pad 2 smd roundrect (at -0.9 -0.4) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 9 /D5))
    (pad 3 smd roundrect (at -0.9 0.4) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 11 /D4))
    (pad 1 smd roundrect (at -0.9 -1.2) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 10 /D6))
    (model ${KIPRJMOD}/000_LOCAL.pretty/3d/R_Array_Convex_4x0603.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000_LOCAL:R_Array_Convex_4x0603 (layer F.Cu) (tedit 60C9CA25)
    (at 153 111.6)
    (descr "Chip Resistor Network, ROHM MNR14 (see mnr_g.pdf)")
    (tags "resistor array")
    (attr smd)
    (fp_text reference RN3 (at 0 -3.2) (layer F.SilkS))
    (fp_text value 100 (at 0 -2.2 unlocked) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 5 smd roundrect (at 0.9 1.2) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 25 /~STROBE))
    (pad 6 smd roundrect (at 0.9 0.4) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 24 /PD0))
    (pad 8 smd roundrect (at 0.9 -1.2) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 22 /PD2))
    (pad 7 smd roundrect (at 0.9 -0.4) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 23 /PD1))
    (pad 4 smd roundrect (at -0.9 1.2) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 13 /WR))
    (pad 2 smd roundrect (at -0.9 -0.4) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 5 /D1))
    (pad 3 smd roundrect (at -0.9 0.4) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 7 /D0))
    (pad 1 smd roundrect (at -0.9 -1.2) (size 0.8 0.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 6 /D2))
    (model ${KIPRJMOD}/000_LOCAL.pretty/3d/R_Array_Convex_4x0603.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000_LOCAL:L_0805_2012Metric (layer F.Cu) (tedit 60C9B4E4)
    (at 147 98.2 180)
    (descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 80, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference FB1 (at -2.1 0 -90 unlocked) (layer F.SilkS))
    (fp_text value 40-1.5A (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.0625 0 180) (size 0.875 1.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 VBUS))
    (pad 1 smd roundrect (at -1.0625 0 180) (size 0.875 1.2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 VCC))
    (model ${KIPRJMOD}/000_LOCAL.pretty/3d/L_0805_2012Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000_LOCAL:C_0805_2012Metric (layer F.Cu) (tedit 60BB0558)
    (at 145.65 95.8 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at 2.5 0.55 270 unlocked) (layer F.SilkS))
    (fp_text value 0.01u (at 3.3 -0.45 270 unlocked) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.95 0 90) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.95 0 90) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 VBUS))
    (model ${KIPRJMOD}/000_LOCAL.pretty/3d/C_0805_2012Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000_LOCAL:C_0805_2012Metric (layer F.Cu) (tedit 60BB0558)
    (at 147.05 104.8 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at 2.4 0.45 -90 unlocked) (layer F.SilkS))
    (fp_text value 0.1u (at 2.9 -0.55 270 unlocked) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.95 0 90) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.95 0 90) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 VCC))
    (model ${KIPRJMOD}/000_LOCAL.pretty/3d/C_0805_2012Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000_LOCAL:DSUB-25_Male_EdgeMount_P2.77mm (layer F.Cu) (tedit 60C163D6)
    (at 157.95 100 90)
    (descr "25-pin D-Sub connector, solder-cups edge-mounted, male, x-pin-pitch 2.77mm, distance of mounting holes 47.1mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
    (tags "25-pin D-Sub connector edge mount solder cup male x-pin-pitch 2.77mm mounting holes distance 47.1mm")
    (fp_text reference J2 (at -15.267 -0.4688 90) (layer F.SilkS) hide)
    (fp_text value "DB25 Male" (at 0 12.95 90) (layer F.Fab))
    (fp_text user "PCB edge" (at 0 2.45 90) (layer Dwgs.User))
    (fp_text user %R (at 0 3.39 90) (layer F.Fab))
    (pad 25 smd roundrect (at 15.235 -0.5 90) (size 2 4.6) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 24 smd roundrect (at 12.465 -0.5 90) (size 2 4.6) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 23 smd roundrect (at 9.695 -0.5 90) (size 2 4.6) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 22 smd roundrect (at 6.925 -0.5 90) (size 2 4.6) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 21 smd roundrect (at 4.155 -0.5 90) (size 2 4.6) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 20 smd roundrect (at 1.385 -0.5 90) (size 2 4.6) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 19 smd roundrect (at -1.385 -0.5 90) (size 2 4.6) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 18 smd roundrect (at -4.155 -0.5 90) (size 2 4.6) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 17 smd roundrect (at -6.925 -0.5 90) (size 2 4.6) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (pad 16 smd roundrect (at -9.695 -0.5 90) (size 2 4.6) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 16 /RST_ERR))
    (pad 15 smd roundrect (at -12.465 -0.5 90) (size 2 4.6) (layers B.Cu B.Mask) (roundrect_rratio 0.25)
      (net 16 /RST_ERR))
    (pad 14 smd roundrect (at -15.235 -0.5 90) (size 2 4.6) (layers B.Cu B.Mask) (roundrect_rratio 0.25))
    (pad 13 smd roundrect (at 16.62 -0.5 90) (size 2 4.6) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
    (pad 12 smd roundrect (at 13.85 -0.5 90) (size 2 4.6) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 11 smd roundrect (at 11.08 -0.5 90) (size 2 4.6) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 27 /BUSY))
    (pad 10 smd roundrect (at 8.31 -0.5 90) (size 2 4.6) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 25 /~STROBE))
    (pad 9 smd roundrect (at 5.54 -0.5 90) (size 2 4.6) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 17 /PD7))
    (pad 8 smd roundrect (at 2.77 -0.5 90) (size 2 4.6) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 18 /PD6))
    (pad 7 smd roundrect (at 0 -0.5 90) (size 2 4.6) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 19 /PD5))
    (pad 6 smd roundrect (at -2.77 -0.5 90) (size 2 4.6) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 20 /PD4))
    (pad 5 smd roundrect (at -5.54 -0.5 90) (size 2 4.6) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 21 /PD3))
    (pad 4 smd roundrect (at -8.31 -0.5 90) (size 2 4.6) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 22 /PD2))
    (pad 3 smd roundrect (at -11.08 -0.5 90) (size 2 4.6) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 23 /PD1))
    (pad 2 smd roundrect (at -13.85 -0.5 90) (size 2 4.6) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 24 /PD0))
    (pad 1 smd roundrect (at -16.62 -0.5 90) (size 2 4.6) (layers F.Cu F.Mask) (roundrect_rratio 0.25)
      (net 25 /~STROBE))
    (model ${KIPRJMOD}/000_LOCAL.pretty/3d/connector_a-ds_25_pp_z.stp_
      (offset (xyz 0 -8.199999999999999 -0.87))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/3d/956-025-010R0.STEP_
      (offset (xyz 0 -9.85 -9.4))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/3d/956-025-010R0.STEP
      (offset (xyz 0 -9.85 7.6))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
    (model ${KIPRJMOD}/000_LOCAL.pretty/3d/171-025-103.step
      (offset (xyz -26.5 -8.300000000000001 -7.2))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module 000_LOCAL:SSOP-28_5.3x10.2mm_P0.65mm (layer F.Cu) (tedit 60BCA611)
    (at 145.75 111.2 90)
    (descr "28-Lead Plastic Shrink Small Outline (SS)-5.30 mm Body [SSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U1 (at 1.05 0) (layer F.SilkS))
    (fp_text value FT245RL (at -1.05 0) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 28 smd roundrect (at 3.6 -4.225 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.18))
    (pad 27 smd roundrect (at 3.6 -3.575 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.18))
    (pad 26 smd roundrect (at 3.6 -2.925 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.18)
      (net 1 GND))
    (pad 25 smd roundrect (at 3.6 -2.275 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.18)
      (net 1 GND))
    (pad 24 smd roundrect (at 3.6 -1.625 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.18))
    (pad 23 smd roundrect (at 3.6 -0.975 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.18))
    (pad 22 smd roundrect (at 3.6 -0.325 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.18)
      (net 14 /~TXE))
    (pad 21 smd roundrect (at 3.6 0.325 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.18)
      (net 1 GND))
    (pad 20 smd roundrect (at 3.6 0.975 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.18)
      (net 15 VCC))
    (pad 19 smd roundrect (at 3.6 1.625 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.18))
    (pad 18 smd roundrect (at 3.6 2.275 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.18)
      (net 1 GND))
    (pad 17 smd roundrect (at 3.6 2.925 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.18)
      (net 2 /3v3))
    (pad 16 smd roundrect (at 3.6 3.575 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.18)
      (net 4 /USB-))
    (pad 15 smd roundrect (at 3.6 4.225 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.18)
      (net 3 /USB+))
    (pad 14 smd roundrect (at -3.6 4.225 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.18)
      (net 13 /WR))
    (pad 13 smd roundrect (at -3.6 3.575 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.18)
      (net 15 VCC))
    (pad 12 smd roundrect (at -3.6 2.925 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.18))
    (pad 11 smd roundrect (at -3.6 2.275 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.18)
      (net 8 /D3))
    (pad 10 smd roundrect (at -3.6 1.625 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.18)
      (net 10 /D6))
    (pad 9 smd roundrect (at -3.6 0.975 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.18)
      (net 9 /D5))
    (pad 8 smd roundrect (at -3.6 0.325 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.18))
    (pad 7 smd roundrect (at -3.6 -0.325 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.18)
      (net 1 GND))
    (pad 6 smd roundrect (at -3.6 -0.975 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.18)
      (net 12 /D7))
    (pad 5 smd roundrect (at -3.6 -1.625 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.18)
      (net 5 /D1))
    (pad 4 smd roundrect (at -3.6 -2.275 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.18)
      (net 15 VCC))
    (pad 3 smd roundrect (at -3.6 -2.925 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.18)
      (net 6 /D2))
    (pad 2 smd roundrect (at -3.6 -3.575 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.18)
      (net 11 /D4))
    (pad 1 smd roundrect (at -3.6 -4.225 90) (size 1.75 0.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.18)
      (net 7 /D0))
    (model ${KIPRJMOD}/000_LOCAL.pretty/3d/SSOP-28_5.3x10.2mm_P0.65mm.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000_LOCAL:R_0805_2012Metric (layer F.Cu) (tedit 60BB056D)
    (at 153 115 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 2 -0.175 270 unlocked) (layer F.SilkS))
    (fp_text value 47K (at 0.7 -1.35) (layer F.SilkS))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2439004878048781)
      (net 15 VCC))
    (pad 1 smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2439004878048781)
      (net 25 /~STROBE))
    (model ${KIPRJMOD}/000_LOCAL.pretty/3d/R_0805_2012Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000_LOCAL:C_0805_2012Metric (layer F.Cu) (tedit 60BB0558)
    (at 145.075 104.8 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at 2.3 0 -90) (layer F.SilkS))
    (fp_text value 4.7u (at -0.46 -1.465 270 unlocked) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.95 0 90) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.95 0 90) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 VCC))
    (model ${KIPRJMOD}/000_LOCAL.pretty/3d/C_0805_2012Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module 000_LOCAL:C_0805_2012Metric (layer F.Cu) (tedit 60BB0558)
    (at 149.025 104.8 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at -2.4 -0.775 270 unlocked) (layer F.SilkS))
    (fp_text value 0.1u (at -2.9 0.275 270 unlocked) (layer F.SilkS))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.95 0 270) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /3v3))
    (pad 1 smd roundrect (at -0.95 0 270) (size 1 1.45) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KIPRJMOD}/000_LOCAL.pretty/3d/C_0805_2012Metric.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 144 96.2) (end 144 103.8) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 142 115) (end 139 115) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 142 85) (end 142 82) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 139 103.8) (end 139 115) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 139 96.2) (end 139 85) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 144 96.2) (end 139 96.2) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 139 103.8) (end 144 103.8) (layer Edge.Cuts) (width 0.05))
  (gr_text Capture (at 142 84 -90) (layer F.SilkS))
  (gr_text v009 (at 148 100 -90) (layer B.SilkS))
  (gr_text 13 (at 154.45 83.425 -90) (layer F.SilkS))
  (gr_text 1 (at 154.45 116.65 -90) (layer F.SilkS))
  (gr_text 14 (at 154.4 115.25 -90) (layer B.SilkS))
  (gr_text 25 (at 154.4 84.8 -90) (layer B.SilkS))
  (gr_text github.com/bkw777/LPT_Capture (at 150 100 -90) (layer B.SilkS))
  (gr_text LPT (at 144 84 -90) (layer F.SilkS))
  (gr_line (start 159.75 82) (end 159.75 118) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 142 82) (end 159.75 82) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 159.75 118) (end 142 118) (layer Edge.Cuts) (width 0.05))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.2) (thermal_bridge_width 0.3) (smoothing fillet) (radius 0.1))
    (polygon
      (pts
        (xy 159.75 118) (xy 139 118) (xy 139 82) (xy 159.75 82)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.2))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.2) (thermal_bridge_width 0.3) (smoothing fillet) (radius 0.1))
    (polygon
      (pts
        (xy 159.75 118) (xy 139 118) (xy 139 82) (xy 159.75 82)
      )
    )
  )
)
