(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 4)
    (no_connects 0)
    (area 118.374999 165.624999 140.095001 165.775001)
    (thickness 1.6)
    (drawings 53)
    (tracks 18)
    (zones 0)
    (modules 13)
    (nets 5)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk true)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory C:/Users/smerrett79/SkyDrive/Documents/Remap/BIRU/sonassist/))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad1)")
  (net 2 "Net-(J1-Pad2)")
  (net 3 "Net-(J1-Pad3)")
  (net 4 "Net-(J1-Pad4)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
  )
  (module BIRU:outlinesL (layer F.Cu) (tedit 0)
    (at 104.91 159.5)
    (fp_text reference Left** (at 0 0) (layer F.SilkS) hide)
    (fp_text value Left (at 0.75 0) (layer F.SilkS) hide)
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 131.75 154.82)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33) (layer F.SilkS))
    (fp_text value CONN_01X04 (at 0 9.95) (layer F.Fab))
    (fp_text user %R (at 0 3.81 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(J1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad4)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module BIRU:4ToesLCU (layer F.Cu) (tedit 596FE549)
    (at 83.62 71.12)
    (fp_text reference G*** (at -4.9 6.7) (layer F.SilkS) hide)
    (fp_text value 4ToesLCU (at -6.4 10.9) (layer F.SilkS) hide)
  )
  (module BIRU:bigToeLCU (layer F.Cu) (tedit 0)
    (at 128.78 53.26)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value bigToeLCU (at 0.75 0) (layer F.SilkS) hide)
  )
  (module BIRU:innerBallLCU (layer F.Cu) (tedit 0)
    (at 128.55 109.88)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value innerBallLCU (at 0.75 0) (layer F.SilkS) hide)
  )
  (module BIRU:outerBallLCU (layer F.Cu) (tedit 0)
    (at 81.7 119.75)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value outerBallLCU (at 0.75 0) (layer F.SilkS) hide)
  )
  (module BIRU:4mmRndPad (layer F.Cu) (tedit 596FF6C4)
    (at 86.7 68.07)
    (fp_text reference P1 (at 0 0.5) (layer F.SilkS))
    (fp_text value 4Toes (at -0.1 -1.6) (layer F.Fab))
    (pad 1 smd circle (at 0.1 6.5) (size 4 4) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(J1-Pad3)"))
  )
  (module BIRU:4mmRndPad (layer F.Cu) (tedit 596FF6C4)
    (at 115.35 56.29)
    (fp_text reference P2 (at 0 0.5) (layer F.SilkS))
    (fp_text value bigToe (at -0.1 -1.6) (layer F.Fab))
    (pad 1 smd circle (at 0.1 6.5) (size 4 4) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(J1-Pad2)"))
  )
  (module BIRU:4mmRndPad (layer F.Cu) (tedit 596FF6C4)
    (at 130.18 124.36)
    (fp_text reference P3 (at 0 0.5) (layer F.SilkS))
    (fp_text value innerBall (at -0.1 -1.6) (layer F.Fab))
    (pad 1 smd circle (at 0.1 6.5) (size 4 4) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(J1-Pad1)"))
  )
  (module BIRU:4mmRndPad (layer F.Cu) (tedit 596FF6C4)
    (at 95.23 127.2)
    (fp_text reference P4 (at 0 0.5) (layer F.SilkS))
    (fp_text value outerBall (at -0.1 -1.6) (layer F.Fab))
    (pad 1 smd circle (at 0.1 6.5) (size 4 4) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(J1-Pad4)"))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 123.94 161.55)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 123.94 74.55)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3 (layer F.Cu) (tedit 56D1B4CB)
    (at 81.44 96.54)
    (descr "Mounting Hole 3.2mm, no annular, M3")
    (tags "mounting hole 3.2mm no annular m3")
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS))
    (fp_text value MountingHole_3.2mm_M3 (at 0 4.2) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (gr_line (start 134.51 140.64) (end 134.75 167.64) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 141.26 133.08) (end 134.51 140.64) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 148.55 119.84) (end 141.26 133.08) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 151.26 109.6) (end 148.55 119.84) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 152.4 97.79) (end 151.26 109.6) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 149.73 89.92) (end 152.4 97.79) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 144.78 86.11) (end 149.73 89.92) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 142.62 80.77) (end 144.78 86.11) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 143.38 77.09) (end 142.62 80.77) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 148.97 71.25) (end 143.38 77.09) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 152.91 63.75) (end 148.97 71.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 153.29 52.32) (end 152.91 63.75) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 150.95 42.32) (end 153.29 52.32) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 144.91 34.14) (end 150.95 42.32) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 139.93 32.36) (end 144.91 34.14) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 134.24 31.83) (end 139.93 32.36) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 116.81 33.07) (end 134.24 31.83) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 95.91 39.42) (end 116.81 33.07) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 84.53 46.74) (end 95.91 39.42) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 73.96 61.57) (end 84.53 46.74) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 66.24 76.61) (end 73.96 61.57) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 61.38 91.06) (end 66.24 76.61) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 57.28 112.71) (end 61.38 91.06) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 59.51 124.33) (end 57.28 112.71) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 74.93 136.91) (end 59.51 124.33) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 91.06 141.48) (end 74.93 136.91) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 103 141.22) (end 91.06 141.48) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 119.51 153.54) (end 103 141.22) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 119.51 167.77) (end 119.51 153.54) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 134.75 167.64) (end 119.51 167.77) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 161.179109 -85.958924) (end 161.179109 -85.958924) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 161.179109 -85.958924) (end 161.179109 -85.958924) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 161.179109 -85.958924) (end 161.179109 -85.958924) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 211.580016 84.251415) (end 211.580016 84.251415) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 161.179109 -85.958924) (end 161.179109 -85.958924) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 211.580016 84.251415) (end 211.580016 84.251415) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 161.179109 -85.958924) (end 161.179109 -85.958924) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 161.179109 -85.958924) (end 161.179109 -85.958924) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 211.580016 84.251415) (end 211.580016 84.251415) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 211.580016 84.251415) (end 211.580016 84.251415) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 161.179109 -85.958924) (end 161.179109 -85.958924) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 161.179109 -85.958924) (end 161.179109 -85.958924) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 211.580016 84.251415) (end 211.580016 84.251415) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 211.580016 84.251415) (end 211.580016 84.251415) (layer Edge.Cuts) (width 0.1))
)
