<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="0" y1="0.3175" x2="18.0975" y2="0.3175" width="0" layer="20"/>
<wire x1="18.0975" y1="0.3175" x2="18.0975" y2="13.6525" width="0" layer="20"/>
<wire x1="18.0975" y1="13.6525" x2="0" y2="13.6525" width="0" layer="20"/>
<wire x1="0" y1="13.6525" x2="0" y2="0.3175" width="0" layer="20"/>
<text>C</text>
<text>A</text>
<text>S</text>
<text>ALPS SKC</text>
<text>KPS 20130907</text>
<text>DATA TRAVEL</text>
<text>BREAKOUT</text>
<text>EXPERIMENTS</text>
<text>&amp;</text>
</plain>
<libraries>
<library name="misc">
<packages>
<package name="SMA+SOD323-P-NOSS">
<description>Pad that combines SMA and SOT323</description>
</package>
</packages>
</library>
<library name="switch">
<packages>
<package name="SW-ALPS-SKC-LED">
</package>
</packages>
</library>
<library name="conn">
<packages>
<package name="J-1-SQUARE-70">
</package>
<package name="J-1-OCTAGON-70">
</package>
<package name="J-1-ROUND-70">
</package>
<package name="J-1-ROUND-74">
<description>0.1" breakaway header pin, round pad.</description>
</package>
<package name="J-1-SQUARE-74">
<description>0.1" breakaway header pin, square pad</description>
</package>
</packages>
</library>
<library name="glyphs">
<packages>
<package name="GLYPH-DT&amp;E-50">
</package>
</packages>
</library>
</libraries>
<attributes>
<attribute name="AUTHOR_NAME" value="KPS"/>
<attribute name="VERSION" value="20130907"/>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="D1" library="misc" package="SMA+SOD323-P-NOSS" value="1N4148">
<attribute name="NAME"/>
</element>
<element name="LA" library="conn" package="J-1-OCTAGON-70" value=" "/>
<element name="LC" library="conn" package="J-1-OCTAGON-70" value=" "/>
<element name="S0" library="conn" package="J-1-ROUND-70" value=" "/>
<element name="A0" library="conn" package="J-1-SQUARE-70" value=" "/>
<element name="C0" library="conn" package="J-1-SQUARE-70" value=" "/>
<element name="C1" library="conn" package="J-1-SQUARE-74" value=" "/>
<element name="A1" library="conn" package="J-1-SQUARE-74" value=" "/>
<element name="S1" library="conn" package="J-1-ROUND-74" value=" "/>
<element name="S2" library="conn" package="J-1-ROUND-74" value=" "/>
<element name="SW1" library="switch" package="SW-ALPS-SKC-LED" value=" "/>
<element name="U$1" library="glyphs" package="GLYPH-DT&amp;E-50" value=""/>
</elements>
<signals>
<signal name="C">
<contactref element="D1" pad="C"/>
<contactref element="C1" pad="1"/>
<contactref element="C0" pad="1"/>
<contactref element="SW1" pad="S1"/>
</signal>
<signal name="S">
<contactref element="S0" pad="1"/>
<contactref element="S2" pad="1"/>
<contactref element="S1" pad="1"/>
<contactref element="SW1" pad="S2"/>
</signal>
<signal name="A">
<contactref element="D1" pad="A"/>
<contactref element="A0" pad="1"/>
<contactref element="A1" pad="1"/>
</signal>
<signal name="LA">
<contactref element="LA" pad="1"/>
<contactref element="SW1" pad="LA"/>
</signal>
<signal name="LC">
<contactref element="LC" pad="1"/>
<contactref element="SW1" pad="LC"/>
</signal>
<signal name="N$1">
</signal>
<signal name="N$2">
</signal>
</signals>
</board>
</drawing>
</eagle>
