(kicad_pcb (version 20171130) (host pcbnew "(5.1.4-0-10_14)")
  (general
    (thickness 1.6)
    (drawings 53)
    (tracks 63)
    (zones 0)
    (modules 12)
    (nets 8)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 3)
    (user_trace_width 0.5)
    (user_trace_width 1)
    (user_trace_width 2)
    (user_trace_width 3)
    (user_trace_width 4)
    (user_trace_width 5)
    (user_trace_width 6)
    (trace_clearance 0.2)
    (zone_clearance 0.5)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 6 6)
    (pad_drill 3)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers/"))
  )
  (net 0 "")
  (net 1 Earth)
  (net 2 +12V)
  (net 3 -12V)
  (net 4 GND)
  (net 5 +5V)
  (net 6 LINE)
  (net 7 NEUT)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net +5V)
    (add_net -12V)
    (add_net Earth)
    (add_net GND)
    (add_net LINE)
    (add_net NEUT)
  )
  (module Symbol:Symbol_Highvoltage_Type1_CopperTop_Small (layer B.Cu) (tedit 0)
    (at 127.8 70.4 180)
    (descr "Symbol, Highvoltage, Type 1, Copper Top, Small,")
    (tags "Symbol, Highvoltage, Type 1, Copper Top, Small,")
    (attr virtual)
    (fp_text reference REF** (at 1.016 5.207) (layer B.Fab) hide)
    (fp_text value Symbol_Highvoltage_Type1_CopperTop_Small (at 0.508 -4.191) (layer B.Fab))
  )
  (module Symbol:Symbol_Danger_CopperTop_Small (layer F.Cu) (tedit 0)
    (at 117.5 72)
    (descr "Symbol, Danger, Copper Top, Small,")
    (tags "Symbol, Danger, Copper Top, Small,")
    (attr virtual)
    (fp_text reference REF** (at 0.254 -4.699) (layer F.Fab) hide)
    (fp_text value Symbol_Danger_CopperTop_Small (at 0.889 4.572) (layer F.Fab))
  )
  (module rt65b-breakout:DIN-7 (layer F.Cu) (tedit 5E220F5E)
    (at 177.75 74)
    (fp_text reference J1 (at -8.5 -15) (layer F.Fab) hide)
    (fp_text value DIN-7 (at 8.75 -15) (layer F.Fab))
    (pad 6 thru_hole circle (at 7.5 -12.5) (size 2.75 2.75) (drill 1.5) (layers *.Cu *.Mask)
      (net 2 +12V))
    (pad 7 thru_hole circle (at -7.5 -12.5) (size 2.75 2.75) (drill 1.5) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 4 thru_hole circle (at 5 -10 90) (size 2.75 2.75) (drill 1.5) (layers *.Cu *.Mask)
      (net 2 +12V))
    (pad 5 thru_hole circle (at -5 -10) (size 2.75 2.75) (drill 1.5) (layers *.Cu *.Mask)
      (net 5 +5V))
    (pad 1 thru_hole circle (at 7.5 -7.5) (size 2.75 2.75) (drill 1.5) (layers *.Cu *.Mask)
      (net 1 Earth))
    (pad 3 thru_hole circle (at -7.5 -7.5) (size 2.75 2.75) (drill 1.5) (layers *.Cu *.Mask)
      (net 5 +5V))
    (pad 2 thru_hole circle (at 0 -7.5) (size 2.75 2.75) (drill 1.5) (layers *.Cu *.Mask)
      (net 3 -12V))
    (pad 10 thru_hole circle (at 5 2.5) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 1 Earth))
    (pad 8 thru_hole circle (at -5 2.5) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 1 Earth))
    (pad 9 thru_hole circle (at 0 0) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 1 Earth))
    (model "${KIPRJMOD}/User Library-DIN-5.STEP"
      (offset (xyz 1.6 14 9))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module rt65b-breakout:MountingHole_3mm_Pad_Via (layer F.Cu) (tedit 5E0D46DD)
    (at 138 44.25)
    (descr "Mounting Hole 3mm")
    (tags "mounting hole 3mm")
    (attr virtual)
    (fp_text reference REF** (at 0 -4) (layer F.Fab) hide)
    (fp_text value NC (at 0 4) (layer F.SilkS))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 0) (size 3 3) (drill 3) (layers *.Cu *.Mask))
  )
  (module rt65b-breakout:KP01.1112.11 (layer F.Cu) (tedit 5DFB1678)
    (at 132.75 79)
    (fp_text reference J3 (at 0 0.5) (layer F.Fab) hide)
    (fp_text value IEC320-C14 (at 0 -0.5) (layer F.Fab))
    (fp_text user E (at 16.5 -13.5) (layer F.SilkS))
    (fp_text user N (at -11.5 -13) (layer F.SilkS))
    (fp_text user L (at -19 -13) (layer F.SilkS))
    (pad 3 thru_hole circle (at 16.51 -16.45) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 1 Earth))
    (pad "" np_thru_hole circle (at -26.67 -12.63) (size 6 6) (drill 6) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 26.67 -7.55) (size 6 6) (drill 6) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at -11.43 -16.45) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 7 NEUT))
    (pad 1 thru_hole circle (at -19.05 -16.45) (size 2.5 2.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 6 LINE))
    (model ${KIPRJMOD}/e_0100.1701c002.step
      (offset (xyz 12.7 -6.2 18.5))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (module rt65b-breakout:MountingHole_3mm_Pad_Via (layer F.Cu) (tedit 5DFAF31D)
    (at 171 44.25)
    (descr "Mounting Hole 3mm")
    (tags "mounting hole 3mm")
    (attr virtual)
    (fp_text reference H1 (at 0 -4) (layer F.Fab) hide)
    (fp_text value 5V (at 0 4) (layer F.SilkS))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 1.59099 -1.59099) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 5 +5V))
    (pad 1 thru_hole circle (at 0 -2.25) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 5 +5V))
    (pad 1 thru_hole circle (at -1.59099 -1.59099) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 5 +5V))
    (pad 1 thru_hole circle (at -2.25 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 5 +5V))
    (pad 1 thru_hole circle (at -1.59099 1.59099) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 5 +5V))
    (pad 1 thru_hole circle (at 0 2.25) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 5 +5V))
    (pad 1 thru_hole circle (at 1.59099 1.59099) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 5 +5V))
    (pad 1 thru_hole circle (at 2.25 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 5 +5V))
    (pad 1 thru_hole rect (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Mask)
      (net 5 +5V))
  )
  (module rt65b-breakout:MountingHole_3mm_Pad_Via (layer F.Cu) (tedit 5DFAF847)
    (at 113.25 44.25)
    (descr "Mounting Hole 3mm")
    (tags "mounting hole 3mm")
    (attr virtual)
    (fp_text reference H5 (at 0 -4) (layer F.Fab) hide)
    (fp_text value LINE (at 0 4) (layer F.SilkS))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Mask)
      (net 6 LINE))
    (pad 1 thru_hole circle (at 2.25 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 6 LINE))
    (pad 1 thru_hole circle (at 1.59099 1.59099) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 6 LINE))
    (pad 1 thru_hole circle (at 0 2.25) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 6 LINE))
    (pad 1 thru_hole circle (at -1.59099 1.59099) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 6 LINE))
    (pad 1 thru_hole circle (at -2.25 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 6 LINE))
    (pad 1 thru_hole circle (at -1.59099 -1.59099) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 6 LINE))
    (pad 1 thru_hole circle (at 0 -2.25) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 6 LINE))
    (pad 1 thru_hole circle (at 1.59099 -1.59099) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 6 LINE))
  )
  (module rt65b-breakout:MountingHole_3mm_Pad_Via (layer F.Cu) (tedit 5DFAF31D)
    (at 129.75 44.25)
    (descr "Mounting Hole 3mm")
    (tags "mounting hole 3mm")
    (attr virtual)
    (fp_text reference H7 (at 0 -4) (layer F.Fab) hide)
    (fp_text value EARTH (at 0 4) (layer F.SilkS))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Mask)
      (net 1 Earth))
    (pad 1 thru_hole circle (at 2.25 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 Earth))
    (pad 1 thru_hole circle (at 1.59099 1.59099) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 Earth))
    (pad 1 thru_hole circle (at 0 2.25) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 Earth))
    (pad 1 thru_hole circle (at -1.59099 1.59099) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 Earth))
    (pad 1 thru_hole circle (at -2.25 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 Earth))
    (pad 1 thru_hole circle (at -1.59099 -1.59099) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 Earth))
    (pad 1 thru_hole circle (at 0 -2.25) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 Earth))
    (pad 1 thru_hole circle (at 1.59099 -1.59099) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 Earth))
  )
  (module rt65b-breakout:MountingHole_3mm_Pad_Via (layer F.Cu) (tedit 5DFAF31D)
    (at 121.5 44.25)
    (descr "Mounting Hole 3mm")
    (tags "mounting hole 3mm")
    (attr virtual)
    (fp_text reference H6 (at 0 -4) (layer F.Fab) hide)
    (fp_text value NEUT (at 0 4) (layer F.SilkS))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Mask)
      (net 7 NEUT))
    (pad 1 thru_hole circle (at 2.25 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 7 NEUT))
    (pad 1 thru_hole circle (at 1.59099 1.59099) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 7 NEUT))
    (pad 1 thru_hole circle (at 0 2.25) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 7 NEUT))
    (pad 1 thru_hole circle (at -1.59099 1.59099) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 7 NEUT))
    (pad 1 thru_hole circle (at -2.25 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 7 NEUT))
    (pad 1 thru_hole circle (at -1.59099 -1.59099) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 7 NEUT))
    (pad 1 thru_hole circle (at 0 -2.25) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 7 NEUT))
    (pad 1 thru_hole circle (at 1.59099 -1.59099) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 7 NEUT))
  )
  (module rt65b-breakout:MountingHole_3mm_Pad_Via (layer F.Cu) (tedit 5DFAF31D)
    (at 162.75 44.25)
    (descr "Mounting Hole 3mm")
    (tags "mounting hole 3mm")
    (attr virtual)
    (fp_text reference H4 (at 0 -4) (layer F.Fab) hide)
    (fp_text value COM (at 0 4) (layer F.SilkS))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 1 thru_hole circle (at 2.25 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 1 thru_hole circle (at 1.59099 1.59099) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 1 thru_hole circle (at 0 2.25) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 1 thru_hole circle (at -1.59099 1.59099) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 1 thru_hole circle (at -2.25 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 1 thru_hole circle (at -1.59099 -1.59099) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 1 thru_hole circle (at 0 -2.25) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 4 GND))
    (pad 1 thru_hole circle (at 1.59099 -1.59099) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 4 GND))
  )
  (module rt65b-breakout:MountingHole_3mm_Pad_Via (layer F.Cu) (tedit 5DFAF31D)
    (at 146.25 44.25)
    (descr "Mounting Hole 3mm")
    (tags "mounting hole 3mm")
    (attr virtual)
    (fp_text reference H3 (at 0 -4) (layer B.CrtYd) hide)
    (fp_text value -12V (at 0 4) (layer F.SilkS))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Mask)
      (net 3 -12V))
    (pad 1 thru_hole circle (at 2.25 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 -12V))
    (pad 1 thru_hole circle (at 1.59099 1.59099) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 -12V))
    (pad 1 thru_hole circle (at 0 2.25) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 -12V))
    (pad 1 thru_hole circle (at -1.59099 1.59099) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 -12V))
    (pad 1 thru_hole circle (at -2.25 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 -12V))
    (pad 1 thru_hole circle (at -1.59099 -1.59099) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 -12V))
    (pad 1 thru_hole circle (at 0 -2.25) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 -12V))
    (pad 1 thru_hole circle (at 1.59099 -1.59099) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 3 -12V))
  )
  (module rt65b-breakout:MountingHole_3mm_Pad_Via (layer F.Cu) (tedit 5DFAF31D)
    (at 154.5 44.25)
    (descr "Mounting Hole 3mm")
    (tags "mounting hole 3mm")
    (attr virtual)
    (fp_text reference H2 (at 0 -4) (layer F.Fab) hide)
    (fp_text value 12V (at 0 4) (layer F.SilkS))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 6 6) (drill 3) (layers *.Cu *.Mask)
      (net 2 +12V))
    (pad 1 thru_hole circle (at 2.25 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 +12V))
    (pad 1 thru_hole circle (at 1.59099 1.59099) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 +12V))
    (pad 1 thru_hole circle (at 0 2.25) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 +12V))
    (pad 1 thru_hole circle (at -1.59099 1.59099) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 +12V))
    (pad 1 thru_hole circle (at -2.25 0) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 +12V))
    (pad 1 thru_hole circle (at -1.59099 -1.59099) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 +12V))
    (pad 1 thru_hole circle (at 0 -2.25) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 +12V))
    (pad 1 thru_hole circle (at 1.59099 -1.59099) (size 0.8 0.8) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 +12V))
  )
  (gr_text "SHOCK RISK!\nUSE ONLY WITH\nAPPROPRIATE CASE" (at 118.4 70) (layer B.SilkS))
  (gr_text "MAINS VOLTAGE\nUSE EXTREME CAUTION" (at 122 72) (layer F.SilkS))
  (gr_arc (start 102 76) (end 99 76) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 189.25 76) (end 189.25 79) (angle -90) (layer Edge.Cuts) (width 0.05))
  (dimension 38.1 (width 0.12) (layer Dwgs.User)
    (gr_text "38.100 mm" (at 207.137 60.071 270) (layer Dwgs.User))
    (feature1 (pts (xy 203.581 79.121) (xy 206.453421 79.121)))
    (feature2 (pts (xy 203.581 41.021) (xy 206.453421 41.021)))
    (crossbar (pts (xy 205.867 41.021) (xy 205.867 79.121)))
    (arrow1a (pts (xy 205.867 79.121) (xy 205.280579 77.994496)))
    (arrow1b (pts (xy 205.867 79.121) (xy 206.453421 77.994496)))
    (arrow2a (pts (xy 205.867 41.021) (xy 205.280579 42.147504)))
    (arrow2b (pts (xy 205.867 41.021) (xy 206.453421 42.147504)))
  )
  (gr_text G (at 170.2 63.8) (layer F.SilkS))
  (gr_text E (at 185.2 68.8) (layer F.SilkS))
  (gr_text -12v (at 177.5 69) (layer F.SilkS))
  (gr_text 12v (at 185.8 64) (layer F.SilkS))
  (gr_text 5v (at 172.8 66.5) (layer F.SilkS))
  (gr_line (start 116.5 64) (end 116.5 52) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 118.25 64) (end 116.5 64) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 118.25 52) (end 118.25 64) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 126.5 64) (end 126.5 52) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 124.75 64) (end 126.5 64) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 124.75 52) (end 124.75 64) (layer Edge.Cuts) (width 0.05))
  (dimension 93.25 (width 0.15) (layer Dwgs.User)
    (gr_text "93.250 mm" (at 145.625 35.3) (layer Dwgs.User))
    (feature1 (pts (xy 192.25 20.5) (xy 192.25 34.586421)))
    (feature2 (pts (xy 99 20.5) (xy 99 34.586421)))
    (crossbar (pts (xy 99 34) (xy 192.25 34)))
    (arrow1a (pts (xy 192.25 34) (xy 191.123496 34.586421)))
    (arrow1b (pts (xy 192.25 34) (xy 191.123496 33.413579)))
    (arrow2a (pts (xy 99 34) (xy 100.126504 34.586421)))
    (arrow2b (pts (xy 99 34) (xy 100.126504 33.413579)))
  )
  (gr_line (start 102 79) (end 189.25 79) (layer Edge.Cuts) (width 0.05))
  (dimension 64.25 (width 0.15) (layer Dwgs.User)
    (gr_text "64.250 mm" (at 142.125 25.2) (layer Dwgs.User))
    (feature1 (pts (xy 174.25 29.75) (xy 174.25 25.913579)))
    (feature2 (pts (xy 110 29.75) (xy 110 25.913579)))
    (crossbar (pts (xy 110 26.5) (xy 174.25 26.5)))
    (arrow1a (pts (xy 174.25 26.5) (xy 173.123496 27.086421)))
    (arrow1b (pts (xy 174.25 26.5) (xy 173.123496 25.913579)))
    (arrow2a (pts (xy 110 26.5) (xy 111.126504 27.086421)))
    (arrow2b (pts (xy 110 26.5) (xy 111.126504 25.913579)))
  )
  (gr_line (start 192.25 52) (end 192.25 76) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 174.25 52) (end 192.25 52) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 166 52) (end 167.75 52) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 174.25 41) (end 174.25 52) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 167.75 52) (end 167.75 41) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 167.75 41) (end 174.25 41) (layer Edge.Cuts) (width 0.05))
  (dimension 11 (width 0.15) (layer F.Fab)
    (gr_text "11.000 mm" (at 83.7 46.5 90) (layer F.Fab))
    (feature1 (pts (xy 89 41) (xy 84.413579 41)))
    (feature2 (pts (xy 89 52) (xy 84.413579 52)))
    (crossbar (pts (xy 85 52) (xy 85 41)))
    (arrow1a (pts (xy 85 41) (xy 85.586421 42.126504)))
    (arrow1b (pts (xy 85 41) (xy 84.413579 42.126504)))
    (arrow2a (pts (xy 85 52) (xy 85.586421 50.873496)))
    (arrow2b (pts (xy 85 52) (xy 84.413579 50.873496)))
  )
  (gr_line (start 99 76) (end 99 52) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 110 52) (end 99 52) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 157.75 52) (end 159.5 52) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 149.5 52) (end 151.25 52) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 141.25 52) (end 143 52) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 133 52) (end 134.75 52) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 159.5 41) (end 166 41) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 166 41) (end 166 52) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 159.5 52) (end 159.5 41) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 151.25 41) (end 157.75 41) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 157.75 41) (end 157.75 52) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 151.25 52) (end 151.25 41) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 143 41) (end 149.5 41) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 149.5 41) (end 149.5 52) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 143 52) (end 143 41) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 134.75 41) (end 141.25 41) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 141.25 41) (end 141.25 52) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 134.75 52) (end 134.75 41) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 126.5 41) (end 133 41) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 133 41) (end 133 52) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 126.5 52) (end 126.5 41) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 118.25 41) (end 124.75 41) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 124.75 41) (end 124.75 52) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 118.25 52) (end 118.25 41) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 116.5 41) (end 116.5 52) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 110 41) (end 116.5 41) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 110 52) (end 110 41) (layer Edge.Cuts) (width 0.05))
)
