<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="32.385" x2="0" y2="2.54" width="0.1524" layer="20"/>
<wire x1="0" y1="2.54" x2="2.54" y2="0" width="0.1524" layer="20" curve="90"/>
<wire x1="2.54" y1="0" x2="34.29" y2="0" width="0.1524" layer="20"/>
<wire x1="34.29" y1="0" x2="36.83" y2="2.54" width="0.1524" layer="20" curve="90"/>
<wire x1="36.83" y1="2.54" x2="36.83" y2="32.385" width="0.1524" layer="20"/>
<wire x1="36.83" y1="32.385" x2="34.29" y2="34.925" width="0.1524" layer="20" curve="90"/>
<wire x1="34.29" y1="34.925" x2="2.54" y2="34.925" width="0.1524" layer="20"/>
<wire x1="2.54" y1="34.925" x2="0" y2="32.385" width="0.1524" layer="20" curve="90"/>
<text>Sparkfun
Pro Micro
RP2040
</text>
<text>nm3210</text>
<text>@2021</text>
<text>nRF24L01</text>
<text>GND</text>
<text>VBUS</text>
<text>LED</text>
<text>D9</text>
<text>+5V</text>
<text>Remote Control
Receive</text>
</plain>
<libraries>
<library name="nm3210_custom">
<packages>
<package name="SF17717_PROMICRORP2040_BREAKOUT">
<description>Sparkfun Pro Micro RP2040 (DEV-17717) Breakout. 

Layout of the Pro Micro board to allow for easy castellated soldering.</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X4">
<description>&lt;h3&gt;Plated Through Hole - 2x4&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:8&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="MOLEX-1X4">
<description>&lt;h3&gt;Molex 4-Pin Plated Through-Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/2pin_molex_set_19iv10.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="POWER_JACK_PTH_BREAD">
<description>&lt;h3&gt;DC Barrel Power Jack/Connector Breadboard Compatible&lt;/h3&gt;
Breadboard-friendly pins. 
5.5mm jack, 2.1mm center pole diameter
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 3&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://cdn.sparkfun.com/datasheets/Prototyping/18742.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;POWER_JACK&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Capacitors&lt;/h3&gt;
This library contains capacitors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CPOL-RADIAL-2.5MM-5MM-KIT">
<description>2.5 mm spaced PTHs with top copper masked</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="nm3210_custom" package="SF17717_PROMICRORP2040_BREAKOUT" value="SF17717_PROMICRORP2040_BREAKOUT"/>
<element name="J2" library="SparkFun-Connectors" package="2X4" value="">
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="CPOL-RADIAL-2.5MM-5MM-KIT" value="10uF">
<attribute name="PROD_ID" value="CAP-08440"/>
</element>
<element name="J4" library="SparkFun-Connectors" package="MOLEX-1X4" value="">
<attribute name="PROD_ID" value="CONN-08186"/>
<attribute name="SF_ID" value="PRT-08231"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="POWER_JACK_PTH_BREAD" value="POWER_JACKPTH_BREAD">
<attribute name="PROD_ID" value="COMP-13253"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U$1" pad="02R_PADB"/>
<contactref element="U$1" pad="02R"/>
<contactref element="U$1" pad="02R_PADT"/>
<contactref element="U$1" pad="10L_PADB"/>
<contactref element="U$1" pad="10L_PADT"/>
<contactref element="U$1" pad="10L"/>
<contactref element="U$1" pad="09L_PADB"/>
<contactref element="U$1" pad="09L"/>
<contactref element="U$1" pad="09L_PADT"/>
<contactref element="U$1" pad="GND_T"/>
<contactref element="U$1" pad="GND_B"/>
<contactref element="J4" pad="3"/>
<contactref element="J1" pad="GNDBREAK"/>
<contactref element="J1" pad="GND"/>
<contactref element="C1" pad="2"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="U$1" pad="04R_PADB"/>
<contactref element="U$1" pad="04R_PADT"/>
<contactref element="U$1" pad="04R"/>
<contactref element="C1" pad="1"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="U$1" pad="D-_B"/>
<contactref element="U$1" pad="D-_T"/>
</signal>
<signal name="D0">
<contactref element="U$1" pad="D0_T"/>
<contactref element="U$1" pad="D0_B"/>
<contactref element="J4" pad="2"/>
</signal>
<signal name="VBUS">
<contactref element="U$1" pad="01R_PADB"/>
<contactref element="U$1" pad="01R"/>
<contactref element="U$1" pad="01R_PADT"/>
<contactref element="U$1" pad="VBUS_B"/>
<contactref element="U$1" pad="VBUS_T"/>
<contactref element="J4" pad="4"/>
<contactref element="J1" pad="PWR"/>
</signal>
<signal name="N$15">
<contactref element="U$1" pad="03R_PADB"/>
<contactref element="U$1" pad="03R"/>
<contactref element="U$1" pad="03R_PADT"/>
</signal>
<signal name="N$16">
<contactref element="U$1" pad="05R_PADB"/>
<contactref element="U$1" pad="05R"/>
<contactref element="U$1" pad="05R_PADT"/>
</signal>
<signal name="N$17">
<contactref element="U$1" pad="06R_PADT"/>
<contactref element="U$1" pad="06R_PADB"/>
<contactref element="U$1" pad="06R"/>
</signal>
<signal name="IRQ">
<contactref element="U$1" pad="07R"/>
<contactref element="U$1" pad="07R_PADB"/>
<contactref element="U$1" pad="07R_PADT"/>
<contactref element="J2" pad="7"/>
</signal>
<signal name="CE">
<contactref element="U$1" pad="08R_PADT"/>
<contactref element="U$1" pad="08R_PADB"/>
<contactref element="U$1" pad="08R"/>
<contactref element="J2" pad="4"/>
</signal>
<signal name="SCK">
<contactref element="U$1" pad="09R"/>
<contactref element="U$1" pad="09R_PADT"/>
<contactref element="U$1" pad="09R_PADB"/>
<contactref element="J2" pad="6"/>
</signal>
<signal name="CIPO">
<contactref element="U$1" pad="10R_PADB"/>
<contactref element="U$1" pad="10R"/>
<contactref element="U$1" pad="10R_PADT"/>
<contactref element="J2" pad="8"/>
</signal>
<signal name="COPI">
<contactref element="U$1" pad="11R_PADB"/>
<contactref element="U$1" pad="11R"/>
<contactref element="U$1" pad="11R_PADT"/>
<contactref element="J2" pad="5"/>
</signal>
<signal name="!CS">
<contactref element="U$1" pad="12R"/>
<contactref element="U$1" pad="12R_PADT"/>
<contactref element="U$1" pad="12R_PADB"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="9">
<contactref element="U$1" pad="01L_PADB"/>
<contactref element="U$1" pad="01L_PADT"/>
<contactref element="U$1" pad="01L"/>
<contactref element="J4" pad="1"/>
</signal>
<signal name="N$27">
<contactref element="U$1" pad="02L_PADT"/>
<contactref element="U$1" pad="02L"/>
<contactref element="U$1" pad="02L_PADB"/>
</signal>
<signal name="SDA_1">
<contactref element="U$1" pad="07L_PADT"/>
<contactref element="U$1" pad="07L_PADB"/>
<contactref element="U$1" pad="07L"/>
</signal>
<signal name="SCL_1">
<contactref element="U$1" pad="08L"/>
<contactref element="U$1" pad="08L_PADB"/>
<contactref element="U$1" pad="08L_PADT"/>
</signal>
<signal name="N$1">
<contactref element="U$1" pad="12L_PADB"/>
<contactref element="U$1" pad="12L"/>
<contactref element="U$1" pad="12L_PADT"/>
</signal>
<signal name="N$2">
<contactref element="U$1" pad="11L"/>
<contactref element="U$1" pad="11L_PADT"/>
<contactref element="U$1" pad="11L_PADB"/>
</signal>
<signal name="N$6">
<contactref element="U$1" pad="06L_PADT"/>
<contactref element="U$1" pad="06L"/>
<contactref element="U$1" pad="06L_PADB"/>
</signal>
<signal name="N$7">
<contactref element="U$1" pad="05L_PADT"/>
<contactref element="U$1" pad="05L_PADB"/>
<contactref element="U$1" pad="05L"/>
</signal>
<signal name="N$8">
<contactref element="U$1" pad="04L_PADT"/>
<contactref element="U$1" pad="04L"/>
<contactref element="U$1" pad="04L_PADB"/>
</signal>
<signal name="N$9">
<contactref element="U$1" pad="03L"/>
<contactref element="U$1" pad="03L_PADT"/>
<contactref element="U$1" pad="03L_PADB"/>
</signal>
<signal name="N$3">
<contactref element="U$1" pad="SWDCK_T"/>
<contactref element="U$1" pad="SWDCK_B"/>
</signal>
<signal name="N$4">
<contactref element="U$1" pad="SWDIO_B"/>
<contactref element="U$1" pad="SWDIO_T"/>
</signal>
<signal name="N$5">
<contactref element="U$1" pad="D+_B"/>
<contactref element="U$1" pad="D+_T"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
