<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="36.609" y2="0" width="0" layer="20"/>
<wire x1="36.609" y1="0" x2="36.609" y2="11.6" width="0" layer="20"/>
<wire x1="36.609" y1="11.6" x2="0" y2="11.6" width="0" layer="20"/>
<wire x1="0" y1="11.6" x2="0" y2="0" width="0" layer="20"/>
<text>11.6mm</text>
<text>36.6mm</text>
<text>1. Solder Mask - RED</text>
<text>2. 1oz Copper after plating</text>
<text>Fab Notes:</text>
<text>3. Board thickness 62mils nominal.</text>
<text>4. Silkscreen - WHITE</text>
<text>5. Materials are to be ROHS and UL 94VO compliant</text>
<text>6. Surface finish is to be ENIG</text>
<text>7. Fabricate to IPC-600 Class 2 spec</text>
<text>(C) 2012, Google Inc.</text>
<text>(C) Google Inc. 2012</text>
<text>2</text>
</plain>
<libraries>
<library name="ftdichip">
<packages>
<package name="QFN32">
<description>&lt;b&gt;QFN 32&lt;/b&gt;&lt;p&gt;
Source: http://www.ftdichip.com/Documents/DataSheets/DS_FT232R_v104.pdf</description>
</package>
</packages>
</library>
<library name="rcl">
<packages>
<package name="C0402">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="R0402">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="led">
<packages>
<package name="CHIPLED_0603">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_LY Q971.pdf</description>
</package>
</packages>
</library>
<library name="USB_DEBUG">
<packages>
<package name="MOLEX_48037-1000">
<description>USB A type PLUG, SMT, Bent Shell Leg</description>
</package>
</packages>
</library>
<library name="wirepad">
<packages>
<package name="2,15/1,0">
<description>&lt;b&gt;THROUGH-HOLE PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="TPS717xx">
<packages>
<package name="SC70-5">
</package>
</packages>
</library>
<library name="untitled">
<packages>
<package name="LOGO_ANDROID_USB">
<description>for usb board</description>
</package>
</packages>
</library>
<library name="frames">
<description>&lt;b&gt;Frames for Sheet and Layout&lt;/b&gt;</description>
<packages>
<package name="DOCFIELD">
<description>&lt;b&gt;DOCUMENT FIELD&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="ftdichip" package="QFN32" value="FT232RQ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MF" value=""/>
<attribute name="MPN" value="FT232RQ"/>
<attribute name="OC_FARNELL" value="1146033"/>
<attribute name="OC_NEWARK" value="91K9919"/>
</element>
<element name="C1" library="rcl" package="C0402" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="rcl" package="C0402" value="4.7uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="rcl" package="C0402" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="rcl" package="C0402" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="rcl" package="R0402" value="120">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="rcl" package="R0402" value="120">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TX" library="led" package="CHIPLED_0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RX" library="led" package="CHIPLED_0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="rcl" package="R0402" value="33">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="rcl" package="C0402" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="USB_DEBUG" package="MOLEX_48037-1000" value="USB_A_PLUG"/>
<element name="PTC1" library="rcl" package="R0603" value="33 Ohm">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="3V3" library="wirepad" package="2,15/1,0" value="WIREPAD2,15/1,0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TXD" library="wirepad" package="2,15/1,0" value="WIREPAD2,15/1,0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RXD" library="wirepad" package="2,15/1,0" value="WIREPAD2,15/1,0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="GND" library="wirepad" package="2,15/1,0" value="WIREPAD2,15/1,0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="rcl" package="C0402" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="GND1" library="wirepad" package="2,15/1,0" value="WIREPAD2,15/1,0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U3" library="TPS717xx" package="SC70-5" value="TPS71718">
<attribute name="VALUE"/>
<attribute name="NAME"/>
<attribute name="U3" value="TPS717"/>
</element>
<element name="U2" library="TPS717xx" package="SC70-5" value="TPS71701">
<attribute name="VALUE"/>
<attribute name="NAME"/>
<attribute name="U2" value="TPS717"/>
</element>
<element name="R4" library="rcl" package="R0402" value="976K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="rcl" package="R0402" value="301K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="rcl" package="C0402" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FB1" library="rcl" package="C0402" value="33">
<attribute name="NAME"/>
</element>
<element name="C8" library="rcl" package="C0402" value="10nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$2" library="untitled" package="LOGO_ANDROID_USB" value=""/>
<element name="U$3" library="frames" package="DOCFIELD" value="">
<attribute name="LAST_DATE_TIME"/>
<attribute name="SHEET"/>
<attribute name="DRAWING_NAME"/>
</element>
</elements>
<signals>
<signal name="TXLED">
<contactref element="U1" pad="22"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="RXLED">
<contactref element="U1" pad="21"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="GND">
<contactref element="U1" pad="4"/>
<contactref element="U1" pad="17"/>
<contactref element="U1" pad="20"/>
<contactref element="U1" pad="24"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="U$1" pad="GND"/>
<contactref element="C4" pad="2"/>
<contactref element="GND" pad="1"/>
<contactref element="C6" pad="2"/>
<contactref element="GND1" pad="1"/>
<contactref element="U1" pad="26"/>
<contactref element="U3" pad="GND"/>
<contactref element="U2" pad="GND"/>
<contactref element="R5" pad="1"/>
<contactref element="C7" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="U$1" pad="SHIELD1"/>
<contactref element="U$1" pad="SHIELD2"/>
</signal>
<signal name="VCC">
<contactref element="U1" pad="19"/>
<contactref element="C2" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="U3" pad="IN"/>
<contactref element="U3" pad="EN"/>
<contactref element="U2" pad="IN"/>
<contactref element="U2" pad="EN"/>
<contactref element="FB1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="TX" pad="C"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="RX" pad="C"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="VDD_3V3">
<contactref element="U1" pad="16"/>
<contactref element="TX" pad="A"/>
<contactref element="RX" pad="A"/>
<contactref element="C1" pad="1"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="RXD">
<contactref element="U1" pad="2"/>
<contactref element="RXD" pad="1"/>
</signal>
<signal name="TXD">
<contactref element="R3" pad="2"/>
<contactref element="TXD" pad="1"/>
</signal>
<signal name="VDD_1V8">
<contactref element="U1" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="U3" pad="OUT"/>
</signal>
<signal name="VBUS_UNFILTERED">
<contactref element="U$1" pad="VDD"/>
<contactref element="FB1" pad="1"/>
<contactref element="C8" pad="1"/>
</signal>
<signal name="USB_D-">
<contactref element="U1" pad="15"/>
<contactref element="U$1" pad="USB_D-"/>
</signal>
<signal name="USB_D+">
<contactref element="U1" pad="14"/>
<contactref element="U$1" pad="USB_D+"/>
</signal>
<signal name="TXD_UNFILTERED">
<contactref element="U1" pad="30"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="MIC_PIN_PROTECTED">
<contactref element="PTC1" pad="2"/>
<contactref element="3V3" pad="1"/>
</signal>
<signal name="VDD_3V36">
<contactref element="PTC1" pad="1"/>
<contactref element="U2" pad="OUT"/>
<contactref element="R4" pad="2"/>
<contactref element="C7" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="R4" pad="1"/>
<contactref element="R5" pad="2"/>
<contactref element="U2" pad="FB"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
