(kicad_pcb (version 20171130) (host pcbnew "(5.0.0-rc2-dev-329-gd1ab62fb4)")
  (general
    (thickness 1.6)
    (drawings 8)
    (tracks 106)
    (zones 0)
    (modules 11)
    (nets 12)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.2)
    (trace_clearance 0.15)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad2)")
  (net 2 GND)
  (net 3 +3V3)
  (net 4 "Net-(D1-Pad1)")
  (net 5 SDA)
  (net 6 CS_XL)
  (net 7 CS_MAG)
  (net 8 INT_MAG)
  (net 9 INT_1_XL)
  (net 10 INT_2_XL)
  (net 11 SCL)
  (net_class Default "This is the default net class."
    (clearance 0.15)
    (trace_width 0.2)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net CS_MAG)
    (add_net CS_XL)
    (add_net GND)
    (add_net INT_1_XL)
    (add_net INT_2_XL)
    (add_net INT_MAG)
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(D1-Pad1)")
    (add_net SCL)
    (add_net SDA)
  )
  (net_class VCC ""
    (clearance 0.2)
    (trace_width 0.35)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 144.78 94.107)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 -1.5) (layer F.SilkS))
    (fp_text value 220nF (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad2)"))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 149.352 93.345)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 0 -1.5) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 149.352 91.186 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at 0 -1.5 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 180) (layer F.Fab))
    (pad 1 smd rect (at -1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 1 0 180) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 5ABD5E64)
    (at 140.716 89.408)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 10K (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 11 SCL))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804)
    (at 140.716 91.948)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 10K (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0.5) (layer F.Fab))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 SDA))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805 (layer F.Cu) (tedit 58E0A804)
    (at 141.671 86.741)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 0 -1.65) (layer F.SilkS))
    (fp_text value 10K (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad1)"))
    (pad 1 smd rect (at -0.95 0) (size 0.7 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LSM303AGRTR:LGA12R50P_200X200X100 (layer F.Cu) (tedit 0)
    (at 144.526 90.932)
    (attr smd)
    (fp_text reference U1 (at -0.642587 -1.40718) (layer F.SilkS))
    (fp_text value LSM303AGRTR (at -0.48927 1.60177) (layer F.SilkS))
    (pad 1 smd rect (at -0.76 -0.75) (size 0.45 0.35) (layers F.Cu F.Paste F.Mask)
      (net 11 SCL))
    (pad 2 smd rect (at -0.76 -0.25) (size 0.45 0.35) (layers F.Cu F.Paste F.Mask)
      (net 6 CS_XL))
    (pad 3 smd rect (at -0.76 0.25) (size 0.45 0.35) (layers F.Cu F.Paste F.Mask)
      (net 7 CS_MAG))
    (pad 4 smd rect (at -0.76 0.75) (size 0.45 0.35) (layers F.Cu F.Paste F.Mask)
      (net 5 SDA))
    (pad 5 smd rect (at -0.25 0.76 90) (size 0.45 0.35) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad2)"))
    (pad 6 smd rect (at 0.25 0.76 90) (size 0.45 0.35) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 7 smd rect (at 0.76 0.75) (size 0.45 0.35) (layers F.Cu F.Paste F.Mask)
      (net 8 INT_MAG))
    (pad 8 smd rect (at 0.76 0.25) (size 0.45 0.35) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 9 smd rect (at 0.76 -0.25) (size 0.45 0.35) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 10 smd rect (at 0.76 -0.75) (size 0.45 0.35) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 11 smd rect (at 0.25 -0.76 90) (size 0.45 0.35) (layers F.Cu F.Paste F.Mask)
      (net 10 INT_2_XL))
    (pad 12 smd rect (at -0.25 -0.76 90) (size 0.45 0.35) (layers F.Cu F.Paste F.Mask)
      (net 9 INT_1_XL))
  )
  (module Pin_Headers:Pin_Header_Straight_1x05_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 139.7 96.52 90)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference J1 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value Conn_01x05 (at 0 12.49 90) (layer F.Fab))
    (fp_text user %R (at 0 5.08 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 CS_XL))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 CS_MAG))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 SCL))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 SDA))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 INT_MAG))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x05_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x05_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 149.86 83.82 270)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference J2 (at 0 -2.33 270) (layer F.SilkS))
    (fp_text value Conn_01x05 (at 0 12.49 270) (layer F.Fab))
    (fp_text user %R (at 0 5.08) (layer F.Fab))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 INT_1_XL))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 INT_2_XL))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x05_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 59959803)
    (at 144.526 87.079 90)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at 0 -1.45 90) (layer F.SilkS))
    (fp_text value LED (at 0 1.55 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 90) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D1-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Capacitors_Tantalum_SMD:CP_Tantalum_Case-T_EIA-3528-12_Reflow (layer F.Cu) (tedit 58CC8C08)
    (at 148.462 87.757)
    (descr "Tantalum capacitor, Case T, EIA 3528-12, 3.5x2.8x1.2mm, Reflow soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference C2 (at 0 -3.15) (layer F.SilkS))
    (fp_text value 10uF (at 0 3.15) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 1.525 0) (size 1.95 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -1.525 0) (size 1.95 2.5) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model Capacitors_Tantalum_SMD.3dshapes/CP_Tantalum_Case-T_EIA-3528-12.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (dimension 16.51 (width 0.3) (layer F.SilkS)
    (gr_text "0.6500 in" (at 162.882 90.043 270) (layer F.SilkS))
    (feature1 (pts (xy 151.892 98.298) (xy 161.368421 98.298)))
    (feature2 (pts (xy 151.892 81.788) (xy 161.368421 81.788)))
    (crossbar (pts (xy 160.782 81.788) (xy 160.782 98.298)))
    (arrow1a (pts (xy 160.782 98.298) (xy 160.195579 97.171496)))
    (arrow1b (pts (xy 160.782 98.298) (xy 161.368421 97.171496)))
    (arrow2a (pts (xy 160.782 81.788) (xy 160.195579 82.914504)))
    (arrow2b (pts (xy 160.782 81.788) (xy 161.368421 82.914504)))
  )
  (dimension 14.224 (width 0.3) (layer F.SilkS)
    (gr_text "0.5600 in" (at 144.78 72.957) (layer F.SilkS))
    (feature1 (pts (xy 151.892 81.788) (xy 151.892 74.470579)))
    (feature2 (pts (xy 137.668 81.788) (xy 137.668 74.470579)))
    (crossbar (pts (xy 137.668 75.057) (xy 151.892 75.057)))
    (arrow1a (pts (xy 151.892 75.057) (xy 150.765496 75.643421)))
    (arrow1b (pts (xy 151.892 75.057) (xy 150.765496 74.470579)))
    (arrow2a (pts (xy 137.668 75.057) (xy 138.794504 75.643421)))
    (arrow2b (pts (xy 137.668 75.057) (xy 138.794504 74.470579)))
  )
  (dimension 14.224 (width 0.3) (layer F.SilkS)
    (gr_text "14.224 mm" (at 144.78 77.148) (layer F.SilkS))
    (feature1 (pts (xy 137.668 81.788) (xy 137.668 78.661579)))
    (feature2 (pts (xy 151.892 81.788) (xy 151.892 78.661579)))
    (crossbar (pts (xy 151.892 79.248) (xy 137.668 79.248)))
    (arrow1a (pts (xy 137.668 79.248) (xy 138.794504 78.661579)))
    (arrow1b (pts (xy 137.668 79.248) (xy 138.794504 79.834421)))
    (arrow2a (pts (xy 151.892 79.248) (xy 150.765496 78.661579)))
    (arrow2b (pts (xy 151.892 79.248) (xy 150.765496 79.834421)))
  )
  (dimension 16.51 (width 0.3) (layer F.SilkS)
    (gr_text "16.510 mm" (at 157.167 90.043 270) (layer F.SilkS))
    (feature1 (pts (xy 151.892 98.298) (xy 155.653421 98.298)))
    (feature2 (pts (xy 151.892 81.788) (xy 155.653421 81.788)))
    (crossbar (pts (xy 155.067 81.788) (xy 155.067 98.298)))
    (arrow1a (pts (xy 155.067 98.298) (xy 154.480579 97.171496)))
    (arrow1b (pts (xy 155.067 98.298) (xy 155.653421 97.171496)))
    (arrow2a (pts (xy 155.067 81.788) (xy 154.480579 82.914504)))
    (arrow2b (pts (xy 155.067 81.788) (xy 155.653421 82.914504)))
  )
  (gr_line (start 137.668 81.788) (end 151.892 81.788) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 137.668 98.298) (end 137.668 81.788) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 151.892 98.298) (end 137.668 98.298) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 151.892 81.788) (end 151.892 98.298) (layer Edge.Cuts) (width 0.2))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 133.56336 101.30536) (xy 153.8 102.2) (xy 152.8 79.2) (xy 134.4 80)
      )
    )
  )
)
