(kicad_pcb (version 4) (host pcbnew 4.0.7-e1-6374~58~ubuntu16.04.1)
  (general
    (links 126)
    (no_connects 0)
    (area 113.004021 57.572699 187.894301 142.340801)
    (thickness 1.6)
    (drawings 132)
    (tracks 471)
    (zones 0)
    (modules 63)
    (nets 43)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.6)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.15)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 4)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "/home/sven/work/avr/4chord-midi/hardware/ATmega328-TQFP32 Revision B/pdf/"))
  )
  (net 0 "")
  (net 1 +3V3)
  (net 2 GND)
  (net 3 /XTAL1)
  (net 4 /XTAL2)
  (net 5 "Net-(C8-Pad1)")
  (net 6 "Net-(C9-Pad1)")
  (net 7 "Net-(C10-Pad1)")
  (net 8 "Net-(C11-Pad1)")
  (net 9 "Net-(C12-Pad1)")
  (net 10 "Net-(C13-Pad1)")
  (net 11 "Net-(C14-Pad1)")
  (net 12 "Net-(C15-Pad1)")
  (net 13 "Net-(D1-Pad2)")
  (net 14 "Net-(D1-Pad1)")
  (net 15 "Net-(D2-Pad2)")
  (net 16 "Net-(D3-Pad2)")
  (net 17 "Net-(D4-Pad2)")
  (net 18 /USB_RESET)
  (net 19 /USB_D-)
  (net 20 /BTN_MENU_SELECT)
  (net 21 /LCD_BACKLIGHT_PWM)
  (net 22 /LCD_#RESET)
  (net 23 /LCD_D#C)
  (net 24 /LCD_#CS)
  (net 25 /SPI_MOSI)
  (net 26 /SPI_MISO)
  (net 27 /SPI_SCK)
  (net 28 /BTN_CHORD_I)
  (net 29 /BTN_CHORD_V)
  (net 30 /BTN_CHORD_vi)
  (net 31 /BTN_CHORD_IV)
  (net 32 /#RESET)
  (net 33 /UART_RX)
  (net 34 /UART_TX)
  (net 35 /USB_D+)
  (net 36 "Net-(P1-Pad2)")
  (net 37 "Net-(P1-Pad3)")
  (net 38 "Net-(P3-Pad1)")
  (net 39 +5V)
  (net 40 "Net-(Q1-Pad1)")
  (net 41 /BTN_MENU_PREV)
  (net 42 /BTN_MENU_NEXT)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /#RESET)
    (add_net /BTN_CHORD_I)
    (add_net /BTN_CHORD_IV)
    (add_net /BTN_CHORD_V)
    (add_net /BTN_CHORD_vi)
    (add_net /BTN_MENU_NEXT)
    (add_net /BTN_MENU_PREV)
    (add_net /BTN_MENU_SELECT)
    (add_net /LCD_#CS)
    (add_net /LCD_#RESET)
    (add_net /LCD_BACKLIGHT_PWM)
    (add_net /LCD_D#C)
    (add_net /SPI_MISO)
    (add_net /SPI_MOSI)
    (add_net /SPI_SCK)
    (add_net /UART_RX)
    (add_net /UART_TX)
    (add_net /USB_D+)
    (add_net /USB_D-)
    (add_net /USB_RESET)
    (add_net /XTAL1)
    (add_net /XTAL2)
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(C12-Pad1)")
    (add_net "Net-(C13-Pad1)")
    (add_net "Net-(C14-Pad1)")
    (add_net "Net-(C15-Pad1)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(C9-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(P1-Pad2)")
    (add_net "Net-(P1-Pad3)")
    (add_net "Net-(P3-Pad1)")
    (add_net "Net-(Q1-Pad1)")
  )
  (net_class Power ""
    (clearance 0.2)
    (trace_width 0.4)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net GND)
  )
  (net_class Signal ""
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module Nokia_5110-3310_LCD:Nokia_5110-3310_LCD (layer F.Cu) (tedit 5985A8F6)
    (at 136.2 70.6)
    (fp_text reference U2 (at 0 6) (layer F.SilkS) hide)
    (fp_text value Nokia_5110_LCD (at 0 8) (layer F.Fab))
    (pad "" thru_hole circle (at 17.25 32.5) (size 2 2) (drill 2) (layers *.Cu))
    (pad "" np_thru_hole circle (at 20.25 23) (size 1.5 1.5) (drill 1.5) (layers *.Mask B.Cu F.SilkS))
    (pad "" np_thru_hole circle (at 20.25 21.75) (size 1.5 1.5) (drill 1.5) (layers *.Mask B.Cu F.SilkS))
    (pad "" np_thru_hole circle (at -20.25 23.25) (size 1.5 1.5) (drill 1.5) (layers *.Mask B.Cu F.SilkS))
    (pad "" np_thru_hole circle (at -20.25 22) (size 1.5 1.5) (drill 1.5) (layers *.Mask B.Cu F.SilkS))
    (pad "" np_thru_hole circle (at -20.25 23.75) (size 1.5 1.5) (drill 1.5) (layers *.Mask B.Cu F.SilkS))
    (pad "" np_thru_hole circle (at -20.25 21.25) (size 1.5 1.5) (drill 1.5) (layers *.Mask B.Cu F.SilkS))
    (pad "" np_thru_hole circle (at -20.25 3.75) (size 1.5 1.5) (drill 1.5) (layers *.Mask B.Cu F.SilkS))
    (pad "" np_thru_hole circle (at -20.25 3.25) (size 1.5 1.5) (drill 1.5) (layers *.Mask B.Cu F.SilkS))
    (pad "" np_thru_hole circle (at -20.25 1.25) (size 1.5 1.5) (drill 1.5) (layers *.Mask B.Cu F.SilkS))
    (pad "" np_thru_hole circle (at -20.25 1.75) (size 1.5 1.5) (drill 1.5) (layers *.Mask B.Cu F.SilkS))
    (pad "" np_thru_hole circle (at 20.25 23.75) (size 1.5 1.5) (drill 1.5) (layers *.Mask B.Cu F.SilkS))
    (pad "" np_thru_hole circle (at 20.25 21.25) (size 1.5 1.5) (drill 1.5) (layers *.Mask B.Cu F.SilkS))
    (pad "" np_thru_hole circle (at 20.25 3) (size 1.5 1.5) (drill 1.5) (layers *.Mask B.Cu F.SilkS))
    (pad "" smd rect (at 19 2.5) (size 1.5 3) (layers B.Cu B.Mask))
    (pad "" smd rect (at 19 22.5) (size 1.5 3) (layers B.Cu B.Mask))
    (pad "" smd rect (at -19 22.5) (size 1.5 3) (layers B.Cu B.Mask))
    (pad "" smd rect (at -19 2.5) (size 1.5 3) (layers B.Cu B.Mask))
    (pad "" np_thru_hole oval (at 20.25 22.5) (size 2 4.5) (drill 1.5) (layers *.Mask B.Cu F.SilkS))
    (pad "" np_thru_hole oval (at -20.25 22.5) (size 2 4.5) (drill 1.5) (layers *.Mask B.Cu F.SilkS))
    (pad "" np_thru_hole oval (at 20.25 2.5) (size 2 4.5) (drill 1.5) (layers *.Mask B.Cu F.SilkS))
    (pad "" np_thru_hole oval (at -20.25 2.5) (size 2 4.5) (drill 1.5) (layers *.Mask B.Cu F.SilkS))
    (pad 9 smd rect (at 4 2.5) (size 0.6 3) (layers F.Cu F.Mask)
      (net 1 +3V3))
    (pad 8 smd rect (at 3 2.5) (size 0.6 3) (layers F.Cu F.Mask)
      (net 27 /SPI_SCK))
    (pad 7 smd rect (at 2 2.5) (size 0.6 3) (layers F.Cu F.Mask)
      (net 25 /SPI_MOSI))
    (pad 6 smd rect (at 1 2.5) (size 0.6 3) (layers F.Cu F.Mask)
      (net 23 /LCD_D#C))
    (pad 1 smd rect (at -4 2.5) (size 0.6 3) (layers F.Cu F.Mask)
      (net 22 /LCD_#RESET))
    (pad 2 smd rect (at -3 2.5) (size 0.6 3) (layers F.Cu F.Mask)
      (net 12 "Net-(C15-Pad1)"))
    (pad 5 smd rect (at 0 2.5) (size 0.6 3) (layers F.Cu F.Mask)
      (net 24 /LCD_#CS))
    (pad 4 smd rect (at -1 2.5) (size 0.6 3) (layers F.Cu F.Mask)
      (net 1 +3V3))
    (pad 3 smd rect (at -2 2.5) (size 0.6 3) (layers F.Cu F.Mask)
      (net 2 GND))
    (pad "" np_thru_hole circle (at 20.25 1.25) (size 1.5 1.5) (drill 1.5) (layers *.Mask B.Cu F.SilkS))
    (pad "" np_thru_hole circle (at 20.25 3.75) (size 1.5 1.5) (drill 1.5) (layers *.Mask B.Cu F.SilkS))
    (pad "" np_thru_hole circle (at 20.25 1.75) (size 1.5 1.5) (drill 1.5) (layers *.Mask B.Cu F.SilkS))
    (pad "" thru_hole circle (at -17.25 6) (size 2 2) (drill 2) (layers *.Cu))
  )
  (module Connect:USB_Mini-B (layer F.Cu) (tedit 59441C46)
    (at 135.9 63.7 270)
    (descr "USB Mini-B 5-pin SMD connector")
    (tags "USB USB_B USB_Mini connector")
    (attr smd)
    (fp_text reference P1 (at -0.65 6.9 270) (layer F.SilkS) hide)
    (fp_text value USB_B (at -0.65 -7.1 270) (layer F.Fab))
    (pad 1 smd rect (at 2.8 -1.6 270) (size 2.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 39 +5V))
    (pad 2 smd rect (at 2.8 -0.8 270) (size 2.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(P1-Pad2)"))
    (pad 3 smd rect (at 2.8 0 270) (size 2.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(P1-Pad3)"))
    (pad 4 smd rect (at 2.8 0.8 270) (size 2.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 5 smd rect (at 2.8 1.6 270) (size 2.3 0.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 6 smd rect (at 2.7 -4.45 270) (size 2.5 2) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at -2.8 -4.45 270) (size 2.5 2) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 2.7 4.45 270) (size 2.5 2) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at -2.8 4.45 270) (size 2.5 2) (layers F.Cu F.Paste F.Mask))
    (pad "" np_thru_hole circle (at 0.2 -2.2 270) (size 0.9 0.9) (drill 0.9) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0.2 2.2 270) (size 0.9 0.9) (drill 0.9) (layers *.Cu *.Mask))
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 5985F6FA)
    (at 131.064 124.841 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 0 1.778 270) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 59594D69)
    (at 146.812 88.392 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at 0 -1.75 360) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 1.75 180) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 59594CCA)
    (at 126.238 91.694 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at 0 1.75 270) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 5985ADC4)
    (at 126.238 85.598 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at 0 -1.778 90) (layer B.SilkS))
    (fp_text value 27p (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 3 /XTAL1))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 5985ADBC)
    (at 126.238 79.629 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at 0 1.778 450) (layer B.SilkS))
    (fp_text value 27p (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 4 /XTAL2))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 59594CB6)
    (at 122 112.7 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C8 (at 0 -1.75 270) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 59594C9C)
    (at 136 112.7 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C9 (at 0 -1.75 270) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(C9-Pad1)"))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 150.1 112.8 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C10 (at 0 1.75 90) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 5985E0C9)
    (at 135.128 134.112 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C11 (at 0 1.778 450) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(C11-Pad1)"))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 59594D51)
    (at 143.3 134.1 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C12 (at 0 -1.75 270) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(C12-Pad1)"))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 59594D35)
    (at 157.3 134.1 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C13 (at 0 -1.75 270) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(C13-Pad1)"))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 171.323 134.239 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C14 (at 0 1.75 90) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 1.75 90) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(C14-Pad1)"))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 58AA84A8)
    (at 134.874 72.517 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C15 (at 0 1.75 270) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75 270) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(C15-Pad1)"))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 59441C57)
    (at 117.5 83.6 270)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at 0 -1.45 270) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.55 270) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D1-Pad2)"))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D1-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 59441C69)
    (at 155 83.6 270)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D2 (at 0 -1.45 270) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.55 270) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(D2-Pad2)"))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D1-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 59441C62)
    (at 117.5 96.7 270)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D3 (at 0 -1.45 270) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.55 270) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(D3-Pad2)"))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D1-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0805 (layer F.Cu) (tedit 59441C6E)
    (at 154.9 96.6 270)
    (descr "LED 0805 smd package")
    (tags "LED led 0805 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D4 (at 0 -1.45 270) (layer F.SilkS) hide)
    (fp_text value LED (at 0 1.55 270) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(D4-Pad2)"))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 1.2) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(D1-Pad1)"))
    (model LEDs.3dshapes/LED_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Housings_QFP:TQFP-32_7x7mm_Pitch0.8mm (layer B.Cu) (tedit 59441C1F)
    (at 139.1 87.5)
    (descr "32-Lead Plastic Thin Quad Flatpack (PT) - 7x7x1.0 mm Body, 2.00 mm [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "QFP 0.8")
    (attr smd)
    (fp_text reference IC1 (at 0 6.05) (layer B.SilkS) hide)
    (fp_text value ATMEGA328P-A (at 0 -6.05) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -4.25 2.8) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at -4.25 2) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 41 /BTN_MENU_PREV))
    (pad 3 smd rect (at -4.25 1.2) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 4 smd rect (at -4.25 0.4) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (pad 5 smd rect (at -4.25 -0.4) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 6 smd rect (at -4.25 -1.2) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (pad 7 smd rect (at -4.25 -2) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 3 /XTAL1))
    (pad 8 smd rect (at -4.25 -2.8) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 4 /XTAL2))
    (pad 9 smd rect (at -2.8 -4.25 270) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 21 /LCD_BACKLIGHT_PWM))
    (pad 10 smd rect (at -2 -4.25 270) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 19 /USB_D-))
    (pad 11 smd rect (at -1.2 -4.25 270) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 18 /USB_RESET))
    (pad 12 smd rect (at -0.4 -4.25 270) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 22 /LCD_#RESET))
    (pad 13 smd rect (at 0.4 -4.25 270) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 23 /LCD_D#C))
    (pad 14 smd rect (at 1.2 -4.25 270) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 24 /LCD_#CS))
    (pad 15 smd rect (at 2 -4.25 270) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 25 /SPI_MOSI))
    (pad 16 smd rect (at 2.8 -4.25 270) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 26 /SPI_MISO))
    (pad 17 smd rect (at 4.25 -2.8) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 27 /SPI_SCK))
    (pad 18 smd rect (at 4.25 -2) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (pad 19 smd rect (at 4.25 -1.2) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 20 smd rect (at 4.25 -0.4) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 21 smd rect (at 4.25 0.4) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 22 smd rect (at 4.25 1.2) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask))
    (pad 23 smd rect (at 4.25 2) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 31 /BTN_CHORD_IV))
    (pad 24 smd rect (at 4.25 2.8) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 30 /BTN_CHORD_vi))
    (pad 25 smd rect (at 2.8 4.25 270) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 29 /BTN_CHORD_V))
    (pad 26 smd rect (at 2 4.25 270) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 28 /BTN_CHORD_I))
    (pad 27 smd rect (at 1.2 4.25 270) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 42 /BTN_MENU_NEXT))
    (pad 28 smd rect (at 0.4 4.25 270) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 20 /BTN_MENU_SELECT))
    (pad 29 smd rect (at -0.4 4.25 270) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 32 /#RESET))
    (pad 30 smd rect (at -1.2 4.25 270) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 33 /UART_RX))
    (pad 31 smd rect (at -2 4.25 270) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 34 /UART_TX))
    (pad 32 smd rect (at -2.8 4.25 270) (size 1.6 0.55) (layers B.Cu B.Paste B.Mask)
      (net 35 /USB_D+))
    (model Housings_QFP.3dshapes/TQFP-32_7x7mm_Pitch0.8mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 59441C29)
    (at 184.9 118.3)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference P3 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value UART (at 0 9.95) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.33) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(P3-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 /UART_RX))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 /UART_TX))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer B.Cu) (tedit 58CE4E7E)
    (at 140.716 77.724 270)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 0 2.5 270) (layer B.SilkS))
    (fp_text value 2N7002 (at 0 -2.5 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1 0.95 270) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 40 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at -1 -0.95 270) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 3 smd rect (at 1 0 270) (size 0.9 0.8) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 148.59 72.644 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 1.7 270) (layer B.SilkS))
    (fp_text value 68R (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 36 "Net-(P1-Pad2)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 19 /USB_D-))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 59594D9F)
    (at 128.9 97.8)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0 -1.8 180) (layer B.SilkS))
    (fp_text value 68R (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 37 "Net-(P1-Pad3)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 35 /USB_D+))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 595907E0)
    (at 151.257 72.644 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 0 -1.8 450) (layer B.SilkS))
    (fp_text value 1k5 (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 36 "Net-(P1-Pad2)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 18 /USB_RESET))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 59594DB6)
    (at 128.9 102.6)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at -0.05 -1.75 180) (layer B.SilkS))
    (fp_text value 1M (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 37 "Net-(P1-Pad3)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 127.508 112.522 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at 0 1.7 270) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 41 /BTN_MENU_PREV))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 5 "Net-(C8-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 5985B654)
    (at 141.478 112.649 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at 0 1.651 270) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 20 /BTN_MENU_SELECT))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 6 "Net-(C9-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 5959071B)
    (at 144.4 112.7 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at 0 -1.7 450) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 42 /BTN_MENU_NEXT))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(C10-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 153.8 128.4 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R8 (at 0 1.7 270) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 28 /BTN_CHORD_I))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(C11-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 5959075C)
    (at 156.2 128.3 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R9 (at 0 -1.8 450) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 29 /BTN_CHORD_V))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 9 "Net-(C12-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 162.8 134.2 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R10 (at 0 1.7 270) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 30 /BTN_CHORD_vi))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(C13-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 59590779)
    (at 165.6 134.2 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R11 (at 0 -1.8 450) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 31 /BTN_CHORD_IV))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(C14-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 118.8 89.3 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R12 (at 0 1.7 180) (layer B.SilkS))
    (fp_text value 100 (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 5959078B)
    (at 159.258 85.979 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R13 (at 0 1.7 90) (layer B.SilkS))
    (fp_text value 100 (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(D2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 118.9 100.8 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R14 (at 0 1.7 180) (layer B.SilkS))
    (fp_text value 100 (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 16 "Net-(D3-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 595907AB)
    (at 159.258 92.583 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R15 (at 0 -1.8 450) (layer B.SilkS))
    (fp_text value 100 (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 17 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 5985AC45)
    (at 139.573 72.644 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R16 (at 0 -1.778 270) (layer B.SilkS))
    (fp_text value 100 (at 0 -1.75 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 40 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 21 /LCD_BACKLIGHT_PWM))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 5985AC27)
    (at 141.986 72.644 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R17 (at 0 -1.651 450) (layer B.SilkS))
    (fp_text value 1M (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 21 /LCD_BACKLIGHT_PWM))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Buttons_Switches_SMD:SW_SPST_EVPBF (layer F.Cu) (tedit 5985A97C)
    (at 122 112.7)
    (descr "Light Touch Switch")
    (attr smd)
    (fp_text reference SW1 (at 0 -3.9) (layer F.SilkS) hide)
    (fp_text value < (at 0.047 5.029) (layer F.SilkS))
    (fp_text user %R (at 0 -3.9) (layer F.Fab))
    (pad 1 smd rect (at 2.88 -2) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -2.88 -2) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -2.88 2) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 2.88 2) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C8-Pad1)"))
  )
  (module Buttons_Switches_SMD:SW_SPST_EVPBF (layer F.Cu) (tedit 5985A986)
    (at 136 112.7)
    (descr "Light Touch Switch")
    (attr smd)
    (fp_text reference SW2 (at 0 -3.9) (layer F.SilkS) hide)
    (fp_text value Select (at 0.017 5.029) (layer F.SilkS))
    (fp_text user %R (at 0 -3.9) (layer F.Fab))
    (pad 1 smd rect (at 2.88 -2) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -2.88 -2) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -2.88 2) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C9-Pad1)"))
    (pad 2 smd rect (at 2.88 2) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C9-Pad1)"))
  )
  (module Buttons_Switches_SMD:SW_SPST_EVPBF (layer F.Cu) (tedit 5985A99A)
    (at 150 112.7)
    (descr "Light Touch Switch")
    (attr smd)
    (fp_text reference SW3 (at 0 -3.9) (layer F.SilkS) hide)
    (fp_text value > (at -0.013 5.029) (layer F.SilkS))
    (fp_text user %R (at 0 -3.9) (layer F.Fab))
    (pad 1 smd rect (at 2.88 -2) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -2.88 -2) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -2.88 2) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C10-Pad1)"))
    (pad 2 smd rect (at 2.88 2) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C10-Pad1)"))
  )
  (module Buttons_Switches_SMD:SW_SPST_EVPBF (layer F.Cu) (tedit 5985A9AD)
    (at 129.3 134.1)
    (descr "Light Touch Switch")
    (attr smd)
    (fp_text reference SW4 (at 0 -3.9) (layer F.SilkS) hide)
    (fp_text value I (at -0.014 4.965) (layer F.SilkS))
    (fp_text user %R (at 0 -3.9) (layer F.Fab))
    (pad 1 smd rect (at 2.88 -2) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -2.88 -2) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -2.88 2) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C11-Pad1)"))
    (pad 2 smd rect (at 2.88 2) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C11-Pad1)"))
  )
  (module Buttons_Switches_SMD:SW_SPST_EVPBF (layer F.Cu) (tedit 5985A9C3)
    (at 143.3 134.1)
    (descr "Light Touch Switch")
    (attr smd)
    (fp_text reference SW5 (at 0 -3.9) (layer F.SilkS) hide)
    (fp_text value V (at -0.044 4.965) (layer F.SilkS))
    (fp_text user %R (at 0 -3.9) (layer F.Fab))
    (pad 1 smd rect (at 2.88 -2) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -2.88 -2) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -2.88 2) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C12-Pad1)"))
    (pad 2 smd rect (at 2.88 2) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C12-Pad1)"))
  )
  (module Buttons_Switches_SMD:SW_SPST_EVPBF (layer F.Cu) (tedit 5985A9D9)
    (at 157.3 134.1)
    (descr "Light Touch Switch")
    (attr smd)
    (fp_text reference SW6 (at 0 -3.9) (layer F.SilkS) hide)
    (fp_text value vi (at 0.053 4.965) (layer F.SilkS))
    (fp_text user %R (at 0 -3.9) (layer F.Fab))
    (pad 1 smd rect (at 2.88 -2) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -2.88 -2) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -2.88 2) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C13-Pad1)"))
    (pad 2 smd rect (at 2.88 2) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C13-Pad1)"))
  )
  (module Buttons_Switches_SMD:SW_SPST_EVPBF (layer F.Cu) (tedit 5985A9E7)
    (at 171.3 134.1)
    (descr "Light Touch Switch")
    (attr smd)
    (fp_text reference SW7 (at 0 -3.9) (layer F.SilkS) hide)
    (fp_text value IV (at 0.023 4.965) (layer F.SilkS))
    (fp_text user %R (at 0 -3.9) (layer F.Fab))
    (pad 1 smd rect (at 2.88 -2) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 1 smd rect (at -2.88 -2) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at -2.88 2) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C14-Pad1)"))
    (pad 2 smd rect (at 2.88 2) (size 2.75 1) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C14-Pad1)"))
  )
  (module TO_SOT_Packages_SMD:SOT-223 (layer B.Cu) (tedit 5986020B)
    (at 123.952 125.984 180)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U1 (at 0.127 0 360) (layer B.SilkS))
    (fp_text value LD1117S33CTR (at 0 -4.5 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 4 smd rect (at 3.15 0 180) (size 2 3.8) (layers B.Cu B.Paste B.Mask))
    (pad 2 smd rect (at -3.15 0 180) (size 2 1.5) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (pad 3 smd rect (at -3.15 -2.3 180) (size 2 1.5) (layers B.Cu B.Paste B.Mask)
      (net 39 +5V))
    (pad 1 smd rect (at -3.15 2.3 180) (size 2 1.5) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:CP_Tantalum_Case-A_EIA-3216-18_Hand (layer B.Cu) (tedit 58CC8C08)
    (at 127.889 131.826)
    (descr "Tantalum capacitor, Case A, EIA 3216-18, 3.2x1.6x1.6mm, Hand soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference C1 (at 0 2.55) (layer B.SilkS))
    (fp_text value 10u (at 0 -2.55) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -2 0) (size 3.2 1.5) (layers B.Cu B.Paste B.Mask)
      (net 39 +5V))
    (pad 2 smd rect (at 2 0) (size 3.2 1.5) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_Tantalum_SMD.3dshapes/CP_Tantalum_Case-A_EIA-3216-18.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_Tantalum_SMD:CP_Tantalum_Case-A_EIA-3216-18_Hand (layer B.Cu) (tedit 5985F6EE)
    (at 128.016 120.015)
    (descr "Tantalum capacitor, Case A, EIA 3216-18, 3.2x1.6x1.6mm, Hand soldering footprint")
    (tags "capacitor tantalum smd")
    (attr smd)
    (fp_text reference C2 (at 0 -2.54) (layer B.SilkS))
    (fp_text value 10u (at 0 -2.55) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -2 0) (size 3.2 1.5) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 2 0) (size 3.2 1.5) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_Tantalum_SMD.3dshapes/CP_Tantalum_Case-A_EIA-3216-18.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystals:Crystal_SMD_HC49-SD (layer B.Cu) (tedit 5986021C)
    (at 129.8 82.6 90)
    (descr "SMD Crystal HC-49-SD http://cdn-reichelt.de/documents/datenblatt/B400/xxx-HC49-SMD.pdf, 11.4x4.7mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference X1 (at 0.05 1.01 90) (layer B.SilkS))
    (fp_text value 12MHz (at 0 -3.55 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -4.25 0 90) (size 4.5 2) (layers B.Cu B.Paste B.Mask)
      (net 3 /XTAL1))
    (pad 2 smd rect (at 4.25 0 90) (size 4.5 2) (layers B.Cu B.Paste B.Mask)
      (net 4 /XTAL2))
    (model ${KISYS3DMOD}/Crystals.3dshapes/Crystal_SMD_HC49-SD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:IDC_Header_Straight_6pins (layer F.Cu) (tedit 5959088D)
    (at 170.3 109.7 270)
    (descr "6 pins through hole IDC header")
    (tags "IDC header socket VASCH AVR ISP")
    (fp_text reference P2 (at 3 -7.5 270) (layer F.SilkS) hide)
    (fp_text value Programmer (at 3 -4.4 270) (layer F.SilkS))
    (fp_text user 1 (at 0.02 1.72 270) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 26 /SPI_MISO))
    (pad 2 thru_hole oval (at 0 -2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 3 thru_hole oval (at 2.54 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 27 /SPI_SCK))
    (pad 4 thru_hole oval (at 2.54 -2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 25 /SPI_MOSI))
    (pad 5 thru_hole oval (at 5.08 0 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 32 /#RESET))
    (pad 6 thru_hole oval (at 5.08 -2.54 270) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (module Pin_Headers:Pin_Header_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 5985AAD0)
    (at 181.229 118.3005)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (fp_text reference P4 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value "UART Power" (at 0 9.95) (layer F.Fab))
    (fp_text user %R (at 0 3.81 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +3V3))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(P3-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(P3-Pad1)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 +5V))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Artwork_4chord-midi:craplab-fraktur-Cu locked (layer F.Cu) (tedit 5985A61A)
    (at 150.622 126.619)
    (fp_text reference G2 (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.Cu) hide)
  )
  (module Artwork_4chord-midi:craplab-fraktur-Mask locked (layer F.Cu) (tedit 5985A5F6)
    (at 150.622 126.619)
    (fp_text reference G1 (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.Mask) hide)
  )
  (module Artwork_4chord-midi:oshw-mask (layer B.Cu) (tedit 5985A674)
    (at 143.637 120.396 180)
    (fp_text reference G3 (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module Artwork_4chord-midi:oshw-cooper (layer B.Cu) (tedit 5985A727)
    (at 143.637 120.396 180)
    (fp_text reference G4 (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 5985EC97)
    (at 179.959 109.982)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C16 (at 0 -1.778) (layer B.SilkS))
    (fp_text value 100n (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.75) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 32 /#RESET))
    (pad 2 smd rect (at 1.25 0) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 179.959 113.538 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R18 (at 0 1.7 180) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 1 +3V3))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 32 /#RESET))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Artwork_4chord-midi:projpage-QR-code-inv (layer F.Cu) (tedit 5985FDA5)
    (at 136.017 88.138)
    (fp_text reference G11 (at 0 0) (layer F.SilkS) hide)
    (fp_text value qr (at 0.75 0) (layer F.SilkS) hide)
  )
  (module Artwork_4chord-midi:4chord-midi (layer B.Cu) (tedit 5985FD99)
    (at 142.113 101.219 180)
    (fp_text reference G12 (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value 4chordmidi (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module Artwork_4chord-midi:craplab (layer B.Cu) (tedit 5986137F)
    (at 165.989 101.6 180)
    (fp_text reference G22 (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value craplab (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module Artwork_4chord-midi:finland (layer B.Cu) (tedit 598618B8)
    (at 163.957 119.38 180)
    (fp_text reference G31 (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value finland (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module Artwork_4chord-midi:craplab-2400 (layer B.Cu) (tedit 0)
    (at 176.53 102.997 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (gr_text VCC (at 187 117.9 90) (layer F.SilkS))
  (gr_text RX (at 187 120.9 90) (layer F.SilkS))
  (gr_text TX (at 187 123.4 90) (layer F.SilkS))
  (gr_text GND (at 187 126.5 90) (layer F.SilkS))
  (gr_text none (at 178.7 122 90) (layer F.SilkS))
  (gr_text 3V3 (at 178.7 118.1 90) (layer F.SilkS))
  (gr_text 5V0 (at 178.8 126.1 90) (layer F.SilkS))
  (gr_text "Designed in Finland, perkele!" (at 158.369 109.601 90) (layer B.SilkS))
  (gr_circle (center 123.531 65.8614) (end 125.231 65.8614) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 116.00302 142.219142) (end 115.76738 142.188825) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.82709 142.242569) (end 116.00302 142.219142) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 118.53033 142.260483) (end 116.82709 142.242569) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 121.40357 142.274263) (end 118.53033 142.260483) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 125.7402 142.282532) (end 121.40357 142.274263) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 131.8326 142.286666) (end 125.7402 142.282532) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 139.9699 142.289422) (end 131.8326 142.286666) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 150.4484 142.2908) (end 139.9699 142.289422) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 160.9256 142.289422) (end 150.4484 142.2908) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 169.0631 142.286666) (end 160.9256 142.289422) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 175.1552 142.282532) (end 169.0631 142.286666) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 179.4919 142.274263) (end 175.1552 142.282532) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 182.3667 142.260483) (end 179.4919 142.274263) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 184.0699 142.242569) (end 182.3667 142.260483) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 184.894 142.219142) (end 184.0699 142.242569) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 185.1311 142.188825) (end 184.894 142.219142) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 185.1667 142.124057) (end 185.1311 142.188825) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 185.1942 141.972473) (end 185.1667 142.124057) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 185.215 141.687218) (end 185.1942 141.972473) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 185.2302 141.22833) (end 185.215 141.687218) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 185.2411 140.55171) (end 185.2302 141.22833) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 185.2468 139.61465) (end 185.2411 140.55171) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 185.2496 138.37303) (end 185.2468 139.61465) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 185.2507 136.78553) (end 185.2496 138.37303) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 185.2507 131.4815) (end 185.2507 136.78553) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 186.4261 131.4815) (end 185.2507 131.4815) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 187.0548 131.4773) (end 186.4261 131.4815) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 187.4266 131.4608) (end 187.0548 131.4773) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 187.6252 131.425) (end 187.4266 131.4608) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 187.73 131.3629) (end 187.6252 131.425) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 187.7684 131.2692) (end 187.73 131.3629) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 187.7988 130.9992) (end 187.7684 131.2692) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 187.821 130.4466) (end 187.7988 130.9992) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 187.8348 129.4999) (end 187.821 130.4466) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 187.8415 128.0501) (end 187.8348 129.4999) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 187.8443 125.99) (end 187.8415 128.0501) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 187.8401 123.2119) (end 187.8443 125.99) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 187.8348 119.6042) (end 187.8401 123.2119) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 187.8111 107.9666) (end 187.8348 119.6042) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 187.6404 107.3424) (end 187.8111 107.9666) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 186.3436 104.4952) (end 187.6404 107.3424) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 183.9292 101.7958) (end 186.3436 104.4952) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 180.1495 99.0286) (end 183.9292 101.7958) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 174.7612 95.9778) (end 180.1495 99.0286) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 170.6975 93.7616) (end 174.7612 95.9778) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 168.1247 92.1177) (end 170.6975 93.7616) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 166.515 90.6145) (end 168.1247 92.1177) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 165.0432 88.6259) (end 166.515 90.6145) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 164.1309 87.0038) (end 165.0432 88.6259) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 163.2574 85.0332) (end 164.1309 87.0038) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 162.2887 82.3845) (end 163.2574 85.0332) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 161.0924 78.7245) (end 162.2887 82.3845) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 160.6899 77.4679) (end 161.0924 78.7245) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 160.2987 76.2607) (end 160.6899 77.4679) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 159.9611 75.2397) (end 160.2987 76.2607) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 159.724 74.5423) (end 159.9611 75.2397) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 158.5831 71.6333) (end 159.724 74.5423) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 157.3498 69.1444) (end 158.5831 71.6333) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 155.9814 66.9989) (end 157.3498 69.1444) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 154.4324 65.1164) (end 155.9814 66.9989) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 151.1582 62.2515) (end 154.4324 65.1164) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 147.3024 60.022) (end 151.1582 62.2515) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 142.985 58.4828) (end 147.3024 60.022) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 138.3231 57.689) (end 142.985 58.4828) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 137.3654 57.6393) (end 138.3231 57.689) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 136.172 57.6227) (end 137.3654 57.6393) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 134.9758 57.6393) (end 136.172 57.6227) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 134.0126 57.6876) (end 134.9758 57.6393) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 128.4315 58.7294) (end 134.0126 57.6876) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 123.3893 60.8513) (end 128.4315 58.7294) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 119.81332 63.307) (end 123.3893 60.8513) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 116.91528 66.2961) (end 119.81332 63.307) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.54276 68.1122) (end 116.91528 66.2961) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.39348 69.9604) (end 115.54276 68.1122) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 113.563897 71.9487) (end 114.39348 69.9604) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 113.153241 74.1867) (end 113.563897 71.9487) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 113.089851 75.0895) (end 113.153241 74.1867) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 113.065046 103.1836) (end 113.089851 75.0895) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 113.058156 111.7328) (end 113.065046 103.1836) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 113.054022 118.3639) (end 113.058156 111.7328) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 113.056778 123.318) (end 113.054022 118.3639) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 113.063668 126.8361) (end 113.056778 123.318) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 113.076071 129.1595) (end 113.063668 126.8361) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 113.096741 130.5306) (end 113.076071 129.1595) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 113.12568 131.1893) (end 113.096741 130.5306) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 113.162887 131.3795) (end 113.12568 131.1893) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 113.485348 131.4608) (end 113.162887 131.3795) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 114.46513 131.4815) (end 113.485348 131.4608) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.64611 131.4815) (end 114.46513 131.4815) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.64611 136.78553) (end 115.64611 131.4815) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.64611 138.37303) (end 115.64611 136.78553) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.64887 139.61465) (end 115.64611 138.37303) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.65576 140.55171) (end 115.64887 139.61465) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.66541 141.22833) (end 115.65576 140.55171) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.68056 141.687218) (end 115.66541 141.22833) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.70261 141.972473) (end 115.68056 141.687218) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.73017 142.124057) (end 115.70261 141.972473) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 115.76738 142.188825) (end 115.73017 142.124057) (layer Edge.Cuts) (width 0.1))
  (gr_circle (center 148.987 65.8614) (end 150.687 65.8614) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 120.1492 137.627) (end 121.8492 137.627) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 180.6032 137.627) (end 182.3032 137.627) (layer Edge.Cuts) (width 0.15))
  (gr_text http://4chord.craplab.fi/ (at 136.1 102.5) (layer F.SilkS))
  (gr_text "...because why not?" (at 164.25 104.75) (layer B.SilkS))
  (gr_text "CERN OHL v.1.2" (at 143.636 126.511) (layer B.Mask))
  (gr_text "Licensed under" (at 143.636 125.111) (layer B.Mask))
  (gr_text 08-2017 (at 136.25 107.25) (layer B.SilkS))
  (gr_text "Revision B" (at 147.75 107.25) (layer B.SilkS))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.38))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 115.6208 131.4196) (xy 115.697 131.4196) (xy 115.697 131.445) (xy 115.697 131.4704) (xy 115.697 134.62)
        (xy 115.7224 140.7922) (xy 115.7224 141.4272) (xy 115.7478 141.8844) (xy 115.7478 141.9352) (xy 115.7732 142.0622)
        (xy 115.7986 142.1384) (xy 116.0018 142.1638) (xy 116.84 142.1892) (xy 119.9388 142.2146) (xy 126.6952 142.2146)
        (xy 140.1826 142.24) (xy 152.4762 142.24) (xy 161.0614 142.24) (xy 171.2722 142.24) (xy 179.9082 142.24)
        (xy 183.1848 142.1892) (xy 184.6834 142.1638) (xy 184.912 142.1638) (xy 185.0898 142.1384) (xy 185.1152 142.113)
        (xy 185.1406 141.9606) (xy 185.166 141.5288) (xy 185.1914 139.7508) (xy 185.1914 135.2296) (xy 185.1914 131.4958)
        (xy 185.1914 131.4704) (xy 185.1914 131.445) (xy 185.2168 131.4196) (xy 185.293 131.4196) (xy 186.6392 131.4196)
        (xy 187.1218 131.4196) (xy 187.452 131.3942) (xy 187.6044 131.3688) (xy 187.6552 131.3434) (xy 187.6806 131.318)
        (xy 187.706 131.2672) (xy 187.7314 131.1402) (xy 187.7568 130.8354) (xy 187.7822 128.6764) (xy 187.7822 126.5174)
        (xy 187.7822 123.0376) (xy 187.7822 121.1834) (xy 187.7822 119.1006) (xy 187.7822 116.1288) (xy 187.7568 109.6518)
        (xy 187.7568 108.0262) (xy 187.7568 107.95) (xy 187.6044 107.4166) (xy 187.579 107.3404) (xy 187.0456 106.172)
        (xy 186.3852 104.7242) (xy 186.309 104.5464) (xy 186.2328 104.4448) (xy 184.7342 102.7938) (xy 183.8452 101.8286)
        (xy 180.6448 99.4664) (xy 180.2384 99.1616) (xy 180.086 99.06) (xy 175.6664 96.5708) (xy 175.3108 96.3676)
        (xy 174.3964 95.8596) (xy 170.6372 93.8022) (xy 168.4274 92.3798) (xy 168.0972 92.1766) (xy 166.4716 90.6526)
        (xy 164.973 88.646) (xy 164.0586 86.995) (xy 163.2712 85.1916) (xy 162.7632 83.82) (xy 162.2298 82.3722)
        (xy 161.6456 80.5942) (xy 160.0454 75.692) (xy 159.6644 74.5236) (xy 158.5722 71.755) (xy 157.3276 69.215)
        (xy 157.226 69.0626) (xy 155.9306 67.0306) (xy 154.3812 65.151) (xy 152.8064 63.7794) (xy 151.13 62.3062)
        (xy 147.32 60.0964) (xy 142.9766 58.547) (xy 138.4554 57.7596) (xy 138.2268 57.7342) (xy 137.287 57.6834)
        (xy 135.8138 57.6834) (xy 135.2296 57.6834) (xy 134.2136 57.7342) (xy 134.0358 57.7342) (xy 128.4986 58.7756)
        (xy 128.3462 58.8264) (xy 125.0188 60.2234) (xy 123.3932 60.9092) (xy 119.8626 63.3476) (xy 116.967 66.3194)
        (xy 115.5954 68.1482) (xy 114.4524 69.977) (xy 113.6142 71.9836) (xy 113.1824 74.2188) (xy 113.157 75.1586)
        (xy 113.157 77.1398) (xy 113.157 79.2226) (xy 113.1316 84.7344) (xy 113.1316 92.1766) (xy 113.1316 108.0262)
        (xy 113.1316 125.1712) (xy 113.1316 127.6604) (xy 113.1824 130.3782) (xy 113.1824 130.81) (xy 113.1824 131.2164)
        (xy 113.2332 131.3434) (xy 113.411 131.3688) (xy 113.665 131.4196) (xy 114.8334 131.4196)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.38))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 137.541 57.7088) (xy 138.2776 57.7342) (xy 138.43 57.7596) (xy 138.7094 57.8104) (xy 139.2936 57.912)
        (xy 140.462 58.0898) (xy 142.9004 58.5216) (xy 143.002 58.547) (xy 143.4338 58.6994) (xy 147.2692 60.071)
        (xy 147.3962 60.1472) (xy 149.3266 61.2648) (xy 151.1554 62.3316) (xy 152.2984 63.3222) (xy 154.3812 65.151)
        (xy 155.8798 66.9544) (xy 157.3022 69.1896) (xy 158.5468 71.6788) (xy 158.7754 72.2884) (xy 159.8422 75.0824)
        (xy 161.036 78.74) (xy 161.4424 80.01) (xy 161.7726 80.9752) (xy 162.306 82.6008) (xy 162.8648 84.1248)
        (xy 163.2458 85.1408) (xy 163.9316 86.6902) (xy 164.1094 87.0712) (xy 164.1348 87.122) (xy 164.592 87.9348)
        (xy 165.0238 88.6968) (xy 165.4556 89.281) (xy 166.4716 90.6526) (xy 166.5224 90.7034) (xy 167.1574 91.2876)
        (xy 168.0464 92.1258) (xy 168.1988 92.2274) (xy 168.6052 92.4814) (xy 169.9006 93.3196) (xy 170.6626 93.8022)
        (xy 171.6532 94.361) (xy 173.2026 95.1738) (xy 174.8536 96.0882) (xy 176.3014 96.9264) (xy 180.086 99.06)
        (xy 180.2892 99.2124) (xy 181.9402 100.4062) (xy 183.8452 101.8032) (xy 183.9214 101.8794) (xy 186.2074 104.4194)
        (xy 186.309 104.5464) (xy 186.4614 104.8766) (xy 186.944 105.9434) (xy 187.579 107.3404) (xy 187.6044 107.4166)
        (xy 187.7568 107.9754) (xy 187.7568 115.1636) (xy 187.7822 121.4628) (xy 187.7822 129.7432) (xy 187.7568 130.8354)
        (xy 187.7314 131.1148) (xy 187.706 131.2926) (xy 187.6552 131.3434) (xy 187.6044 131.3688) (xy 187.452 131.3942)
        (xy 187.071 131.4196) (xy 185.2168 131.4196) (xy 185.1914 131.4704) (xy 185.1914 140.4874) (xy 185.166 141.6558)
        (xy 185.1406 141.9606) (xy 185.1152 142.113) (xy 185.0898 142.1384) (xy 184.912 142.1638) (xy 184.2262 142.1892)
        (xy 177.927 142.2146) (xy 172.6946 142.24) (xy 157.7086 142.2146) (xy 145.7706 142.24) (xy 132.8674 142.24)
        (xy 124.9934 142.2146) (xy 119.9388 142.2146) (xy 117.348 142.1892) (xy 116.8654 142.1892) (xy 116.0018 142.1638)
        (xy 115.7986 142.1384) (xy 115.7732 142.0622) (xy 115.7478 141.9352) (xy 115.7478 141.8336) (xy 115.7224 141.3764)
        (xy 115.7224 141.0462) (xy 115.697 139.065) (xy 115.697 131.445) (xy 115.6716 131.4196) (xy 114.0714 131.4196)
        (xy 113.4364 131.3942) (xy 113.3348 131.3688) (xy 113.2078 131.3434) (xy 113.1824 131.2164) (xy 113.157 130.7846)
        (xy 113.1316 129.2606) (xy 113.1316 93.1164) (xy 113.157 80.8482) (xy 113.157 75.0316) (xy 113.2078 74.1934)
        (xy 113.6142 71.9836) (xy 113.9444 71.1708) (xy 114.4778 69.9262) (xy 115.1382 68.8848) (xy 115.57 68.199)
        (xy 115.697 68.0212) (xy 116.7892 66.5734) (xy 117.0686 66.1924) (xy 119.761 63.4746) (xy 119.888 63.3476)
        (xy 123.3932 60.9092) (xy 123.5202 60.8584) (xy 125.2474 60.1472) (xy 128.4986 58.7756) (xy 131.3942 58.2422)
        (xy 133.9088 57.7596) (xy 134.5184 57.7088) (xy 135.509 57.6834) (xy 136.9822 57.6834)
      )
    )
  )
  (zone (net 1) (net_name +3V3) (layer B.Cu) (hatch edge 0.508)
    (priority 2)
    (connect_pads (clearance 0.6))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 125.73 124.968) (xy 128.397 124.968) (xy 128.397 127) (xy 122.174 127) (xy 122.174 123.19)
        (xy 117.602 123.19) (xy 117.602 118.618) (xy 125.73 118.618) (xy 125.73 124.841)
      )
    )
  )
  (zone (net 39) (net_name +5V) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.6))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 122.174 127.254) (xy 128.397 127.254) (xy 128.397 129.286) (xy 125.73 129.286) (xy 125.73 133.223)
        (xy 117.602 133.223) (xy 117.602 128.778) (xy 122.174 128.778) (xy 122.174 127.381)
      )
    )
  )
)
