(kicad_pcb (version 20171130) (host pcbnew "(5.1.5-0-10_14)")
  (general
    (thickness 1.6)
    (drawings 50)
    (tracks 97)
    (zones 0)
    (modules 39)
    (nets 1)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module alexglow-footprints:pn2222a (layer B.Cu) (tedit 6221BA93)
    (at 161.75 48.5)
    (fp_text reference " " (at 0 1.5) (layer B.SilkS))
    (fp_text value PN2222A (at 0 -1.5) (layer B.Fab))
    (pad 1 thru_hole circle (at -3 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 3 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module alexglow-footprints:pn2222a (layer B.Cu) (tedit 6221BA93)
    (at 137.25 48.5)
    (fp_text reference " " (at 0 1.5) (layer B.SilkS))
    (fp_text value PN2222A (at 0 -1.5) (layer B.Fab))
    (pad 3 thru_hole circle (at 3 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -3 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module alexglow-footprints:pn2222a (layer B.Cu) (tedit 6221BA93)
    (at 128.5 88 90)
    (fp_text reference " " (at 0 1.5 90) (layer B.SilkS))
    (fp_text value PN2222A (at 0 -1.5 90) (layer B.Fab))
    (pad 1 thru_hole circle (at -3 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 0 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad 3 thru_hole circle (at 3 0 90) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module alexglow-footprints:pn2222a (layer B.Cu) (tedit 6221BA93)
    (at 173 93 180)
    (fp_text reference " " (at 0 1.5) (layer B.SilkS))
    (fp_text value PN2222A (at 0 -1.5) (layer B.Fab))
    (pad 3 thru_hole circle (at 3 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -3 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module alexglow-footprints:pn2222a (layer B.Cu) (tedit 6221BA93)
    (at 173 97.5 180)
    (fp_text reference " " (at 0 1.5) (layer B.SilkS))
    (fp_text value PN2222A (at 0 -1.5) (layer B.Fab))
    (pad 3 thru_hole circle (at 3 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad 2 thru_hole circle (at 0 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
    (pad 1 thru_hole circle (at -3 0 180) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  )
  (module Connectors:1X12_MACHINE-PIN-HEADER_LOCK.004 (layer F.Cu) (tedit 5963D9EF)
    (at 172.4 81.275 90)
    (descr "PLATED THROUGH HOLE -12 PIN MACHINE PIN HEADERS")
    (tags "PLATED THROUGH HOLE -12 PIN MACHINE PIN HEADERS")
    (attr virtual)
    (fp_text reference " " (at 0 -2.032 90) (layer F.SilkS))
    (fp_text value " " (at 0 2.032 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 2 thru_hole circle (at 2.54 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 3 thru_hole circle (at 5.08 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 4 thru_hole circle (at 7.62 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 5 thru_hole circle (at 10.16 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 6 thru_hole circle (at 12.7 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 7 thru_hole circle (at 15.24 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 8 thru_hole circle (at 17.78 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 9 thru_hole circle (at 20.32 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 10 thru_hole circle (at 22.86 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 11 thru_hole circle (at 25.4 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 12 thru_hole circle (at 27.94 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
  )
  (module alexglow-footprints:2-pin-power (layer F.Cu) (tedit 614915E7)
    (at 177.75 90 90)
    (descr "PLATED THROUGH HOLE -12 PIN MACHINE PIN HEADERS")
    (tags "PLATED THROUGH HOLE -12 PIN MACHINE PIN HEADERS")
    (attr virtual)
    (fp_text reference " " (at 0 -2.032 90) (layer F.SilkS))
    (fp_text value " " (at 0 2.032 90) (layer F.SilkS))
    (fp_text user - (at 2.54 1.524 90) (layer F.SilkS))
    (fp_text user + (at 0 1.524 90) (layer F.SilkS))
    (pad 1 thru_hole circle (at 0 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 2 thru_hole circle (at 2.54 -0.1 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
  )
  (module alexglow-footprints:hlogoTiny (layer F.Cu) (tedit 600E2129)
    (at 149.75 97.75)
    (fp_text reference " " (at 0 0) (layer F.SilkS) hide)
    (fp_text value " " (at 0.75 0) (layer F.SilkS) hide)
  )
  (module cbot-breadboard:herz-whole-mask-neg-520 (layer B.Cu) (tedit 0)
    (at 141.91 68.707 180)
    (fp_text reference G*** (at 0 0) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer B.SilkS) hide)
  )
  (module cbot-breadboard:coretext-520 (layer B.Cu) (tedit 0)
    (at 149.87036 94.5 180)
    (fp_text reference G*** (at 0 0) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer B.SilkS) hide)
  )
  (module cbot-breadboard:bow-smol-neg-385 (layer B.Cu) (tedit 0)
    (at 149.59096 71.5772 180)
    (fp_text reference G*** (at 0 0) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer B.SilkS) hide)
  )
  (module alexglow-footprints:round-pad (layer B.Cu) (tedit 61442FED)
    (at 148.26 55.88)
    (descr "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (tags "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (attr smd)
    (fp_text reference " " (at 0 1.27) (layer B.SilkS))
    (fp_text value " " (at 0 -1.27) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0) (size 1.27 1.27) (layers B.Cu B.Paste B.Mask)
      (solder_mask_margin 0.1016))
  )
  (module alexglow-footprints:round-pad (layer B.Cu) (tedit 61442FED)
    (at 148.26 78.74)
    (descr "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (tags "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (attr smd)
    (fp_text reference " " (at 0 1.27) (layer B.SilkS))
    (fp_text value " " (at 0 -1.27) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0) (size 1.27 1.27) (layers B.Cu B.Paste B.Mask)
      (solder_mask_margin 0.1016))
  )
  (module alexglow-footprints:round-pad (layer B.Cu) (tedit 61442FED)
    (at 150.8 58.42)
    (descr "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (tags "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (attr smd)
    (fp_text reference " " (at 0 1.27) (layer B.SilkS))
    (fp_text value " " (at 0 -1.27) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0) (size 1.27 1.27) (layers B.Cu B.Paste B.Mask)
      (solder_mask_margin 0.1016))
  )
  (module alexglow-footprints:round-pad (layer B.Cu) (tedit 61442FED)
    (at 150.8 81.28)
    (descr "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (tags "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (attr smd)
    (fp_text reference " " (at 0 1.27) (layer B.SilkS))
    (fp_text value " " (at 0 -1.27) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0) (size 1.27 1.27) (layers B.Cu B.Paste B.Mask)
      (solder_mask_margin 0.1016))
  )
  (module alexglow-footprints:round-pad (layer B.Cu) (tedit 61442FED)
    (at 148.26 81.28)
    (descr "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (tags "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (attr smd)
    (fp_text reference " " (at 0 1.27) (layer B.SilkS))
    (fp_text value " " (at 0 -1.27) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0) (size 1.27 1.27) (layers B.Cu B.Paste B.Mask)
      (solder_mask_margin 0.1016))
  )
  (module alexglow-footprints:round-pad (layer B.Cu) (tedit 61442FED)
    (at 148.26 58.42)
    (descr "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (tags "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (attr smd)
    (fp_text reference " " (at 0 1.27) (layer B.SilkS))
    (fp_text value " " (at 0 -1.27) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0) (size 1.27 1.27) (layers B.Cu B.Paste B.Mask)
      (solder_mask_margin 0.1016))
  )
  (module alexglow-footprints:round-pad (layer B.Cu) (tedit 61442FED)
    (at 150.8 60.96)
    (descr "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (tags "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (attr smd)
    (fp_text reference " " (at 0 1.27) (layer B.SilkS))
    (fp_text value " " (at 0 -1.27) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0) (size 1.27 1.27) (layers B.Cu B.Paste B.Mask)
      (solder_mask_margin 0.1016))
  )
  (module alexglow-footprints:round-pad (layer B.Cu) (tedit 61442FED)
    (at 148.26 60.96)
    (descr "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (tags "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (attr smd)
    (fp_text reference " " (at 0 1.27) (layer B.SilkS))
    (fp_text value " " (at 0 -1.27) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0) (size 1.27 1.27) (layers B.Cu B.Paste B.Mask)
      (solder_mask_margin 0.1016))
  )
  (module alexglow-footprints:round-pad (layer B.Cu) (tedit 61442FED)
    (at 150.8 63.5)
    (descr "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (tags "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (attr smd)
    (fp_text reference " " (at 0 1.27) (layer B.SilkS))
    (fp_text value " " (at 0 -1.27) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0) (size 1.27 1.27) (layers B.Cu B.Paste B.Mask)
      (solder_mask_margin 0.1016))
  )
  (module alexglow-footprints:round-pad (layer B.Cu) (tedit 61442FED)
    (at 148.26 63.5)
    (descr "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (tags "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (attr smd)
    (fp_text reference " " (at 0 1.27) (layer B.SilkS))
    (fp_text value " " (at 0 -1.27) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0) (size 1.27 1.27) (layers B.Cu B.Paste B.Mask)
      (solder_mask_margin 0.1016))
  )
  (module alexglow-footprints:round-pad (layer B.Cu) (tedit 61442FED)
    (at 150.8 66.04)
    (descr "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (tags "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (attr smd)
    (fp_text reference " " (at 0 1.27) (layer B.SilkS))
    (fp_text value " " (at 0 -1.27) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0) (size 1.27 1.27) (layers B.Cu B.Paste B.Mask)
      (solder_mask_margin 0.1016))
  )
  (module alexglow-footprints:round-pad (layer B.Cu) (tedit 61442FED)
    (at 148.26 66.04)
    (descr "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (tags "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (attr smd)
    (fp_text reference " " (at 0 1.27) (layer B.SilkS))
    (fp_text value " " (at 0 -1.27) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0) (size 1.27 1.27) (layers B.Cu B.Paste B.Mask)
      (solder_mask_margin 0.1016))
  )
  (module alexglow-footprints:round-pad (layer B.Cu) (tedit 61442FED)
    (at 150.8 68.58)
    (descr "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (tags "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (attr smd)
    (fp_text reference " " (at 0 1.27) (layer B.SilkS))
    (fp_text value " " (at 0 -1.27) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0) (size 1.27 1.27) (layers B.Cu B.Paste B.Mask)
      (solder_mask_margin 0.1016))
  )
  (module alexglow-footprints:round-pad (layer B.Cu) (tedit 61442FED)
    (at 148.26 68.58)
    (descr "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (tags "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (attr smd)
    (fp_text reference " " (at 0 1.27) (layer B.SilkS))
    (fp_text value " " (at 0 -1.27) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0) (size 1.27 1.27) (layers B.Cu B.Paste B.Mask)
      (solder_mask_margin 0.1016))
  )
  (module alexglow-footprints:round-pad (layer B.Cu) (tedit 61442FED)
    (at 150.8 71.12)
    (descr "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (tags "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (attr smd)
    (fp_text reference " " (at 0 1.27) (layer B.SilkS))
    (fp_text value " " (at 0 -1.27) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0) (size 1.27 1.27) (layers B.Cu B.Paste B.Mask)
      (solder_mask_margin 0.1016))
  )
  (module alexglow-footprints:round-pad (layer B.Cu) (tedit 61442FED)
    (at 148.26 71.12)
    (descr "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (tags "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (attr smd)
    (fp_text reference " " (at 0 1.27) (layer B.SilkS))
    (fp_text value " " (at 0 -1.27) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0) (size 1.27 1.27) (layers B.Cu B.Paste B.Mask)
      (solder_mask_margin 0.1016))
  )
  (module alexglow-footprints:round-pad (layer B.Cu) (tedit 61442FED)
    (at 150.8 73.66)
    (descr "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (tags "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (attr smd)
    (fp_text reference " " (at 0 1.27) (layer B.SilkS))
    (fp_text value " " (at 0 -1.27) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0) (size 1.27 1.27) (layers B.Cu B.Paste B.Mask)
      (solder_mask_margin 0.1016))
  )
  (module alexglow-footprints:round-pad (layer B.Cu) (tedit 61442FED)
    (at 148.26 73.66)
    (descr "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (tags "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (attr smd)
    (fp_text reference " " (at 0 1.27) (layer B.SilkS))
    (fp_text value " " (at 0 -1.27) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0) (size 1.27 1.27) (layers B.Cu B.Paste B.Mask)
      (solder_mask_margin 0.1016))
  )
  (module alexglow-footprints:round-pad (layer B.Cu) (tedit 61442FED)
    (at 150.8 76.2)
    (descr "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (tags "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (attr smd)
    (fp_text reference " " (at 0 1.27) (layer B.SilkS))
    (fp_text value " " (at 0 -1.27) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0) (size 1.27 1.27) (layers B.Cu B.Paste B.Mask)
      (solder_mask_margin 0.1016))
  )
  (module alexglow-footprints:round-pad (layer B.Cu) (tedit 61442FED)
    (at 148.26 76.2)
    (descr "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (tags "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (attr smd)
    (fp_text reference " " (at 0 1.27) (layer B.SilkS))
    (fp_text value " " (at 0 -1.27) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0) (size 1.27 1.27) (layers B.Cu B.Paste B.Mask)
      (solder_mask_margin 0.1016))
  )
  (module alexglow-footprints:round-pad (layer B.Cu) (tedit 61442FED)
    (at 150.8 78.74)
    (descr "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (tags "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (attr smd)
    (fp_text reference " " (at 0 1.27) (layer B.SilkS))
    (fp_text value " " (at 0 -1.27) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0) (size 1.27 1.27) (layers B.Cu B.Paste B.Mask)
      (solder_mask_margin 0.1016))
  )
  (module alexglow-footprints:round-pad (layer B.Cu) (tedit 61442FED)
    (at 150.8 53.34)
    (descr "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (tags "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (attr smd)
    (fp_text reference " " (at 0 1.27) (layer B.SilkS))
    (fp_text value " " (at 0 -1.27) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0) (size 1.27 1.27) (layers B.Cu B.Paste B.Mask)
      (solder_mask_margin 0.1016))
  )
  (module alexglow-footprints:round-pad (layer B.Cu) (tedit 61442FED)
    (at 150.8 55.88)
    (descr "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (tags "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (attr smd)
    (fp_text reference " " (at 0 1.27) (layer B.SilkS))
    (fp_text value " " (at 0 -1.27) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0) (size 1.27 1.27) (layers B.Cu B.Paste B.Mask)
      (solder_mask_margin 0.1016))
  )
  (module alexglow-footprints:round-pad (layer B.Cu) (tedit 61442FED)
    (at 148.26 53.34)
    (descr "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (tags "ELECTRICALLY CONDUCTIVE PAD 0.05\" CIRCLE")
    (attr smd)
    (fp_text reference " " (at 0 1.27) (layer B.SilkS))
    (fp_text value " " (at 0 -1.27) (layer B.SilkS))
    (pad P$1 smd circle (at 0 0) (size 1.27 1.27) (layers B.Cu B.Paste B.Mask)
      (solder_mask_margin 0.1016))
  )
  (module Connectors:1X12_MACHINE-PIN-HEADER_LOCK.004 (layer F.Cu) (tedit 5963D9EF)
    (at 129.21 81.28 90)
    (descr "PLATED THROUGH HOLE -12 PIN MACHINE PIN HEADERS")
    (tags "PLATED THROUGH HOLE -12 PIN MACHINE PIN HEADERS")
    (attr virtual)
    (fp_text reference " " (at 0 -2.032 90) (layer F.SilkS))
    (fp_text value " " (at 0 2.032 90) (layer F.SilkS))
    (pad 12 thru_hole circle (at 27.94 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 11 thru_hole circle (at 25.4 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 10 thru_hole circle (at 22.86 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 9 thru_hole circle (at 20.32 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 8 thru_hole circle (at 17.78 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 7 thru_hole circle (at 15.24 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 6 thru_hole circle (at 12.7 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 5 thru_hole circle (at 10.16 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 4 thru_hole circle (at 7.62 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 3 thru_hole circle (at 5.08 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 2 thru_hole circle (at 2.54 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at 0 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
  )
  (module Connectors:1X12_MACHINE-PIN-HEADER_LOCK.004 (layer F.Cu) (tedit 5963D9EF)
    (at 177.48 81.28 90)
    (descr "PLATED THROUGH HOLE -12 PIN MACHINE PIN HEADERS")
    (tags "PLATED THROUGH HOLE -12 PIN MACHINE PIN HEADERS")
    (attr virtual)
    (fp_text reference " " (at 0 -2.032 90) (layer F.SilkS))
    (fp_text value " " (at 0 2.032 90) (layer F.SilkS))
    (pad 12 thru_hole circle (at 27.94 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 11 thru_hole circle (at 25.4 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 10 thru_hole circle (at 22.86 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 9 thru_hole circle (at 20.32 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 8 thru_hole circle (at 17.78 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 7 thru_hole circle (at 15.24 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 6 thru_hole circle (at 12.7 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 5 thru_hole circle (at 10.16 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 4 thru_hole circle (at 7.62 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 3 thru_hole circle (at 5.08 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 2 thru_hole circle (at 2.54 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at 0 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
  )
  (module Connectors:1X12_MACHINE-PIN-HEADER_LOCK.004 (layer F.Cu) (tedit 5963D9EF)
    (at 174.94 81.28 90)
    (descr "PLATED THROUGH HOLE -12 PIN MACHINE PIN HEADERS")
    (tags "PLATED THROUGH HOLE -12 PIN MACHINE PIN HEADERS")
    (attr virtual)
    (fp_text reference " " (at 0 -2.032 90) (layer F.SilkS))
    (fp_text value " " (at 0 2.032 90) (layer F.SilkS))
    (pad 12 thru_hole circle (at 27.94 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 11 thru_hole circle (at 25.4 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 10 thru_hole circle (at 22.86 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 9 thru_hole circle (at 20.32 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 8 thru_hole circle (at 17.78 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 7 thru_hole circle (at 15.24 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 6 thru_hole circle (at 12.7 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 5 thru_hole circle (at 10.16 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 4 thru_hole circle (at 7.62 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 3 thru_hole circle (at 5.08 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 2 thru_hole circle (at 2.54 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at 0 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
  )
  (module Connectors:1X12_MACHINE-PIN-HEADER_LOCK.004 (layer F.Cu) (tedit 5963D9EF)
    (at 169.85 81.28 90)
    (descr "PLATED THROUGH HOLE -12 PIN MACHINE PIN HEADERS")
    (tags "PLATED THROUGH HOLE -12 PIN MACHINE PIN HEADERS")
    (attr virtual)
    (fp_text reference " " (at 0 -2.032 90) (layer F.SilkS))
    (fp_text value " " (at 0 2.032 90) (layer F.SilkS))
    (pad 12 thru_hole circle (at 27.94 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 11 thru_hole circle (at 25.4 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 10 thru_hole circle (at 22.86 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 9 thru_hole circle (at 20.32 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 8 thru_hole circle (at 17.78 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 7 thru_hole circle (at 15.24 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 6 thru_hole circle (at 12.7 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 5 thru_hole circle (at 10.16 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 4 thru_hole circle (at 7.62 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 3 thru_hole circle (at 5.08 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 2 thru_hole circle (at 2.54 0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
    (pad 1 thru_hole circle (at 0 -0.1016 90) (size 1.8796 1.8796) (drill 0.889) (layers *.Cu *.Mask)
      (solder_mask_margin 0.1016))
  )
  (gr_text M3 (at 128.75 98) (layer F.SilkS))
  (gr_text 03/2022 (at 138.75 94.75) (layer F.SilkS))
  (gr_text "<3, alex" (at 160.25 94.75) (layer F.SilkS))
  (gr_text "Companion Bot core: designed for use with\nTeensy and Arduino Nano 33 BLE Sense.\n\nStick a mini breadboard in this box,\naligned with the breakout header rows.\nSolder M/F headers on (as labeled).\n\n^ Install board with USB jack UP ^\nConnect the breadboard GPIO pins\nto breakout header rows with M/M wires.\n\nSolder a stripped USB-A cable for power.\nConnect “gnd” row to the controller’s GND.\n\n<—— Need to use one of these pins?    \nUse the pads on the back to connect\n    to an unused header over here. ——>\n\nUse transistors for switching motors,\nheaters, etc. Attach device to +/- pins.\n\nCheck the pins of your transistor!\nCheck the pins of your NeoPixels!\nHACK ON!" (at 149.5 72.5) (layer F.SilkS))
  (gr_text - (at 158.75 50 180) (layer F.SilkS))
  (gr_text + (at 164.75 50 180) (layer F.SilkS))
  (gr_text D (at 161.75 50) (layer F.SilkS))
  (gr_text + (at 140.25 50 180) (layer F.SilkS))
  (gr_text D (at 137.25 50) (layer F.SilkS))
  (gr_text - (at 134.25 50 180) (layer F.SilkS))
  (gr_text + (at 130 85 270) (layer F.SilkS))
  (gr_text D (at 130 88 270) (layer F.SilkS))
  (gr_text - (at 130 91 270) (layer F.SilkS))
  (gr_text M (at 177.5 51) (layer F.SilkS))
  (gr_text M (at 175 51) (layer F.SilkS))
  (gr_text M (at 172.5 51) (layer F.SilkS))
  (gr_text F (at 170 51) (layer F.SilkS))
  (gr_text F (at 129.25 51.25) (layer F.SilkS))
  (gr_text - (at 176 96) (layer F.SilkS))
  (gr_text - (at 176 91.5) (layer F.SilkS))
  (gr_text D (at 173 96) (layer F.SilkS))
  (gr_text D (at 173 91.5) (layer F.SilkS))
  (gr_text + (at 170 96) (layer F.SilkS))
  (gr_text + (at 170 91.5) (layer F.SilkS))
  (gr_line (start 178.5 102.75) (end 128.25 102.75) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 178.5 46.5) (end 128.2 46.5) (layer Edge.Cuts) (width 0.05))
  (gr_text "v3\nalex glow\n@glowascii" (at 149.55 86) (layer B.SilkS))
  (gr_line (start 178.5 102.75) (end 180.25 101) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 180.25 100.5) (end 180.25 101) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 180.25 48.25) (end 178.5 46.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 180.25 48.25) (end 180.25 100.5) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 128.2 46.5) (end 126.45 48.15) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 126.45 100.9) (end 128.25 102.75) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 126.45 100.4) (end 126.45 100.9) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 126.45 48.15) (end 126.45 100.4) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 128.7 100.4) (end 130.2 100.4) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 128.7 48.65) (end 130.2 48.65) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 178 100.5) (end 179.5 100.5) (layer Edge.Cuts) (width 0.05))
  (gr_circle (center 178 48.75) (end 179.5 48.75) (layer Edge.Cuts) (width 0.05))
  (gr_text "“MITTLER ZWISCHEN HIRN UND HANDEN MUSS DAS HERZ SEIN!”" (at 154 100.7) (layer B.SilkS))
  (gr_text gnd (at 177.353 84.282 90) (layer F.SilkS))
  (gr_text 5v (at 174.94 83.901 90) (layer F.SilkS))
  (gr_text USB (at 178.5 93 90) (layer F.SilkS))
  (gr_text gpio (at 169.85 82.885 90) (layer F.SilkS))
)
