(kicad_pcb (version 20171130) (host pcbnew "(5.1.5)-3")
  (general
    (thickness 1.6)
    (drawings 10)
    (tracks 40)
    (zones 0)
    (modules 4)
    (nets 9)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 1)
    (user_trace_width 1)
    (user_trace_width 1.5)
    (user_trace_width 2)
    (user_trace_width 2.5)
    (user_trace_width 3)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "Gerber/"))
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad1)")
  (net 2 "Net-(D1-Pad2)")
  (net 3 "Net-(J1-Pad1)")
  (net 4 "Net-(J1-Pad2)")
  (net 5 "Net-(J1-Pad3)")
  (net 6 "Net-(J2-PadTN)")
  (net 7 "Net-(J2-PadRN)")
  (net 8 "Net-(J2-PadR)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J2-PadR)")
    (add_net "Net-(J2-PadRN)")
    (add_net "Net-(J2-PadTN)")
  )
  (module Diode_THT:D_DO-41_SOD81_P10.16mm_Horizontal (layer F.Cu) (tedit 5AE50CD5)
    (at 128.5 95 270)
    (descr "Diode, DO-41_SOD81 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=5.2*2.7mm^2, , http://www.diodes.com/_files/packages/DO-41%20(Plastic).pdf")
    (tags "Diode DO-41_SOD81 series Axial Horizontal pin pitch 10.16mm  length 5.2mm diameter 2.7mm")
    (fp_text reference D1 (at 5.5 -0.75 90) (layer F.SilkS))
    (fp_text value 1N4001 (at 5.5 0.75 90) (layer F.SilkS))
    (fp_text user %R (at 5.5 -0.75 90) (layer F.Fab))
    (fp_text user K (at -2 0 90) (layer F.Fab))
    (fp_text user K (at -2 0 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 2.2 2.2) (drill 1.1) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-41_SOD81_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TerminalBlock:TerminalBlock_bornier-3_P5.08mm (layer F.Cu) (tedit 59FF03B9)
    (at 155 105 90)
    (descr "simple 3-pin terminal block, pitch 5.08mm, revamped version of bornier3")
    (tags "terminal block bornier3")
    (fp_text reference J1 (at 5.05 -2.75 90) (layer F.SilkS))
    (fp_text value Screw_Terminal_01x03 (at 5.08 5.08 90) (layer F.Fab))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad1)"))
    (pad 2 thru_hole circle (at 5.08 0 90) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad2)"))
    (pad 3 thru_hole circle (at 10.16 0 90) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad3)"))
    (model ${KISYS3DMOD}/TerminalBlock.3dshapes/TerminalBlock_bornier-3_P5.08mm.wrl
      (offset (xyz 5.079999923706055 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Relay_THT:Relay_SPDT_SANYOU_SRD_Series_Form_C (layer F.Cu) (tedit 58FA3148)
    (at 132 100)
    (descr "relay Sanyou SRD series Form C http://www.sanyourelay.ca/public/products/pdf/SRD.pdf")
    (tags "relay Sanyu SRD form C")
    (fp_text reference K1 (at 9 6) (layer F.SilkS))
    (fp_text value SANYOU_SRD_Form_C (at 8 -9.6) (layer F.Fab))
    (fp_text user 1 (at 0 -2.3) (layer F.Fab))
    (fp_text user %R (at 7.1 0.025) (layer F.Fab))
    (pad 2 thru_hole circle (at 1.95 6.05 90) (size 2.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (pad 3 thru_hole circle (at 14.15 6.05 90) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 3 "Net-(J1-Pad1)"))
    (pad 4 thru_hole circle (at 14.2 -6 90) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 5 "Net-(J1-Pad3)"))
    (pad 5 thru_hole circle (at 1.95 -5.95 90) (size 2.5 2.5) (drill 1) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 3 3) (drill 1.3) (layers *.Cu *.Mask)
      (net 4 "Net-(J1-Pad2)"))
    (model ${KISYS3DMOD}/Relay_THT.3dshapes/Relay_SPDT_SANYOU_SRD_Series_Form_C.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_Audio:Jack_3.5mm_Ledino_KB3SPRS_Horizontal (layer F.Cu) (tedit 5BC12D58)
    (at 117.65 104.6)
    (descr https://www.reichelt.de/index.html?ACTION=7&LA=3&OPEN=0&INDEX=0&FILENAME=C160%252FKB3SPRS.pdf)
    (tags "jack stereo TRS")
    (fp_text reference J2 (at -0.4 -4.35 90) (layer F.SilkS))
    (fp_text value "3.5mm KB3SPRS" (at 1.1 -11.85) (layer F.SilkS))
    (fp_text user %R (at 2.7 -4.6) (layer F.Fab))
    (pad T thru_hole rect (at 0 0) (size 4 2.2) (drill 1.3) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (pad TN thru_hole oval (at 7.3 -0.5 90) (size 4 2.2) (drill 1.3) (layers *.Cu *.Mask)
      (net 6 "Net-(J2-PadTN)"))
    (pad RN thru_hole oval (at 2.9 -7.1) (size 4 2.2) (drill 1.3) (layers *.Cu *.Mask)
      (net 7 "Net-(J2-PadRN)"))
    (pad R thru_hole oval (at 4.1 -9.8) (size 4 2.2) (drill 1.3) (layers *.Cu *.Mask)
      (net 8 "Net-(J2-PadR)"))
    (pad S thru_hole oval (at -3.9 -4.6) (size 2.2 4) (drill 1.3) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_Audio.3dshapes/Jack_3.5mm_Ledino_KB3SPRS_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "NO=Normally Open" (at 145.25 103.25) (layer B.SilkS))
  (gr_text "NC=Normally Closed" (at 144.5 96.75) (layer B.SilkS))
  (gr_text NO (at 157.75 104.75 90) (layer B.SilkS))
  (gr_text NC (at 157.75 94.5 90) (layer B.SilkS))
  (gr_text COM (at 157.75 100 90) (layer B.SilkS))
  (gr_text "12v AVR Trigger" (at 133.75 100) (layer B.SilkS))
  (gr_line (start 112 108.25) (end 112 91.75) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 158.75 108.25) (end 112 108.25) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 158.75 91.75) (end 158.75 108.25) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 112 91.75) (end 158.75 91.75) (layer Edge.Cuts) (width 0.05))
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 159.5 109.5) (xy 109.5 109.5) (xy 109.5 90.5) (xy 159.5 90.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 160 110) (xy 109 110) (xy 109 90) (xy 160 90)
      )
    )
  )
)
