(kicad_pcb (version 20171130) (host pcbnew "(5.1.10)-1")
  (general
    (thickness 1.5748)
    (drawings 6)
    (tracks 0)
    (zones 0)
    (modules 1)
    (nets 5)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.127)
    (user_trace_width 0.1524)
    (user_trace_width 0.2032)
    (user_trace_width 0.254)
    (user_trace_width 0.3048)
    (user_trace_width 0.381)
    (user_trace_width 0.508)
    (user_trace_width 0.635)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.127)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.508)
    (via_min_drill 0.3048)
    (user_via 0.6858 0.3302)
    (user_via 0.8128 0.4064)
    (user_via 1.2192 0.6096)
    (user_via 1.4224 0.8128)
    (blind_buried_vias_allowed yes)
    (uvia_size 0.3)
    (uvia_drill 0.1016)
    (uvias_allowed yes)
    (uvia_min_size 0.2032)
    (uvia_min_drill 0.1016)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 3.8 3.8)
    (pad_drill 2.2)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7EFFF77F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(J1-Pad7)")
  (net 3 /signal)
  (net 4 /bias)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1016)
    (add_net /bias)
    (add_net /signal)
    (add_net GND)
    (add_net "Net-(J1-Pad7)")
  )
  (module MSAG_Misc:Omnetics_A115061-001 (layer F.Cu) (tedit 61A933C1)
    (at -101.6 0 90)
    (descr "Through hole righ angle nano strip conn, 1x10, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x10 1.27mm single row")
    (fp_text reference JSSD1 (at 7.2644 7.4168) (layer F.SilkS))
    (fp_text value "Omnetics A115061-001" (at 0.381 2.032 90) (layer F.Fab))
    (fp_text user %R (at -0.595 0.02 90) (layer F.Fab))
    (pad 10 thru_hole oval (at -5.675 4.1275) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 9 thru_hole oval (at -4.445 6.6675) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 8 thru_hole oval (at -3.135 4.1275) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 7 thru_hole oval (at -1.905 6.6675) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 2 "Net-(J1-Pad7)"))
    (pad 6 thru_hole oval (at -0.595 4.1275) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 5 thru_hole oval (at 0.675 6.6675) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole oval (at 1.945 4.1275) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 3 /signal))
    (pad 3 thru_hole oval (at 3.215 6.6675) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 2 thru_hole oval (at 4.485 4.1275) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 4 /bias))
    (pad 1 thru_hole rect (at 5.755 6.6675) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 1 GND))
    (model "${MSAG}/MSAG_KiCad3d/Omnetics A115061-001 REV 2.STEP"
      (offset (xyz 0 0 0.8890000000000001))
      (scale (xyz 1 1 1))
      (rotate (xyz 90 180 0))
    )
  )
  (gr_line (start -91.2368 -6.7564) (end -91.2368 6.7564) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start -92.5068 6.7564) (end -91.2368 6.7564) (angle 90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start -103.124 8.0264) (end -92.5068 8.0264) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start -92.5068 -6.7564) (end -91.2368 -6.7564) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start -103.124 -8.0264) (end -92.5068 -8.0264) (layer Edge.Cuts) (width 0.05))
  (gr_line (start -103.124 -8.0264) (end -103.124 8.0264) (layer Edge.Cuts) (width 0.05))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -91.2368 8.0264) (xy -103.124 8.0264) (xy -103.0732 -8.0264) (xy -91.2368 -8.0264)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -91.2368 8.0264) (xy -103.124 8.0264) (xy -103.0732 -8.0264) (xy -91.2368 -8.0264)
      )
    )
  )
)
