<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.1.3">
<drawing>
<board>
<plain>
<text>ALICAD Sensor Board V2.0</text>
<text>ALICAD 
Sensor 
Board 
V2.0</text>
<wire x1="100" y1="5" x2="100" y2="55" width="0.1524" layer="20"/>
<wire x1="100" y1="55" x2="95" y2="60" width="0.1524" layer="20" curve="90"/>
<wire x1="95" y1="60" x2="5" y2="60" width="0.1524" layer="20"/>
<wire x1="5" y1="60" x2="0" y2="55" width="0.1524" layer="20" curve="90"/>
<wire x1="0" y1="55" x2="0" y2="5" width="0.1524" layer="20"/>
<wire x1="0" y1="5" x2="5" y2="0" width="0.1524" layer="20" curve="90"/>
<wire x1="5" y1="0" x2="95" y2="0" width="0.1524" layer="20"/>
<wire x1="95" y1="0" x2="100" y2="5" width="0.1524" layer="20" curve="90"/>
<text>GND</text>
<text>3.3V</text>
<text>SDA</text>
<text>SCL</text>
<text>Node
Name</text>
<text>+5V</text>
<text>GND</text>
<text>5VDC</text>
<text>LORA UID</text>
<text>GPIO26</text>
<text>GPIO19</text>
<text>GPIO13</text>
<text>GPIO06</text>
<text>GPIO05</text>
</plain>
<libraries>
<library name="Alicad">
<packages>
<package name="GPS-RECEIVER-NEO6M-GENERIC">
<description>&lt;b&gt;GPS Receiver Module&lt;/b&gt; based on &lt;b&gt;NEO-6&lt;/b&gt; device</description>
</package>
<package name="DISPLAY-OLED-128X64-I2C">
<description>&lt;b&gt;128x64 Dot Matrix OLED Module&lt;/b&gt;&lt;br /&gt;
Variant with I2C interface</description>
</package>
<package name="RFM95W">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="DCJACK_2MM_PTH">
<description>DJ Jack 2.0mm PTH Right-Angle</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
<package name="0207/10">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0207, grid 10 mm</description>
</package>
<package name="DO41-10">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 2.54 mm, horizontal, grid 10.16 mm</description>
</package>
</packages>
</library>
<library name="Seeed-Connector">
<packages>
<package name="H4-2.54">
</package>
</packages>
</library>
<library name="raspberrypi_bastelstube_v13">
<description>&lt;b&gt;Raspberry Pi&lt;/b&gt; by &lt;b&gt;Martin's Bastelstube&lt;/b&gt;
&lt;p&gt;
Different shapes of piggyback boards for the famous &amp;amp; fabulous
&lt;a href="http://www.raspberrypi.org/"&gt;Raspberry Pi&lt;/a&gt; computer.
&lt;p&gt;
The outline of the Raspberry Pi board is drawn on layer 52 bDocu, so you can make it invisible if necessary.&lt;br/&gt;
Recommendation: Start your design with RASPI_BOARD_*_FULL, so you are aware of all the big components and
connectors when you're drawing the dimensions of your board and placing your own components.&lt;br/&gt;
Later, you can simply change the package of your Raspberry Pi connector to the RASPI_BOARD_*_EDGES type,
so you can concentrate on your own design.
&lt;p&gt;
Most of my board packages don't have the outline drawn in layer 20 Dimension (except the HATs). This allows you to deviate from the original Raspberry Pi board shape, e.g. when you need more space behind the GPIO connector for the routing of the power supply lines. If you want to stick exactly to the Raspberry Pi board shape, then just draw the Dimension layer right on the lines in layer bDocu.

&lt;hr&gt;&lt;br/&gt;

Version 1.3
&lt;ul&gt;
&lt;li&gt;Added the shape and dimensions of the HAT board with &amp;amp; without the camera and display flex cutout&lt;/li&gt;
&lt;li&gt;New GPIO connector version (suffix &amp;quot;#&amp;quot;) with all pins connected (no more &amp;quot;n.c.&amp;quot; pins)&lt;/li&gt;
&lt;li&gt;Two more &amp;quot;AB-&amp;quot; boards with 5 and 6 drill holes / pads, mechanically compatible with all RasPi versions&lt;/li&gt;
&lt;/ul&gt;

Version 1.2
&lt;ul&gt;
&lt;li&gt;Added a 26-pin GPIO connector with board dimensions of model B+&lt;br/&gt;
       for backwards compatibility with models A and B, named &amp;quot;B-&amp;quot;&lt;/li&gt;
&lt;/ul&gt;

Version 1.1
&lt;ul&gt;
&lt;li&gt;New GPIO connector and board dimensions of model B+&lt;/li&gt;
&lt;li&gt;Old connector and board (for models A and B) renamed to AB&lt;/li&gt;
&lt;li&gt;GPIO pin numbers on connector changed to match Rev2 board design&lt;/li&gt;
&lt;/ul&gt;

Version 1.0
&lt;ul&gt;
&lt;li&gt;More detailed descriptions for all components&lt;/li&gt;
&lt;li&gt;Published on Cadsoft webpage&lt;/li&gt;
&lt;/ul&gt;

&lt;hr&gt;&lt;br/&gt;

Designed by &lt;a href="http://bastelstube.rocci.net/"&gt;Martin's Bastelstube&lt;/a&gt;&lt;br&gt;
Comments / complaints / bug reports / suggestions to &lt;author&gt;eightbit@web.de&lt;/author&gt;</description>
<packages>
<package name="RASPI_BOARD_B+_EDGES_3DRILL_PAD">
<description>Raspberry Pi board model B+, outline is only marked by its edges&lt;br&gt;
with 3 mounting pads (top left pad is missing to allow routing of power supply lines)</description>
</package>
</packages>
</library>
<library name="SparkFun-Switches">
<description>&lt;h3&gt;SparkFun Switches, Buttons, Encoders&lt;/h3&gt;
In this library you'll find switches, buttons, joysticks, and anything that moves to create or disrupt an electrical connection.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE_SWITCH_PTH_6.0MM">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - PTH, 6.0mm Square&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.omron.com/ecb/products/pdf/en-b3f.pdf"&gt;Datasheet&lt;/a&gt; (B3F-1000)&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X05">
<description>&lt;h3&gt;Plated Through Hole - 5 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:5&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_05&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="GPS1" library="Alicad" package="GPS-RECEIVER-NEO6M-GENERIC" value="GPS">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="Alicad" package="DISPLAY-OLED-128X64-I2C" value="DISPLAY">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$2" library="Alicad" package="RFM95W" value="RFM95W"/>
<element name="CN1" library="adafruit" package="DCJACK_2MM_PTH" value=""/>
<element name="GPSLOCK" library="adafruit" package="LED3MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="adafruit" package="0207/10" value="220R"/>
<element name="I2C" library="Seeed-Connector" package="H4-2.54" value="">
<attribute name="MPN" value="P125-1104A0BS116A1"/>
</element>
<element name="X1" library="raspberrypi_bastelstube_v13" package="RASPI_BOARD_B+_EDGES_3DRILL_PAD" value="RASPI_BOARD_B+#_E3P"/>
<element name="S1" library="SparkFun-Switches" package="TACTILE_SWITCH_PTH_6.0MM" value="">
<attribute name="PROD_ID" value=" SWCH-08441"/>
<attribute name="SF_SKU" value="COM-00097"/>
</element>
<element name="S2" library="SparkFun-Switches" package="TACTILE_SWITCH_PTH_6.0MM" value="">
<attribute name="PROD_ID" value=" SWCH-08441"/>
<attribute name="SF_SKU" value="COM-00097"/>
</element>
<element name="S3" library="SparkFun-Switches" package="TACTILE_SWITCH_PTH_6.0MM" value="">
<attribute name="PROD_ID" value=" SWCH-08441"/>
<attribute name="SF_SKU" value="COM-00097"/>
</element>
<element name="D2" library="adafruit" package="DO41-10" value="1N4004"/>
<element name="G" library="SparkFun-Connectors" package="1X05" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="V" library="SparkFun-Connectors" package="1X05" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S" library="SparkFun-Connectors" package="1X05" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="D1" pad="1"/>
<contactref element="GPS1" pad="2"/>
<contactref element="U$2" pad="2"/>
<contactref element="CN1" pad="GND"/>
<contactref element="R1" pad="1"/>
<contactref element="X1" pad="6"/>
<contactref element="X1" pad="9"/>
<contactref element="X1" pad="14"/>
<contactref element="X1" pad="20"/>
<contactref element="X1" pad="25"/>
<contactref element="X1" pad="30"/>
<contactref element="X1" pad="34"/>
<contactref element="X1" pad="39"/>
<contactref element="I2C" pad="1"/>
<contactref element="S1" pad="1"/>
<contactref element="S2" pad="1"/>
<contactref element="S3" pad="1"/>
<contactref element="D2" pad="A"/>
<contactref element="G" pad="5"/>
<contactref element="G" pad="4"/>
<contactref element="G" pad="3"/>
<contactref element="G" pad="2"/>
<contactref element="G" pad="1"/>
</signal>
<signal name="RXD">
<contactref element="GPS1" pad="3"/>
<contactref element="X1" pad="8"/>
</signal>
<signal name="3.3V">
<contactref element="GPS1" pad="1"/>
<contactref element="D1" pad="2"/>
<contactref element="U$2" pad="1"/>
<contactref element="X1" pad="1"/>
<contactref element="X1" pad="17"/>
<contactref element="I2C" pad="2"/>
<contactref element="V" pad="5"/>
<contactref element="V" pad="4"/>
<contactref element="V" pad="3"/>
<contactref element="V" pad="2"/>
<contactref element="V" pad="1"/>
</signal>
<signal name="SDA">
<contactref element="D1" pad="4"/>
<contactref element="I2C" pad="3"/>
<contactref element="X1" pad="3"/>
</signal>
<signal name="SCL">
<contactref element="D1" pad="3"/>
<contactref element="I2C" pad="4"/>
<contactref element="X1" pad="5"/>
</signal>
<signal name="MOSI">
<contactref element="U$2" pad="7"/>
<contactref element="X1" pad="19"/>
</signal>
<signal name="MISO">
<contactref element="U$2" pad="6"/>
<contactref element="X1" pad="21"/>
</signal>
<signal name="SCLK">
<contactref element="U$2" pad="5"/>
<contactref element="X1" pad="23"/>
</signal>
<signal name="CE1">
<contactref element="U$2" pad="8"/>
<contactref element="X1" pad="26"/>
</signal>
<signal name="5V">
<contactref element="CN1" pad="PWR"/>
<contactref element="X1" pad="4"/>
<contactref element="X1" pad="2"/>
<contactref element="D2" pad="C"/>
</signal>
<signal name="TXD">
<contactref element="GPS1" pad="4"/>
<contactref element="X1" pad="10"/>
</signal>
<signal name="RFMIRQ">
<contactref element="U$2" pad="4"/>
<contactref element="X1" pad="15"/>
</signal>
<signal name="RFMRST">
<contactref element="U$2" pad="9"/>
<contactref element="X1" pad="22"/>
</signal>
<signal name="GNDBREAK">
<contactref element="CN1" pad="GNDBREAK"/>
</signal>
<signal name="N$1">
<contactref element="R1" pad="2"/>
<contactref element="GPSLOCK" pad="K"/>
</signal>
<signal name="GPIO18">
<contactref element="S1" pad="3"/>
<contactref element="X1" pad="12"/>
</signal>
<signal name="GPIO23">
<contactref element="S2" pad="3"/>
<contactref element="X1" pad="16"/>
</signal>
<signal name="GPIO24">
<contactref element="S3" pad="3"/>
<contactref element="X1" pad="18"/>
</signal>
<signal name="GPIO17">
<contactref element="X1" pad="11"/>
<contactref element="GPSLOCK" pad="A"/>
</signal>
<signal name="GPIO13">
<contactref element="X1" pad="33"/>
<contactref element="S" pad="3"/>
</signal>
<signal name="GPIO19">
<contactref element="X1" pad="35"/>
<contactref element="S" pad="2"/>
</signal>
<signal name="GPIO26">
<contactref element="X1" pad="37"/>
<contactref element="S" pad="1"/>
</signal>
<signal name="GPIO05">
<contactref element="S" pad="5"/>
<contactref element="X1" pad="29"/>
</signal>
<signal name="GPIO06">
<contactref element="S" pad="4"/>
<contactref element="X1" pad="31"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
