(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "/RED")
	(net 2 "/V+")
	(net 3 "/GRN")
	(net 4 "/BLU")
	(footprint "Alpenglow:TestPoint_Pad_1.5x1.5mm"
		(layer "F.Cu")
		(at 139.573 114.3)
		(descr "SMD rectangular pad as test Point, square 1.5mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "H4"
			(at -0.2 -2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "V+"
			(at 0 1.75 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Alpenglow:TestPoint_Pad_1.5x1.5mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC Part #" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "Root")
		(sheetfile "SideLEDTest.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom dnp)
		(fp_text user "${REFERENCE}"
			(at 0.4 -2 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0 0)
			(size 1.5 1.5)
			(layers "F.Cu" "F.Mask")
			(net 2 "/V+")
			(pinfunction "1")
			(pintype "input")
		)
	)
	(footprint "Alpenglow:LED_1204_4321"
		(layer "F.Cu")
		(at 140.8415 108.815)
		(property "Reference" "D1"
			(at 0 3 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LED_GBAR"
			(at 0.4 4.8 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "Alpenglow:LED_1204_4321"
			(at -0.1 0.2 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at -0.1 0.2 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "RGB LED, green/blue/anode/red"
			(at -0.1 0.2 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "Root")
		(sheetfile "SideLEDTest.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at 1.7 0.2 180)
			(size 0.8 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "/GRN")
			(pinfunction "GK")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "2" smd rect
			(at 0.55 0.2 180)
			(size 0.5 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "/BLU")
			(pinfunction "BK")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "3" smd rect
			(at -0.6 0.2 180)
			(size 0.6 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "/V+")
			(pinfunction "A")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "4" smd rect
			(at -1.9 0.2 180)
			(size 0.8 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "/RED")
			(pinfunction "RK")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
	)
	(footprint "Alpenglow:TestPoint_Pad_1.5x1.5mm"
		(layer "F.Cu")
		(at 139.065 111.125)
		(descr "SMD rectangular pad as test Point, square 1.5mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "H1"
			(at -0.2 -2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "RED"
			(at 0 1.75 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Alpenglow:TestPoint_Pad_1.5x1.5mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC Part #" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "Root")
		(sheetfile "SideLEDTest.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom dnp)
		(fp_text user "${REFERENCE}"
			(at 0.4 -2 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0 0)
			(size 1.5 1.5)
			(layers "F.Cu" "F.Mask")
			(net 1 "/RED")
			(pinfunction "1")
			(pintype "input")
		)
	)
	(footprint "Alpenglow:TestPoint_Pad_1.5x1.5mm"
		(layer "F.Cu")
		(at 141.605 111.125)
		(descr "SMD rectangular pad as test Point, square 1.5mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "H3"
			(at -0.2 -2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "BLU"
			(at 0 1.75 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Alpenglow:TestPoint_Pad_1.5x1.5mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC Part #" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "Root")
		(sheetfile "SideLEDTest.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom dnp)
		(fp_text user "${REFERENCE}"
			(at 0.4 -2 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0 0)
			(size 1.5 1.5)
			(layers "F.Cu" "F.Mask")
			(net 4 "/BLU")
			(pinfunction "1")
			(pintype "input")
		)
	)
	(footprint "Alpenglow:TestPoint_Pad_1.5x1.5mm"
		(layer "F.Cu")
		(at 141.986 114.3)
		(descr "SMD rectangular pad as test Point, square 1.5mm side length")
		(tags "test point SMD pad rectangle square")
		(property "Reference" "H2"
			(at -0.2 -2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "GRN"
			(at 0 1.75 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Alpenglow:TestPoint_Pad_1.5x1.5mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC Part #" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "Root")
		(sheetfile "SideLEDTest.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom dnp)
		(fp_text user "${REFERENCE}"
			(at 0.4 -2 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 0 0)
			(size 1.5 1.5)
			(layers "F.Cu" "F.Mask")
			(net 3 "/GRN")
			(pinfunction "1")
			(pintype "input")
		)
	)
	(gr_line
		(start 143.891 107.823)
		(end 137.541 107.823)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.891 115.189)
		(end 143.891 107.823)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 137.541 107.823)
		(end 137.541 115.189)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 137.541 115.189)
		(end 143.891 115.189)
		(layer "Edge.Cuts")
	)
	(gr_text "A"
		(at 139.573 113.538 0)
		(layer "F.SilkS")
	)
	(gr_text "G"
		(at 141.986 113.538 0)
		(layer "F.SilkS")
	)
	(gr_text "B"
		(at 140.462 113.157 0)
		(layer "F.SilkS")
	)
	(gr_text "R"
		(at 138.049 113.157 0)
		(layer "F.SilkS")
	)
)
