(kicad_pcb (version 20171130) (host pcbnew "(5.0.1-3-g963ef8bb5)")
  (general
    (thickness 1.6)
    (drawings 63)
    (tracks 1284)
    (zones 0)
    (modules 92)
    (nets 109)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.2032)
    (trace_clearance 0.1524)
    (zone_clearance 0.3)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.762)
    (via_drill 0.381)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1 6)
    (pad_drill 0)
    (pad_to_mask_clearance 0.0508)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (grid_origin 113.445 94.488)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber/"))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 /D0)
  (net 3 /D1)
  (net 4 /D2)
  (net 5 GND)
  (net 6 /D3)
  (net 7 /D4)
  (net 8 /D5)
  (net 9 /D6)
  (net 10 /D7)
  (net 11 "Net-(U2-Pad60)")
  (net 12 "Net-(U2-Pad55)")
  (net 13 "Net-(U2-Pad51)")
  (net 14 "Net-(U2-Pad31)")
  (net 15 "Net-(U2-Pad30)")
  (net 16 "Net-(U2-Pad29)")
  (net 17 "Net-(U2-Pad4)")
  (net 18 "Net-(U2-Pad3)")
  (net 19 "Net-(U2-Pad2)")
  (net 20 "Net-(U2-Pad1)")
  (net 21 "Net-(U3-Pad9)")
  (net 22 "Net-(U3-Pad7)")
  (net 23 "Net-(U3-Pad5)")
  (net 24 "Net-(U3-Pad3)")
  (net 25 +3V3)
  (net 26 /SWDIO)
  (net 27 /SWCLK)
  (net 28 /CLK)
  (net 29 /WR)
  (net 30 /RD)
  (net 31 /CS)
  (net 32 /A0)
  (net 33 /A1)
  (net 34 /A2)
  (net 35 /A3)
  (net 36 /A4)
  (net 37 /A5)
  (net 38 /A6)
  (net 39 /A7)
  (net 40 /A8)
  (net 41 /A9)
  (net 42 /A10)
  (net 43 /A11)
  (net 44 /A12)
  (net 45 /A13)
  (net 46 /A14)
  (net 47 /A15)
  (net 48 /RESET)
  (net 49 /DATA_OE)
  (net 50 /DIR)
  (net 51 "Net-(J1-Pad1)")
  (net 52 "Net-(J2-Pad1)")
  (net 53 /3V_D0)
  (net 54 /3V_D1)
  (net 55 /3V_D2)
  (net 56 /3V_D3)
  (net 57 /3V_D4)
  (net 58 /3V_D5)
  (net 59 /3V_D6)
  (net 60 /3V_D7)
  (net 61 "Net-(U7-Pad4)")
  (net 62 /GB_RESET)
  (net 63 /SAMD_RESET)
  (net 64 "Net-(J3-Pad9)")
  (net 65 "Net-(J3-Pad8)")
  (net 66 "Net-(J3-Pad7)")
  (net 67 VBUS)
  (net 68 "Net-(J4-Pad4)")
  (net 69 /3V_A12)
  (net 70 /3V_A13)
  (net 71 /3V_A14)
  (net 72 /3V_A15)
  (net 73 /3V_A11)
  (net 74 /3V_A10)
  (net 75 /3V_A9)
  (net 76 /3V_A8)
  (net 77 /3V_A7)
  (net 78 /3V_A6)
  (net 79 /3V_A5)
  (net 80 /3V_A4)
  (net 81 /3V_CLK)
  (net 82 /3V_WR)
  (net 83 /3V_RD)
  (net 84 /3V_CS)
  (net 85 /3V_A0)
  (net 86 /3V_A1)
  (net 87 /3V_A2)
  (net 88 /3V_A3)
  (net 89 /USB_D-)
  (net 90 /USB_D+)
  (net 91 "Net-(D3-Pad1)")
  (net 92 /LED)
  (net 93 +BATT)
  (net 94 "Net-(TP31-Pad1)")
  (net 95 /SWO)
  (net 96 "Net-(C14-Pad2)")
  (net 97 "Net-(TP44-Pad1)")
  (net 98 /MIDI_IN)
  (net 99 "Net-(J6-PadR)")
  (net 100 /MIDI_OUT)
  (net 101 "Net-(J6-PadT)")
  (net 102 "Net-(J5-PadT)")
  (net 103 "Net-(D4-Pad1)")
  (net 104 "Net-(U8-Pad1)")
  (net 105 "Net-(D4-Pad2)")
  (net 106 "Net-(U8-Pad7)")
  (net 107 "Net-(U8-Pad4)")
  (net 108 /SHIELD)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.2032)
    (via_dia 0.762)
    (via_drill 0.381)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net +5V)
    (add_net +BATT)
    (add_net /3V_A0)
    (add_net /3V_A1)
    (add_net /3V_A10)
    (add_net /3V_A11)
    (add_net /3V_A12)
    (add_net /3V_A13)
    (add_net /3V_A14)
    (add_net /3V_A15)
    (add_net /3V_A2)
    (add_net /3V_A3)
    (add_net /3V_A4)
    (add_net /3V_A5)
    (add_net /3V_A6)
    (add_net /3V_A7)
    (add_net /3V_A8)
    (add_net /3V_A9)
    (add_net /3V_CLK)
    (add_net /3V_CS)
    (add_net /3V_D0)
    (add_net /3V_D1)
    (add_net /3V_D2)
    (add_net /3V_D3)
    (add_net /3V_D4)
    (add_net /3V_D5)
    (add_net /3V_D6)
    (add_net /3V_D7)
    (add_net /3V_RD)
    (add_net /3V_WR)
    (add_net /A0)
    (add_net /A1)
    (add_net /A10)
    (add_net /A11)
    (add_net /A12)
    (add_net /A13)
    (add_net /A14)
    (add_net /A15)
    (add_net /A2)
    (add_net /A3)
    (add_net /A4)
    (add_net /A5)
    (add_net /A6)
    (add_net /A7)
    (add_net /A8)
    (add_net /A9)
    (add_net /CLK)
    (add_net /CS)
    (add_net /D0)
    (add_net /D1)
    (add_net /D2)
    (add_net /D3)
    (add_net /D4)
    (add_net /D5)
    (add_net /D6)
    (add_net /D7)
    (add_net /DATA_OE)
    (add_net /DIR)
    (add_net /GB_RESET)
    (add_net /LED)
    (add_net /MIDI_IN)
    (add_net /MIDI_OUT)
    (add_net /RD)
    (add_net /RESET)
    (add_net /SAMD_RESET)
    (add_net /SHIELD)
    (add_net /SWCLK)
    (add_net /SWDIO)
    (add_net /SWO)
    (add_net /USB_D+)
    (add_net /USB_D-)
    (add_net /WR)
    (add_net GND)
    (add_net "Net-(C14-Pad2)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J3-Pad7)")
    (add_net "Net-(J3-Pad8)")
    (add_net "Net-(J3-Pad9)")
    (add_net "Net-(J4-Pad4)")
    (add_net "Net-(J5-PadT)")
    (add_net "Net-(J6-PadR)")
    (add_net "Net-(J6-PadT)")
    (add_net "Net-(TP31-Pad1)")
    (add_net "Net-(TP44-Pad1)")
    (add_net "Net-(U2-Pad1)")
    (add_net "Net-(U2-Pad2)")
    (add_net "Net-(U2-Pad29)")
    (add_net "Net-(U2-Pad3)")
    (add_net "Net-(U2-Pad30)")
    (add_net "Net-(U2-Pad31)")
    (add_net "Net-(U2-Pad4)")
    (add_net "Net-(U2-Pad51)")
    (add_net "Net-(U2-Pad55)")
    (add_net "Net-(U2-Pad60)")
    (add_net "Net-(U3-Pad3)")
    (add_net "Net-(U3-Pad5)")
    (add_net "Net-(U3-Pad7)")
    (add_net "Net-(U3-Pad9)")
    (add_net "Net-(U7-Pad4)")
    (add_net "Net-(U8-Pad1)")
    (add_net "Net-(U8-Pad4)")
    (add_net "Net-(U8-Pad7)")
    (add_net VBUS)
  )
  (module cui-audio:CUI_SJ-3523-SMT-TR (layer F.Cu) (tedit 5C457822)
    (at 116.3025 45.339 270)
    (attr smd)
    (fp_text reference J6 (at -3.46549 -6.14473 270) (layer F.SilkS) hide)
    (fp_text value "MIDI OUT" (at 0 3.556 270) (layer F.SilkS) hide)
    (pad "" np_thru_hole circle (at 3.5 0 270) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at -3.5 0 270) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask F.SilkS))
    (pad R smd rect (at -2.6 -3.675 270) (size 2.2 2.8) (layers F.Cu F.Paste F.Mask)
      (net 99 "Net-(J6-PadR)"))
    (pad T smd rect (at 4.8 3.675 270) (size 2.8 2.8) (layers F.Cu F.Paste F.Mask)
      (net 101 "Net-(J6-PadT)"))
    (pad S smd rect (at -4.6 3.675 270) (size 2.2 2.8) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
  )
  (module keystone:5015-SMT-TestPoint (layer F.Cu) (tedit 5B1E1383)
    (at 142.2105 77.978 90)
    (fp_text reference TP47 (at 0 2.25 90) (layer F.SilkS) hide)
    (fp_text value D0 (at 0 -0.5 90) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 3.43 1.78) (layers F.Cu F.Paste F.Mask)
      (net 2 /D0))
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 113.064 65.786 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C17 (at 0.1905 1.524 90) (layer F.SilkS))
    (fp_text value C_Small (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 +3V3))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module cui-audio:CUI_SJ-3523-SMT-TR (layer F.Cu) (tedit 5C4571E8)
    (at 105.825 45.339 270)
    (attr smd)
    (fp_text reference J5 (at -3.46549 -6.14473 270) (layer F.SilkS) hide)
    (fp_text value "MIDI IN" (at 0.508 4.2545 270) (layer F.SilkS) hide)
    (pad S smd rect (at -4.6 3.675 270) (size 2.3 2.8) (layers F.Cu F.Paste F.Mask)
      (net 108 /SHIELD))
    (pad T smd rect (at 4.7 3.675 270) (size 2.8 2.6) (layers F.Cu F.Paste F.Mask)
      (net 102 "Net-(J5-PadT)"))
    (pad R smd rect (at -2.7 -3.675 270) (size 2.4 2.55) (layers F.Cu F.Paste F.Mask)
      (net 105 "Net-(D4-Pad2)"))
    (pad "" np_thru_hole circle (at -3.5 0 270) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask F.SilkS))
    (pad "" np_thru_hole circle (at 3.5 0 270) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask F.SilkS))
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 121.446 56.0705 135)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C16 (at 4.041115 0.538815 135) (layer F.SilkS))
    (fp_text value C_Small (at 0 1.43 135) (layer F.Fab))
    (fp_text user %R (at 0 0 135) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 135) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 /SAMD_RESET))
    (pad 2 smd roundrect (at 0.875 0 135) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diode_SMD:D_SOD-123 (layer F.Cu) (tedit 58645DC7)
    (at 106.206 54.1655 180)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D4 (at 3.429 0 180) (layer F.SilkS))
    (fp_text value 1N4148W (at 0 2.1 180) (layer F.Fab))
    (fp_text user %R (at 0 -2 180) (layer F.Fab))
    (pad 1 smd rect (at -1.65 0 180) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 103 "Net-(D4-Pad1)"))
    (pad 2 smd rect (at 1.65 0 180) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 105 "Net-(D4-Pad2)"))
    (model ${KISYS3DMOD}/Diode_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_DIP:SMDIP-8_W9.53mm (layer F.Cu) (tedit 5A02E8C5)
    (at 106.587 61.4045 270)
    (descr "8-lead surface-mounted (SMD) DIP package, row spacing 9.53 mm (375 mils)")
    (tags "SMD DIP DIL PDIP SMDIP 2.54mm 9.53mm 375mil")
    (attr smd)
    (fp_text reference U8 (at -0.254 5.7785 270) (layer F.SilkS))
    (fp_text value 6N137S (at 0 6.14 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -4.765 -3.81 270) (size 2 1.78) (layers F.Cu F.Paste F.Mask)
      (net 104 "Net-(U8-Pad1)"))
    (pad 5 smd rect (at 4.765 3.81 270) (size 2 1.78) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 2 smd rect (at -4.765 -1.27 270) (size 2 1.78) (layers F.Cu F.Paste F.Mask)
      (net 103 "Net-(D4-Pad1)"))
    (pad 6 smd rect (at 4.765 1.27 270) (size 2 1.78) (layers F.Cu F.Paste F.Mask)
      (net 98 /MIDI_IN))
    (pad 3 smd rect (at -4.765 1.27 270) (size 2 1.78) (layers F.Cu F.Paste F.Mask)
      (net 105 "Net-(D4-Pad2)"))
    (pad 7 smd rect (at 4.765 -1.27 270) (size 2 1.78) (layers F.Cu F.Paste F.Mask)
      (net 106 "Net-(U8-Pad7)"))
    (pad 4 smd rect (at -4.765 3.81 270) (size 2 1.78) (layers F.Cu F.Paste F.Mask)
      (net 107 "Net-(U8-Pad4)"))
    (pad 8 smd rect (at 4.765 -3.81 270) (size 2 1.78) (layers F.Cu F.Paste F.Mask)
      (net 25 +3V3))
    (model ${KISYS3DMOD}/Package_DIP.3dshapes/SMDIP-8_W9.53mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 110.0795 53.34 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R5 (at 2.667 0 90) (layer F.SilkS))
    (fp_text value R_Small (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 102 "Net-(J5-PadT)"))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 103 "Net-(D4-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 112.175 53.467 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R6 (at -0.762 1.524 90) (layer F.SilkS))
    (fp_text value R_Small (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 +3V3))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 101 "Net-(J6-PadT)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 120.684 46.7995 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R7 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value R_Small (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 99 "Net-(J6-PadR)"))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 100 /MIDI_OUT))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 109.3175 68.2625 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R8 (at 0 -1.43 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.43 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 +3V3))
    (pad 2 smd roundrect (at 0.875 0 180) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 98 /MIDI_IN))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module keystone:5015-SMT-TestPoint (layer F.Cu) (tedit 5B1E1383)
    (at 135.162 64.5795 90)
    (fp_text reference TP46 (at 0 2.25 90) (layer F.SilkS) hide)
    (fp_text value data0 (at 0 -0.5 90) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 3.43 1.78) (layers F.Cu F.Paste F.Mask)
      (net 53 /3V_D0))
  )
  (module gameboy:Cartridge (layer F.Cu) (tedit 5B6F11B9)
    (at 123.445 96.988)
    (fp_text reference U1 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value CARTRIDGE (at 0 -0.5) (layer F.Fab))
    (pad 1 smd rect (at -22 -2.54) (size 1.4 6) (drill (offset -0.2 0)) (layers F.Cu F.Mask)
      (net 93 +BATT))
    (pad 2 smd rect (at -20.5 -2.5) (size 1 6) (layers F.Cu F.Mask)
      (net 28 /CLK))
    (pad 3 smd rect (at -19 -2.5) (size 1 6) (layers F.Cu F.Mask)
      (net 29 /WR))
    (pad 4 smd rect (at -17.5 -2.5) (size 1 6) (layers F.Cu F.Mask)
      (net 30 /RD))
    (pad 5 smd rect (at -16 -2.5) (size 1 6) (layers F.Cu F.Mask)
      (net 31 /CS))
    (pad 6 smd rect (at -14.5 -2.5) (size 1 6) (layers F.Cu F.Mask)
      (net 32 /A0))
    (pad 7 smd rect (at -13 -2.5) (size 1 6) (layers F.Cu F.Mask)
      (net 33 /A1))
    (pad 8 smd rect (at -11.5 -2.5) (size 1 6) (layers F.Cu F.Mask)
      (net 34 /A2))
    (pad 9 smd rect (at -10 -2.5) (size 1 6) (layers F.Cu F.Mask)
      (net 35 /A3))
    (pad 10 smd rect (at -8.5 -2.5) (size 1 6) (layers F.Cu F.Mask)
      (net 36 /A4))
    (pad 11 smd rect (at -7 -2.5) (size 1 6) (layers F.Cu F.Mask)
      (net 37 /A5))
    (pad 12 smd rect (at -5.5 -2.5) (size 1 6) (layers F.Cu F.Mask)
      (net 38 /A6))
    (pad 13 smd rect (at -4 -2.5) (size 1 6) (layers F.Cu F.Mask)
      (net 39 /A7))
    (pad 14 smd rect (at -2.5 -2.5) (size 1 6) (layers F.Cu F.Mask)
      (net 40 /A8))
    (pad 15 smd rect (at -1 -2.5) (size 1 6) (layers F.Cu F.Mask)
      (net 41 /A9))
    (pad 16 smd rect (at 0.5 -2.5) (size 1 6) (layers F.Cu F.Mask)
      (net 42 /A10))
    (pad 17 smd rect (at 2 -2.5) (size 1 6) (layers F.Cu F.Mask)
      (net 43 /A11))
    (pad 18 smd rect (at 3.5 -2.5) (size 1 6) (layers F.Cu F.Mask)
      (net 44 /A12))
    (pad 19 smd rect (at 5 -2.5) (size 1 6) (layers F.Cu F.Mask)
      (net 45 /A13))
    (pad 20 smd rect (at 6.5 -2.5) (size 1 6) (layers F.Cu F.Mask)
      (net 46 /A14))
    (pad 21 smd rect (at 8 -2.5) (size 1 6) (layers F.Cu F.Mask)
      (net 47 /A15))
    (pad 22 smd rect (at 9.5 -2.5) (size 1 6) (layers F.Cu F.Mask)
      (net 2 /D0))
    (pad 23 smd rect (at 11 -2.5) (size 1 6) (layers F.Cu F.Mask)
      (net 3 /D1))
    (pad 24 smd rect (at 12.5 -2.5) (size 1 6) (layers F.Cu F.Mask)
      (net 4 /D2))
    (pad 25 smd rect (at 14 -2.5) (size 1 6) (layers F.Cu F.Mask)
      (net 6 /D3))
    (pad 26 smd rect (at 15.5 -2.5) (size 1 6) (layers F.Cu F.Mask)
      (net 7 /D4))
    (pad 27 smd rect (at 17 -2.5) (size 1 6) (layers F.Cu F.Mask)
      (net 8 /D5))
    (pad 28 smd rect (at 18.5 -2.5) (size 1 6) (layers F.Cu F.Mask)
      (net 9 /D6))
    (pad 29 smd rect (at 20 -2.5) (size 1 6) (layers F.Cu F.Mask)
      (net 10 /D7))
    (pad 30 smd rect (at 21.5 -2.5) (size 1 6) (layers F.Cu F.Mask)
      (net 48 /RESET))
    (pad 31 smd rect (at 23 -2.5) (size 1 6) (layers F.Cu F.Mask)
      (net 94 "Net-(TP31-Pad1)"))
    (pad 32 smd rect (at 24.5 -2.5) (size 1.4 6) (drill (offset 0.2 0)) (layers F.Cu F.Mask)
      (net 5 GND))
  )
  (module "gameboy:Test Point" (layer F.Cu) (tedit 5B6F0FD6)
    (at 110.445 87.738)
    (fp_text reference TP7 (at 2.75 0) (layer F.SilkS) hide)
    (fp_text value Test_Point (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 33 /A1))
  )
  (module "gameboy:Test Point" (layer F.Cu) (tedit 5B6F0FD6)
    (at 120.945 87.738)
    (fp_text reference TP14 (at 2.75 0) (layer F.SilkS) hide)
    (fp_text value Test_Point (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 40 /A8))
  )
  (module "gameboy:Test Point" (layer F.Cu) (tedit 5B6F0FD6)
    (at 111.945 87.738)
    (fp_text reference TP8 (at 2.75 0) (layer F.SilkS) hide)
    (fp_text value Test_Point (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 34 /A2))
  )
  (module "gameboy:Test Point" (layer F.Cu) (tedit 5B6F0FD6)
    (at 108.945 87.738)
    (fp_text reference TP6 (at 2.75 0) (layer F.SilkS) hide)
    (fp_text value Test_Point (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 32 /A0))
  )
  (module "gameboy:Test Point" (layer F.Cu) (tedit 5B6F0FD6)
    (at 107.445 87.738)
    (fp_text reference TP5 (at 2.75 0) (layer F.SilkS) hide)
    (fp_text value Test_Point (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 31 /CS))
  )
  (module "gameboy:Test Point" (layer F.Cu) (tedit 5B6F0FD6)
    (at 105.945 87.738)
    (fp_text reference TP4 (at 2.75 0) (layer F.SilkS) hide)
    (fp_text value Test_Point (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 30 /RD))
  )
  (module "gameboy:Test Point" (layer F.Cu) (tedit 5B6F0FD6)
    (at 104.445 87.738)
    (fp_text reference TP3 (at 2.75 0) (layer F.SilkS) hide)
    (fp_text value Test_Point (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 29 /WR))
  )
  (module "gameboy:Test Point" (layer F.Cu) (tedit 5B6F0FD6)
    (at 102.945 87.738)
    (fp_text reference TP2 (at 2.75 0) (layer F.SilkS) hide)
    (fp_text value Test_Point (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 28 /CLK))
  )
  (module "gameboy:Test Point" (layer F.Cu) (tedit 5B6F0FD6)
    (at 101.219 87.738)
    (fp_text reference TP1 (at 2.75 0) (layer F.SilkS) hide)
    (fp_text value Test_Point (at 0 -0.5) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 93 +BATT))
  )
  (module "gameboy:Test Point" (layer F.Cu) (tedit 5B6F0FD6)
    (at 122.445 87.738)
    (fp_text reference TP15 (at 2.75 0) (layer F.SilkS) hide)
    (fp_text value Test_Point (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 41 /A9))
  )
  (module "gameboy:Test Point" (layer F.Cu) (tedit 5B6F0FD6)
    (at 123.945 87.738)
    (fp_text reference TP16 (at 2.75 0) (layer F.SilkS) hide)
    (fp_text value Test_Point (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 42 /A10))
  )
  (module "gameboy:Test Point" (layer F.Cu) (tedit 5B6F0FD6)
    (at 125.445 87.738)
    (fp_text reference TP17 (at 2.75 0) (layer F.SilkS) hide)
    (fp_text value Test_Point (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 43 /A11))
  )
  (module "gameboy:Test Point" (layer F.Cu) (tedit 5B6F0FD6)
    (at 126.945 87.738)
    (fp_text reference TP18 (at 2.75 0) (layer F.SilkS) hide)
    (fp_text value Test_Point (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 44 /A12))
  )
  (module "gameboy:Test Point" (layer F.Cu) (tedit 5B6F0FD6)
    (at 128.445 87.738)
    (fp_text reference TP19 (at 2.75 0) (layer F.SilkS) hide)
    (fp_text value Test_Point (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 45 /A13))
  )
  (module "gameboy:Test Point" (layer F.Cu) (tedit 5B6F0FD6)
    (at 114.945 87.738)
    (fp_text reference TP10 (at 2.75 0) (layer F.SilkS) hide)
    (fp_text value Test_Point (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 36 /A4))
  )
  (module "gameboy:Test Point" (layer F.Cu) (tedit 5B6F0FD6)
    (at 129.945 87.738)
    (fp_text reference TP20 (at 2.75 0) (layer F.SilkS) hide)
    (fp_text value Test_Point (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 46 /A14))
  )
  (module "gameboy:Test Point" (layer F.Cu) (tedit 5B6F0FD6)
    (at 116.445 87.738)
    (fp_text reference TP11 (at 2.75 0) (layer F.SilkS) hide)
    (fp_text value Test_Point (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 37 /A5))
  )
  (module "gameboy:Test Point" (layer F.Cu) (tedit 5B6F0FD6)
    (at 117.945 87.738)
    (fp_text reference TP12 (at 2.75 0) (layer F.SilkS) hide)
    (fp_text value Test_Point (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 38 /A6))
  )
  (module "gameboy:Test Point" (layer F.Cu) (tedit 5B6F0FD6)
    (at 131.445 87.738)
    (fp_text reference TP21 (at 2.75 0) (layer F.SilkS) hide)
    (fp_text value Test_Point (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 47 /A15))
  )
  (module "gameboy:Test Point" (layer F.Cu) (tedit 5B6F0FD6)
    (at 132.945 87.738)
    (fp_text reference TP22 (at 2.75 0) (layer F.SilkS) hide)
    (fp_text value Test_Point (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 2 /D0))
  )
  (module "gameboy:Test Point" (layer F.Cu) (tedit 5B6F0FD6)
    (at 134.445 87.738)
    (fp_text reference TP23 (at 2.75 0) (layer F.SilkS) hide)
    (fp_text value Test_Point (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 3 /D1))
  )
  (module "gameboy:Test Point" (layer F.Cu) (tedit 5B6F0FD6)
    (at 135.945 87.738)
    (fp_text reference TP24 (at 2.75 0) (layer F.SilkS) hide)
    (fp_text value Test_Point (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 4 /D2))
  )
  (module "gameboy:Test Point" (layer F.Cu) (tedit 5B6F0FD6)
    (at 137.445 87.738)
    (fp_text reference TP25 (at 2.75 0) (layer F.SilkS) hide)
    (fp_text value Test_Point (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 6 /D3))
  )
  (module "gameboy:Test Point" (layer F.Cu) (tedit 5B6F0FD6)
    (at 138.945 87.738)
    (fp_text reference TP26 (at 2.75 0) (layer F.SilkS) hide)
    (fp_text value Test_Point (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 7 /D4))
  )
  (module "gameboy:Test Point" (layer F.Cu) (tedit 5B6F0FD6)
    (at 140.445 87.738)
    (fp_text reference TP27 (at 2.75 0) (layer F.SilkS) hide)
    (fp_text value Test_Point (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 8 /D5))
  )
  (module "gameboy:Test Point" (layer F.Cu) (tedit 5B6F0FD6)
    (at 141.945 87.738)
    (fp_text reference TP28 (at 2.75 0) (layer F.SilkS) hide)
    (fp_text value Test_Point (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 9 /D6))
  )
  (module "gameboy:Test Point" (layer F.Cu) (tedit 5B6F0FD6)
    (at 143.445 87.738)
    (fp_text reference TP29 (at 2.75 0) (layer F.SilkS) hide)
    (fp_text value Test_Point (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 10 /D7))
  )
  (module "gameboy:Test Point" (layer F.Cu) (tedit 5B6F0FD6)
    (at 144.945 87.738)
    (fp_text reference TP30 (at 2.75 0) (layer F.SilkS) hide)
    (fp_text value Test_Point (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 48 /RESET))
  )
  (module "gameboy:Test Point" (layer F.Cu) (tedit 5B6F0FD6)
    (at 145.795 85.738)
    (fp_text reference TP31 (at 2.75 0) (layer F.SilkS) hide)
    (fp_text value Test_Point (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 94 "Net-(TP31-Pad1)"))
  )
  (module "gameboy:Test Point" (layer F.Cu) (tedit 5B6F0FD6)
    (at 148.045 87.688)
    (fp_text reference TP32 (at 2.75 0) (layer F.SilkS) hide)
    (fp_text value Test_Point (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 5 GND))
  )
  (module "gameboy:Test Point" (layer F.Cu) (tedit 5B6F0FD6)
    (at 119.445 87.738)
    (fp_text reference TP13 (at 2.75 0) (layer F.SilkS) hide)
    (fp_text value Test_Point (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 39 /A7))
  )
  (module "gameboy:Test Point" (layer F.Cu) (tedit 5B6F0FD6)
    (at 113.445 87.738)
    (fp_text reference TP9 (at 2.75 0) (layer F.SilkS) hide)
    (fp_text value Test_Point (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 smd rect (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 35 /A3))
  )
  (module keystone:5015-SMT-TestPoint (layer F.Cu) (tedit 5B1E1383)
    (at 142.195 67.988 90)
    (fp_text reference TP33 (at 0 2.25 90) (layer F.SilkS) hide)
    (fp_text value Test_Point (at 0 -0.5 90) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 3.43 1.78) (layers F.Cu F.Paste F.Mask)
      (net 50 /DIR))
  )
  (module keystone:5015-SMT-TestPoint (layer F.Cu) (tedit 5B1E1383)
    (at 133.695 71.738 135)
    (fp_text reference TP40 (at 0 2.25 135) (layer F.SilkS) hide)
    (fp_text value clk (at 0 -0.5 135) (layer F.Fab))
    (pad 1 smd rect (at 0 0 135) (size 3.43 1.78) (layers F.Cu F.Paste F.Mask)
      (net 81 /3V_CLK))
  )
  (module keystone:5015-SMT-TestPoint (layer F.Cu) (tedit 5B1E1383)
    (at 104.3645 76.708 90)
    (fp_text reference TP41 (at 0 2.25 90) (layer F.SilkS) hide)
    (fp_text value rd (at 0 -0.5 90) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 3.43 1.78) (layers F.Cu F.Paste F.Mask)
      (net 83 /3V_RD))
  )
  (module keystone:5015-SMT-TestPoint (layer F.Cu) (tedit 5B1E1383)
    (at 108.6825 73.7235 45)
    (fp_text reference TP42 (at 0 2.25 45) (layer F.SilkS) hide)
    (fp_text value wr (at 0 -0.5 45) (layer F.Fab))
    (pad 1 smd rect (at 0 0 45) (size 3.43 1.78) (layers F.Cu F.Paste F.Mask)
      (net 82 /3V_WR))
  )
  (module keystone:5015-SMT-TestPoint (layer F.Cu) (tedit 5B1E1383)
    (at 137.945 74.988)
    (fp_text reference TP43 (at 0 2.25) (layer F.SilkS) hide)
    (fp_text value a15 (at 0 -0.5) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 3.43 1.78) (layers F.Cu F.Paste F.Mask)
      (net 72 /3V_A15))
  )
  (module keystone:5015-SMT-TestPoint (layer F.Cu) (tedit 5B1E1383)
    (at 133.003 51.7525 45)
    (fp_text reference TP44 (at 0 2.25 45) (layer F.SilkS) hide)
    (fp_text value PB17 (at 0 -0.5 45) (layer F.Fab))
    (pad 1 smd rect (at 0 0 45) (size 3.43 1.78) (layers F.Cu F.Paste F.Mask)
      (net 97 "Net-(TP44-Pad1)"))
  )
  (module keystone:5015-SMT-TestPoint (layer F.Cu) (tedit 5B1E1383)
    (at 112.2385 69.596 45)
    (fp_text reference TP45 (at 0 2.25 45) (layer F.SilkS) hide)
    (fp_text value cs (at 0 -0.5 45) (layer F.Fab))
    (pad 1 smd rect (at 0 0 45) (size 3.43 1.78) (layers F.Cu F.Paste F.Mask)
      (net 84 /3V_CS))
  )
  (module keystone:5015-SMT-TestPoint (layer F.Cu) (tedit 5B1E1383)
    (at 139.445 65.488 90)
    (fp_text reference TP35 (at 0 2.25 90) (layer F.SilkS) hide)
    (fp_text value GB_RESET (at 0 -0.5 90) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 3.43 1.78) (layers F.Cu F.Paste F.Mask)
      (net 62 /GB_RESET))
  )
  (module keystone:5015-SMT-TestPoint (layer F.Cu) (tedit 5B1E1383)
    (at 139.445 69.738 90)
    (fp_text reference TP34 (at 0 2.25 90) (layer F.SilkS) hide)
    (fp_text value DATA_OE (at 0 -0.5 90) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 3.43 1.78) (layers F.Cu F.Paste F.Mask)
      (net 49 /DATA_OE))
  )
  (module keystone:5015-SMT-TestPoint (layer F.Cu) (tedit 5B1E13A2)
    (at 113.7625 60.833 270)
    (fp_text reference TP38 (at 0 2.25 270) (layer F.SilkS) hide)
    (fp_text value 3.3v (at 0 -0.5 270) (layer F.Fab))
    (pad 1 smd rect (at 0 0 270) (size 3.43 1.78) (layers F.Cu F.Paste F.Mask)
      (net 25 +3V3))
  )
  (module keystone:5015-SMT-TestPoint (layer F.Cu) (tedit 5B1E13A5)
    (at 101.507 69.723 90)
    (fp_text reference TP39 (at 0 2.25 90) (layer F.SilkS) hide)
    (fp_text value batt (at 0 -0.5 90) (layer F.Fab))
    (pad 1 smd rect (at 0 0 90) (size 3.43 1.78) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
  )
  (module keystone:5015-SMT-TestPoint (layer F.Cu) (tedit 5B1E1A42)
    (at 145.945 47.738)
    (fp_text reference TP37 (at 0 2.25) (layer F.SilkS) hide)
    (fp_text value gnd (at 0 -0.5) (layer F.Fab))
    (pad 1 smd rect (at 0 0) (size 3.43 1.78) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
  )
  (module keystone:5015-SMT-TestPoint (layer F.Cu) (tedit 5B1E1B14)
    (at 122.081 53.975 135)
    (fp_text reference TP36 (at 0 2.25 135) (layer F.SilkS) hide)
    (fp_text value SAMD_RESET (at 0 -0.5 135) (layer F.Fab))
    (pad 1 smd rect (at 0 0 135) (size 3.43 1.78) (layers F.Cu F.Paste F.Mask)
      (net 63 /SAMD_RESET))
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 119.745 58.688 315)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C14 (at -3.323402 0.070711 315) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.5 315) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 315) (layer F.Fab))
    (pad 1 smd rect (at -0.949999 0 315) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 2 smd rect (at 0.949999 0 315) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 96 "Net-(C14-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 120.845 57.638 315)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C15 (at -3.358757 0.176777 315) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.5 315) (layer F.Fab))
    (fp_text user %R (at -3.323402 0.141421 315) (layer F.Fab))
    (pad 2 smd rect (at 0.949999 0 315) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 96 "Net-(C14-Pad2)"))
    (pad 1 smd rect (at -0.949999 0 315) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603_HandSoldering (layer F.Cu) (tedit 595FC9C0)
    (at 132.6855 40.5765 270)
    (descr "LED SMD 0603, hand soldering")
    (tags "LED 0603")
    (attr smd)
    (fp_text reference D3 (at 2.921 0 270) (layer F.SilkS))
    (fp_text value LED (at 0 1.55 270) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 25 +3V3))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 91 "Net-(D3-Pad1)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 134.4635 40.5765 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 2.921 0.168 270) (layer F.SilkS))
    (fp_text value 1k (at 0 1.55 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 91 "Net-(D3-Pad1)"))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 92 /LED))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 137.668 61.214)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at -3.048 0) (layer F.SilkS))
    (fp_text value 10k (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 49 /DATA_OE))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 25 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-123 (layer F.Cu) (tedit 58645DC7)
    (at 101.473 74.041 270)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D2 (at 3.247 -0.922 270) (layer F.SilkS))
    (fp_text value MBR120 (at 0 2.1 270) (layer F.Fab))
    (fp_text user %R (at 0 -2 270) (layer F.Fab))
    (pad 1 smd rect (at -1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.65 0 270) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 93 +BATT))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-123 (layer F.Cu) (tedit 58645DC7)
    (at 126.399 46.9265)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D1 (at -0.023 2.244) (layer F.SilkS))
    (fp_text value MBR120 (at 0 2.1) (layer F.Fab))
    (fp_text user %R (at 0 -2) (layer F.Fab))
    (pad 2 smd rect (at 1.65 0) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 67 VBUS))
    (pad 1 smd rect (at -1.65 0) (size 0.9 1.2) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fci:Mini-USB-B-OshPark (layer F.Cu) (tedit 592BBFBF)
    (at 126.399 39.5605 180)
    (fp_text reference J4 (at -6.78 -1.46 180) (layer F.SilkS) hide)
    (fp_text value USB_B_Micro (at -0.02 -4.63 180) (layer F.Fab))
    (pad 6 smd rect (at -3.4 -2.45 180) (size 2 1.4) (drill (offset -0.2 0)) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 6 smd rect (at 3.4 -2.45 180) (size 2 1.4) (drill (offset 0.2 0)) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 1 smd rect (at -1.3 -2.675 180) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 67 VBUS))
    (pad 2 smd rect (at -0.65 -2.675 180) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 89 /USB_D-))
    (pad 3 smd rect (at 0 -2.675 180) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 90 /USB_D+))
    (pad 4 smd rect (at 0.65 -2.675 180) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 68 "Net-(J4-Pad4)"))
    (pad 5 smd rect (at 1.3 -2.675 180) (size 0.4 1.35) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 6 smd rect (at -1.2 0 180) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 6 smd rect (at 1.2 0 180) (size 1.9 1.9) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 6 thru_hole oval (at -3.3 0 180) (size 2.6 1.6) (drill 1.2 (offset -0.5 0)) (layers *.Cu *.Mask F.SilkS)
      (net 5 GND))
    (pad 6 thru_hole oval (at 3.3 0 180) (size 2.6 1.6) (drill 1.2 (offset 0.5 0)) (layers *.Cu *.Mask F.SilkS)
      (net 5 GND))
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 107.476 71.0565 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C13 (at 0 1.8415 180) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 90) (layer F.Fab))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 25 +3V3))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 121.412 79.121 45)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C12 (at 0 -1.25 45) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.5 45) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 45) (layer F.Fab))
    (pad 1 smd rect (at -0.949999 0 45) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 25 +3V3))
    (pad 2 smd rect (at 0.949999 0 45) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 111.887 77.724)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C11 (at 0.542 -1.25) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.25) (layer F.Fab))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 25 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5C454AC0)
    (at 104.682 73.914 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C10 (at -2.6035 -0.4445 270) (layer F.SilkS) hide)
    (fp_text value 1uF (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 129.445 80.137 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C9 (at -2.794 -0.127 270) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 270) (layer F.Fab))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 25 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 137.541 59.563)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C8 (at -3.048 0) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.25) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 25 +3V3))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 141.605 59.563 180)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C7 (at -2.921 0 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 180) (layer F.Fab))
    (pad 2 smd rect (at 0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 1 smd rect (at -0.95 0 180) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 127.923 58.9915 225)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at -0.898026 1.257236 225) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.5 225) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 225) (layer F.Fab))
    (pad 1 smd rect (at -0.949999 0 225) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 2 smd rect (at 0.949999 0 225) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 25 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 133.3205 67.31 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at 2.7305 0.0635 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 90) (layer F.Fab))
    (pad 2 smd rect (at 0.949999 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 25 +3V3))
    (pad 1 smd rect (at -0.949999 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 127.889 75.565 45)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 2.783879 0.089803 45) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.5 45) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 45) (layer F.Fab))
    (pad 1 smd rect (at -0.949999 0 45) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 2 smd rect (at 0.949999 0 45) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 25 +3V3))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 118.237 74.041 45)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 0 -1.25 45) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.5 45) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 45) (layer F.Fab))
    (pad 2 smd rect (at 0.949999 0 45) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 25 +3V3))
    (pad 1 smd rect (at -0.949999 0 45) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 118.618 59.817 135)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 3.592102 0 135) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.5 135) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 135) (layer F.Fab))
    (pad 1 smd rect (at -0.949999 0 135) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 96 "Net-(C14-Pad2)"))
    (pad 2 smd rect (at 0.949999 0 135) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 117.602 60.96 315)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at -3.681905 0.089803 315) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.5 315) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 315) (layer F.Fab))
    (pad 2 smd rect (at 0.949999 0 315) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 25 +3V3))
    (pad 1 smd rect (at -0.949999 0 315) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x05_Pitch1.27mm_SMD (layer F.Cu) (tedit 59650536)
    (at 139.1625 43.4975 270)
    (descr "surface-mounted straight pin header, 2x05, 1.27mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x05 1.27mm double row")
    (attr smd)
    (fp_text reference J3 (at 2.0955 3.7465 270) (layer F.SilkS))
    (fp_text value Conn_ARM_JTAG_SWD_10 (at 0 4.235 270) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 10 smd rect (at 1.95 2.54 270) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 63 /SAMD_RESET))
    (pad 9 smd rect (at -1.95 2.54 270) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 64 "Net-(J3-Pad9)"))
    (pad 8 smd rect (at 1.95 1.27 270) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 65 "Net-(J3-Pad8)"))
    (pad 7 smd rect (at -1.95 1.27 270) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 66 "Net-(J3-Pad7)"))
    (pad 6 smd rect (at 1.95 0 270) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 95 /SWO))
    (pad 5 smd rect (at -1.95 0 270) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 4 smd rect (at 1.95 -1.27 270) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 27 /SWCLK))
    (pad 3 smd rect (at -1.95 -1.27 270) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 2 smd rect (at 1.95 -2.54 270) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 26 /SWDIO))
    (pad 1 smd rect (at -1.95 -2.54 270) (size 2.4 0.74) (layers F.Cu F.Paste F.Mask)
      (net 25 +3V3))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x05_Pitch1.27mm_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 137.287 65.532 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at -2.4765 0.0295) (layer F.SilkS))
    (fp_text value 10k (at 0 1.55 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 25 +3V3))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 62 /GB_RESET))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 122.2715 50.927 315)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0 -1.45 315) (layer F.SilkS))
    (fp_text value 10k (at 0 1.55 315) (layer F.Fab))
    (fp_text user %R (at 0 0 315) (layer F.Fab))
    (pad 2 smd rect (at 1.099999 0 315) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 63 /SAMD_RESET))
    (pad 1 smd rect (at -1.099999 0 315) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 25 +3V3))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23 (layer F.Cu) (tedit 58CE4E7E)
    (at 136.271 69.723 270)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 2.515 -0.674) (layer F.SilkS))
    (fp_text value BSS138 (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 3 smd rect (at 1 0 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 48 /RESET))
    (pad 2 smd rect (at -1 0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 1 smd rect (at -1 -0.95 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 62 /GB_RESET))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_SMD:SOT-23-5 (layer F.Cu) (tedit 58CE4E7E)
    (at 104.682 71.12)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U7 (at -0.127 -2.413) (layer F.SilkS))
    (fp_text value AP2204K-3.3 (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 5 smd rect (at 1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 25 +3V3))
    (pad 4 smd rect (at 1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(U7-Pad4)"))
    (pad 3 smd rect (at -1.1 0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 1 smd rect (at -1.1 -0.95) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "gameboy:Large Hole" (layer F.Cu) (tedit 5AE8088A)
    (at 124.65 82.35)
    (fp_text reference J2 (at 0 0.5) (layer F.SilkS))
    (fp_text value Conn_01x01 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 7.4 7.4) (drill 7.3) (layers *.Cu *.Mask)
      (net 52 "Net-(J2-Pad1)"))
  )
  (module "gameboy:Small Hole" (layer F.Cu) (tedit 5AE80885)
    (at 124.65 57.3)
    (fp_text reference J1 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value Conn_01x01 (at 0 -0.5) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 2.3 2.3) (drill 2.2) (layers *.Cu *.Mask)
      (net 51 "Net-(J1-Pad1)"))
  )
  (module Housings_QFP:LQFP-64_10x10mm_Pitch0.5mm (layer F.Cu) (tedit 5AE96B50)
    (at 124.714 68.072 45)
    (descr "64 LEAD LQFP 10x10mm (see MICREL LQFP10x10-64LD-PL-1.pdf)")
    (tags "QFP 0.5")
    (attr smd)
    (fp_text reference U2 (at 5.632106 -5.658976 180) (layer F.SilkS))
    (fp_text value SAMD51J (at 0 7.2 45) (layer F.Fab))
    (fp_text user %R (at 0 0 45) (layer F.Fab))
    (pad 64 smd rect (at -3.75 -5.7 135) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 88 /3V_A3))
    (pad 63 smd rect (at -3.25 -5.7 135) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 87 /3V_A2))
    (pad 62 smd rect (at -2.75 -5.7 135) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 86 /3V_A1))
    (pad 61 smd rect (at -2.25 -5.7 135) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 85 /3V_A0))
    (pad 60 smd rect (at -1.75 -5.7 135) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(U2-Pad60)"))
    (pad 59 smd rect (at -1.25 -5.7 135) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 95 /SWO))
    (pad 58 smd rect (at -0.75 -5.7 135) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 26 /SWDIO))
    (pad 57 smd rect (at -0.25 -5.7 135) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 27 /SWCLK))
    (pad 56 smd rect (at 0.25 -5.7 135) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 25 +3V3))
    (pad 55 smd rect (at 0.75 -5.7 135) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(U2-Pad55)"))
    (pad 54 smd rect (at 1.25 -5.7 135) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 53 smd rect (at 1.75 -5.7 135) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 96 "Net-(C14-Pad2)"))
    (pad 52 smd rect (at 2.25 -5.7 135) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 63 /SAMD_RESET))
    (pad 51 smd rect (at 2.75 -5.7 135) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(U2-Pad51)"))
    (pad 50 smd rect (at 3.25 -5.7 135) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 92 /LED))
    (pad 49 smd rect (at 3.75 -5.7 135) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 62 /GB_RESET))
    (pad 48 smd rect (at 5.7 -3.75 45) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 25 +3V3))
    (pad 47 smd rect (at 5.7 -3.25 45) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 46 smd rect (at 5.7 -2.75 45) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 90 /USB_D+))
    (pad 45 smd rect (at 5.7 -2.25 45) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 89 /USB_D-))
    (pad 44 smd rect (at 5.7 -1.75 45) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 60 /3V_D7))
    (pad 43 smd rect (at 5.7 -1.25 45) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 59 /3V_D6))
    (pad 42 smd rect (at 5.7 -0.75 45) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 58 /3V_D5))
    (pad 41 smd rect (at 5.7 -0.25 45) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 57 /3V_D4))
    (pad 40 smd rect (at 5.7 0.25 45) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 97 "Net-(TP44-Pad1)"))
    (pad 39 smd rect (at 5.7 0.75 45) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 84 /3V_CS))
    (pad 38 smd rect (at 5.7 1.25 45) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 56 /3V_D3))
    (pad 37 smd rect (at 5.7 1.75 45) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 55 /3V_D2))
    (pad 36 smd rect (at 5.7 2.25 45) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 54 /3V_D1))
    (pad 35 smd rect (at 5.7 2.75 45) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 53 /3V_D0))
    (pad 34 smd rect (at 5.7 3.25 45) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 25 +3V3))
    (pad 33 smd rect (at 5.7 3.75 45) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 32 smd rect (at 3.75 5.7 135) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 81 /3V_CLK))
    (pad 31 smd rect (at 3.25 5.7 135) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(U2-Pad31)"))
    (pad 30 smd rect (at 2.75 5.7 135) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(U2-Pad30)"))
    (pad 29 smd rect (at 2.25 5.7 135) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(U2-Pad29)"))
    (pad 28 smd rect (at 1.75 5.7 135) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 72 /3V_A15))
    (pad 27 smd rect (at 1.25 5.7 135) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 71 /3V_A14))
    (pad 26 smd rect (at 0.75 5.7 135) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 70 /3V_A13))
    (pad 25 smd rect (at 0.25 5.7 135) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 69 /3V_A12))
    (pad 24 smd rect (at -0.25 5.7 135) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 73 /3V_A11))
    (pad 23 smd rect (at -0.75 5.7 135) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 74 /3V_A10))
    (pad 22 smd rect (at -1.25 5.7 135) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 21 smd rect (at -1.75 5.7 135) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 25 +3V3))
    (pad 20 smd rect (at -2.25 5.7 135) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 50 /DIR))
    (pad 19 smd rect (at -2.75 5.7 135) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 81 /3V_CLK))
    (pad 18 smd rect (at -3.25 5.7 135) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 82 /3V_WR))
    (pad 17 smd rect (at -3.75 5.7 135) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 72 /3V_A15))
    (pad 16 smd rect (at -5.7 3.75 45) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 49 /DATA_OE))
    (pad 15 smd rect (at -5.7 3.25 45) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 83 /3V_RD))
    (pad 14 smd rect (at -5.7 2.75 45) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 72 /3V_A15))
    (pad 13 smd rect (at -5.7 2.25 45) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 81 /3V_CLK))
    (pad 12 smd rect (at -5.7 1.75 45) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 75 /3V_A9))
    (pad 11 smd rect (at -5.7 1.25 45) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 76 /3V_A8))
    (pad 10 smd rect (at -5.7 0.75 45) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 77 /3V_A7))
    (pad 9 smd rect (at -5.7 0.25 45) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 78 /3V_A6))
    (pad 8 smd rect (at -5.7 -0.25 45) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 25 +3V3))
    (pad 7 smd rect (at -5.7 -0.75 45) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 6 smd rect (at -5.7 -1.25 45) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 79 /3V_A5))
    (pad 5 smd rect (at -5.7 -1.75 45) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 80 /3V_A4))
    (pad 4 smd rect (at -5.7 -2.25 45) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(U2-Pad4)"))
    (pad 3 smd rect (at -5.7 -2.75 45) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(U2-Pad3)"))
    (pad 2 smd rect (at -5.7 -3.25 45) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(U2-Pad2)"))
    (pad 1 smd rect (at -5.7 -3.75 45) (size 1 0.25) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(U2-Pad1)"))
    (model ${KISYS3DMOD}/Housings_QFP.3dshapes/LQFP-64_10x10mm_Pitch0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:TSSOP-20_4.4x6.5mm_Pitch0.65mm (layer F.Cu) (tedit 54130A77)
    (at 105.664 82.296)
    (descr "20-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U6 (at 0.923 -4.1275) (layer F.SilkS))
    (fp_text value 74LS244 (at 0 4.3) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 20 smd rect (at 2.95 -2.925) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 25 +3V3))
    (pad 19 smd rect (at 2.95 -2.275) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 18 smd rect (at 2.95 -1.625) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 81 /3V_CLK))
    (pad 17 smd rect (at 2.95 -0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 35 /A3))
    (pad 16 smd rect (at 2.95 -0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 82 /3V_WR))
    (pad 15 smd rect (at 2.95 0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 34 /A2))
    (pad 14 smd rect (at 2.95 0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 83 /3V_RD))
    (pad 13 smd rect (at 2.95 1.625) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 33 /A1))
    (pad 12 smd rect (at 2.95 2.275) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 84 /3V_CS))
    (pad 11 smd rect (at 2.95 2.925) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 32 /A0))
    (pad 10 smd rect (at -2.95 2.925) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 9 smd rect (at -2.95 2.275) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 85 /3V_A0))
    (pad 8 smd rect (at -2.95 1.625) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 31 /CS))
    (pad 7 smd rect (at -2.95 0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 86 /3V_A1))
    (pad 6 smd rect (at -2.95 0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 30 /RD))
    (pad 5 smd rect (at -2.95 -0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 87 /3V_A2))
    (pad 4 smd rect (at -2.95 -0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 29 /WR))
    (pad 3 smd rect (at -2.95 -1.625) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 88 /3V_A3))
    (pad 2 smd rect (at -2.95 -2.275) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 28 /CLK))
    (pad 1 smd rect (at -2.95 -2.925) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (model ${KISYS3DMOD}/Housings_SSOP.3dshapes/TSSOP-20_4.4x6.5mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:TSSOP-20_4.4x6.5mm_Pitch0.65mm (layer F.Cu) (tedit 54130A77)
    (at 115.824 82.296)
    (descr "20-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U4 (at 0 -4.3) (layer F.SilkS))
    (fp_text value 74LS244 (at 0 4.3) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2.95 -2.925) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 2 smd rect (at -2.95 -2.275) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 36 /A4))
    (pad 3 smd rect (at -2.95 -1.625) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 73 /3V_A11))
    (pad 4 smd rect (at -2.95 -0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 37 /A5))
    (pad 5 smd rect (at -2.95 -0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 74 /3V_A10))
    (pad 6 smd rect (at -2.95 0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 38 /A6))
    (pad 7 smd rect (at -2.95 0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 75 /3V_A9))
    (pad 8 smd rect (at -2.95 1.625) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 39 /A7))
    (pad 9 smd rect (at -2.95 2.275) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 76 /3V_A8))
    (pad 10 smd rect (at -2.95 2.925) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 11 smd rect (at 2.95 2.925) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 40 /A8))
    (pad 12 smd rect (at 2.95 2.275) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 77 /3V_A7))
    (pad 13 smd rect (at 2.95 1.625) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 41 /A9))
    (pad 14 smd rect (at 2.95 0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 78 /3V_A6))
    (pad 15 smd rect (at 2.95 0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 42 /A10))
    (pad 16 smd rect (at 2.95 -0.325) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 79 /3V_A5))
    (pad 17 smd rect (at 2.95 -0.975) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 43 /A11))
    (pad 18 smd rect (at 2.95 -1.625) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 80 /3V_A4))
    (pad 19 smd rect (at 2.95 -2.275) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 20 smd rect (at 2.95 -2.925) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 25 +3V3))
    (model ${KISYS3DMOD}/Housings_SSOP.3dshapes/TSSOP-20_4.4x6.5mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:TSSOP-20_4.4x6.5mm_Pitch0.65mm (layer F.Cu) (tedit 54130A77)
    (at 133.945 80.738 90)
    (descr "20-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U3 (at 0 4.318 90) (layer F.SilkS))
    (fp_text value 74LS244 (at 0 4.3 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 20 smd rect (at 2.95 -2.925 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 25 +3V3))
    (pad 19 smd rect (at 2.95 -2.275 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 25 +3V3))
    (pad 18 smd rect (at 2.95 -1.625 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 69 /3V_A12))
    (pad 17 smd rect (at 2.95 -0.975 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 16 smd rect (at 2.95 -0.325 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 70 /3V_A13))
    (pad 15 smd rect (at 2.95 0.325 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 14 smd rect (at 2.95 0.975 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 71 /3V_A14))
    (pad 13 smd rect (at 2.95 1.625 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 12 smd rect (at 2.95 2.275 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 72 /3V_A15))
    (pad 11 smd rect (at 2.95 2.925 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 10 smd rect (at -2.95 2.925 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 9 smd rect (at -2.95 2.275 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(U3-Pad9)"))
    (pad 8 smd rect (at -2.95 1.625 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 47 /A15))
    (pad 7 smd rect (at -2.95 0.975 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(U3-Pad7)"))
    (pad 6 smd rect (at -2.95 0.325 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 46 /A14))
    (pad 5 smd rect (at -2.95 -0.325 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(U3-Pad5)"))
    (pad 4 smd rect (at -2.95 -0.975 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 45 /A13))
    (pad 3 smd rect (at -2.95 -1.625 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(U3-Pad3)"))
    (pad 2 smd rect (at -2.95 -2.275 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 44 /A12))
    (pad 1 smd rect (at -2.95 -2.925 90) (size 1.45 0.45) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (model ${KISYS3DMOD}/Housings_SSOP.3dshapes/TSSOP-20_4.4x6.5mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SSOP:TSSOP-24_4.4x7.8mm_Pitch0.65mm (layer F.Cu) (tedit 57B061D2)
    (at 139.446 54.229 180)
    (descr "TSSOP24: plastic thin shrink small outline package; 24 leads; body width 4.4 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot355-1_po.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U5 (at -4.7965 0.0635 180) (layer F.SilkS))
    (fp_text value 74x4245 (at 0 4.95 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 24 smd rect (at 2.85 -3.575 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 25 +3V3))
    (pad 23 smd rect (at 2.85 -2.925 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 25 +3V3))
    (pad 22 smd rect (at 2.85 -2.275 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 49 /DATA_OE))
    (pad 21 smd rect (at 2.85 -1.625 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 53 /3V_D0))
    (pad 20 smd rect (at 2.85 -0.975 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 54 /3V_D1))
    (pad 19 smd rect (at 2.85 -0.325 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 55 /3V_D2))
    (pad 18 smd rect (at 2.85 0.325 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 56 /3V_D3))
    (pad 17 smd rect (at 2.85 0.975 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 57 /3V_D4))
    (pad 16 smd rect (at 2.85 1.625 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 58 /3V_D5))
    (pad 15 smd rect (at 2.85 2.275 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 59 /3V_D6))
    (pad 14 smd rect (at 2.85 2.925 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 60 /3V_D7))
    (pad 13 smd rect (at 2.85 3.575 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 12 smd rect (at -2.85 3.575 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 11 smd rect (at -2.85 2.925 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 5 GND))
    (pad 10 smd rect (at -2.85 2.275 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 10 /D7))
    (pad 9 smd rect (at -2.85 1.625 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 9 /D6))
    (pad 8 smd rect (at -2.85 0.975 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 8 /D5))
    (pad 7 smd rect (at -2.85 0.325 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 7 /D4))
    (pad 6 smd rect (at -2.85 -0.325 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 6 /D3))
    (pad 5 smd rect (at -2.85 -0.975 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 4 /D2))
    (pad 4 smd rect (at -2.85 -1.625 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 3 /D1))
    (pad 3 smd rect (at -2.85 -2.275 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 2 /D0))
    (pad 2 smd rect (at -2.85 -2.925 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 50 /DIR))
    (pad 1 smd rect (at -2.85 -3.575 180) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Housings_SSOP.3dshapes/TSSOP-24_4.4x7.8mm_Pitch0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module chickadee:chickadee_2mm_fcu (layer F.Cu) (tedit 0)
    (at 145.957 44.3865)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (gr_text D0 (at 142.2105 75.565) (layer F.SilkS))
  (gr_text OUT (at 112.1115 45.466 90) (layer F.SilkS))
  (gr_text IN (at 101.634 45.5295 90) (layer F.SilkS))
  (gr_text GND (at 145.995 49.488) (layer F.SilkS))
  (gr_text PB17 (at 134.019 53.0225 45) (layer F.SilkS))
  (gr_text +3.3V (at 113.6355 63.4365) (layer F.SilkS))
  (gr_text +5V (at 101.0625 66.4845 90) (layer F.SilkS))
  (gr_text RESET (at 124.5575 54.0385 315) (layer F.SilkS))
  (gr_text CLK (at 132.195 72.638 315) (layer F.SilkS))
  (gr_text A15 (at 137.845 73.488) (layer F.SilkS))
  (gr_text OE (at 139.4165 72.136) (layer F.SilkS))
  (gr_text DIR (at 142.147 70.4215) (layer F.SilkS))
  (gr_text GB_RS (at 140.496 63.0555) (layer F.SilkS))
  (gr_text "RD\n" (at 106.0155 75.5015 90) (layer F.SilkS))
  (gr_text WR (at 111.032 72.263 45) (layer F.SilkS))
  (gr_text CS (at 113.8895 70.1675 45) (layer F.SilkS))
  (gr_text "Data 3V" (at 132.345 59.188 45) (layer F.SilkS))
  (gr_text SAMD51 (at 119.695 62.838 45) (layer F.SilkS))
  (gr_text "LED\nPB23" (at 131.352 46.6725 45) (layer F.SilkS))
  (gr_text USB (at 126.399 44.831) (layer F.SilkS))
  (gr_text Debug (at 139.099 48.1965) (layer F.SilkS))
  (gr_text Address (at 111.2225 74.549 45) (layer F.SilkS))
  (gr_text Data (at 142.782 82.296 45) (layer F.SilkS))
  (gr_text ckd.tech/pygb/v3 (at 147.1 66.3575 90) (layer F.SilkS))
  (gr_text GND (at 147.945 91.44 90) (layer F.SilkS))
  (gr_text AUD (at 146.445 91.44 90) (layer F.SilkS))
  (gr_text RST (at 144.945 91.44 90) (layer F.SilkS))
  (gr_text D7 (at 143.445 91.44 90) (layer F.SilkS))
  (gr_text D6 (at 141.945 91.44 90) (layer F.SilkS))
  (gr_text D5 (at 140.445 91.44 90) (layer F.SilkS))
  (gr_text D4 (at 138.945 91.44 90) (layer F.SilkS))
  (gr_text D3 (at 137.445 91.44 90) (layer F.SilkS))
  (gr_text D2 (at 135.945 91.44 90) (layer F.SilkS))
  (gr_text D1 (at 134.445 91.44 90) (layer F.SilkS))
  (gr_text D0 (at 132.945 91.44 90) (layer F.SilkS))
  (gr_text A15 (at 131.445 91.44 90) (layer F.SilkS))
  (gr_text A14 (at 129.945 91.44 90) (layer F.SilkS))
  (gr_text A13 (at 128.445 91.44 90) (layer F.SilkS))
  (gr_text A12 (at 126.945 91.44 90) (layer F.SilkS))
  (gr_text A11 (at 125.445 91.44 90) (layer F.SilkS))
  (gr_text A10 (at 123.945 91.44 90) (layer F.SilkS))
  (gr_text A9 (at 122.445 91.44 90) (layer F.SilkS))
  (gr_text A8 (at 120.945 91.44 90) (layer F.SilkS))
  (gr_text A7 (at 119.445 91.44 90) (layer F.SilkS))
  (gr_text A6 (at 117.945 91.44 90) (layer F.SilkS))
  (gr_text A5 (at 116.445 91.44 90) (layer F.SilkS))
  (gr_text A4 (at 114.945 91.44 90) (layer F.SilkS))
  (gr_text A3 (at 113.445 91.44 90) (layer F.SilkS))
  (gr_text A2 (at 111.945 91.44 90) (layer F.SilkS))
  (gr_text A1 (at 110.445 91.44 90) (layer F.SilkS))
  (gr_text A0 (at 108.945 91.44 90) (layer F.SilkS))
  (gr_text CS (at 107.442 91.44 90) (layer F.SilkS))
  (gr_text RD (at 105.945 91.44 90) (layer F.SilkS))
  (gr_text WR (at 104.445 91.44 90) (layer F.SilkS))
  (gr_text CLK (at 102.945 91.44 90) (layer F.SilkS))
  (gr_text +5V (at 101.219 91.44 90) (layer F.SilkS))
  (gr_line (start 143.3 42.3) (end 143.3 38.3) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 149.3 42.3) (end 143.3 42.3) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 149.3 98) (end 100 98) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 149.3 42.3) (end 149.3 98) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 100 38.3) (end 143.3 38.3) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 100 38.3) (end 100 98) (layer Edge.Cuts) (width 0.15))
  (zone (net 5) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 111.2225 38.4175) (xy 111.2225 61.722) (xy 100.11 61.595) (xy 99.949 98.044) (xy 149.352 98.044)
        (xy 149.352 38.227) (xy 149.352 38.1)
      )
    )
  )
  (zone (net 5) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.3048) (thermal_bridge_width 0.3048))
    (polygon
      (pts
        (xy 149.352 98.044) (xy 149.352 37.973) (xy 111.4765 38.354) (xy 111.4765 61.1505) (xy 100.0465 61.1505)
        (xy 100.076 98.044)
      )
    )
  )
  (zone (net 108) (net_name /SHIELD) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 100.0465 38.2905) (xy 110.905 38.227) (xy 110.7145 60.579) (xy 100.491 60.3885)
      )
    )
  )
  (zone (net 108) (net_name /SHIELD) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 100.0465 60.8965) (xy 99.983 38.4175) (xy 110.524 38.4175) (xy 110.3335 60.8965)
      )
    )
  )
)
