(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 46)
    (no_connects 0)
    (area 136.564999 33.095 188.428002 96.346001)
    (thickness 1.6)
    (drawings 6)
    (tracks 119)
    (zones 0)
    (modules 33)
    (nets 21)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 1)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory R:/Kicad/Bridge/plot/))
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad1)")
  (net 2 "Net-(D1-Pad2)")
  (net 3 "Net-(D2-Pad1)")
  (net 4 "Net-(D3-Pad1)")
  (net 5 "Net-(D3-Pad2)")
  (net 6 "Net-(D5-Pad1)")
  (net 7 "Net-(D5-Pad2)")
  (net 8 "Net-(D6-Pad1)")
  (net 9 "Net-(D7-Pad1)")
  (net 10 "Net-(D7-Pad2)")
  (net 11 "Net-(P2-Pad2)")
  (net 12 "Net-(P3-Pad2)")
  (net 13 "Net-(P6-Pad2)")
  (net 14 "Net-(P7-Pad2)")
  (net 15 "Net-(D4-Pad1)")
  (net 16 "Net-(D8-Pad1)")
  (net 17 /HV)
  (net 18 /OV)
  (net 19 /B2)
  (net 20 /B1)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 1)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D5-Pad1)")
    (add_net "Net-(D5-Pad2)")
    (add_net "Net-(D6-Pad1)")
    (add_net "Net-(D7-Pad1)")
    (add_net "Net-(D7-Pad2)")
    (add_net "Net-(D8-Pad1)")
    (add_net "Net-(P2-Pad2)")
    (add_net "Net-(P3-Pad2)")
    (add_net "Net-(P6-Pad2)")
    (add_net "Net-(P7-Pad2)")
  )
  (net_class HVPower ""
    (clearance 1)
    (trace_width 3)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /B1)
    (add_net /B2)
    (add_net /HV)
    (add_net /OV)
  )
  (module Capacitors_ThroughHole:C_Rect_L41.5mm_W20.0mm_P37.50mm_MKS4 (layer F.Cu) (tedit 59C8EFC4)
    (at 162.433 84.074 90)
    (descr "C, Rect series, Radial, pin pitch=37.50mm, , length*width=41.5*20mm^2, Capacitor, http://www.wima.com/EN/WIMA_MKS_4.pdf")
    (tags "C Rect series Radial pin pitch 37.50mm  length 41.5mm width 20mm Capacitor")
    (fp_text reference C1 (at 18.796 0 90) (layer F.SilkS))
    (fp_text value C (at 18.75 11.31 90) (layer F.Fab) hide)
    (fp_text user %R (at 18.75 0 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.8 2.8) (drill 1.4) (layers *.Cu *.Mask)
      (net 17 /HV))
    (pad 2 thru_hole circle (at 37.5 0 90) (size 2.8 2.8) (drill 1.4) (layers *.Cu *.Mask)
      (net 18 /OV))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Rect_L41.5mm_W20.0mm_P37.50mm_MKS4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_ThroughHole:D_DO-35_SOD27_P10.16mm_Horizontal (layer F.Cu) (tedit 5921392E)
    (at 155.829 68.961 270)
    (descr "D, DO-35_SOD27 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "D DO-35_SOD27 series Axial Horizontal pin pitch 10.16mm  length 4mm diameter 2mm")
    (fp_text reference D1 (at 5.08 -2.06 270) (layer F.SilkS))
    (fp_text value D_Zener (at 5.08 2.06 270) (layer F.Fab))
    (fp_text user %R (at 5.08 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-35_SOD27_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_ThroughHole:D_DO-35_SOD27_P10.16mm_Horizontal (layer F.Cu) (tedit 5921392E)
    (at 160.147 68.961 270)
    (descr "D, DO-35_SOD27 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "D DO-35_SOD27 series Axial Horizontal pin pitch 10.16mm  length 4mm diameter 2mm")
    (fp_text reference D2 (at 5.08 -2.06 270) (layer F.SilkS))
    (fp_text value D_Zener (at 5.08 2.06 270) (layer F.Fab))
    (fp_text user %R (at 5.08 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 "Net-(D2-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-35_SOD27_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_ThroughHole:D_DO-35_SOD27_P10.16mm_Horizontal (layer F.Cu) (tedit 59C90AAF)
    (at 155.829 61.849 90)
    (descr "D, DO-35_SOD27 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "D DO-35_SOD27 series Axial Horizontal pin pitch 10.16mm  length 4mm diameter 2mm")
    (fp_text reference D3 (at 5.08 2.032 90) (layer F.SilkS))
    (fp_text value D_Zener (at 5.08 2.06 90) (layer F.Fab))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 4 "Net-(D3-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(D3-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-35_SOD27_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_ThroughHole:D_DO-35_SOD27_P10.16mm_Horizontal (layer F.Cu) (tedit 59C90AA6)
    (at 160.401 61.849 90)
    (descr "D, DO-35_SOD27 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "D DO-35_SOD27 series Axial Horizontal pin pitch 10.16mm  length 4mm diameter 2mm")
    (fp_text reference D4 (at 5.08 2.159 90) (layer F.SilkS))
    (fp_text value D_Zener (at 5.08 2.06 90) (layer F.Fab))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(D4-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 5 "Net-(D3-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-35_SOD27_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_ThroughHole:D_DO-35_SOD27_P10.16mm_Horizontal (layer F.Cu) (tedit 5921392E)
    (at 168.656 68.961 270)
    (descr "D, DO-35_SOD27 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "D DO-35_SOD27 series Axial Horizontal pin pitch 10.16mm  length 4mm diameter 2mm")
    (fp_text reference D5 (at 5.08 -2.06 270) (layer F.SilkS))
    (fp_text value D_Zener (at 5.08 2.06 270) (layer F.Fab))
    (fp_text user %R (at 5.08 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 6 "Net-(D5-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(D5-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-35_SOD27_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_ThroughHole:D_DO-35_SOD27_P10.16mm_Horizontal (layer F.Cu) (tedit 5921392E)
    (at 164.719 68.961 270)
    (descr "D, DO-35_SOD27 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "D DO-35_SOD27 series Axial Horizontal pin pitch 10.16mm  length 4mm diameter 2mm")
    (fp_text reference D6 (at 5.08 -2.06 270) (layer F.SilkS))
    (fp_text value D_Zener (at 5.08 2.06 270) (layer F.Fab))
    (fp_text user %R (at 5.08 0 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 "Net-(D6-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0 270) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(D5-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-35_SOD27_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_ThroughHole:D_DO-35_SOD27_P10.16mm_Horizontal (layer F.Cu) (tedit 59C90A8F)
    (at 168.529 61.849 90)
    (descr "D, DO-35_SOD27 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "D DO-35_SOD27 series Axial Horizontal pin pitch 10.16mm  length 4mm diameter 2mm")
    (fp_text reference D7 (at 5.08 1.905 90) (layer F.SilkS))
    (fp_text value D_Zener (at 5.08 2.06 90) (layer F.Fab))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(D7-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(D7-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-35_SOD27_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_ThroughHole:D_DO-35_SOD27_P10.16mm_Horizontal (layer F.Cu) (tedit 59C90A9A)
    (at 164.719 61.849 90)
    (descr "D, DO-35_SOD27 series, Axial, Horizontal, pin pitch=10.16mm, , length*diameter=4*2mm^2, , http://www.diodes.com/_files/packages/DO-35.pdf")
    (tags "D DO-35_SOD27 series Axial Horizontal pin pitch 10.16mm  length 4mm diameter 2mm")
    (fp_text reference D8 (at 5.08 1.905 90) (layer F.SilkS))
    (fp_text value D_Zener (at 5.08 2.06 90) (layer F.Fab))
    (fp_text user %R (at 5.08 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 16 "Net-(D8-Pad1)"))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(D7-Pad2)"))
    (model ${KISYS3DMOD}/Diodes_THT.3dshapes/D_DO-35_SOD27_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wire_Pads:SolderWirePad_2x_1mmDrill (layer F.Cu) (tedit 59C8EE94)
    (at 144.272 90.17)
    (fp_text reference P1 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value HV1+ (at 0.381 2.921) (layer F.SilkS))
    (pad 1 thru_hole circle (at -1.905 0) (size 2.49936 2.49936) (drill 1.00076) (layers *.Cu *.Mask)
      (net 17 /HV))
    (pad 1 thru_hole circle (at 1.905 0) (size 2.49936 2.49936) (drill 1.00076) (layers *.Cu *.Mask)
      (net 17 /HV))
  )
  (module Connectors_Molex:Molex_KK-6410-02_02x2.54mm_Straight (layer F.Cu) (tedit 59C80822)
    (at 151.892 91.694)
    (descr "Connector Headers with Friction Lock, 22-27-2021, http://www.molex.com/pdm_docs/sd/022272021_sd.pdf")
    (tags "connector molex kk_6410 22-27-2021")
    (fp_text reference P2 (at 1 -4.5) (layer F.SilkS) hide)
    (fp_text value GDT1 (at 1.143 -4.191) (layer F.SilkS))
    (fp_text user %R (at 1.27 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 3 "Net-(D2-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 11 "Net-(P2-Pad2)"))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_KK-6410-02_02x2.54mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Molex:Molex_KK-6410-02_02x2.54mm_Straight (layer F.Cu) (tedit 59C8EE5B)
    (at 152.019 39.37)
    (descr "Connector Headers with Friction Lock, 22-27-2021, http://www.molex.com/pdm_docs/sd/022272021_sd.pdf")
    (tags "connector molex kk_6410 22-27-2021")
    (fp_text reference P3 (at 1 -4.5) (layer F.SilkS) hide)
    (fp_text value GDT2 (at 1.27 4.5) (layer F.SilkS))
    (fp_text user %R (at 1.27 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 15 "Net-(D4-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 12 "Net-(P3-Pad2)"))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_KK-6410-02_02x2.54mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wire_Pads:SolderWirePad_2x_1mmDrill (layer F.Cu) (tedit 59C8EE82)
    (at 180.34 40.513)
    (fp_text reference P4 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value OV1 (at 0.127 2.794) (layer F.SilkS))
    (pad 1 thru_hole circle (at -1.905 0) (size 2.49936 2.49936) (drill 1.00076) (layers *.Cu *.Mask)
      (net 18 /OV))
    (pad 1 thru_hole circle (at 1.905 0) (size 2.49936 2.49936) (drill 1.00076) (layers *.Cu *.Mask)
      (net 18 /OV))
  )
  (module Wire_Pads:SolderWirePad_2x_1mmDrill (layer F.Cu) (tedit 59C8F052)
    (at 144.272 65.532)
    (fp_text reference P5 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value B1 (at 0 2.794) (layer F.SilkS))
    (pad 1 thru_hole circle (at -1.905 0) (size 2.49936 2.49936) (drill 1.00076) (layers *.Cu *.Mask)
      (net 20 /B1))
    (pad 1 thru_hole circle (at 1.905 0) (size 2.49936 2.49936) (drill 1.00076) (layers *.Cu *.Mask)
      (net 20 /B1))
  )
  (module Connectors_Molex:Molex_KK-6410-02_02x2.54mm_Straight (layer F.Cu) (tedit 59C807F6)
    (at 169.799 91.821)
    (descr "Connector Headers with Friction Lock, 22-27-2021, http://www.molex.com/pdm_docs/sd/022272021_sd.pdf")
    (tags "connector molex kk_6410 22-27-2021")
    (fp_text reference P6 (at 1 -4.5) (layer F.SilkS) hide)
    (fp_text value GDT3 (at 1.143 -4.318) (layer F.SilkS))
    (fp_text user %R (at 1.27 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 8 "Net-(D6-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 13 "Net-(P6-Pad2)"))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_KK-6410-02_02x2.54mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Molex:Molex_KK-6410-02_02x2.54mm_Straight (layer F.Cu) (tedit 59C8EE63)
    (at 169.799 39.37)
    (descr "Connector Headers with Friction Lock, 22-27-2021, http://www.molex.com/pdm_docs/sd/022272021_sd.pdf")
    (tags "connector molex kk_6410 22-27-2021")
    (fp_text reference P7 (at 1 -4.5) (layer F.SilkS) hide)
    (fp_text value GDT4 (at 1.27 4.5) (layer F.SilkS))
    (fp_text user %R (at 1.27 0) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 16 "Net-(D8-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0) (size 2 2.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 14 "Net-(P7-Pad2)"))
    (model ${KISYS3DMOD}/Connectors_Molex.3dshapes/Molex_KK-6410-02_02x2.54mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wire_Pads:SolderWirePad_2x_1mmDrill (layer F.Cu) (tedit 59C8EE8B)
    (at 180.34 90.17)
    (fp_text reference P8 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value HV+ (at 0.381 2.921) (layer F.SilkS))
    (pad 1 thru_hole circle (at -1.905 0) (size 2.49936 2.49936) (drill 1.00076) (layers *.Cu *.Mask)
      (net 17 /HV))
    (pad 1 thru_hole circle (at 1.905 0) (size 2.49936 2.49936) (drill 1.00076) (layers *.Cu *.Mask)
      (net 17 /HV))
  )
  (module Wire_Pads:SolderWirePad_2x_1mmDrill (layer F.Cu) (tedit 59C8F03C)
    (at 180.34 65.659)
    (fp_text reference P9 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value B2 (at 0 2.413) (layer F.SilkS))
    (pad 1 thru_hole circle (at -1.905 0) (size 2.49936 2.49936) (drill 1.00076) (layers *.Cu *.Mask)
      (net 19 /B2))
    (pad 1 thru_hole circle (at 1.905 0) (size 2.49936 2.49936) (drill 1.00076) (layers *.Cu *.Mask)
      (net 19 /B2))
  )
  (module Wire_Pads:SolderWirePad_2x_1mmDrill (layer F.Cu) (tedit 59C8EE7C)
    (at 144.272 40.513)
    (fp_text reference P10 (at 0 -3.81) (layer F.SilkS) hide)
    (fp_text value 0V (at -0.127 2.794) (layer F.SilkS))
    (pad 1 thru_hole circle (at -1.905 0) (size 2.49936 2.49936) (drill 1.00076) (layers *.Cu *.Mask)
      (net 18 /OV))
    (pad 1 thru_hole circle (at 1.905 0) (size 2.49936 2.49936) (drill 1.00076) (layers *.Cu *.Mask)
      (net 18 /OV))
  )
  (module TO_SOT_Packages_THT:TO-247_TO-3P_Vertical (layer F.Cu) (tedit 59C808EE)
    (at 144.272 84.074 90)
    (descr "TO-247, Vertical, RM 5.45mm, TO-3P")
    (tags "TO-247 Vertical RM 5.45mm TO-3P")
    (fp_text reference Q1 (at 5.45 -3.45 90) (layer F.SilkS))
    (fp_text value 10R (at 7.239 6.604 90) (layer F.SilkS))
    (fp_text user %R (at 5.45 -3.45 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.5 4.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 2 thru_hole oval (at 5.461 0.254 90) (size 2.5 4.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 17 /HV))
    (pad 3 thru_hole oval (at 10.9 0 90) (size 2.5 4.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 20 /B1))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-247_TO-3P_Vertical.wrl
      (at (xyz 0.212598 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-247_TO-3P_Vertical (layer F.Cu) (tedit 59C808FA)
    (at 144.526 58.674 90)
    (descr "TO-247, Vertical, RM 5.45mm, TO-3P")
    (tags "TO-247 Vertical RM 5.45mm TO-3P")
    (fp_text reference Q2 (at 5.45 -3.45 90) (layer F.SilkS))
    (fp_text value 10R (at 4.572 6.096 90) (layer F.SilkS))
    (fp_text user %R (at 5.45 -3.45 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.5 4.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 4 "Net-(D3-Pad1)"))
    (pad 2 thru_hole oval (at 5.45 0 90) (size 2.5 4.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 20 /B1))
    (pad 3 thru_hole oval (at 10.9 0 90) (size 2.5 4.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 18 /OV))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-247_TO-3P_Vertical.wrl
      (at (xyz 0.212598 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-247_TO-3P_Vertical (layer F.Cu) (tedit 59C808E5)
    (at 180.594 73.279 270)
    (descr "TO-247, Vertical, RM 5.45mm, TO-3P")
    (tags "TO-247 Vertical RM 5.45mm TO-3P")
    (fp_text reference Q3 (at 5.45 -3.45 270) (layer F.SilkS))
    (fp_text value 10R (at 3.683 6.985 270) (layer F.SilkS))
    (fp_text user %R (at 5.45 -3.45 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.5 4.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 6 "Net-(D5-Pad1)"))
    (pad 2 thru_hole oval (at 5.45 0 270) (size 2.5 4.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 17 /HV))
    (pad 3 thru_hole oval (at 10.9 0 270) (size 2.5 4.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 19 /B2))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-247_TO-3P_Vertical.wrl
      (at (xyz 0.212598 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-247_TO-3P_Vertical (layer F.Cu) (tedit 59C80908)
    (at 180.34 47.879 270)
    (descr "TO-247, Vertical, RM 5.45mm, TO-3P")
    (tags "TO-247 Vertical RM 5.45mm TO-3P")
    (fp_text reference Q4 (at 5.45 -3.45 270) (layer F.SilkS))
    (fp_text value 10R (at 6.223 6.731 270) (layer F.SilkS))
    (fp_text user %R (at 5.45 -3.45 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 2.5 4.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 9 "Net-(D7-Pad1)"))
    (pad 2 thru_hole oval (at 5.45 0 270) (size 2.5 4.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 19 /B2))
    (pad 3 thru_hole oval (at 10.9 0 270) (size 2.5 4.5) (drill 1.5) (layers *.Cu *.Mask)
      (net 18 /OV))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-247_TO-3P_Vertical.wrl
      (at (xyz 0.212598 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0411_L9.9mm_D3.6mm_P15.24mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 151.003 69.469 270)
    (descr "Resistor, Axial_DIN0411 series, Axial, Horizontal, pin pitch=15.24mm, 1W = 1/1W, length*diameter=9.9*3.6mm^2")
    (tags "Resistor Axial_DIN0411 series Axial Horizontal pin pitch 15.24mm 1W = 1/1W length 9.9mm diameter 3.6mm")
    (fp_text reference R1 (at 7.62 -2.86 270) (layer F.SilkS))
    (fp_text value R (at 7.62 2.86 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 2 thru_hole oval (at 15.24 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 11 "Net-(P2-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0411_L9.9mm_D3.6mm_P15.24mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0411_L9.9mm_D3.6mm_P15.24mm_Horizontal (layer F.Cu) (tedit 59C8EEF6)
    (at 150.749 61.595 90)
    (descr "Resistor, Axial_DIN0411 series, Axial, Horizontal, pin pitch=15.24mm, 1W = 1/1W, length*diameter=9.9*3.6mm^2")
    (tags "Resistor Axial_DIN0411 series Axial Horizontal pin pitch 15.24mm 1W = 1/1W length 9.9mm diameter 3.6mm")
    (fp_text reference R2 (at 7.747 2.921 90) (layer F.SilkS))
    (fp_text value R (at 7.62 2.86 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 4 "Net-(D3-Pad1)"))
    (pad 2 thru_hole oval (at 15.24 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 12 "Net-(P3-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0411_L9.9mm_D3.6mm_P15.24mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0411_L9.9mm_D3.6mm_P15.24mm_Horizontal (layer F.Cu) (tedit 5874F706)
    (at 173.482 69.342 270)
    (descr "Resistor, Axial_DIN0411 series, Axial, Horizontal, pin pitch=15.24mm, 1W = 1/1W, length*diameter=9.9*3.6mm^2")
    (tags "Resistor Axial_DIN0411 series Axial Horizontal pin pitch 15.24mm 1W = 1/1W length 9.9mm diameter 3.6mm")
    (fp_text reference R3 (at 7.62 -2.86 270) (layer F.SilkS))
    (fp_text value R (at 7.62 2.86 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 6 "Net-(D5-Pad1)"))
    (pad 2 thru_hole oval (at 15.24 0 270) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 13 "Net-(P6-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0411_L9.9mm_D3.6mm_P15.24mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_ThroughHole:R_Axial_DIN0411_L9.9mm_D3.6mm_P15.24mm_Horizontal (layer F.Cu) (tedit 59C8EEEE)
    (at 173.482 61.468 90)
    (descr "Resistor, Axial_DIN0411 series, Axial, Horizontal, pin pitch=15.24mm, 1W = 1/1W, length*diameter=9.9*3.6mm^2")
    (tags "Resistor Axial_DIN0411 series Axial Horizontal pin pitch 15.24mm 1W = 1/1W length 9.9mm diameter 3.6mm")
    (fp_text reference R4 (at 9.017 2.667 90) (layer F.SilkS))
    (fp_text value R (at 7.62 2.86 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 9 "Net-(D7-Pad1)"))
    (pad 2 thru_hole oval (at 15.24 0 90) (size 2.4 2.4) (drill 1.2) (layers *.Cu *.Mask)
      (net 14 "Net-(P7-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0411_L9.9mm_D3.6mm_P15.24mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_DIN965 (layer F.Cu) (tedit 59C807DA)
    (at 162.433 90.17)
    (descr "Mounting Hole 3.2mm, no annular, M3, DIN965")
    (tags "mounting hole 3.2mm no annular m3 din965")
    (fp_text reference MK1 (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value Mounting_Hole (at 0 3.8) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_DIN965 (layer F.Cu) (tedit 59C80978)
    (at 162.306 40.64)
    (descr "Mounting Hole 3.2mm, no annular, M3, DIN965")
    (tags "mounting hole 3.2mm no annular m3 din965")
    (fp_text reference MK2 (at 0 -3.8) (layer F.SilkS) hide)
    (fp_text value Mounting_Hole (at 0 3.8) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 3.2 3.2) (drill 3.2) (layers *.Cu *.Mask))
  )
  (module djwLibrary:netjoin (layer F.Cu) (tedit 59C8EFAB)
    (at 149.987 64.008 180)
    (fp_text reference U1 (at 0 0.5 180) (layer F.SilkS) hide)
    (fp_text value netjoin (at 0 -0.5 180) (layer F.Fab))
    (pad 1 smd trapezoid (at -2.54 -1.524 180) (size 0.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D2-Pad1)"))
    (pad 2 smd trapezoid (at 1.905 -1.524 180) (size 0.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 20 /B1))
  )
  (module djwLibrary:netjoin (layer F.Cu) (tedit 59C8EFA3)
    (at 172.72 67.183)
    (fp_text reference U3 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value netjoin (at 0 -0.5) (layer F.Fab))
    (pad 1 smd trapezoid (at -2.54 -1.524) (size 0.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D6-Pad1)"))
    (pad 2 smd trapezoid (at 1.905 -1.524) (size 0.2 0.2) (layers F.Cu F.Paste F.Mask)
      (net 19 /B2))
  )
  (module djwLibrary:netjoin-B (layer F.Cu) (tedit 59C8EF56)
    (at 166.243 57.531 90)
    (fp_text reference U4 (at -4.318 0.508 90) (layer F.SilkS) hide)
    (fp_text value netjoin (at 0 -0.5 90) (layer F.Fab))
    (pad 1 smd trapezoid (at -2.54 -1.524 90) (size 0.2 0.2) (layers B.Cu F.Paste F.Mask)
      (net 16 "Net-(D8-Pad1)"))
    (pad 2 smd trapezoid (at 1.905 -1.524 90) (size 0.2 0.2) (layers B.Cu F.Paste F.Mask)
      (net 18 /OV))
  )
  (module djwLibrary:netjoin-B (layer F.Cu) (tedit 59C8EF4E)
    (at 161.925 57.531 90)
    (fp_text reference U2 (at -4.445 0.635 90) (layer F.SilkS) hide)
    (fp_text value netjoin (at 0 -0.5 90) (layer F.Fab))
    (pad 1 smd trapezoid (at -2.54 -1.524 90) (size 0.2 0.2) (layers B.Cu F.Paste F.Mask)
      (net 15 "Net-(D4-Pad1)"))
    (pad 2 smd trapezoid (at 1.905 -1.524 90) (size 0.2 0.2) (layers B.Cu F.Paste F.Mask)
      (net 18 /OV))
  )
  (gr_text www.extremeelectronics.co.uk (at 185.674 54.102 90) (layer F.SilkS))
  (gr_text "IGBT Bridge V3" (at 139.192 45.593 90) (layer F.SilkS))
  (gr_line (start 137.414 95.631) (end 137.414 35.814) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 187.579 35.814) (end 187.579 95.631) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 187.579 95.631) (end 137.414 95.631) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 137.414 35.814) (end 187.579 35.814) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 17) (net_name /HV) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 137.668 75.692) (xy 187.198 75.565) (xy 187.198 95.377) (xy 137.668 95.25) (xy 137.795 75.692)
      )
    )
  )
  (zone (net 18) (net_name /OV) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 137.795 36.195) (xy 187.198 36.068) (xy 187.198 55.88) (xy 137.795 55.88) (xy 137.922 36.195)
      )
    )
  )
  (zone (net 20) (net_name /B1) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 137.414 62.992) (xy 149.352 62.992) (xy 149.352 73.914) (xy 137.541 73.914) (xy 137.414 63.119)
      )
    )
  )
  (zone (net 19) (net_name /B2) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 187.071 63.119) (xy 174.371 63.119) (xy 174.371 73.914) (xy 187.071 73.914)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 165.354 43.688) (xy 159.258 43.688) (xy 159.258 37.592) (xy 165.354 37.592)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 165.608 93.218) (xy 159.385 93.218) (xy 159.385 87.122) (xy 165.608 87.122)
      )
    )
  )
  (zone (net 20) (net_name /B1) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 137.414 62.992) (xy 149.352 62.992) (xy 149.352 73.914) (xy 137.414 73.914)
      )
    )
  )
  (zone (net 19) (net_name /B2) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 174.371 63.119) (xy 187.198 63.119) (xy 187.198 73.914) (xy 174.371 73.914)
      )
    )
  )
)
