(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 44)
    (no_connects 1)
    (area 64.696768 31.97616 178.510001 123.265001)
    (thickness 1.6)
    (drawings 94)
    (tracks 144)
    (zones 0)
    (modules 18)
    (nets 58)
  )
  (page USLetter)
  (title_block
    (title "Project Title")
  )
  (layers
    (0 F.Cu jumper)
    (31 B.Cu signal hide)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.1524)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.1524)
    (edge_width 0.1524)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.3556)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0)
    (uvia_min_drill 0)
    (pcb_text_width 0.1524)
    (pcb_text_size 1.016 1.016)
    (mod_edge_width 0.1524)
    (mod_text_size 1.016 1.016)
    (mod_text_width 0.1524)
    (pad_size 0.2 0.2)
    (pad_drill 0)
    (pad_to_mask_clearance 0.0762)
    (solder_mask_min_width 0.1016)
    (pad_to_paste_clearance -0.0762)
    (aux_axis_origin 196.5452 123.5456)
    (grid_origin -114.10188 32.77616)
    (visible_elements FFFFEFFF)
    (pcbplotparams
      (layerselection 0x310fc_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerbers))
  )
  (net 0 "")
  (net 1 "Net-(J1-Pad2)")
  (net 2 "Net-(J1-Pad1)")
  (net 3 "Net-(J1-Pad3)")
  (net 4 "Net-(J1-Pad4)")
  (net 5 "Net-(J1-Pad5)")
  (net 6 "Net-(J1-Pad6)")
  (net 7 "Net-(J1-Pad7)")
  (net 8 "Net-(J1-Pad8)")
  (net 9 "Net-(J1-Pad9)")
  (net 10 "Net-(J1-Pad10)")
  (net 11 "Net-(J1-Pad12)")
  (net 12 "Net-(J1-Pad18)")
  (net 13 "Net-(J1-Pad19)")
  (net 14 "Net-(J1-Pad20)")
  (net 15 "Net-(J1-Pad21)")
  (net 16 "Net-(J1-Pad22)")
  (net 17 "Net-(J1-Pad23)")
  (net 18 "Net-(C2-Pad1)")
  (net 19 "Net-(C2-Pad2)")
  (net 20 VGH)
  (net 21 PRVGL)
  (net 22 VGL)
  (net 23 VDD)
  (net 24 VSH)
  (net 25 VGH2)
  (net 26 VSL)
  (net 27 VCOM)
  (net 28 GDR)
  (net 29 RESE)
  (net 30 BUSY)
  (net 31 ^RES)
  (net 32 ^D/C)
  (net 33 ^CS)
  (net 34 SCK)
  (net 35 DOUT)
  (net 36 VPP)
  (net 37 VDDIO)
  (net 38 "Net-(J1-Pad0)")
  (net 39 "Net-(J1-PadPGM)")
  (net 40 "Net-(J1-PadDAC)")
  (net 41 "Net-(J1-Pad3V2)")
  (net 42 "Net-(J1-PadVIN)")
  (net 43 "Net-(J1-PadVBAT)")
  (net 44 GND)
  (net 45 "Net-(J2-Pad2)")
  (net 46 "Net-(J2-Pad1)")
  (net 47 "Net-(J2-Pad3)")
  (net 48 "Net-(J2-Pad4)")
  (net 49 "Net-(J2-Pad5)")
  (net 50 "Net-(J2-Pad30)")
  (net 51 "Net-(J2-Pad31)")
  (net 52 "Net-(J2-Pad32)")
  (net 53 "Net-(J2-Pad33)")
  (net 54 "Net-(J2-Pad34)")
  (net 55 "Net-(J2-Pad6)")
  (net 56 "Net-(J2-Pad11)")
  (net 57 "Net-(J2-Pad12)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.3556)
    (uvia_drill 0.254)
    (add_net BUSY)
    (add_net DOUT)
    (add_net GDR)
    (add_net GND)
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(J1-Pad0)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad18)")
    (add_net "Net-(J1-Pad19)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad20)")
    (add_net "Net-(J1-Pad21)")
    (add_net "Net-(J1-Pad22)")
    (add_net "Net-(J1-Pad23)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad3V2)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J1-Pad9)")
    (add_net "Net-(J1-PadDAC)")
    (add_net "Net-(J1-PadPGM)")
    (add_net "Net-(J1-PadVBAT)")
    (add_net "Net-(J1-PadVIN)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad11)")
    (add_net "Net-(J2-Pad12)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J2-Pad3)")
    (add_net "Net-(J2-Pad30)")
    (add_net "Net-(J2-Pad31)")
    (add_net "Net-(J2-Pad32)")
    (add_net "Net-(J2-Pad33)")
    (add_net "Net-(J2-Pad34)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J2-Pad6)")
    (add_net PRVGL)
    (add_net RESE)
    (add_net SCK)
    (add_net VCOM)
    (add_net VDD)
    (add_net VDDIO)
    (add_net VGH)
    (add_net VGH2)
    (add_net VGL)
    (add_net VPP)
    (add_net VSH)
    (add_net VSL)
    (add_net ^CS)
    (add_net ^D/C)
    (add_net ^RES)
  )
  (module hirose-34pos-bigger-gnd-pads:CONN-HEADER-FH34SRJ-34S-0.5SH-BIG-GND (layer F.Cu) (tedit 58E8619F)
    (at 74.49812 60.37616 90)
    (fp_text reference J2 (at -0.225 -0.325 270) (layer F.Fab))
    (fp_text value HEADER-FEMALE-34POS-FFC-SMT-1x34-P0.5MM (at 0 2.9 90) (layer F.Fab) hide)
    (fp_text user %R (at -10.425 -0.075 180) (layer F.SilkS))
    (pad 2 smd rect (at 9.652 -1.778 180) (size 2 2) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(J2-Pad2)"))
    (pad 1 smd rect (at -8.225 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 46 "Net-(J2-Pad1)"))
    (pad 2 smd rect (at -7.725 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 45 "Net-(J2-Pad2)"))
    (pad 3 smd rect (at -7.225 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(J2-Pad3)"))
    (pad 4 smd rect (at -6.725 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(J2-Pad4)"))
    (pad 5 smd rect (at -6.225 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(J2-Pad5)"))
    (pad 6 smd rect (at -5.725 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 55 "Net-(J2-Pad6)"))
    (pad 7 smd rect (at -5.225 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 28 GDR))
    (pad 8 smd rect (at -4.725 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 29 RESE))
    (pad 9 smd rect (at -4.225 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 22 VGL))
    (pad 10 smd rect (at -3.725 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 20 VGH))
    (pad 11 smd rect (at -3.225 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 56 "Net-(J2-Pad11)"))
    (pad 12 smd rect (at -2.725 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 57 "Net-(J2-Pad12)"))
    (pad 13 smd rect (at -2.225 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 44 GND))
    (pad 14 smd rect (at -1.725 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 30 BUSY))
    (pad 15 smd rect (at -1.225 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 31 ^RES))
    (pad 16 smd rect (at -0.725 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 32 ^D/C))
    (pad 17 smd rect (at -0.225 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 33 ^CS))
    (pad 18 smd rect (at 0.275 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 34 SCK))
    (pad 19 smd rect (at 0.775 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 35 DOUT))
    (pad 20 smd rect (at 1.275 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 37 VDDIO))
    (pad 21 smd rect (at 1.775 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 37 VDDIO))
    (pad 22 smd rect (at 2.275 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 44 GND))
    (pad 23 smd rect (at 2.775 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 23 VDD))
    (pad 24 smd rect (at 3.275 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 36 VPP))
    (pad 25 smd rect (at 3.775 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 24 VSH))
    (pad 26 smd rect (at 4.275 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 25 VGH2))
    (pad 27 smd rect (at 4.775 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 26 VSL))
    (pad 28 smd rect (at 5.275 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 21 PRVGL))
    (pad 29 smd rect (at 5.775 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 27 VCOM))
    (pad 30 smd rect (at 6.275 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(J2-Pad30)"))
    (pad 31 smd rect (at 6.775 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(J2-Pad31)"))
    (pad 32 smd rect (at 7.275 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(J2-Pad32)"))
    (pad 33 smd rect (at 7.775 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(J2-Pad33)"))
    (pad 34 smd rect (at 8.275 1.175 180) (size 0.8 0.3) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(J2-Pad34)"))
    (pad e smd rect (at -9.652 -1.778 180) (size 2 2) (layers F.Cu F.Paste F.Mask))
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58EB4E25)
    (at 86.05812 70.31616 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C5 (at 1.278 1.726 180) (layer F.SilkS))
    (fp_text value CAP-CER-1UF (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 44 GND))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 22 VGL))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58EB4E0C)
    (at 129.90312 43.92616 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at -0.845 -2.19 180) (layer F.SilkS))
    (fp_text value CAP-CER-1UF (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 44 GND))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 37 VDDIO))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58EB4E5F)
    (at 79.44612 76.46416 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at -3.048 0 360) (layer F.SilkS))
    (fp_text value CAP-CER-2.2UF (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(C2-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58EB4E1C)
    (at 86.05012 65.28816 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at -3.556 0 180) (layer F.SilkS))
    (fp_text value CAP-CER-1UF (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 44 GND))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 20 VGH))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58EB4DE7)
    (at 110.20112 42.72916 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C4 (at -3.737 0.063 180) (layer F.SilkS))
    (fp_text value CAP-CER-1UF (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 44 GND))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 21 PRVGL))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58EB4E14)
    (at 97.22612 57.66816 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C6 (at -3.556 0 180) (layer F.SilkS))
    (fp_text value CAP-CER-1UF (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 44 GND))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 23 VDD))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58EB4E04)
    (at 110.39412 49.80216 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C7 (at -3.654 0.106 180) (layer F.SilkS))
    (fp_text value CAP-CER-1UF (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 44 GND))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 24 VSH))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58EB4DFD)
    (at 110.35112 47.60416 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C8 (at -3.647 0.038 180) (layer F.SilkS))
    (fp_text value CAP-CER-1UF (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 44 GND))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 25 VGH2))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58EB4DE0)
    (at 110.20112 40.35416 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C9 (at -3.717 0.058 180) (layer F.SilkS))
    (fp_text value CAP-CER-1UF (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 44 GND))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 27 VCOM))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58EB4DF3)
    (at 110.25112 45.05416 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C10 (at -4.157 0.048 180) (layer F.SilkS))
    (fp_text value CAP-CER-1UF (at 0 2.1 180) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 44 GND))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 26 VSL))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:SOD-123 (layer F.Cu) (tedit 58EB4E4B)
    (at 75.15812 76.83616 90)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D1 (at -3.438 -0.03 180) (layer F.SilkS))
    (fp_text value DIODE (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.635 0 90) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 44 GND))
    (pad 2 smd rect (at 1.635 0 90) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C2-Pad1)"))
  )
  (module Diodes_SMD:SOD-123 (layer F.Cu) (tedit 58EB4E47)
    (at 83.00212 76.21016 270)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D2 (at 3.556 0 360) (layer F.SilkS))
    (fp_text value DIODE (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.635 0 270) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 20 VGH))
    (pad 2 smd rect (at 1.635 0 270) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(C2-Pad2)"))
  )
  (module Diodes_SMD:SOD-123 (layer F.Cu) (tedit 58EB4E55)
    (at 70.31812 76.79616 270)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D3 (at -3.126 0.016 360) (layer F.SilkS))
    (fp_text value DIODE (at 0 2.1 270) (layer F.Fab))
    (pad 1 smd rect (at -1.635 0 270) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1.635 0 270) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 21 PRVGL))
  )
  (module Wickerlib:TEENSY-3.2-SILK (layer F.Cu) (tedit 58E9D464)
    (at 161.99612 51.31816)
    (fp_text reference J1 (at -2 0 270) (layer F.Fab))
    (fp_text value TEENSY3.2-72MHz (at -2.54 20.32) (layer F.Fab) hide)
    (fp_text user VIN (at 8.382095 -10.16) (layer F.SilkS))
    (fp_text user %R (at 5.08 -12.7) (layer F.SilkS))
    (fp_text user AGND (at 9.144 -7.62) (layer F.SilkS))
    (fp_text user 3.3V (at 8.810666 -5.08) (layer F.SilkS))
    (fp_text user 23 (at 8.144 -2.54) (layer F.SilkS))
    (fp_text user 22 (at 8.144 0) (layer F.SilkS))
    (fp_text user 21 (at 8.144 2.54) (layer F.SilkS))
    (fp_text user 20 (at 8.144 5.08) (layer F.SilkS))
    (fp_text user 19 (at 8.144 7.62) (layer F.SilkS))
    (fp_text user 18 (at 8.144 10.16) (layer F.SilkS))
    (fp_text user 17 (at 8.144 12.7) (layer F.SilkS))
    (fp_text user 16 (at 8.144 15.24) (layer F.SilkS))
    (fp_text user 15 (at 8.144 17.78) (layer F.SilkS))
    (fp_text user 14 (at 8.144 20.32) (layer F.SilkS))
    (fp_text user 13 (at 8.144 22.86) (layer F.SilkS))
    (fp_text user 0 (at -12.668381 -7.62) (layer F.SilkS))
    (fp_text user GND (at -13.716 -10.16) (layer F.SilkS))
    (fp_text user VBAT (at -7.62 26.416 90) (layer F.SilkS))
    (fp_text user 3.3V (at -5.08 26.416 90) (layer F.SilkS))
    (fp_text user GND (at -2.54 26.416 90) (layer F.SilkS))
    (fp_text user PGM (at 0 26.416 90) (layer F.SilkS))
    (fp_text user DAC (at 2.54 26.416 90) (layer F.SilkS))
    (fp_text user 1 (at -12.668381 -5.08) (layer F.SilkS))
    (fp_text user 2 (at -12.668381 -2.54) (layer F.SilkS))
    (fp_text user 3 (at -12.668381 0) (layer F.SilkS))
    (fp_text user 4 (at -12.668381 2.54) (layer F.SilkS))
    (fp_text user 5 (at -12.668381 5.08) (layer F.SilkS))
    (fp_text user 6 (at -12.668381 7.62) (layer F.SilkS))
    (fp_text user 7 (at -12.668381 10.16) (layer F.SilkS))
    (fp_text user 8 (at -12.668381 12.7) (layer F.SilkS))
    (fp_text user 9 (at -12.668381 15.24) (layer F.SilkS))
    (fp_text user 10 (at -13.144571 17.78) (layer F.SilkS))
    (fp_text user 11 (at -13.144571 20.32) (layer F.SilkS))
    (fp_text user 12 (at -13.144571 22.86) (layer F.SilkS))
    (pad G1 thru_hole circle (at -10.16 -10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 44 GND))
    (pad 0 thru_hole circle (at -10.16 -7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 38 "Net-(J1-Pad0)"))
    (pad 1 thru_hole circle (at -10.16 -5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(J1-Pad1)"))
    (pad 2 thru_hole circle (at -10.16 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(J1-Pad2)"))
    (pad 3 thru_hole circle (at -10.16 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(J1-Pad3)"))
    (pad 4 thru_hole circle (at -10.16 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(J1-Pad4)"))
    (pad 5 thru_hole circle (at -10.16 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(J1-Pad5)"))
    (pad 6 thru_hole circle (at -10.16 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(J1-Pad6)"))
    (pad 7 thru_hole circle (at -10.16 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(J1-Pad7)"))
    (pad 8 thru_hole circle (at -10.16 12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(J1-Pad8)"))
    (pad 9 thru_hole circle (at -10.16 15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(J1-Pad9)"))
    (pad 10 thru_hole circle (at -10.16 17.78) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(J1-Pad10)"))
    (pad 11 thru_hole circle (at -10.16 20.32) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 35 DOUT))
    (pad 12 thru_hole circle (at -10.16 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(J1-Pad12)"))
    (pad VBAT thru_hole circle (at -7.62 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 43 "Net-(J1-PadVBAT)"))
    (pad 3V1 thru_hole circle (at -5.08 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 37 VDDIO))
    (pad G2 thru_hole circle (at -2.54 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 44 GND))
    (pad PGM thru_hole circle (at 0 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 39 "Net-(J1-PadPGM)"))
    (pad DAC thru_hole circle (at 2.54 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 40 "Net-(J1-PadDAC)"))
    (pad 13 thru_hole circle (at 5.08 22.86) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 34 SCK))
    (pad 16 thru_hole circle (at 5.08 15.24) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 32 ^D/C))
    (pad 3V2 thru_hole circle (at 5.08 -5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 41 "Net-(J1-Pad3V2)"))
    (pad 18 thru_hole circle (at 5.08 10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(J1-Pad18)"))
    (pad 17 thru_hole circle (at 5.08 12.7) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 33 ^CS))
    (pad AG thru_hole circle (at 5.08 -7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 44 GND))
    (pad 22 thru_hole circle (at 5.08 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(J1-Pad22)"))
    (pad VIN thru_hole circle (at 5.08 -10.16) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 42 "Net-(J1-PadVIN)"))
    (pad 21 thru_hole circle (at 5.08 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(J1-Pad21)"))
    (pad 20 thru_hole circle (at 5.08 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(J1-Pad20)"))
    (pad 19 thru_hole circle (at 5.08 7.62) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(J1-Pad19)"))
    (pad 23 thru_hole circle (at 5.08 -2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(J1-Pad23)"))
    (pad 14 thru_hole circle (at 5.08 20.32) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 31 ^RES))
    (pad 15 thru_hole circle (at 5.08 17.78) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 30 BUSY))
  )
  (module Inductors:Inductor_1212 (layer F.Cu) (tedit 5652586A)
    (at 104.61812 75.66616 180)
    (attr smd)
    (fp_text reference L1 (at 0 2.75 180) (layer F.SilkS))
    (fp_text value INDUCTOR (at 0 -2.75 180) (layer F.Fab))
    (pad 1 smd rect (at -1.75 0 180) (size 2.5 2.5) (layers F.Cu F.Paste F.Mask)
      (net 37 VDDIO))
    (pad 2 smd rect (at 1.75 0 180) (size 2.5 2.5) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(C2-Pad2)"))
  )
  (module TO_SOT_Packages_SMD:SOT-23_Handsoldering (layer F.Cu) (tedit 54E9291B)
    (at 95.93812 74.25616 180)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 0 -3.81 180) (layer F.SilkS))
    (fp_text value Q_NMOS_GDS (at 0 3.81 180) (layer F.Fab))
    (pad 1 smd rect (at -0.95 1.50114 180) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 28 GDR))
    (pad 2 smd rect (at 0.95 1.50114 180) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 29 RESE))
    (pad 3 smd rect (at 0 -1.50114 180) (size 0.8001 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(C2-Pad2)"))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-23_Handsoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 96.27812 65.30616)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 -2.1) (layer F.SilkS))
    (fp_text value "2.2R 1%" (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 29 RESE))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 44 GND))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "Drew Fustini\ndrew@oshpark.com" (at 160.98012 56.39816 270) (layer B.SilkS))
  (gr_text github.com/pdp7/kicad-teensy-epaper (at 155.90012 56.39816 270) (layer B.SilkS))
  (gr_line (start 78.64812 33.72616) (end 86.22312 33.72616) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 86.22312 33.72616) (end 86.94812 34.45116) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 86.94812 34.45116) (end 86.94812 35.75116) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 86.94812 35.75116) (end 86.94812 36.12616) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 86.94812 36.12616) (end 86.17312 36.90116) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 86.17312 36.90116) (end 78.22312 36.90116) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 78.22312 36.90116) (end 77.59812 36.27616) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 77.59812 36.27616) (end 77.59812 34.30116) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 77.59812 34.30116) (end 78.17312 33.72616) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 78.17312 33.72616) (end 79.14812 33.72616) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 156.62312 33.82616) (end 157.59812 33.82616) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 156.04812 34.40116) (end 156.62312 33.82616) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 156.04812 36.37616) (end 156.04812 34.40116) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 156.67312 37.00116) (end 156.04812 36.37616) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 164.62312 37.00116) (end 156.67312 37.00116) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 165.39812 36.22616) (end 164.62312 37.00116) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 165.39812 35.85116) (end 165.39812 36.22616) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 165.39812 34.55116) (end 165.39812 35.85116) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 164.67312 33.82616) (end 165.39812 34.55116) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 157.09812 33.82616) (end 164.67312 33.82616) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_circle (center 70.02312 37.37616) (end 68.29812 34.17616) (layer Edge.Cuts) (width 0.1524))
  (gr_circle (center 69.89812 84.27616) (end 68.17312 81.07616) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 173.34812 59.65116) (end 173.32312 59.65116) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 173.34812 60.12616) (end 173.34812 59.65116) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 173.04812 60.42616) (end 173.34812 60.12616) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 171.92312 60.42616) (end 173.04812 60.42616) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 171.67312 60.17616) (end 171.92312 60.42616) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 171.67312 56.60116) (end 171.67312 60.17616) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 171.89812 56.37616) (end 171.67312 56.60116) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 172.14812 56.37616) (end 171.89812 56.37616) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 172.34812 56.37616) (end 172.14812 56.37616) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 173.14812 56.37616) (end 172.34812 56.37616) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 173.32312 56.55116) (end 173.14812 56.37616) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 173.32312 59.75116) (end 173.32312 56.55116) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 172.84812 37.90116) (end 172.84812 34.70116) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 172.84812 34.70116) (end 172.67312 34.52616) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 172.67312 34.52616) (end 171.87312 34.52616) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 171.87312 34.52616) (end 171.67312 34.52616) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 171.67312 34.52616) (end 171.42312 34.52616) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 171.42312 34.52616) (end 171.19812 34.75116) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 171.19812 34.75116) (end 171.19812 38.32616) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 171.19812 38.32616) (end 171.44812 38.57616) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 171.44812 38.57616) (end 172.57312 38.57616) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 172.57312 38.57616) (end 172.87312 38.27616) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 172.87312 38.27616) (end 172.87312 37.80116) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 172.87312 37.80116) (end 172.84812 37.80116) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 173.12312 86.22616) (end 173.09812 86.22616) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 173.12312 86.70116) (end 173.12312 86.22616) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 172.82312 87.00116) (end 173.12312 86.70116) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 171.69812 87.00116) (end 172.82312 87.00116) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 171.44812 86.75116) (end 171.69812 87.00116) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 171.44812 83.17616) (end 171.44812 86.75116) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 171.67312 82.95116) (end 171.44812 83.17616) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 171.92312 82.95116) (end 171.67312 82.95116) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 172.12312 82.95116) (end 171.92312 82.95116) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 172.92312 82.95116) (end 172.12312 82.95116) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 173.09812 83.12616) (end 172.92312 82.95116) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 173.09812 86.32616) (end 173.09812 83.12616) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 64.77312 34.00116) (end 64.77312 87.17616) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 66.74812 32.12616) (end 68.19812 32.12616) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_arc (start 66.67312 34.02616) (end 64.77312 34.00116) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_arc (start 66.84812 87.25116) (end 66.82312 89.32616) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 170.89812 32.12616) (end 67.59812 32.12616) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 170.89812 89.32616) (end 66.67312 89.32616) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 175.19812 35.45116) (end 175.17312 35.47616) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 175.19812 85.57616) (end 175.19812 35.45116) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_arc (start 171.17312 85.35116) (end 175.17312 85.60116) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_arc (start 171.26212 36.02916) (end 170.90212 32.11916) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_text "https://github.com/pdp7/kicad-teensy-epaper\n2017-04-10" (at 118.66812 85.95616 180) (layer B.SilkS))
  (gr_text "https://github.com/pdp7/kicad-teensy-epaper\n2017-04-10" (at 117.44812 36.61616) (layer B.SilkS))
  (gr_line (start 66.84612 72.05016) (end 69.38612 72.05016) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 66.84612 48.68216) (end 66.84612 72.05016) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 69.38612 48.68216) (end 66.84612 48.68216) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_line (start 69.38612 72.05016) (end 69.38612 48.68216) (angle 90) (layer Edge.Cuts) (width 0.1524))
  (gr_text "https://github.com/pdp7/kicad-teensy-epaper\n2017-04-10" (at 95.75812 85.21616) (layer F.SilkS))
  (zone (net 44) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 174.92312 34.60116) (xy 175.24805 89.27616) (xy 65.02312 89.27616) (xy 64.99812 78.95116) (xy 64.94812 32.12616)
        (xy 171.34812 32.00116) (xy 174.44812 32.82616)
      )
    )
  )
  (zone (net 37) (net_name VDDIO) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 175.74812 37.65116) (xy 175.22312 89.25116) (xy 65.02312 89.25116) (xy 64.92312 32.25116) (xy 173.27312 31.97616)
      )
    )
  )
)
