(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "USLetter")
  (title_block
    (title "py32_dev")
    (rev "A")
    (company "bit-builder.com")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "+3.3V")
  (net 2 "GND")
  (net 3 "OSCIN")
  (net 4 "OSCOUT")
  (net 5 "OSC32IN")
  (net 6 "OSC32OUT")
  (net 7 "MCU_RST")
  (net 8 "BOOT0_PRE")
  (net 9 "Net-(D1-Pad2)")
  (net 10 "Net-(J1-PadB5)")
  (net 11 "Net-(J1-PadA5)")
  (net 12 "Net-(D2-Pad2)")
  (net 13 "BOOT0")
  (net 14 "SWDIO")
  (net 15 "SWCLK")
  (net 16 "/VBUS")
  (net 17 "unconnected-(J1-PadS1)")
  (net 18 "PB7")
  (net 19 "PB6")
  (net 20 "PB5")
  (net 21 "PB4")
  (net 22 "PB3")
  (net 23 "PA15")
  (net 24 "PA8")
  (net 25 "PF3")
  (net 26 "PA0")
  (net 27 "PA1")
  (net 28 "PA2")
  (net 29 "PA3")
  (net 30 "PA4")
  (net 31 "PA5")
  (net 32 "PA6")
  (net 33 "PA7")
  (net 34 "PB0")
  (net 35 "PB1")
  (net 36 "VDD")
  (net 37 "PA12")
  (net 38 "PA11")
  (footprint "Button_Switch_SMD:SW_Push_1P1T_NO_Vertical_Wuerth_434133025816" (layer "F.Cu")
    (tedit 5DB98283)
    (at 174.3 116.125)
    (descr "https://katalog.we-online.com/em/datasheet/434133025816.pdf")
    (tags "tactile switch Wurth Wuerth")
    (property "Sheetfile" "py32_dev.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "SW1" (at -4.325 0.325) (layer "F.SilkS"))
    (fp_text value "Usr" (at 0 2.55) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.05 0) (layer "F.Fab"))
    (pad "1" smd rect (at 2.075 -1.075) (size 1.05 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "1") (pintype "passive"))
    (pad "1" smd rect (at -2.075 -1.075) (size 1.05 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect (at -2.075 1.075) (size 1.05 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "PA11") (pinfunction "2") (pintype "passive"))
    (pad "2" smd rect (at 2.05 1.075) (size 1.05 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 38 "PA11") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_Push_1P1T_NO_Vertical_Wuerth_434133025816.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.5mm_Pad" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 186 97)
    (descr "Mounting Hole 2.5mm")
    (tags "mounting hole 2.5mm")
    (property "Sheetfile" "py32_dev.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H2" (at -3.55 -2.525) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 8.6 -5.275) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 5 5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 178.975 116.05 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "py32_dev.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R4" (at 0 1.675 180) (layer "F.SilkS"))
    (fp_text value "1.5K" (at 0 1.43 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "PA11") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3.3V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 159.175 100.76)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "py32_dev.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R7" (at -2.495 -0.5 180) (layer "F.SilkS"))
    (fp_text value "10K" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "BOOT0_PRE") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "BOOT0") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Button_Switch_SMD:SW_Push_1P1T_NO_Vertical_Wuerth_434133025816" (layer "F.Cu")
    (tedit 5DB98283)
    (at 155 111.625 -90)
    (descr "https://katalog.we-online.com/em/datasheet/434133025816.pdf")
    (tags "tactile switch Wurth Wuerth")
    (property "Sheetfile" "py32_dev.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "SW2" (at -3.525 0.075 -180) (layer "F.SilkS"))
    (fp_text value "Reset" (at 0 2.55 -270) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0.05 0 -270) (layer "F.Fab"))
    (pad "1" smd rect (at -2.075 -1.075 270) (size 1.05 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "1") (pintype "passive"))
    (pad "1" smd rect (at 2.075 -1.075 270) (size 1.05 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect (at -2.075 1.075 270) (size 1.05 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "MCU_RST") (pinfunction "2") (pintype "passive"))
    (pad "2" smd rect (at 2.05 1.075 270) (size 1.05 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 7 "MCU_RST") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_Push_1P1T_NO_Vertical_Wuerth_434133025816.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 139.725 110.275 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "py32_dev.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C4" (at 2.4 0.5) (layer "F.SilkS"))
    (fp_text value "0.1uf" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_Tantalum_SMD:CP_EIA-3216-18_Kemet-A_Pad1.58x1.35mm_HandSolder" (layer "F.Cu")
    (tedit 5EBA9318)
    (at 138.7 106.925 180)
    (descr "Tantalum Capacitor SMD Kemet-A (3216-18 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (property "Sheetfile" "py32_dev.kicad_sch")
    (property "Sheetname" "")
    (property "Voltage" "35V")
    (attr smd)
    (fp_text reference "C2" (at 3.5125 0.9) (layer "F.SilkS"))
    (fp_text value "0.33uf" (at 0 1.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4375 0 180) (size 1.575 1.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.185185)
      (net 36 "VDD") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4375 0 180) (size 1.575 1.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.185185)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-3216-18_Kemet-A.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x18_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 134 97 90)
    (descr "Through hole straight pin header, 1x18, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x18 2.54mm single row")
    (property "Sheetfile" "py32_dev.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 0.075 -2.625 180) (layer "F.SilkS"))
    (fp_text value "Conn_01x18" (at 2.75 40.3 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.3 21.45) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "+3.3V") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "BOOT0_PRE") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "PB7") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "PB6") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 "PB5") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole oval (at 0 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "PB4") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole oval (at 0 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "PB3") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" thru_hole oval (at 0 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 "PA15") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" thru_hole oval (at 0 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "PA12") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" thru_hole oval (at 0 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "PA11") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" thru_hole oval (at 0 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 "PA8") (pinfunction "Pin_18") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x18_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Crystal:Crystal_SMD_TXC_7M-4Pin_3.2x2.5mm" (layer "F.Cu")
    (tedit 5A0FD1B2)
    (at 153.4 102.35 90)
    (descr "SMD Crystal TXC 7M http://www.txccrystal.com/images/pdf/7m-accuracy.pdf, 3.2x2.5mm^2 package")
    (tags "SMD SMT crystal")
    (property "Sheetfile" "py32_dev.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "Y1" (at 0.075 2.85 180) (layer "F.SilkS"))
    (fp_text value "24MHz" (at 0 2.45 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -1.1 0.85 90) (size 1.4 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "OSCOUT") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect (at 1.1 0.85 90) (size 1.4 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "2") (pintype "passive"))
    (pad "3" smd rect (at 1.1 -0.85 90) (size 1.4 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "OSCIN") (pinfunction "3") (pintype "passive"))
    (pad "4" smd rect (at -1.1 -0.85 90) (size 1.4 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Crystal.3dshapes/Crystal_SMD_TXC_7M-4Pin_3.2x2.5mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_Tantalum_SMD:CP_EIA-3216-18_Kemet-A_Pad1.58x1.35mm_HandSolder" (layer "F.Cu")
    (tedit 5EBA9318)
    (at 132.7625 104.15)
    (descr "Tantalum Capacitor SMD Kemet-A (3216-18 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (property "Sheetfile" "py32_dev.kicad_sch")
    (property "Sheetname" "")
    (property "Voltage" "35V")
    (attr smd)
    (fp_text reference "C1" (at -0.9125 -1.8) (layer "F.SilkS"))
    (fp_text value "0.1uf" (at 0 1.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4375 0) (size 1.575 1.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.185185)
      (net 16 "/VBUS") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4375 0) (size 1.575 1.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.185185)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-3216-18_Kemet-A.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Fuse:Fuse_Bourns_MF-SM_7.98x5.44mm" (layer "F.Cu")
    (tedit 5ABAF57A)
    (at 132.625 113.725 -90)
    (descr "https://www.bourns.com/docs/Product-Datasheets/mfsm.pdf")
    (tags "bourns ptc resettable fuse polyfuse MF-SM MF-SMHT")
    (property "Sheetfile" "py32_dev.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "F1" (at -6.125 0.025 180) (layer "F.SilkS"))
    (fp_text value "Polyfuse" (at 0.275 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -3.7 0 270) (size 2.3 3.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "/VBUS") (pintype "passive"))
    (pad "2" smd rect (at 3.7 0 270) (size 2.3 3.1) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 36 "VDD") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Fuse.3dshapes/Fuse_Bourns_MF-SM_7.98x5.44mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 141.45 115.85 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "py32_dev.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at 0.65 -1.625) (layer "F.SilkS"))
    (fp_text value "470" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(D1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Jumper:SolderJumper-3_P1.3mm_Open_Pad1.0x1.5mm_NumberLabels" (layer "F.Cu")
    (tedit 5A3F6CCC)
    (at 143.83 102.2 180)
    (descr "SMD Solder Jumper, 1x1.5mm Pads, 0.3mm gap, open, labeled with numbers")
    (tags "solder jumper open")
    (property "Sheetfile" "py32_dev.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "JP5" (at 0.14 -1.97 180) (layer "F.SilkS"))
    (fp_text value "Boot" (at 0.14 3.13) (layer "F.Fab"))
    (fp_text user "3" (at 1.86 1.93 180) (layer "F.SilkS"))
    (fp_text user "1" (at -1.92 1.97 180) (layer "F.SilkS"))
    (pad "1" smd rect (at -1.3 0 180) (size 1 1.5) (layers "F.Cu" "F.Mask")
      (net 2 "GND") (pinfunction "A") (pintype "passive"))
    (pad "2" smd rect (at 0 0 180) (size 1 1.5) (layers "F.Cu" "F.Mask")
      (net 8 "BOOT0_PRE") (pinfunction "C") (pintype "passive"))
    (pad "3" smd rect (at 1.3 0 180) (size 1 1.5) (layers "F.Cu" "F.Mask")
      (net 1 "+3.3V") (pinfunction "B") (pintype "passive"))
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 145.725 115.825 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "py32_dev.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C11" (at -0.5 1.375) (layer "F.SilkS"))
    (fp_text value "0.1uf" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "MCU_RST") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Crystal:Crystal_DS15_D1.5mm_L5.0mm_Horizontal" (layer "F.Cu")
    (tedit 5A0FD1B2)
    (at 172.35 107.45 90)
    (descr "Crystal THT DS15 5.0mm length 1.5mm diameter http://www.microcrystal.com/images/_Product-Documentation/03_TF_metal_Packages/01_Datasheet/DS-Series.pdf")
    (tags "['DS15']")
    (property "Sheetfile" "py32_dev.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "Y2" (at 0.875 3.975) (layer "F.SilkS"))
    (fp_text value "32.768KHz" (at 3.12 1.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1 4) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 6 "OSC32OUT") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 1.7 0 90) (size 1 1) (drill 0.5) (layers *.Cu *.Mask)
      (net 5 "OSC32IN") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Crystal.3dshapes/Crystal_DS15_D1.5mm_L5.0mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_QFP:LQFP-32_7x7mm_P0.8mm" (layer "F.Cu")
    (tedit 5D9F72AF)
    (at 163.825 108.475)
    (descr "LQFP, 32 Pin (https://www.nxp.com/docs/en/package-information/SOT358-1.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "LQFP QFP")
    (property "Sheetfile" "py32_dev.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U2" (at 0 -5.88) (layer "F.SilkS"))
    (fp_text value "PY32F030K1xT" (at -2.65 6) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -4.175 -2.8) (size 1.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
    (pad "2" smd roundrect (at -4.175 -2) (size 1.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "OSCIN") (pinfunction "OSCIN-PF0") (pintype "input"))
    (pad "3" smd roundrect (at -4.175 -1.2) (size 1.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "OSCOUT") (pinfunction "OSCOUT-PF1") (pintype "output"))
    (pad "4" smd roundrect (at -4.175 -0.4) (size 1.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "MCU_RST") (pinfunction "PF2-NRST") (pintype "input"))
    (pad "5" smd roundrect (at -4.175 0.4) (size 1.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "PF3") (pinfunction "PF3") (pintype "bidirectional"))
    (pad "6" smd roundrect (at -4.175 1.2) (size 1.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "PA0") (pinfunction "PA0") (pintype "bidirectional"))
    (pad "7" smd roundrect (at -4.175 2) (size 1.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "PA1") (pinfunction "PA1") (pintype "bidirectional"))
    (pad "8" smd roundrect (at -4.175 2.8) (size 1.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "PA2") (pinfunction "PA2") (pintype "bidirectional"))
    (pad "9" smd roundrect (at -2.8 4.175) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 29 "PA3") (pinfunction "PA3") (pintype "bidirectional"))
    (pad "10" smd roundrect (at -2 4.175) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "PA4") (pinfunction "PA4") (pintype "bidirectional"))
    (pad "11" smd roundrect (at -1.2 4.175) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "PA5") (pinfunction "PA5") (pintype "bidirectional"))
    (pad "12" smd roundrect (at -0.4 4.175) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "PA6") (pinfunction "PA6") (pintype "bidirectional"))
    (pad "13" smd roundrect (at 0.4 4.175) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "PA7") (pinfunction "PA7") (pintype "bidirectional"))
    (pad "14" smd roundrect (at 1.2 4.175) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "PB0") (pinfunction "PB0") (pintype "bidirectional"))
    (pad "15" smd roundrect (at 2 4.175) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 35 "PB1") (pinfunction "PB1") (pintype "bidirectional"))
    (pad "16" smd roundrect (at 2.8 4.175) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "VSS") (pintype "passive"))
    (pad "17" smd roundrect (at 4.175 2.8) (size 1.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3.3V") (pinfunction "VCC") (pintype "power_in"))
    (pad "18" smd roundrect (at 4.175 2) (size 1.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 24 "PA8") (pinfunction "PA8") (pintype "bidirectional"))
    (pad "19" smd roundrect (at 4.175 1.2) (size 1.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "OSC32OUT") (pinfunction "PA9-OSC32OUT") (pintype "bidirectional"))
    (pad "20" smd roundrect (at 4.175 0.4) (size 1.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "OSC32IN") (pinfunction "PA10-OSC32IN") (pintype "bidirectional"))
    (pad "21" smd roundrect (at 4.175 -0.4) (size 1.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "PA11") (pinfunction "PA11") (pintype "bidirectional"))
    (pad "22" smd roundrect (at 4.175 -1.2) (size 1.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 37 "PA12") (pinfunction "PA12") (pintype "bidirectional"))
    (pad "23" smd roundrect (at 4.175 -2) (size 1.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "SWDIO") (pinfunction "PA13") (pintype "bidirectional"))
    (pad "24" smd roundrect (at 4.175 -2.8) (size 1.5 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "SWCLK") (pinfunction "PA14") (pintype "bidirectional"))
    (pad "25" smd roundrect (at 2.8 -4.175) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "PA15") (pinfunction "PA15") (pintype "bidirectional"))
    (pad "26" smd roundrect (at 2 -4.175) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "PB3") (pinfunction "PB3") (pintype "bidirectional"))
    (pad "27" smd roundrect (at 1.2 -4.175) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "PB4") (pinfunction "PB4") (pintype "bidirectional"))
    (pad "28" smd roundrect (at 0.4 -4.175) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "PB5") (pinfunction "PB5") (pintype "bidirectional"))
    (pad "29" smd roundrect (at -0.4 -4.175) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "PB6") (pinfunction "PB6") (pintype "bidirectional"))
    (pad "30" smd roundrect (at -1.2 -4.175) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "PB7") (pinfunction "PB7") (pintype "bidirectional"))
    (pad "31" smd roundrect (at -2 -4.175) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "BOOT0") (pinfunction "PF4-BOOT0") (pintype "input"))
    (pad "32" smd roundrect (at -2.8 -4.175) (size 0.5 1.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "VSS") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_QFP.3dshapes/LQFP-32_7x7mm_P0.8mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_Tantalum_SMD:CP_EIA-3216-18_Kemet-A_Pad1.58x1.35mm_HandSolder" (layer "F.Cu")
    (tedit 5EBA9318)
    (at 138.65 113.15 180)
    (descr "Tantalum Capacitor SMD Kemet-A (3216-18 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
    (tags "capacitor tantalum")
    (property "Sheetfile" "py32_dev.kicad_sch")
    (property "Sheetname" "")
    (property "Voltage" "10V")
    (attr smd)
    (fp_text reference "C3" (at 2.125 1.725) (layer "F.SilkS"))
    (fp_text value "10uf" (at 0 1.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.4375 0 180) (size 1.575 1.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.185185)
      (net 1 "+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 1.4375 0 180) (size 1.575 1.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.185185)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-3216-18_Kemet-A.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 177.5875 112.35 180)
    (descr "Diode SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "diode")
    (property "Sheetfile" "py32_dev.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D2" (at -2.6375 0) (layer "F.SilkS"))
    (fp_text value "GREEN" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 37 "PA12") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(D2-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Custom:SHOUHAN TYPE-C 6P" (layer "F.Cu")
    (tedit 0)
    (at 128.475 109 180)
    (descr "USB Type C Power Only")
    (property "Sheetfile" "py32_dev.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J1" (at 4.915 0 unlocked) (layer "F.SilkS"))
    (fp_text value "Board Pwr" (at 8.275 0.225 90 unlocked) (layer "F.Fab"))
    (pad "A5" smd rect (at 0.11 0.5 180) (size 1 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "Net-(J1-PadA5)") (pinfunction "CC1") (pintype "bidirectional"))
    (pad "A9" smd rect (at 0.11 -1.5 180) (size 1 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "/VBUS") (pinfunction "VBUS") (pintype "passive"))
    (pad "A12" smd rect (at 0.11 -2.7 180) (size 1 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "B5" smd rect (at 0.11 -0.5 180) (size 1 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "Net-(J1-PadB5)") (pinfunction "CC2") (pintype "bidirectional"))
    (pad "B9" smd rect (at 0.11 1.5 180) (size 1 0.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "/VBUS") (pinfunction "VBUS") (pintype "passive"))
    (pad "B12" smd rect (at 0.11 2.7 180) (size 1 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "passive"))
    (pad "S1" thru_hole oval (at 0.16 4.32 180) (size 1.8 1) (drill oval 1.4 0.6) (layers *.Cu *.Mask)
      (net 17 "unconnected-(J1-PadS1)") (pinfunction "SHIELD") (pintype "passive"))
    (pad "S1" thru_hole oval (at 3.96 4.32 180) (size 1.8 1) (drill oval 1.4 0.6) (layers *.Cu *.Mask)
      (net 17 "unconnected-(J1-PadS1)") (pinfunction "SHIELD") (pintype "passive"))
    (pad "S1" thru_hole oval (at 0.16 -4.32 180) (size 1.8 1) (drill oval 1.4 0.6) (layers *.Cu *.Mask)
      (net 17 "unconnected-(J1-PadS1)") (pinfunction "SHIELD") (pintype "passive"))
    (pad "S1" thru_hole oval (at 3.96 -4.32 180) (size 1.8 1) (drill oval 1.4 0.6) (layers *.Cu *.Mask)
      (net 17 "unconnected-(J1-PadS1)") (pinfunction "SHIELD") (pintype "passive"))
  )
  (footprint "MountingHole:MountingHole_2.5mm_Pad" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 186 121)
    (descr "Mounting Hole 2.5mm")
    (tags "mounting hole 2.5mm")
    (property "Sheetfile" "py32_dev.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H3" (at -3.55 2.2) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at 9.625 4.7) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 5 5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 173 104.15 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "py32_dev.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C9" (at -2.65 0.875) (layer "F.SilkS"))
    (fp_text value "12.5pf" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "OSC32IN") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 174.225 112.325)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "py32_dev.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R6" (at -2.375 1.125) (layer "F.SilkS"))
    (fp_text value "680" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(D2-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 150.15 115.825 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "py32_dev.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R5" (at -0.075 -1.775) (layer "F.SilkS"))
    (fp_text value "10K" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 180) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "MCU_RST") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 149.975 101 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "py32_dev.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C6" (at 2.8 0) (layer "F.SilkS"))
    (fp_text value "22pf" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "OSCIN") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 180) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x18_P2.54mm_Vertical" (layer "F.Cu")
    (tedit 59FED5CC)
    (at 134 121 90)
    (descr "Through hole straight pin header, 1x18, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x18 2.54mm single row")
    (property "Sheetfile" "py32_dev.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J3" (at -0.15 -2.625 180) (layer "F.SilkS"))
    (fp_text value "Conn_01x18" (at -2.75 40.075 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -2.025 21.525) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "VDD") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "+3.3V") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "MCU_RST") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "SWCLK") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "SWDIO") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "GND") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 0 17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 "PF3") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 "PA0") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval (at 0 22.86 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 "PA1") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" thru_hole oval (at 0 25.4 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 "PA2") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" thru_hole oval (at 0 27.94 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 "PA3") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" thru_hole oval (at 0 30.48 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "PA4") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" thru_hole oval (at 0 33.02 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "PA5") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" thru_hole oval (at 0 35.56 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "PA6") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" thru_hole oval (at 0 38.1 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "PA7") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" thru_hole oval (at 0 40.64 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "PB0") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" thru_hole oval (at 0 43.18 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "PB1") (pinfunction "Pin_18") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x18_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 136.975 102.275)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "py32_dev.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R3" (at 0.15 1.65) (layer "F.SilkS"))
    (fp_text value "R" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(J1-PadA5)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-223-3_TabPin2" (layer "F.Cu")
    (tedit 5A02FF57)
    (at 146.075 110.275)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (property "Sheetfile" "py32_dev.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U1" (at 0 -4.5) (layer "F.SilkS"))
    (fp_text value "uA7805" (at -0.925 -1.125) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -3.15 -2.3) (size 2 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 36 "VDD") (pinfunction "IN") (pintype "power_in"))
    (pad "2" smd rect (at 3.15 0) (size 2 3.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "2" smd rect (at -3.15 0) (size 2 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "3" smd rect (at -3.15 2.3) (size 2 1.5) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "+3.3V") (pinfunction "OUT") (pintype "power_out"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-223.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.5mm_Pad" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 126 97)
    (descr "Mounting Hole 2.5mm")
    (tags "mounting hole 2.5mm")
    (property "Sheetfile" "py32_dev.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at 3.575 -2.7) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at -9.9 -6.1) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 5 5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 149.95 103.75)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "py32_dev.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C7" (at -2.725 0.05) (layer "F.SilkS"))
    (fp_text value "22pf" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "OSCOUT") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 169.55 113.525 -90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "py32_dev.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C5" (at 0.95 1.8) (layer "F.SilkS"))
    (fp_text value "0.1uf" (at -3.45 -0.15 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+3.3V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 270) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 137.7125 115.85)
    (descr "Diode SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "diode")
    (property "Sheetfile" "py32_dev.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D1" (at -0.0125 1.625) (layer "F.SilkS"))
    (fp_text value "RED" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(D1-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 137 100.3)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "py32_dev.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R2" (at -2.675 -0.35) (layer "F.SilkS"))
    (fp_text value "R" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(J1-PadB5)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "MountingHole:MountingHole_2.5mm_Pad" (layer "F.Cu")
    (tedit 56D1B4CB)
    (at 126 121)
    (descr "Mounting Hole 2.5mm")
    (tags "mounting hole 2.5mm")
    (property "Sheetfile" "py32_dev.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "H4" (at 3.5 2.275) (layer "F.SilkS"))
    (fp_text value "MountingHole" (at -9.95 5.6) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 5 5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 173 109.05)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "py32_dev.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C8" (at 2.425 0.925) (layer "F.SilkS"))
    (fp_text value "12.5pf" (at 0 1.43) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "OSC32OUT") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect (start 122 93) (end 190 125) (layer "Edge.Cuts") (width 0.1) (fill none))
  (gr_text "bit-builder.com\npy32_dev rev A" (at 160.175 116.8) (layer "F.SilkS"))
  (dimension (type aligned) (layer "F.Fab")
    (pts (xy 126 97) (xy 186 97))
    (height -8.35)
    (gr_text "60.0000 mm" (at 156 87.5) (layer "F.Fab"))
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.1) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "F.Fab")
    (pts (xy 134 97) (xy 122 97))
    (height 11.75)
    (gr_text "12.0000 mm" (at 128 84.1) (layer "F.Fab"))
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.1) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "F.Fab")
    (pts (xy 190 125) (xy 122 125))
    (height -4.575)
    (gr_text "68.0000 mm" (at 156 128.425) (layer "F.Fab"))
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.1) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "F.Fab")
    (pts (xy 122 125) (xy 122 93))
    (height -5.925)
    (gr_text "32.0000 mm" (at 114.925 109 90) (layer "F.Fab"))
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.1) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (dimension (type aligned) (layer "F.Fab")
    (pts (xy 186 97) (xy 186 121))
    (height -12.620409)
    (gr_text "24.0000 mm" (at 197.470409 109 90) (layer "F.Fab"))
    (format (units 3) (units_format 1) (precision 4))
    (style (thickness 0.1) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
  )
  (zone (net 36) (net_name "VDD") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.35))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 144.275 105.775)
        (xy 144.25 108.825)
        (xy 139.625 108.775)
        (xy 134.55 115.775)
        (xy 134.575 118.875)
        (xy 130.7 118.85)
        (xy 130.7 115.825)
        (xy 138.4 105.8)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 180.75 110.3)
        (xy 169 110.3)
        (xy 169 107.85)
        (xy 170.5 102.125)
        (xy 180.775 102.125)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 161 105.675)
        (xy 161 108.025)
        (xy 157.45 108.025)
        (xy 154.7 105.375)
        (xy 147.775 105.35)
        (xy 147.775 99.375)
        (xy 155.3 99.35)
      )
    )
  )
  (zone (net 1) (net_name "+3.3V") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 145.725 111.5)
        (xy 145.725 114.4)
        (xy 143.525 114.4)
        (xy 143.525 115.075)
        (xy 143.55 111.5)
      )
    )
  )
  (zone (net 1) (net_name "+3.3V") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 141.35 111.5)
        (xy 143.6 111.5)
        (xy 143.6 116.9)
        (xy 141.6 116.9)
        (xy 141.6 114.55)
        (xy 138.775 114.55)
        (xy 138.775 111.35)
        (xy 139.7 111.35)
        (xy 139.875 109.825)
        (xy 141.35 109.825)
      )
    )
  )
  (zone (net 36) (net_name "VDD") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 135.27 119.53)
        (xy 135.26 122.91)
        (xy 132.23 122.9)
        (xy 130.7 118.49)
        (xy 134.57 118.49)
      )
    )
  )
  (zone (net 16) (net_name "/VBUS") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads yes (clearance 0.3))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 134.17 109.13)
        (xy 131.22 109.13)
        (xy 131.22 111.07)
        (xy 127.8 110.94)
        (xy 127.81 107)
        (xy 130.43 104.73)
        (xy 132.18 104.72)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 190 93)
        (xy 190 125)
        (xy 122 125)
        (xy 122 93)
      )
    )
  )
)
