(kicad_pcb (version 20171130) (host pcbnew "(5.1.6)-1")
  (general
    (thickness 1.6)
    (drawings 121)
    (tracks 411)
    (zones 0)
    (modules 55)
    (nets 38)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.2)
    (user_trace_width 0.15)
    (user_trace_width 0.3)
    (user_trace_width 0.5)
    (trace_clearance 0.2)
    (zone_clearance 0.254)
    (zone_45_only no)
    (trace_min 0.127)
    (via_size 0.55)
    (via_drill 0.3)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFDFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber/"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 GNDA)
  (net 3 +3V3)
  (net 4 /ROI_SEL)
  (net 5 /BW0)
  (net 6 /TEST_MODE)
  (net 7 /CS1)
  (net 8 /BW1)
  (net 9 /CS0)
  (net 10 /RD_DIR)
  (net 11 /GAIN)
  (net 12 /HOR_BIN)
  (net 13 /VIDEO_P)
  (net 14 /EPC_VDD)
  (net 15 /ADC_VDD)
  (net 16 /I_BIAS)
  (net 17 /ADC_DATA)
  (net 18 /ANA_TEST2)
  (net 19 /ANA_TEST1)
  (net 20 /PWR_DOWN)
  (net 21 /CLR_DATA)
  (net 22 /DATA_RDY)
  (net 23 /CLR_PIX)
  (net 24 /SHUTTER)
  (net 25 /READ)
  (net 26 /SDA)
  (net 27 /SCL)
  (net 28 /ADC_CS)
  (net 29 /ADC_CLK)
  (net 30 /VIDEO_CM)
  (net 31 /ADC_P)
  (net 32 /EXT_ADC_P)
  (net 33 /EXT_ADC_N)
  (net 34 "Net-(R5-Pad2)")
  (net 35 /VDD_7V0)
  (net 36 /VDD_5V0)
  (net 37 /VDD_1V8)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.55)
    (via_drill 0.3)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net /ADC_CLK)
    (add_net /ADC_CS)
    (add_net /ADC_DATA)
    (add_net /ADC_P)
    (add_net /ADC_VDD)
    (add_net /ANA_TEST1)
    (add_net /ANA_TEST2)
    (add_net /BW0)
    (add_net /BW1)
    (add_net /CLR_DATA)
    (add_net /CLR_PIX)
    (add_net /CS0)
    (add_net /CS1)
    (add_net /DATA_RDY)
    (add_net /EPC_VDD)
    (add_net /EXT_ADC_N)
    (add_net /EXT_ADC_P)
    (add_net /GAIN)
    (add_net /HOR_BIN)
    (add_net /I_BIAS)
    (add_net /PWR_DOWN)
    (add_net /RD_DIR)
    (add_net /READ)
    (add_net /ROI_SEL)
    (add_net /SCL)
    (add_net /SDA)
    (add_net /SHUTTER)
    (add_net /TEST_MODE)
    (add_net /VDD_1V8)
    (add_net /VDD_5V0)
    (add_net /VDD_7V0)
    (add_net /VIDEO_CM)
    (add_net /VIDEO_P)
    (add_net GND)
    (add_net GNDA)
    (add_net "Net-(R5-Pad2)")
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 120.2 108.4 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C10 (at -2.9 0 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 118.4 108.54 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C9 (at -2.6 0 90) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 130.1 97.4)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP10 (at 0 -0.8 90) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -0.8 90) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 30 /VIDEO_CM))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x10_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 115 88.54 180)
    (descr "Through hole straight pin header, 2x10, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x10 2.54mm double row")
    (fp_text reference J1 (at 5.5 0.04) (layer B.SilkS) hide)
    (fp_text value Conn_02x10_Odd_Even (at 1.27 -25.19) (layer B.Fab))
    (fp_text user %R (at 1.27 -11.43 270) (layer B.Fab))
    (pad 20 thru_hole oval (at 2.54 -22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /SCL))
    (pad 19 thru_hole oval (at 0 -22.86 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /SDA))
    (pad 18 thru_hole oval (at 2.54 -20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /READ))
    (pad 17 thru_hole oval (at 0 -20.32 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 16 thru_hole oval (at 2.54 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 15 thru_hole oval (at 0 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 14 thru_hole oval (at 2.54 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /ADC_CS))
    (pad 13 thru_hole oval (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /ADC_DATA))
    (pad 12 thru_hole oval (at 2.54 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /ADC_CLK))
    (pad 11 thru_hole oval (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 10 thru_hole oval (at 2.54 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GNDA))
    (pad 9 thru_hole oval (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 /EXT_ADC_N))
    (pad 8 thru_hole oval (at 2.54 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /EXT_ADC_P))
    (pad 7 thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GNDA))
    (pad 6 thru_hole oval (at 2.54 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /CLR_PIX))
    (pad 5 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /SHUTTER))
    (pad 4 thru_hole oval (at 2.54 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /CLR_DATA))
    (pad 3 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /DATA_RDY))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /PWR_DOWN))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x10_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 128.3 93 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at 0 -1.43 90) (layer F.SilkS))
    (fp_text value 0R (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GNDA))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 /EXT_ADC_N))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 126.7 98.2 270)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at -2.4 0 90) (layer F.SilkS))
    (fp_text value 0R (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GNDA))
    (pad 1 smd roundrect (at -0.7875 0 270) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 /VIDEO_CM))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 128.3 98.2 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 2.4 0 90) (layer F.SilkS))
    (fp_text value DNP (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 /VIDEO_CM))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 124.5 93.3 180)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (fp_text reference JP2 (at 2.8 -2.4 90) (layer B.SilkS))
    (fp_text value Jumper_3_Bridged12 (at 0 -7.41) (layer B.Fab))
    (fp_text user %R (at 0 -2.54 270) (layer B.Fab))
    (pad 3 thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 /ADC_P))
    (pad 2 thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /VIDEO_P))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 /EXT_ADC_P))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical (layer B.Cu) (tedit 59FED5CC)
    (at 130.7 110.6 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference JP1 (at 0 2.8 180) (layer B.SilkS))
    (fp_text value Jumper_NC_Small (at 0 -4.87 90) (layer B.Fab))
    (fp_text user %R (at 0 -1.27 180) (layer B.Fab))
    (pad 2 thru_hole oval (at 0 -2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GNDA))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer B.Cu) (tedit 5B301BBD)
    (at 143.8 98.5 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 0 1.5 270) (layer B.SilkS))
    (fp_text value "56K 1% 100ppm/K" (at 0 -1.43 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 16 /I_BIAS))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 150.5 95)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP7 (at 0 2.3 90) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 2.2 90) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 16 /I_BIAS))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 150.4 104.1)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP6 (at 0 -1.448) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 35 /VDD_7V0))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 152.8 104.1)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP5 (at 0 1.625) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 1.575) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 36 /VDD_5V0))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 147.7 89.8)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP4 (at 0 -0.9 90) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -0.9 90) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 37 /VDD_1V8))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 150.5 92.6)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP9 (at 0 -0.8 90) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -0.8 90) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 18 /ANA_TEST2))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 152.9 92.6)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP8 (at 0 -0.8 90) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 -0.8 90) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 19 /ANA_TEST1))
  )
  (module epc901:epc901 (layer F.Cu) (tedit 5F5FE4B6)
    (at 139.8 99.95 270)
    (solder_mask_margin 0.05)
    (zone_connect 0)
    (attr smd)
    (fp_text reference U1 (at -3.65 2.4 180) (layer F.SilkS))
    (fp_text value EPC901 (at 0 0 90) (layer F.Fab))
    (pad 32 smd circle (at -3.7 -0.43 270) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 37 /VDD_1V8) (zone_connect 0))
    (pad 31 smd circle (at -3.2 -0.43 270) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 1 GND) (zone_connect 0))
    (pad 30 smd circle (at -2.7 -0.43 270) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 6 /TEST_MODE) (zone_connect 0))
    (pad 29 smd circle (at -2.2 -0.43 270) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 18 /ANA_TEST2) (zone_connect 0))
    (pad 28 smd circle (at -1.7 -0.43 270) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 19 /ANA_TEST1) (zone_connect 0))
    (pad 27 smd circle (at -1.2 -0.43 270) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 16 /I_BIAS) (zone_connect 0))
    (pad 26 smd circle (at -0.7 -0.43 270) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 14 /EPC_VDD) (zone_connect 0))
    (pad 25 smd circle (at -0.2 -0.43 270) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 12 /HOR_BIN) (zone_connect 0))
    (pad 24 smd circle (at 0.3 -0.43 270) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 10 /RD_DIR) (zone_connect 0))
    (pad 23 smd circle (at 0.8 -0.43 270) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 8 /BW1) (zone_connect 0))
    (pad 22 smd circle (at 1.3 -0.43 270) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 5 /BW0) (zone_connect 0))
    (pad 21 smd circle (at 1.8 -0.43 270) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 11 /GAIN) (zone_connect 0))
    (pad 20 smd circle (at 2.3 -0.43 270) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 35 /VDD_7V0) (zone_connect 0))
    (pad 19 smd circle (at 2.8 -0.43 270) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 9 /CS0) (zone_connect 0))
    (pad 18 smd circle (at 3.3 -0.43 270) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 36 /VDD_5V0) (zone_connect 0))
    (pad 17 smd circle (at 3.8 -0.43 270) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 7 /CS1) (zone_connect 0))
    (pad 1 smd circle (at -3.7 0.43 270) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDA) (zone_connect 0))
    (pad 2 smd circle (at -3.2 0.43 270) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 20 /PWR_DOWN) (zone_connect 0))
    (pad 3 smd circle (at -2.7 0.43 270) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 21 /CLR_DATA) (zone_connect 0))
    (pad 4 smd circle (at -2.2 0.43 270) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 22 /DATA_RDY) (zone_connect 0))
    (pad 5 smd circle (at -1.7 0.43 270) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 23 /CLR_PIX) (zone_connect 0))
    (pad 6 smd circle (at -1.2 0.43 270) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 24 /SHUTTER) (zone_connect 0))
    (pad 7 smd circle (at -0.7 0.43 270) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDA) (zone_connect 0))
    (pad 8 smd circle (at -0.2 0.43 270) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 33 /EXT_ADC_N) (zone_connect 0))
    (pad 9 smd circle (at 0.3 0.43 270) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 13 /VIDEO_P) (zone_connect 0))
    (pad 10 smd circle (at 0.8 0.43 270) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3) (zone_connect 0))
    (pad 11 smd circle (at 1.3 0.43 270) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 30 /VIDEO_CM) (zone_connect 0))
    (pad 12 smd circle (at 1.8 0.43 270) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 25 /READ) (zone_connect 0))
    (pad 13 smd circle (at 2.3 0.43 270) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 26 /SDA) (zone_connect 0))
    (pad 14 smd circle (at 2.8 0.43 270) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 27 /SCL) (zone_connect 0))
    (pad 15 smd circle (at 3.3 0.43 270) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 4 /ROI_SEL) (zone_connect 0))
    (pad 16 smd circle (at 3.8 0.43 270) (size 0.3 0.3) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDA) (zone_connect 0))
    (model ${KIPRJMOD}/epc901.pretty/EPC901_V3.step
      (offset (xyz 0.05 0.19 0.15))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 125.1 110 180)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP2 (at 2.3 0) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 2.3 0) (layer F.Fab))
    (pad 1 smd circle (at 0 0 180) (size 1 1) (layers F.Cu F.Mask)
      (net 15 /ADC_VDD))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 152.8 95)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP3 (at 0 2.3 90) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at 0 2.3 90) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 14 /EPC_VDD))
  )
  (module TestPoint:TestPoint_Pad_D1.0mm (layer F.Cu) (tedit 5A0F774F)
    (at 121.9 112.5)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (attr virtual)
    (fp_text reference TP1 (at -2.2 0) (layer F.SilkS) hide)
    (fp_text value TestPoint (at 0 1.55) (layer F.Fab))
    (fp_text user %R (at -2.2 0) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 3 +3V3))
  )
  (module MountingHole:MountingHole_2.2mm_M2_DIN965_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 169 85)
    (descr "Mounting Hole 2.2mm, M2, DIN965")
    (tags "mounting hole 2.2mm m2 din965")
    (zone_connect 2)
    (attr virtual)
    (fp_text reference H4 (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value MountingHole_Pad (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.8 3.8) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
  )
  (module MountingHole:MountingHole_2.2mm_M2_DIN965_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 169 115)
    (descr "Mounting Hole 2.2mm, M2, DIN965")
    (tags "mounting hole 2.2mm m2 din965")
    (zone_connect 2)
    (attr virtual)
    (fp_text reference H3 (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value MountingHole_Pad (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.8 3.8) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
  )
  (module MountingHole:MountingHole_2.2mm_M2_DIN965_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 114 115)
    (descr "Mounting Hole 2.2mm, M2, DIN965")
    (tags "mounting hole 2.2mm m2 din965")
    (zone_connect 2)
    (attr virtual)
    (fp_text reference H2 (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value MountingHole_Pad (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.8 3.8) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
  )
  (module MountingHole:MountingHole_2.2mm_M2_DIN965_Pad (layer F.Cu) (tedit 56D1B4CB)
    (at 114 85)
    (descr "Mounting Hole 2.2mm, M2, DIN965")
    (tags "mounting hole 2.2mm m2 din965")
    (zone_connect 2)
    (attr virtual)
    (fp_text reference H1 (at 0 -2.9) (layer F.SilkS) hide)
    (fp_text value MountingHole_Pad (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.8 3.8) (drill 2.2) (layers *.Cu *.Mask)
      (net 1 GND) (zone_connect 2))
  )
  (module epc901:lensholder-m12-20mm (layer F.Cu) (tedit 5F5EC079)
    (at 140 100 90)
    (descr "M12 Lenses Inc. PT-LH009P, M12 thread, 20mm hole spacing, plastic")
    (fp_text reference H0 (at 0 6.7 90) (layer F.SilkS) hide)
    (fp_text value LensMount (at 0 -6.6 90) (layer F.Fab))
    (pad "" np_thru_hole circle (at 10 0 90) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -10 0 90) (size 2.2 2.2) (drill 2.2) (layers *.Cu *.Mask))
    (model ${KIPRJMOD}/epc901.pretty/PT-LH009P.stp
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-6 (layer F.Cu) (tedit 5A02FF57)
    (at 124 102.7 180)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U3 (at 0 2.4) (layer F.SilkS))
    (fp_text value AD747x (at 0 2.9) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 5 smd rect (at 1.1 0 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(R5-Pad2)"))
    (pad 6 smd rect (at 1.1 -0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 28 /ADC_CS))
    (pad 4 smd rect (at 1.1 0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 29 /ADC_CLK))
    (pad 3 smd rect (at -1.1 0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 31 /ADC_P))
    (pad 2 smd rect (at -1.1 0 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDA))
    (pad 1 smd rect (at -1.1 -0.95 180) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask)
      (net 15 /ADC_VDD))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57)
    (at 127.4 106.8 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference U2 (at 0 2.7) (layer F.SilkS))
    (fp_text value REF3030 (at 0 2.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 3 smd rect (at 1 0 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 2 GNDA))
    (pad 2 smd rect (at -1 0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 15 /ADC_VDD))
    (pad 1 smd rect (at -1 -0.95 90) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 120.4 102.7)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at 0 -1.43) (layer F.SilkS))
    (fp_text value 100R (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 "Net-(R5-Pad2)"))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 /ADC_DATA))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 155.8 94.5 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R25 (at 3 0) (layer F.SilkS) hide)
    (fp_text value DNP (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 /HOR_BIN))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 158.8 94.5 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R24 (at -3.2 0) (layer F.SilkS) hide)
    (fp_text value DNP (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 /HOR_BIN))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 155.8 102.1 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R17 (at 3 0) (layer F.SilkS) hide)
    (fp_text value DNP (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /GAIN))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 158.8 102.1 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R16 (at -3.2 0) (layer F.SilkS) hide)
    (fp_text value DNP (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 /GAIN))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 155.8 96.4 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R23 (at 3 0) (layer F.SilkS) hide)
    (fp_text value DNP (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 /RD_DIR))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 158.8 96.4 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R22 (at -3.2 0) (layer F.SilkS) hide)
    (fp_text value 10K (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 /RD_DIR))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 155.8 104 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R15 (at 3 0) (layer F.SilkS) hide)
    (fp_text value DNP (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 /CS0))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 158.8 104 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R14 (at -3.2 0) (layer F.SilkS) hide)
    (fp_text value DNP (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 /CS0))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 155.8 98.3 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R21 (at 3 0) (layer F.SilkS) hide)
    (fp_text value DNP (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 /BW1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 158.8 98.3 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R20 (at -2.7 0) (layer F.SilkS) hide)
    (fp_text value 10K (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 /BW1))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 155.8 105.9 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R13 (at 2.6 0) (layer F.SilkS) hide)
    (fp_text value DNP (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 /CS1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 158.8 105.9 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R12 (at -2.7 0) (layer F.SilkS) hide)
    (fp_text value DNP (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 /CS1))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 155.8 92.6 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R27 (at 2.6 0) (layer F.SilkS) hide)
    (fp_text value 10K (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /TEST_MODE))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 158.7875 92.6 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R26 (at -2.7125 0) (layer F.SilkS) hide)
    (fp_text value DNP (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /TEST_MODE))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 155.8 100.2 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R19 (at 2.6 0) (layer F.SilkS) hide)
    (fp_text value DNP (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /BW0))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 158.8 100.2 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R18 (at -2.7 0) (layer F.SilkS) hide)
    (fp_text value 10K (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /BW0))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 155.8 107.8 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R11 (at 2.7 0) (layer F.SilkS) hide)
    (fp_text value DNP (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 /ROI_SEL))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0603_1608Metric (layer F.Cu) (tedit 5B301BBD)
    (at 158.8 107.8 180)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R10 (at -2.7 0) (layer F.SilkS) hide)
    (fp_text value DNP (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 /ROI_SEL))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Inductor_SMD:L_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 143 100.8)
    (descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags inductor)
    (attr smd)
    (fp_text reference L1 (at 2.4 0) (layer B.SilkS))
    (fp_text value "600R @100M" (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 14 /EPC_VDD))
    (model ${KISYS3DMOD}/Inductor_SMD.3dshapes/L_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 126.8 103.5 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C8 (at 2.7 0 90) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GNDA))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 /ADC_VDD))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 128.4 103.5 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C7 (at 2.7 0 90) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GNDA))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 /ADC_VDD))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer F.Cu) (tedit 5B301BBE)
    (at 124.7 107 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6 (at 0 -1.4 90) (layer F.SilkS))
    (fp_text value 1uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 GNDA))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 143 96.2)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at 2.5 0) (layer B.SilkS))
    (fp_text value 1uF (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 37 /VDD_1V8))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 143 103.8)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at 2.5 0) (layer B.SilkS))
    (fp_text value 2.2uF (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GNDA))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 36 /VDD_5V0))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 143 102.3)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at 2.5 -0.1) (layer B.SilkS))
    (fp_text value 2.2uF (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GNDA))
    (pad 1 smd roundrect (at -0.7875 0) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 35 /VDD_7V0))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 136.6 101 180)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at 0 -1.5) (layer B.SilkS))
    (fp_text value 1uF (at 0 -1.43) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 2 GNDA))
    (pad 1 smd roundrect (at -0.7875 0 180) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric (layer B.Cu) (tedit 5B301BBE)
    (at 142.3 98.5 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 0 -1.5 270) (layer B.SilkS))
    (fp_text value 1uF (at 0 -1.43 90) (layer B.Fab))
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -0.7875 0 90) (size 0.875 0.95) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 14 /EPC_VDD))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text 3V3 (at 121.9 113.3 90) (layer F.SilkS))
  (gr_text ADC_VDD (at 125.1 110.8 90) (layer F.SilkS))
  (gr_text VDD_5V0 (at 152.8 104.9 90) (layer F.SilkS))
  (gr_text VDD_7V0 (at 150.4 104.9 90) (layer F.SilkS))
  (gr_text EPC_VDD (at 152.8 95.8 90) (layer F.SilkS))
  (gr_text I_BIAS (at 150.5 95.8 90) (layer F.SilkS))
  (gr_text ANA_TEST1 (at 152.9 91.7 90) (layer F.SilkS))
  (gr_text ANA_TEST2 (at 150.5 91.7 90) (layer F.SilkS))
  (gr_text VDD_1V8 (at 147.7 89 90) (layer F.SilkS))
  (gr_text VIDEO_CM (at 130.1 96.6 90) (layer F.SilkS))
  (gr_text ON-BOARD (at 127.6 97.7) (layer B.SilkS))
  (gr_text EXTERNAL (at 127.6 94.2) (layer B.SilkS))
  (gr_text "ADC SELECTION" (at 130.1 90.3) (layer B.SilkS))
  (gr_text "STAR GND" (at 129.5 108) (layer B.SilkS))
  (gr_text 2 (at 157.5 91) (layer B.SilkS))
  (gr_text 4 (at 157.5 93) (layer B.SilkS))
  (gr_text 6 (at 157.5 95) (layer B.SilkS))
  (gr_text 8 (at 157.5 97) (layer B.SilkS))
  (gr_text 10 (at 157.5 99) (layer B.SilkS))
  (gr_text 12 (at 157.5 101) (layer B.SilkS))
  (gr_text 14 (at 157.5 103) (layer B.SilkS))
  (gr_text 16 (at 157.5 105) (layer B.SilkS))
  (gr_text 18 (at 157.5 107) (layer B.SilkS))
  (gr_text 20 (at 157.5 109) (layer B.SilkS))
  (gr_text 19 (at 160.5 109) (layer B.SilkS))
  (gr_text 17 (at 160.5 107) (layer B.SilkS))
  (gr_text 15 (at 160.5 105) (layer B.SilkS))
  (gr_text 13 (at 160.5 103) (layer B.SilkS))
  (gr_text 11 (at 160.5 101) (layer B.SilkS))
  (gr_text 9 (at 160.5 99) (layer B.SilkS))
  (gr_text 7 (at 160.5 97) (layer B.SilkS))
  (gr_text 5 (at 160.5 95) (layer B.SilkS))
  (gr_text 3 (at 160.5 93) (layer B.SilkS))
  (gr_text 1 (at 160.5 91) (layer B.SilkS))
  (gr_text GND (at 162.5 107) (layer B.SilkS))
  (gr_text GND (at 162.5 105) (layer B.SilkS))
  (gr_text ADC_DATA (at 162.5 103) (layer B.SilkS))
  (gr_text ADC_CS (at 155.5 103) (layer B.SilkS))
  (gr_text ADC_CLK (at 155.5 101) (layer B.SilkS))
  (gr_text GND (at 162.5 101) (layer B.SilkS))
  (gr_text VIDEO_N (at 162.5 99) (layer B.SilkS))
  (gr_text VIDEO_P (at 155.5 97) (layer B.SilkS))
  (gr_text GNDA (at 155.5 99) (layer B.SilkS))
  (gr_text GNDA (at 162.5 97) (layer B.SilkS))
  (gr_text "Breakout Board    REV A" (at 141.5 115) (layer B.SilkS))
  (dimension 55 (width 0.15) (layer Dwgs.User)
    (gr_text "55.000 mm" (at 141.5 73.2) (layer Dwgs.User))
    (feature1 (pts (xy 169 76.5) (xy 169 73.913579)))
    (feature2 (pts (xy 114 76.5) (xy 114 73.913579)))
    (crossbar (pts (xy 114 74.5) (xy 169 74.5)))
    (arrow1a (pts (xy 169 74.5) (xy 167.873496 75.086421)))
    (arrow1b (pts (xy 169 74.5) (xy 167.873496 73.913579)))
    (arrow2a (pts (xy 114 74.5) (xy 115.126504 75.086421)))
    (arrow2b (pts (xy 114 74.5) (xy 115.126504 73.913579)))
  )
  (dimension 30 (width 0.15) (layer Dwgs.User)
    (gr_text "30.000 mm" (at 180.8 100 270) (layer Dwgs.User))
    (feature1 (pts (xy 177.5 115) (xy 180.086421 115)))
    (feature2 (pts (xy 177.5 85) (xy 180.086421 85)))
    (crossbar (pts (xy 179.5 85) (xy 179.5 115)))
    (arrow1a (pts (xy 179.5 115) (xy 178.913579 113.873496)))
    (arrow1b (pts (xy 179.5 115) (xy 180.086421 113.873496)))
    (arrow2a (pts (xy 179.5 85) (xy 178.913579 86.126504)))
    (arrow2b (pts (xy 179.5 85) (xy 180.086421 86.126504)))
  )
  (dimension 36 (width 0.15) (layer Dwgs.User)
    (gr_text "36.000 mm" (at 175.8 100 270) (layer Dwgs.User))
    (feature1 (pts (xy 173 118) (xy 175.086421 118)))
    (feature2 (pts (xy 173 82) (xy 175.086421 82)))
    (crossbar (pts (xy 174.5 82) (xy 174.5 118)))
    (arrow1a (pts (xy 174.5 118) (xy 173.913579 116.873496)))
    (arrow1b (pts (xy 174.5 118) (xy 175.086421 116.873496)))
    (arrow2a (pts (xy 174.5 82) (xy 173.913579 83.126504)))
    (arrow2b (pts (xy 174.5 82) (xy 175.086421 83.126504)))
  )
  (dimension 61 (width 0.15) (layer Dwgs.User)
    (gr_text "61.000 mm" (at 141.5 77.7) (layer Dwgs.User))
    (feature1 (pts (xy 172 81) (xy 172 78.413579)))
    (feature2 (pts (xy 111 81) (xy 111 78.413579)))
    (crossbar (pts (xy 111 79) (xy 172 79)))
    (arrow1a (pts (xy 172 79) (xy 170.873496 79.586421)))
    (arrow1b (pts (xy 172 79) (xy 170.873496 78.413579)))
    (arrow2a (pts (xy 111 79) (xy 112.126504 79.586421)))
    (arrow2b (pts (xy 111 79) (xy 112.126504 78.413579)))
  )
  (gr_text "epc901 1024x1 CCD Sensor" (at 141.5 85.5) (layer B.SilkS))
  (gr_text CONFIG (at 160.5 90.6) (layer F.SilkS))
  (gr_text SHUTTER (at 162.5 95) (layer B.SilkS))
  (gr_text CLR_PIX (at 155.5 95) (layer B.SilkS))
  (gr_text DATA_RDY (at 162.5 93) (layer B.SilkS))
  (gr_text CLR_DATA (at 155.5 93) (layer B.SilkS))
  (gr_text PWR_DOWN (at 155.5 91) (layer B.SilkS))
  (gr_text SCL (at 155.5 109) (layer B.SilkS))
  (gr_text SDA (at 162.5 109) (layer B.SilkS))
  (gr_text READ (at 155.5 107) (layer B.SilkS))
  (gr_text 3V3 (at 155.5 105) (layer B.SilkS))
  (gr_text GND (at 162.5 91) (layer B.SilkS))
  (gr_line (start 114 118) (end 169 118) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 111 85) (end 111 115) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 169 82) (end 114 82) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 172 115) (end 172 85) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 169 115) (end 169 118) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 114 115) (end 111 115) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 114 85) (end 114 82) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 169 85) (end 172 85) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_text TEST_MODE (at 160.5 92.6) (layer F.SilkS))
  (gr_text HDR_BIN (at 160.5 94.5) (layer F.SilkS))
  (gr_text RD_DIR (at 160.5 96.4) (layer F.SilkS))
  (gr_text CS0 (at 160.5 104) (layer F.SilkS))
  (gr_text CS1 (at 160.5 105.9) (layer F.SilkS))
  (gr_text GAIN (at 160.5 102.1) (layer F.SilkS))
  (gr_text BW1 (at 160.5 98.3) (layer F.SilkS))
  (gr_text BW0 (at 160.5 100.2) (layer F.SilkS))
  (gr_text ROI_SEL (at 160.5 107.8) (layer F.SilkS))
  (gr_text H (at 158.8 90.6) (layer F.SilkS))
  (gr_text L (at 155.8 90.6) (layer F.SilkS))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.5))
    (polygon
      (pts
        (xy 116.5 117.5) (xy 111.5 117.5) (xy 111.5 112.5) (xy 116.5 112.5)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 171.5 117.5) (xy 111.5 117.5) (xy 111.5 82.5) (xy 171.5 82.5)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.254))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.5))
    (polygon
      (pts
        (xy 116.5 87.4) (xy 111.5 87.4) (xy 111.5 82.5) (xy 116.5 82.5)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.5))
    (polygon
      (pts
        (xy 171.5 87.5) (xy 166.5 87.5) (xy 166.5 82.5) (xy 171.5 82.5)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.254))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.5))
    (polygon
      (pts
        (xy 171.5 117.5) (xy 166.5 117.5) (xy 166.5 112.5) (xy 171.5 112.5)
      )
    )
  )
  (zone (net 2) (net_name GNDA) (layer B.Cu) (hatch edge 0.508)
    (priority 1)
    (connect_pads (clearance 0.254))
    (min_thickness 0.2)
    (fill yes (arc_segments 32) (thermal_gap 0.254) (thermal_bridge_width 0.508) (smoothing fillet) (radius 0.5))
    (polygon
      (pts
        (xy 132 94) (xy 140.7 94) (xy 140.7 101.5) (xy 145.7 101.5) (xy 145.7 106.1)
        (xy 134.9 106.1) (xy 134.9 112) (xy 129.5 112) (xy 129.5 108.8) (xy 124 108.8)
        (xy 124 100) (xy 119.5 100) (xy 111.5 100) (xy 111.5 95) (xy 119 95)
        (xy 122.9 91.1) (xy 129.1 91.1)
      )
    )
  )
)
