(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "USLetter")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0.0508)
    (aux_axis_origin 25.225 185.25)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "/HALL1_VCC")
  (net 2 "/HALL1_GND")
  (net 3 "/HALL1_VOUT")
  (net 4 "/HALL1_~{SLEEP_IN}")
  (net 5 "/~{SLEEP1}")
  (footprint "Resistor_SMD:R_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 26.325 179.535 90)
    (descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "D:/Dropbox/Hardware_projects/MusselGapeTracker/KiCad_files/MusselGapeTracker_RevE.kicad_sch")
    (property "Sheetname" "MusselGapeTracker_RevE_0")
    (attr smd)
    (fp_text reference "R1" (at 0.085 -1.225 90) (layer "F.SilkS"))
    (fp_text value "10kΩ" (at 0.035 0.975 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "/HALL1_~{SLEEP_IN}") (pinfunction "1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.825 0 90) (size 0.8 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "/~{SLEEP1}") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0603_1608Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 29.075 179.535 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "D:/Dropbox/Hardware_projects/MusselGapeTracker/KiCad_files/MusselGapeTracker_RevE.kicad_sch")
    (property "Sheetname" "MusselGapeTracker_RevE_0")
    (attr smd)
    (fp_text reference "C1" (at 0.135 1.25 90) (layer "F.SilkS"))
    (fp_text value "0.1µF" (at 0.085 -1.05 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "/HALL1_VCC") (pinfunction "1") (pintype "passive"))
    (pad "2" smd roundrect (at 0.775 0 90) (size 0.9 0.95) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "/HALL1_GND") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "A1395SEHLT-T:SENSOR_A1395SEHLT-T" (layer "F.Cu")
    (tedit 628FF9BA)
    (at 27.559 176.53 180)
    (property "MANUFACTURER" "Allegro Microsystems")
    (property "PARTREV" "7")
    (property "STANDARD" "Manufacturer Recommendation")
    (property "Sheetfile" "D:/Dropbox/Hardware_projects/MusselGapeTracker/KiCad_files/MusselGapeTracker_RevE.kicad_sch")
    (property "Sheetname" "MusselGapeTracker_RevE_0")
    (attr through_hole)
    (fp_text reference "U1" (at 0.635145 -2.159495) (layer "F.SilkS") hide)
    (fp_text value "A1395SEHLT-T" (at -1.016 2.794) (layer "F.Fab") hide)
    (pad "1" smd rect locked (at -1.35 -0.5 180) (size 1 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/HALL1_VCC") (pinfunction "VCC") (pintype "power_in"))
    (pad "2" smd rect locked (at -1.35 0 180) (size 1 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "/HALL1_VOUT") (pinfunction "OUT") (pintype "output"))
    (pad "3" smd rect locked (at 0 0.5 90) (size 0.3 3.7) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/HALL1_GND") (pinfunction "GND") (pintype "power_in"))
    (pad "4" smd rect locked (at 0 -0.05 180) (size 1.25 0.8) (layers "F.Cu" "F.Mask")
      (net 2 "/HALL1_GND") (pinfunction "GND") (pintype "power_in"))
    (pad "5" smd rect locked (at 1.35 0 180) (size 1 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "/~{SLEEP1}") (pinfunction "~{SLEEP}") (pintype "input"))
    (pad "6" smd rect locked (at 1.35 -0.5 180) (size 1 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "/HALL1_VCC") (pinfunction "VREF") (pintype "power_in"))
  )
  (footprint "Miller_parts:2X2_2.25MM" (layer "F.Cu")
    (tedit 629673BA)
    (at 27.625 183.325 180)
    (descr "2X2 header 1.5mm pitch<p>\n0.8mm drill")
    (property "Sheetfile" "D:/Dropbox/Hardware_projects/MusselGapeTracker/KiCad_files/MusselGapeTracker_RevE.kicad_sch")
    (property "Sheetname" "MusselGapeTracker_RevE_0")
    (fp_text reference "HALL1_HEADER1" (at -1.85 -1.9 180) (layer "F.SilkS") hide)
    (fp_text value "PINHD-2X21.5MM_SILK" (at -2.7 2.35 180) (layer "F.Fab") hide)
    (pad "P$1" thru_hole roundrect (at -1.125 -1.125 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.25) (chamfer top_left top_right bottom_left bottom_right)
      (net 2 "/HALL1_GND") (pinfunction "1") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "P$2" thru_hole roundrect (at 1.125 -1.125 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.25) (chamfer top_left top_right bottom_left bottom_right)
      (net 1 "/HALL1_VCC") (pinfunction "2") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "P$3" thru_hole roundrect (at -1.125 1.125 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.25) (chamfer top_left top_right bottom_left bottom_right)
      (net 3 "/HALL1_VOUT") (pinfunction "3") (pintype "passive") (solder_mask_margin 0.0762))
    (pad "P$4" thru_hole roundrect (at 1.125 1.125 180) (size 1.27 1.27) (drill 0.8) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (chamfer_ratio 0.25) (chamfer top_left top_right bottom_left bottom_right)
      (net 4 "/HALL1_~{SLEEP_IN}") (pinfunction "4") (pintype "passive") (solder_mask_margin 0.0762))
  )
  (gr_poly
    (pts
      (xy 30.875 176.125)
      (xy 30.875 185.65)
      (xy 24.525 185.65)
      (xy 24.525 176.125)
      (xy 25.35 175.25)
      (xy 30.05 175.25)
    ) (layer "Edge.Cuts") (width 0.05) (fill none))
  (gr_text "GND" (at 30.1 184.5 -90) (layer "B.SilkS"))
  (gr_text "VCC" (at 25.125 184.475 -90) (layer "B.SilkS"))
  (gr_text "SLP" (at 25.125 181.95 -90) (layer "B.SilkS"))
  (gr_text "Hall\nEffect\nSensor" (at 27.575 177.275) (layer "B.SilkS"))
  (gr_text "VOUT" (at 30.125 181.725 -90) (layer "B.SilkS"))
  (gr_text "GND" (at 30.175 184.5 90) (layer "F.SilkS"))
  (gr_text "VCC" (at 25.2 184.475 90) (layer "F.SilkS"))
  (gr_text "VOUT" (at 30.2 181.8 90) (layer "F.SilkS"))
  (gr_text "SLP" (at 25.225 182.025 90) (layer "F.SilkS"))
)
