<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="158.75" y2="0" width="0" layer="20"/>
<wire x1="158.75" y1="0" x2="158.75" y2="57.15" width="0" layer="20"/>
<wire x1="158.75" y1="57.15" x2="0" y2="57.15" width="0" layer="20"/>
<wire x1="0" y1="57.15" x2="0" y2="0" width="0" layer="20"/>
<text>-12V</text>
<text>+12V</text>
<text>N_BNK
(GND-DC)</text>
<text>GND</text>
<text>RECEIVER INTERCONNECT  BOARD</text>
<text>PN:0004692 REV B</text>
<text>AUG-2016</text>
<text>+5V
OUT</text>
<text>L1_BNK
(+12DC)</text>
<text>N</text>
<text>CLOSED</text>
<text>OPEN</text>
<text>+12</text>
<text>GND</text>
<text>HOME3</text>
<text>TO AMP BOX</text>
<text>TO SCB BOX</text>
<text>TO REC HEAD</text>
<text>SHIELD</text>
<text>+12</text>
<text>-12</text>
<text>+5</text>
<text>GND</text>
<text>GAIN1</text>
<text>GAIN2</text>
<text>GAIN3</text>
<text>GAIN4</text>
<text>1X</text>
<text>10X</text>
<text>100X</text>
<text>SHIELD</text>
<text>GND</text>
<text>HOME3</text>
<text>DCRELAY</text>
<text>GAIN1</text>
<text>GAIN2</text>
<text>GAIN3</text>
<text>GAIN4</text>
<text>100X</text>
<text>10X</text>
<text>1X</text>
<text>GND</text>
<text>INPUT SEL</text>
<text>INPUT SEL</text>
<text>GND</text>
</plain>
<libraries>
<library name="con-phoenix-350">
<packages>
<package name="1985234">
</package>
<package name="1985250">
</package>
<package name="1990122">
</package>
</packages>
</library>
<library name="logo.SBE">
<packages>
<package name="SPARKY_A">
</package>
<package name="BRANDED">
</package>
</packages>
</library>
<library name="SBE_Mounting_ClearZones">
<packages>
<package name="HEX_SNDOFF_CLEARZONE">
</package>
</packages>
</library>
<library name="con-tycoelectronics">
<packages>
<package name="RJ11-NO_SHIELD">
<description>&lt;b&gt;RJ11 Low Profile&lt;/b&gt; No Shield&lt;/b&gt;&lt;p&gt;
For all RJ11 N and Z Series Models&lt;br&gt;
Source: www.tycoelectronics.com .. ENG_DS_1654001_1099_RJ_L_0507.pdf</description>
</package>
</packages>
</library>
<library name="rcl.SBE">
<packages>
<package name="R1210">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-stewart">
<packages>
<package name="SS-7188VS">
</package>
</packages>
</library>
<library name="rcl">
<packages>
<package name="C1210">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="relay.SBE">
<packages>
<package name="G2RE">
<description>&lt;b&gt;RELAY&lt;/b&gt;&lt;p&gt;
1 x switch, high current, Omron</description>
</package>
</packages>
</library>
<library name="linear">
<description>&lt;b&gt;Linear Devices&lt;/b&gt;&lt;p&gt;
Operational amplifiers,  comparators, voltage regulators, ADCs, DACs, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO220V">
<description>&lt;b&gt;TO 200 vertical&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J2" library="con-phoenix-350" package="1985250" value="1985250">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="logo.SBE" package="SPARKY_A" value=""/>
<element name="U$2" library="logo.SBE" package="BRANDED" value=""/>
<element name="J3" library="con-phoenix-350" package="1990122" value="1990122">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J4" library="con-phoenix-350" package="1990122" value="1990122">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$3" library="SBE_Mounting_ClearZones" package="HEX_SNDOFF_CLEARZONE" value=""/>
<element name="U$4" library="SBE_Mounting_ClearZones" package="HEX_SNDOFF_CLEARZONE" value=""/>
<element name="U$6" library="SBE_Mounting_ClearZones" package="HEX_SNDOFF_CLEARZONE" value=""/>
<element name="U$7" library="SBE_Mounting_ClearZones" package="HEX_SNDOFF_CLEARZONE" value=""/>
<element name="U$8" library="SBE_Mounting_ClearZones" package="HEX_SNDOFF_CLEARZONE" value=""/>
<element name="ZETA4" library="con-tycoelectronics" package="RJ11-NO_SHIELD" value="RJ11-2L-B">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="rcl.SBE" package="R1210" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J5" library="con-stewart" package="SS-7188VS" value="SS7188VS">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="rcl.SBE" package="R1210" value="2K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="rcl" package="C1210" value="1000p">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="K1" library="relay.SBE" package="G2RE" value="G2RE">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X1" library="con-phoenix-350" package="1985234" value="1985234">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="linear" package="TO220V" value="7805TV"/>
<element name="C1" library="rcl" package="C1210" value="1000p"/>
<element name="C3" library="rcl" package="C1210" value="1000p"/>
</elements>
<signals>
<signal name="N$2">
<contactref element="K1" pad="O1"/>
<contactref element="K1" pad="O0"/>
<contactref element="X1" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="K1" pad="S1"/>
<contactref element="K1" pad="S0"/>
<contactref element="X1" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="J2" pad="8"/>
<contactref element="K1" pad="P1"/>
<contactref element="K1" pad="P0"/>
</signal>
<signal name="N$5">
<contactref element="J4" pad="6"/>
<contactref element="X1" pad="5"/>
</signal>
<signal name="N$6">
<contactref element="J3" pad="1"/>
<contactref element="J4" pad="13"/>
</signal>
<signal name="N$7">
<contactref element="J3" pad="2"/>
<contactref element="J4" pad="12"/>
</signal>
<signal name="N$8">
<contactref element="J3" pad="3"/>
<contactref element="J4" pad="11"/>
</signal>
<signal name="N$9">
<contactref element="J3" pad="4"/>
<contactref element="J4" pad="10"/>
</signal>
<signal name="N$10">
<contactref element="J3" pad="5"/>
<contactref element="J4" pad="9"/>
</signal>
<signal name="N$11">
<contactref element="J3" pad="6"/>
<contactref element="J4" pad="8"/>
</signal>
<signal name="N$12">
<contactref element="J3" pad="7"/>
<contactref element="J4" pad="7"/>
</signal>
<signal name="N$13">
<contactref element="J2" pad="2"/>
<contactref element="J3" pad="10"/>
<contactref element="X1" pad="6"/>
<contactref element="IC1" pad="1"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="J2" pad="7"/>
<contactref element="X1" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="J4" pad="3"/>
<contactref element="K1" pad="2"/>
</signal>
<signal name="N$17">
<contactref element="J2" pad="3"/>
<contactref element="J3" pad="9"/>
</signal>
<signal name="GND">
<contactref element="J5" pad="S1"/>
<contactref element="J5" pad="S2"/>
<contactref element="J5" pad="1"/>
<contactref element="J5" pad="3"/>
<contactref element="J5" pad="5"/>
<contactref element="J5" pad="7"/>
<contactref element="R4" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="J2" pad="1"/>
<contactref element="J3" pad="12"/>
<contactref element="J4" pad="1"/>
<contactref element="J4" pad="2"/>
<contactref element="J3" pad="13"/>
<contactref element="J3" pad="14"/>
<contactref element="J4" pad="14"/>
<contactref element="X1" pad="4"/>
<contactref element="IC1" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="N$16">
<contactref element="J5" pad="6"/>
</signal>
<signal name="N$20">
<contactref element="ZETA4" pad="1"/>
<contactref element="J5" pad="4"/>
</signal>
<signal name="N$21">
<contactref element="R1" pad="1"/>
<contactref element="ZETA4" pad="6"/>
<contactref element="J5" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="N$18">
<contactref element="ZETA4" pad="5"/>
<contactref element="ZETA4" pad="3"/>
<contactref element="R1" pad="2"/>
<contactref element="K1" pad="1"/>
<contactref element="J3" pad="8"/>
<contactref element="IC1" pad="3"/>
<contactref element="J2" pad="4"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="J3" pad="11"/>
<contactref element="J4" pad="5"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
