(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010f0_ffffffff)
      (disableapertmacros false)
      (usegerberextensions true)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "remote-rpi_gbr/")
    )
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad2)")
  (net 2 "VDD")
  (net 3 "/GP24")
  (net 4 "/MOSI")
  (net 5 "GND")
  (net 6 "/MISO")
  (net 7 "/GP25")
  (net 8 "/SCLK")
  (net 9 "/CE0")
  (footprint "LED_SMD:LED_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEF1)
    (at 16.002 9.144)
    (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "LED")
    (property "Sheetfile" "File: remote-rpi.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D1" (at -2.667 0) (layer "F.SilkS"))
    (fp_text value "LTST-C170KFKT" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "/GP25") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9375 0) (size 0.975 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "Net-(D1-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Symbol:OSHW-Logo_5.7x6mm_SilkScreen" (layer "F.Cu")
    (tedit 0)
    (at 9.144 8.382)
    (descr "Open Source Hardware Logo")
    (tags "Logo OSHW")
    (property "Sheetfile" "File: remote-rpi.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "LOGO1" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "Logo_Open_Hardware_Small" (at 0.75 0) (layer "F.Fab") hide)
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 16.002 6.858)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "File: remote-rpi.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at -2.667 0) (layer "F.SilkS"))
    (fp_text value "22R" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 2 "VDD") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902439)
      (net 1 "Net-(D1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "NF-03:Ai-Thinker-NF-03" (layer "B.Cu")
    (tedit 0)
    (at 18.08 1.696 -90)
    (property "Sheetfile" "File: remote-rpi.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U1" (at 9.068 9 unlocked) (layer "B.SilkS"))
    (fp_text value "Ai-Thinker NF-03" (at 12.7 9 unlocked) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 9.068 9 unlocked) (layer "B.Fab"))
    (pad "1" smd roundrect (at 0 0.5 270) (size 0.813 2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 2 "VDD") (pinfunction "VCC") (pintype "power_in"))
    (pad "2" smd roundrect (at 1.27 0.5 270) (size 0.813 2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 5 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "3" smd roundrect (at 2.54 0.5 270) (size 0.813 2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 3 "/GP24") (pinfunction "CE") (pintype "input"))
    (pad "4" smd roundrect (at 3.81 0.5 270) (size 0.813 2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 9 "/CE0") (pinfunction "~{CSN}") (pintype "input"))
    (pad "5" smd roundrect (at 5.08 0.5 270) (size 0.813 2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 8 "/SCLK") (pinfunction "SCK") (pintype "input"))
    (pad "6" smd roundrect (at 6.35 0.5 270) (size 0.813 2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 4 "/MOSI") (pinfunction "MOSI") (pintype "input"))
    (pad "7" smd roundrect (at 7.62 0.5 270) (size 0.813 2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 6 "/MISO") (pinfunction "MISO") (pintype "output"))
    (pad "8" smd roundrect (at 8.89 0.5 270) (size 0.813 2) (layers "B.Cu" "B.Paste" "B.Mask") (roundrect_rratio 0.25)
      (net 7 "/GP25") (pinfunction "IRQ") (pintype "output"))
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_2x04_P2.54mm_Vertical" (layer "B.Cu")
    (tedit 5A19A422)
    (at 21.062 2.29 180)
    (descr "Through hole straight socket strip, 2x04, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 2x04 2.54mm double row")
    (property "Sheetfile" "File: remote-rpi.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J1" (at -1.27 2.77) (layer "B.SilkS") hide)
    (fp_text value "Conn_02x04_Odd_Even" (at -1.27 -10.39) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at -1.27 -3.81 90) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 "VDD") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at -2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 "/GP24") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 "/MOSI") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at -2.54 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 "GND") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 "/MISO") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at -2.54 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 "/GP25") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 "/SCLK") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at -2.54 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "/CE0") (pinfunction "Pin_8") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 25.025 11.325) (end 25.025 0.875) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 0 0) (end 18.825 0) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 18.825 12.2) (end 0 12.2) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 19.7 11.325) (end 25.025 11.325) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 0 12.2) (end 0 0) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 18.825 12.2) (end 19.7 11.325) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 18.825 0) (end 19.7 0.875) (layer "Edge.Cuts") (width 0.1))
  (gr_line (start 25.025 0.875) (end 19.7 0.875) (layer "Edge.Cuts") (width 0.1))
  (gr_text "3.3V\nMOSI\nMISO\nSCK" (at 10.541 6.096) (layer "B.SilkS"))
  (gr_text "CE\nGND\nIRQ\nCSN" (at 11.557 6.096) (layer "B.SilkS"))
  (gr_text "CSL @ Taipei Tech\nnRF24L01+ for RPi\nDANCHOUZHOU\n2022-11-04" (at 8.89 2.54) (layer "F.SilkS"))
)
