(kicad_pcb (version 20171130) (host pcbnew "(5.1.4-0)")
  (general
    (thickness 1.6)
    (drawings 15)
    (tracks 94)
    (zones 0)
    (modules 15)
    (nets 13)
  )
  (page A4)
  (title_block
    (date 2019-06-20)
    (rev 1.1)
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.3048)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "manufacturing/"))
  )
  (net 0 "")
  (net 1 "Net-(U2-Pad6)")
  (net 2 /5VDC)
  (net 3 /DAC)
  (net 4 /SCL)
  (net 5 /GND)
  (net 6 /SDA)
  (net 7 /3.3VDC)
  (net 8 /AMP_REF)
  (net 9 "Net-(C1-Pad2)")
  (net 10 "Net-(R2-Pad1)")
  (net 11 "Net-(J2-PadT)")
  (net 12 "Net-(J2-PadS)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /3.3VDC)
    (add_net /5VDC)
    (add_net /AMP_REF)
    (add_net /DAC)
    (add_net /GND)
    (add_net /SCL)
    (add_net /SDA)
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J2-PadS)")
    (add_net "Net-(J2-PadT)")
    (add_net "Net-(R2-Pad1)")
    (add_net "Net-(RV1-Pad1)")
    (add_net "Net-(RV1-Pad2)")
    (add_net "Net-(RV1-Pad3)")
    (add_net "Net-(U2-Pad6)")
  )
  (module asl_footprints:RJ45_SMD (layer F.Cu) (tedit 5D49D52B)
    (at 132.08 76.2 180)
    (descr "SMD RJ45")
    (fp_text reference J1 (at 0 0) (layer F.SilkS) hide)
    (fp_text value RJ45_HRZ_SMD (at 0 0) (layer F.SilkS) hide)
    (pad G2 smd rect (at 7.35 -7.88 180) (size 3.7 2.2) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at 4.445 -18.205 270) (size 6.35 0.76) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at 3.175 -18.205 270) (size 6.35 0.76) (layers F.Cu F.Paste F.Mask))
    (pad 6 smd rect (at 1.905 -18.205 270) (size 6.35 0.76) (layers F.Cu F.Paste F.Mask)
      (net 2 /5VDC))
    (pad 5 smd rect (at 0.635 -18.205 270) (size 6.35 0.76) (layers F.Cu F.Paste F.Mask)
      (net 3 /DAC))
    (pad 1 smd rect (at -4.445 -18.205 270) (size 6.35 0.76) (layers F.Cu F.Paste F.Mask)
      (net 4 /SCL))
    (pad 2 smd rect (at -3.175 -18.205 270) (size 6.35 0.76) (layers F.Cu F.Paste F.Mask)
      (net 5 /GND))
    (pad 3 smd rect (at -1.905 -18.205 270) (size 6.35 0.76) (layers F.Cu F.Paste F.Mask))
    (pad G1 smd rect (at -7.35 -7.88 180) (size 3.7 2.2) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at -0.635 -18.205 270) (size 6.35 0.76) (layers F.Cu F.Paste F.Mask)
      (net 6 /SDA))
  )
  (module Potentiometer_THT:Potentiometer_Bourns_3386F_Vertical (layer F.Cu) (tedit 5AA07388)
    (at 128.397 110.998 270)
    (descr "Potentiometer, vertical, Bourns 3386F, https://www.bourns.com/pdfs/3386.pdf")
    (tags "Potentiometer vertical Bourns 3386F")
    (fp_text reference RV2 (at -3.048 1.27 180) (layer F.SilkS))
    (fp_text value "50KΩ Trimpot" (at 2.655 3.475 90) (layer F.Fab))
    (fp_text user %R (at -1.11 -2.54) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 /AMP_REF))
    (pad 2 thru_hole circle (at 5.08 -2.54 270) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(R2-Pad1)"))
    (pad 3 thru_hole circle (at 0 -5.08 270) (size 1.44 1.44) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_3386F_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module asl_footprints:MonoJack (layer F.Cu) (tedit 5D49CFC1)
    (at 154.432 84.796)
    (fp_text reference J2 (at -4.318 -7.199) (layer F.SilkS))
    (fp_text value "Mono Audio Jack" (at 0.254 12.446) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad "" np_thru_hole circle (at 0 4.5) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 -2.5) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
    (pad T smd rect (at -3.7 5.8) (size 2.8 2.8) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(J2-PadT)"))
    (pad TN smd rect (at 0.75 9.8) (size 2.8 2.6) (layers F.Cu F.Paste F.Mask))
    (pad S smd rect (at -3.7 -3.6) (size 2.8 2.2) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J2-PadS)"))
  )
  (module Package_SO:TSSOP-8_3x3mm_P0.65mm (layer F.Cu) (tedit 5A02F25C)
    (at 145.669 102.362)
    (descr "TSSOP8: plastic thin shrink small outline package; 8 leads; body width 3 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot505-1_po.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U2 (at 0 -2.55) (layer F.SilkS))
    (fp_text value MCP4541 (at 0 2.55) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2.15 -0.975) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 5 /GND))
    (pad 2 smd rect (at -2.15 -0.325) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 4 /SCL))
    (pad 3 smd rect (at -2.15 0.325) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 6 /SDA))
    (pad 4 smd rect (at -2.15 0.975) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 5 /GND))
    (pad 5 smd rect (at 2.15 0.975) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(R2-Pad1)"))
    (pad 6 smd rect (at 2.15 0.325) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(U2-Pad6)"))
    (pad 7 smd rect (at 2.15 -0.325) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J2-PadS)"))
    (pad 8 smd rect (at 2.15 -0.975) (size 1.1 0.4) (layers F.Cu F.Paste F.Mask)
      (net 7 /3.3VDC))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSSOP-8_3x3mm_P0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 140.335 116.84 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 /AMP_REF))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 140.335 108.712 270)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 0 1.524 90) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(C1-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 /DAC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric (layer F.Cu) (tedit 5B301BBE)
    (at 137.414 102.616 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at 0 2.032 90) (layer F.SilkS))
    (fp_text value 22µF (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 5 /GND))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 7 /3.3VDC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric (layer F.Cu) (tedit 5B301BBE)
    (at 126.746 102.616 270)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at 0 2.032 90) (layer F.SilkS))
    (fp_text value 10µF (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 5 /GND))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 2 /5VDC))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 140.335 112.776 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at 0 1.651 90) (layer F.SilkS))
    (fp_text value 10KΩ (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 "Net-(C1-Pad2)"))
    (pad 1 smd roundrect (at -0.9375 0 90) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 /AMP_REF))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 138.303 112.776 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 0 1.524 90) (layer F.SilkS))
    (fp_text value 15KΩ (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 /AMP_REF))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 "Net-(R2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 147.574 96.774 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at 0 -1.65 90) (layer F.SilkS))
    (fp_text value 2.2KΩ (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 /SDA))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 /3.3VDC))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_0805_2012Metric (layer F.Cu) (tedit 5B36C52B)
    (at 143.51 96.774 270)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at 0 1.524 90) (layer F.SilkS))
    (fp_text value 2.2KΩ (at 0 1.65 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 /SCL))
    (pad 1 smd roundrect (at -0.9375 0 270) (size 0.975 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 /3.3VDC))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module asl_footprints:SOT-223 (layer F.Cu) (tedit 5D0BDDAA)
    (at 132.08 103.124 270)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U1 (at 3.048 -3.048 180) (layer F.SilkS))
    (fp_text value ZLDO1117 (at 0 4.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -3.2 -2.3 270) (size 1.6 1.2) (layers F.Cu F.Paste F.Mask)
      (net 5 /GND))
    (pad 3 smd rect (at -3.2 2.3 270) (size 1.6 1.2) (layers F.Cu F.Paste F.Mask)
      (net 2 /5VDC))
    (pad 2 smd rect (at -3.2 0 270) (size 1.6 1.2) (layers F.Cu F.Paste F.Mask)
      (net 7 /3.3VDC))
    (pad 4 smd rect (at 3.2 0 270) (size 1.6 3.3) (layers F.Cu F.Paste F.Mask))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-8_3.9x4.9mm_P1.27mm (layer F.Cu) (tedit 5C97300E)
    (at 154.94 102.362)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (attr smd)
    (fp_text reference U3 (at 0 -3.4) (layer F.SilkS))
    (fp_text value NCS2211 (at 0 3.4) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -2.475 -1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /GND))
    (pad 2 smd roundrect (at -2.475 -0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 /AMP_REF))
    (pad 3 smd roundrect (at -2.475 0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 /AMP_REF))
    (pad 4 smd roundrect (at -2.475 1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(U2-Pad6)"))
    (pad 5 smd roundrect (at 2.475 1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(J2-PadS)"))
    (pad 6 smd roundrect (at 2.475 0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 /3.3VDC))
    (pad 7 smd roundrect (at 2.475 -0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 /GND))
    (pad 8 smd roundrect (at 2.475 -1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 "Net-(J2-PadT)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module asl_footprints:DIN_Clip (layer F.Cu) (tedit 5D0BF83A)
    (at 145.288 97.844)
    (fp_text reference DRA1 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value "DIN Rail Adapter" (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 0 -12.5) (size 3 3) (drill 3) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 0 12.5) (size 3 3) (drill 3) (layers *.Cu *.Mask))
  )
  (gr_arc (start 124.46 78.74) (end 124.46 76.2) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 157.988 78.74) (end 160.528 78.74) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 157.988 116.84) (end 157.988 119.38) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 124.46 116.84) (end 121.92 116.84) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_text "Licensed under the TAPR Open Hardware License\n(www.tapr.org/OHL)" (at 124.206 97.282 270) (layer B.SilkS))
  (gr_text "Audio\nBoard\nv1.1" (at 157.48 113.7285) (layer F.SilkS))
  (gr_text +Vol (at 123.825 109.601) (layer F.SilkS))
  (gr_line (start 121.92 116.84) (end 121.92 78.74) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 157.988 119.38) (end 124.46 119.38) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 160.528 78.74) (end 160.528 116.84) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 124.46 76.2) (end 157.988 76.2) (layer Edge.Cuts) (width 0.05))
  (zone (net 5) (net_name /GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 114.3 71.12) (xy 175.26 71.12) (xy 175.26 127) (xy 114.3 127)
      )
    )
  )
  (zone (net 5) (net_name /GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 111.76 68.58) (xy 177.8 68.58) (xy 177.8 129.54) (xy 111.76 129.54)
      )
    )
  )
)
