(kicad_pcb (version 4) (host pcbnew "(2015-01-16 BZR 5376)-product")
  (general
    (links 47)
    (no_connects 0)
    (area 33.949999 24.949999 164.050001 133.050001)
    (thickness 1.6)
    (drawings 7327)
    (tracks 181)
    (zones 0)
    (modules 30)
    (nets 40)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
  )
  (setup
    (last_trace_width 0.254)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.254)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.889)
    (via_drill 0.635)
    (via_min_size 0.889)
    (via_min_drill 0.508)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /SwitchGrounds)
  (net 2 /YLimit)
  (net 3 /Z0Stepper0)
  (net 4 /Z0Stepper1)
  (net 5 /Z0Stepper2)
  (net 6 /Z0Stepper3)
  (net 7 /LManipGrounds)
  (net 8 /LManipVac)
  (net 9 /Z0Limit)
  (net 10 /Z1Limit)
  (net 11 /Z2Limit)
  (net 12 /CollisionLimit)
  (net 13 /Z1Stepper0)
  (net 14 /Z1Stepper1)
  (net 15 /Z1Stepper2)
  (net 16 /Z1Stepper3)
  (net 17 /LManipAir)
  (net 18 /SManipGrounds)
  (net 19 /SManipVac)
  (net 20 /SManipAir)
  (net 21 /Z2Stepper0)
  (net 22 /Z2Stepper1)
  (net 23 /Z2Stepper2)
  (net 24 /Z2Stepper3)
  (net 25 /LEDGND)
  (net 26 /LEDVCC)
  (net 27 /PressureGND)
  (net 28 /PressureVCC)
  (net 29 /PressureSignal)
  (net 30 "Net-(P14-Pad1)")
  (net 31 "Net-(P17-Pad1)")
  (net 32 "Net-(P18-Pad1)")
  (net 33 "Net-(P19-Pad1)")
  (net 34 "Net-(P20-Pad1)")
  (net 35 "Net-(P11-Pad2)")
  (net 36 "Net-(P21-Pad1)")
  (net 37 "Net-(P22-Pad1)")
  (net 38 "Net-(P23-Pad1)")
  (net 39 "Net-(P24-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.889)
    (via_drill 0.635)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net /CollisionLimit)
    (add_net /LEDGND)
    (add_net /LEDVCC)
    (add_net /LManipAir)
    (add_net /LManipGrounds)
    (add_net /LManipVac)
    (add_net /PressureGND)
    (add_net /PressureSignal)
    (add_net /PressureVCC)
    (add_net /SManipAir)
    (add_net /SManipGrounds)
    (add_net /SManipVac)
    (add_net /SwitchGrounds)
    (add_net /YLimit)
    (add_net /Z0Limit)
    (add_net /Z0Stepper0)
    (add_net /Z0Stepper1)
    (add_net /Z0Stepper2)
    (add_net /Z0Stepper3)
    (add_net /Z1Limit)
    (add_net /Z1Stepper0)
    (add_net /Z1Stepper1)
    (add_net /Z1Stepper2)
    (add_net /Z1Stepper3)
    (add_net /Z2Limit)
    (add_net /Z2Stepper0)
    (add_net /Z2Stepper1)
    (add_net /Z2Stepper2)
    (add_net /Z2Stepper3)
    (add_net "Net-(P11-Pad2)")
    (add_net "Net-(P14-Pad1)")
    (add_net "Net-(P17-Pad1)")
    (add_net "Net-(P18-Pad1)")
    (add_net "Net-(P19-Pad1)")
    (add_net "Net-(P20-Pad1)")
    (add_net "Net-(P21-Pad1)")
    (add_net "Net-(P22-Pad1)")
    (add_net "Net-(P23-Pad1)")
    (add_net "Net-(P24-Pad1)")
  )
  (module Socket_Strips:Socket_Strip_Straight_1x03_Pitch2.54mm (layer F.Cu) (tedit 58A25A71)
    (at 46 128.2 90)
    (descr "Through hole straight socket strip, 1x03, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x03 2.54mm single row")
    (fp_text reference P1 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value YLIMIT (at -2.4 0.8 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /YLimit))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /SwitchGrounds))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /PressureVCC))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x03_Pitch2.54mm.wrl
      (at (xyz 0 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 58A25717)
    (at 98.6 34.8 90)
    (descr "Through hole straight socket strip, 1x04, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x04 2.54mm single row")
    (fp_text reference P2 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value Z0-M3 (at -2.8 4.2 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /Z0Stepper0))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /Z0Stepper1))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /Z0Stepper2))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /Z0Stepper3))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 58A22DDD)
    (at 86.2 124.1 90)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (fp_text reference P3 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value LMANIPVAC (at -2.5 1.4 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /LManipGrounds))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /LManipVac))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 58A22F5A)
    (at 64.3 128.2 270)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (fp_text reference P4 (at 0 -2.33 270) (layer F.SilkS) hide)
    (fp_text value Z0LIMIT (at -2.4 1.2 360) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /SwitchGrounds))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /Z0Limit))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_2x15_Pitch2.54mm (layer B.Cu) (tedit 58A22E4D)
    (at 84.6 78.1 270)
    (descr "Through hole straight socket strip, 2x15, 2.54mm pitch, double rows")
    (tags "Through hole socket strip THT 2x15 2.54mm double row")
    (fp_text reference P5 (at -1.27 2.33 270) (layer B.SilkS) hide)
    (fp_text value RIBBON (at -1.2 -41.1 270) (layer B.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /Z0Stepper0))
    (pad 2 thru_hole oval (at -2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /Z0Stepper1))
    (pad 3 thru_hole oval (at 0 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /Z0Stepper2))
    (pad 4 thru_hole oval (at -2.54 -2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /Z0Stepper3))
    (pad 5 thru_hole oval (at 0 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /SwitchGrounds))
    (pad 6 thru_hole oval (at -2.54 -5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 /YLimit))
    (pad 7 thru_hole oval (at 0 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /Z0Limit))
    (pad 8 thru_hole oval (at -2.54 -7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /Z1Limit))
    (pad 9 thru_hole oval (at 0 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /Z2Limit))
    (pad 10 thru_hole oval (at -2.54 -10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /CollisionLimit))
    (pad 11 thru_hole oval (at 0 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /Z1Stepper0))
    (pad 12 thru_hole oval (at -2.54 -12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /Z1Stepper1))
    (pad 13 thru_hole oval (at 0 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /Z1Stepper2))
    (pad 14 thru_hole oval (at -2.54 -15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /Z1Stepper3))
    (pad 15 thru_hole oval (at 0 -17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /LManipGrounds))
    (pad 16 thru_hole oval (at -2.54 -17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /LManipVac))
    (pad 17 thru_hole oval (at 0 -20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /LManipAir))
    (pad 18 thru_hole oval (at -2.54 -20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /SManipGrounds))
    (pad 19 thru_hole oval (at 0 -22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /SManipVac))
    (pad 20 thru_hole oval (at -2.54 -22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /SManipAir))
    (pad 21 thru_hole oval (at 0 -25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /Z2Stepper0))
    (pad 22 thru_hole oval (at -2.54 -25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /Z2Stepper1))
    (pad 23 thru_hole oval (at 0 -27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /Z2Stepper2))
    (pad 24 thru_hole oval (at -2.54 -27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /Z2Stepper3))
    (pad 25 thru_hole oval (at 0 -30.48 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /LEDGND))
    (pad 26 thru_hole oval (at -2.54 -30.48 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /LEDVCC))
    (pad 27 thru_hole oval (at 0 -33.02 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /PressureGND))
    (pad 28 thru_hole oval (at -2.54 -33.02 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 28 /PressureVCC))
    (pad 29 thru_hole oval (at 0 -35.56 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 29 /PressureSignal))
    (pad 30 thru_hole oval (at -2.54 -35.56 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(P14-Pad1)"))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_2x15_Pitch2.54mm.wrl
      (at (xyz -0.05 -0.7 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 58A2571B)
    (at 123.8 34.6 90)
    (descr "Through hole straight socket strip, 1x04, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x04 2.54mm single row")
    (fp_text reference P6 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value Z1-M4 (at -2.6 3.5 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /Z1Stepper0))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /Z1Stepper1))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 /Z1Stepper2))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /Z1Stepper3))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 58A25AB8)
    (at 129.2 124.2 90)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (fp_text reference P7 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value LED (at -2.4 1.2 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /LEDGND))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /LEDVCC))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 58A22E27)
    (at 109.8 124.2 90)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (fp_text reference P8 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value LMANIPAIR (at -2.5 1.3 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /LManipGrounds))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /LManipAir))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 58A22DB3)
    (at 40.7 128.2 270)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (fp_text reference P9 (at 0 -2.33 270) (layer F.SilkS) hide)
    (fp_text value Z1LIMIT (at -2.3 1.3 360) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /SwitchGrounds))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /Z1Limit))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 58A22DF8)
    (at 155.1 124.1 90)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (fp_text reference P10 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value SMANIPVAC (at -2.6 1.3 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /SManipGrounds))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /SManipVac))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 58A22E72)
    (at 38.8 48)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (fp_text reference P11 (at 0 -2.33) (layer F.SilkS) hide)
    (fp_text value PRESSURE (at 3 0.9 90) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 27 /PressureGND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 "Net-(P11-Pad2)"))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x04_Pitch2.54mm (layer F.Cu) (tedit 58A2571E)
    (at 147.5 34.9 90)
    (descr "Through hole straight socket strip, 1x04, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x04 2.54mm single row")
    (fp_text reference P12 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value Z2-M5 (at -2.9 4 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /Z2Stepper0))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /Z2Stepper1))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /Z2Stepper2))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /Z2Stepper3))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x04_Pitch2.54mm.wrl
      (at (xyz 0 -0.15 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 58A22F4F)
    (at 56.4 128.2 270)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (fp_text reference P13 (at 0 -2.33 270) (layer F.SilkS) hide)
    (fp_text value Z2LIMIT (at -2.3 1 360) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /SwitchGrounds))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /Z2Limit))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x01_Pitch2.54mm (layer B.Cu) (tedit 58A22E56)
    (at 140.5 75.5)
    (descr "Through hole straight socket strip, 1x01, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x01 2.54mm single row")
    (fp_text reference P14 (at 0 2.33) (layer B.SilkS) hide)
    (fp_text value SPARE (at 0 -2.33) (layer B.SilkS))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 30 "Net-(P14-Pad1)"))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 58A22DE6)
    (at 120.2 124.2 90)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (fp_text reference P15 (at 0 -2.33 90) (layer F.SilkS) hide)
    (fp_text value SMANIPAIR (at -2.4 1.3 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /SManipGrounds))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /SManipAir))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 58A22F5F)
    (at 72.2 128.2 270)
    (descr "Through hole straight socket strip, 1x02, 2.54mm pitch, single row")
    (tags "Through hole socket strip THT 1x02 2.54mm single row")
    (fp_text reference P16 (at 0 -2.33 270) (layer F.SilkS) hide)
    (fp_text value COLLIMIT (at -2.4 1.7 360) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 /SwitchGrounds))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /CollisionLimit))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 270))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_Pad (layer F.Cu) (tedit 58A21DAE)
    (at 38.7 29.9)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (fp_text reference P17 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MOUNT (at 0 4.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 31 "Net-(P17-Pad1)"))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_Pad (layer F.Cu) (tedit 58A21DB3)
    (at 137.8 29.9)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (fp_text reference P18 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MOUNT (at 0 4.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 32 "Net-(P18-Pad1)"))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_Pad (layer F.Cu) (tedit 58A22DA2)
    (at 45.2 122.8)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (fp_text reference P19 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MOUNT (at 0 4.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 33 "Net-(P19-Pad1)"))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_Pad (layer F.Cu) (tedit 58A22DED)
    (at 137.6 127.8)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (fp_text reference P20 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MOUNT (at 0 4.2) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 34 "Net-(P20-Pad1)"))
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58A22E65)
    (at 44.9 48.3 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 2.1 90) (layer B.SilkS))
    (fp_text value R (at 0 -2.1 90) (layer B.SilkS) hide)
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 35 "Net-(P11-Pad2)"))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 27 /PressureGND))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58A22E60)
    (at 44.9 54 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0 2.1 90) (layer B.SilkS))
    (fp_text value R (at 0 -2.1 90) (layer B.SilkS) hide)
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 29 /PressureSignal))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 35 "Net-(P11-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-123 (layer B.Cu) (tedit 58A22E14)
    (at 87.6 119.2)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D1 (at 0 2) (layer B.SilkS))
    (fp_text value DIODE (at 0 -2.1) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.65 0) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask)
      (net 7 /LManipGrounds))
    (pad 2 smd rect (at 1.65 0) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask)
      (net 8 /LManipVac))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-123 (layer B.Cu) (tedit 58A22E19)
    (at 111.1 119.2)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D2 (at 0 2) (layer B.SilkS))
    (fp_text value DIODE (at 0 -2.1) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.65 0) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask)
      (net 7 /LManipGrounds))
    (pad 2 smd rect (at 1.65 0) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask)
      (net 17 /LManipAir))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-123 (layer B.Cu) (tedit 58A22E09)
    (at 153.4 119.2)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D3 (at 0 2) (layer B.SilkS))
    (fp_text value DIODE (at 0 -2.1) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.65 0) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask)
      (net 18 /SManipGrounds))
    (pad 2 smd rect (at 1.65 0) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask)
      (net 19 /SManipVac))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_SOD-123 (layer B.Cu) (tedit 58A22E0E)
    (at 121.5 119.2)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D4 (at 0 2) (layer B.SilkS))
    (fp_text value DIODE (at 0 -2.1) (layer F.SilkS) hide)
    (pad 1 smd rect (at -1.65 0) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask)
      (net 18 /SManipGrounds))
    (pad 2 smd rect (at 1.65 0) (size 0.9 1.2) (layers B.Cu B.Paste B.Mask)
      (net 20 /SManipAir))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_SOD-123.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_Pad (layer F.Cu) (tedit 58A26240)
    (at 39.37 63.5)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (fp_text reference P21 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MOUNT (at 0 4.2) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 36 "Net-(P21-Pad1)"))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_Pad (layer F.Cu) (tedit 58A26246)
    (at 39.37 101.6)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (fp_text reference P22 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MOUNT (at 0 4.2) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 37 "Net-(P22-Pad1)"))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_Pad (layer F.Cu) (tedit 58A26254)
    (at 153.67 63.5)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (fp_text reference P23 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MOUNT (at 0 4.2) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 38 "Net-(P23-Pad1)"))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_Pad (layer F.Cu) (tedit 58A2624D)
    (at 153.67 101.6)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (fp_text reference P24 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MOUNT (at 0 4.2) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 39 "Net-(P24-Pad1)"))
  )
  (gr_line (start 34 133) (end 34 25) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_text 30 (at 120.35 70) (layer B.SilkS))
  (gr_text 29 (at 120.55 82.7) (layer B.SilkS))
  (gr_text 2 (at 83.45 69.9) (layer B.SilkS))
  (gr_text 1 (at 83.4 82.45) (layer B.SilkS))
  (gr_line (start 164 133) (end 34 133) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 164 25) (end 164 133) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 34 25) (end 164 25) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_text "COPYRIGHT (C) FLYSORTER LLC\nDATE CODE: 20170213" (at 132.2 112.1) (layer B.SilkS))
)
