<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.1.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="0" y2="12" width="0.127" layer="20"/>
<wire x1="0" y1="12" x2="25.25" y2="12" width="0.127" layer="20"/>
<wire x1="25.25" y1="12" x2="25.25" y2="0" width="0.127" layer="20"/>
<wire x1="0" y1="0" x2="25.25" y2="0" width="0.127" layer="20"/>
<text>Blinky
Tape</text>
<text>Rev H</text>
<text>5V</text>
<text>D13</text>
<text>GND</text>
<text>blinkinlabs.com</text>
<text>5V</text>
<text>D13</text>
<text>GND</text>
<text>5V</text>
<text>GND</text>
<text>A9</text>
<text>D7</text>
<text>D11</text>
<text>Slot drill with copper</text>
<text>11/2013</text>
</plain>
<libraries>
<library name="blinkiverse">
<description>Library of parts that we use for our Blinkiverse designs. Some parts copied (and modified) from the excellent Sparkfun libraries.
</description>
<packages>
<package name="CRSYTAL_2520">
</package>
<package name="QFN44ML_7X7_LONGLEADS_MOD">
</package>
<package name="MICRO_USB_FCI_THRUHOLE">
</package>
<package name="TEST_VIA_.5MM">
</package>
<package name="CAP_0402_KEMET_MEDIAN">
</package>
<package name="RES_0402_KEMET_MEDIAN">
</package>
<package name="TEST_PAD_SMT">
</package>
<package name="OSHW-LOGO-S">
</package>
<package name="GLOWBOARD_KMR211G_SWITCH">
<description>KMR211G momentary surface mount switch</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="C0603K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 0603 Reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 1608</description>
</package>
</packages>
</library>
<library name="blinkinlabs">
<description>Library of parts that we use for our Blinkinlabs designs. Some parts copied (and modified) from the excellent Sparkfun libraries.
</description>
<packages>
<package name="WS2812B_WIDE_CONNECTOR">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R2" library="blinkiverse" package="RES_0402_KEMET_MEDIAN" value="22"/>
<element name="R1" library="blinkiverse" package="RES_0402_KEMET_MEDIAN" value="22"/>
<element name="C5" library="blinkiverse" package="CAP_0402_KEMET_MEDIAN" value="1uF"/>
<element name="C3" library="blinkiverse" package="CAP_0402_KEMET_MEDIAN" value="0.1uF"/>
<element name="C6" library="blinkiverse" package="CAP_0402_KEMET_MEDIAN" value="18pF"/>
<element name="C7" library="blinkiverse" package="CAP_0402_KEMET_MEDIAN" value="18pF"/>
<element name="C2" library="blinkiverse" package="CAP_0402_KEMET_MEDIAN" value="0.1uF"/>
<element name="C1" library="adafruit" package="C0603K" value="10uF"/>
<element name="U$2" library="blinkiverse" package="QFN44ML_7X7_LONGLEADS_MOD" value="ARDUINO_LEONARDO-REV3B_SMARTPRJ_ATMEGA32U4-XUMU_MODDED"/>
<element name="S1" library="blinkiverse" package="GLOWBOARD_KMR211G_SWITCH" value="Normally open"/>
<element name="Q1" library="blinkiverse" package="CRSYTAL_2520" value="16 MHz"/>
<element name="C4" library="blinkiverse" package="CAP_0402_KEMET_MEDIAN" value="0.1uF"/>
<element name="U$4" library="blinkiverse" package="MICRO_USB_FCI_THRUHOLE" value="MICRO_USBSMT+THRUHULE"/>
<element name="U$1" library="blinkiverse" package="TEST_VIA_.5MM" value="TEST_VIA"/>
<element name="U$3" library="blinkiverse" package="TEST_VIA_.5MM" value="TEST_VIA"/>
<element name="U$5" library="blinkiverse" package="TEST_VIA_.5MM" value="TEST_VIA"/>
<element name="U$6" library="blinkiverse" package="TEST_VIA_.5MM" value="TEST_VIA"/>
<element name="U$7" library="blinkiverse" package="TEST_VIA_.5MM" value="TEST_VIA"/>
<element name="U$8" library="blinkiverse" package="TEST_VIA_.5MM" value="TEST_VIA"/>
<element name="U$10" library="blinkiverse" package="TEST_PAD_SMT" value="TEST_PAD_SMT"/>
<element name="U$11" library="blinkiverse" package="TEST_PAD_SMT" value="TEST_PAD_SMT"/>
<element name="U$12" library="blinkiverse" package="TEST_PAD_SMT" value="TEST_PAD_SMT"/>
<element name="U$13" library="blinkiverse" package="TEST_PAD_SMT" value="TEST_PAD_SMT"/>
<element name="U$14" library="blinkiverse" package="TEST_PAD_SMT" value="TEST_PAD_SMT"/>
<element name="U$15" library="blinkiverse" package="OSHW-LOGO-S" value=""/>
<element name="U$9" library="blinkinlabs" package="WS2812B_WIDE_CONNECTOR" value="WS2812B_CONNECTORWIDE"/>
<element name="R3" library="blinkiverse" package="RES_0402_KEMET_MEDIAN" value="??"/>
</elements>
<signals>
<signal name="GND">
<contactref element="C5" pad="P$2"/>
<contactref element="C3" pad="P$2"/>
<contactref element="C6" pad="P$2"/>
<contactref element="C7" pad="P$2"/>
<contactref element="U$2" pad="5"/>
<contactref element="U$2" pad="35"/>
<contactref element="U$2" pad="23"/>
<contactref element="U$2" pad="15"/>
<contactref element="U$2" pad="43"/>
<contactref element="U$2" pad="PAD@1"/>
<contactref element="S1" pad="P$1"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="P$2"/>
<contactref element="C4" pad="P$2"/>
<contactref element="U$2" pad="PAD@2"/>
<contactref element="U$2" pad="PAD@3"/>
<contactref element="U$2" pad="PAD@4"/>
<contactref element="U$2" pad="PAD@5"/>
<contactref element="U$2" pad="PAD@6"/>
<contactref element="U$2" pad="PAD@7"/>
<contactref element="U$2" pad="PAD@8"/>
<contactref element="U$2" pad="PAD@9"/>
<contactref element="U$2" pad="PAD@10"/>
<contactref element="U$2" pad="PAD@11"/>
<contactref element="U$2" pad="PAD@12"/>
<contactref element="U$2" pad="PAD@13"/>
<contactref element="U$2" pad="PAD@14"/>
<contactref element="U$2" pad="PAD@15"/>
<contactref element="U$2" pad="PAD@16"/>
<contactref element="U$4" pad="PIN$5"/>
<contactref element="U$7" pad="P$1"/>
<contactref element="U$13" pad="P$1"/>
<contactref element="Q1" pad="P$4"/>
<contactref element="Q1" pad="P$2"/>
<contactref element="U$9" pad="GND1"/>
<contactref element="U$9" pad="GND_1"/>
<contactref element="U$9" pad="GND_2"/>
<contactref element="U$9" pad="GND"/>
</signal>
<signal name="MOSI">
<contactref element="U$2" pad="10"/>
<contactref element="U$3" pad="P$1"/>
</signal>
<signal name="MISO">
<contactref element="U$2" pad="11"/>
<contactref element="U$1" pad="P$1"/>
</signal>
<signal name="SCK">
<contactref element="U$2" pad="9"/>
<contactref element="U$5" pad="P$1"/>
</signal>
<signal name="RST">
<contactref element="U$2" pad="13"/>
<contactref element="U$6" pad="P$1"/>
</signal>
<signal name="N$9">
<contactref element="C7" pad="P$1"/>
<contactref element="U$2" pad="17"/>
<contactref element="Q1" pad="P$1"/>
</signal>
<signal name="N$8">
<contactref element="C6" pad="P$1"/>
<contactref element="U$2" pad="16"/>
<contactref element="Q1" pad="P$3"/>
</signal>
<signal name="D+_IN">
<contactref element="R1" pad="P$1"/>
<contactref element="U$4" pad="PIN$3"/>
</signal>
<signal name="D-_IN">
<contactref element="R2" pad="P$1"/>
<contactref element="U$4" pad="PIN$2"/>
</signal>
<signal name="D-">
<contactref element="R2" pad="P$2"/>
<contactref element="U$2" pad="3"/>
</signal>
<signal name="D+">
<contactref element="U$2" pad="4"/>
<contactref element="R1" pad="P$2"/>
</signal>
<signal name="D10">
<contactref element="S1" pad="P$4"/>
<contactref element="U$2" pad="30"/>
</signal>
<signal name="AREF">
<contactref element="U$2" pad="42"/>
</signal>
<signal name="N$2">
<contactref element="U$2" pad="6"/>
<contactref element="C5" pad="P$1"/>
</signal>
<signal name="LED_DATA">
<contactref element="U$9" pad="DATA1"/>
<contactref element="U$9" pad="DATA_1"/>
<contactref element="U$9" pad="DATA_2"/>
<contactref element="U$9" pad="DATA"/>
<contactref element="R3" pad="P$2"/>
</signal>
<signal name="VCC">
<contactref element="C1" pad="1"/>
<contactref element="U$2" pad="34"/>
<contactref element="U$2" pad="44"/>
<contactref element="U$2" pad="24"/>
<contactref element="U$2" pad="14"/>
<contactref element="U$2" pad="2"/>
<contactref element="U$2" pad="7"/>
<contactref element="C2" pad="P$1"/>
<contactref element="C3" pad="P$1"/>
<contactref element="C4" pad="P$1"/>
<contactref element="U$8" pad="P$1"/>
<contactref element="U$4" pad="PIN$1"/>
<contactref element="U$12" pad="P$1"/>
<contactref element="U$9" pad="5V_1"/>
<contactref element="U$9" pad="5V1"/>
<contactref element="U$9" pad="5V"/>
<contactref element="U$9" pad="5V_2"/>
</signal>
<signal name="N$3">
</signal>
<signal name="N$4">
</signal>
<signal name="N$5">
</signal>
<signal name="N$6">
</signal>
<signal name="N$1">
</signal>
<signal name="D11">
<contactref element="U$2" pad="12"/>
<contactref element="U$14" pad="P$1"/>
</signal>
<signal name="D7">
<contactref element="U$2" pad="1"/>
<contactref element="U$10" pad="P$1"/>
</signal>
<signal name="A9">
<contactref element="U$2" pad="29"/>
<contactref element="U$11" pad="P$1"/>
</signal>
<signal name="SHIELD">
<contactref element="U$4" pad="PAD$8"/>
<contactref element="U$4" pad="PAD$10"/>
<contactref element="U$4" pad="PAD$2"/>
<contactref element="U$4" pad="PAD$4"/>
<contactref element="U$4" pad="PAD$5"/>
<contactref element="U$4" pad="PAD$7"/>
<contactref element="U$4" pad="PAD$6"/>
<contactref element="U$4" pad="PAD$1"/>
<contactref element="U$4" pad="PAD$3"/>
<contactref element="U$4" pad="PAD$9"/>
</signal>
<signal name="D13">
<contactref element="U$2" pad="32"/>
<contactref element="R3" pad="P$1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
