(kicad_pcb (version 4) (host pcbnew 4.0.6+dfsg1-1)
  (general
    (links 5)
    (no_connects 1)
    (area 67.177145 77.31 128.462855 145.875)
    (thickness 1.6)
    (drawings 54)
    (tracks 6)
    (zones 0)
    (modules 9)
    (nets 5)
  )
  (page USLetter)
  (title_block
    (title "OSH Park Badge")
    (company www.MakersBox.us)
    (comment 1 "K. Olsen")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.1524)
    (user_trace_width 0.254)
    (user_trace_width 0.3048)
    (user_trace_width 0.4064)
    (user_trace_width 0.6096)
    (user_trace_width 2.032)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.254)
    (edge_width 0.254)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (user_via 1 0.5)
    (uvia_size 0.762)
    (uvia_drill 0.508)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.8 1.8)
    (pad_drill 0.9)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (grid_origin 210.82 95.25)
    (visible_elements 7FFFEFFF)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerbers/))
  )
  (net 0 "")
  (net 1 "Net-(D1-Pad1)")
  (net 2 "Net-(BT1-Pad2)")
  (net 3 "Net-(BT1-Pad1)")
  (net 4 "Net-(D1-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.762)
    (uvia_drill 0.508)
    (add_net "Net-(BT1-Pad1)")
    (add_net "Net-(BT1-Pad2)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D1-Pad2)")
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 5ADA5840)
    (at 99.822 88.265)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at -0.6 -0.5) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 0.9) (layer F.Fab))
    (pad "" thru_hole circle (at 0.18 -0.25) (size 5 5) (drill 2) (layers *.Cu B.Mask))
  )
  (module myFootPrints:MadeInOregonRev25 (layer F.Cu) (tedit 0)
    (at 108.585 93.091)
    (fp_text reference VAL (at 0 0) (layer F.SilkS) hide)
    (fp_text value MadeInOregonRev25 (at 0 0) (layer F.SilkS) hide)
  )
  (module footprints:BATT_CR2032_SMD (layer B.Cu) (tedit 5ADA578A)
    (at 100.22 105.55 180)
    (tags battery)
    (fp_text reference BT1 (at 0 -5.08 180) (layer B.SilkS) hide)
    (fp_text value Battery (at 0 2.54 180) (layer B.SilkS) hide)
    (pad 2 smd circle (at 0.33 0.25 180) (size 17.78 17.78) (layers B.Cu B.Paste B.Mask)
      (net 2 "Net-(BT1-Pad2)"))
    (pad 1 smd rect (at -11.43 0 180) (size 2.54 5.08) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(BT1-Pad1)"))
    (pad 1 smd rect (at 11.43 0 180) (size 2.54 5.08) (layers B.Cu B.Paste B.Mask)
      (net 3 "Net-(BT1-Pad1)"))
  )
  (module footprints:LED_D5.0mm (layer F.Cu) (tedit 5ADA641B)
    (at 101.346 93.345 180)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (fp_text reference D1 (at 1.27 -3.96 180) (layer F.SilkS) hide)
    (fp_text value LED (at 1.27 3.96 180) (layer F.Fab))
    (fp_text user + (at 2.5 1.6 180) (layer F.SilkS))
    (fp_text user %R (at 1.25 0 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 4 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/LEDs.3dshapes/LED_D5.0mm.wrl
      (at (xyz 0 0 -0.12))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5ADA5E91)
    (at 87.63 93.345)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R1 (at 3.81 0) (layer F.SilkS))
    (fp_text value 100 (at 3.556 -2.286) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 "Net-(BT1-Pad1)"))
    (pad 2 thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 4 "Net-(D1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module footprints:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal (layer F.Cu) (tedit 5ADA5E91)
    (at 112.395 93.345 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.16666666666666666W = 1/6W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.16666666666666666W = 1/6W length 3.6mm diameter 1.6mm")
    (fp_text reference R2 (at 3.81 0 180) (layer F.SilkS))
    (fp_text value 100 (at 3.556 -2.286 180) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 "Net-(BT1-Pad2)"))
    (pad 2 thru_hole oval (at 7.62 0 180) (size 1.4 1.4) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module badgelife_dev_board:wrench-neg-mask (layer F.Cu) (tedit 0)
    (at 98.92 116.9)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module badgelife_dev_board:wrench-neg (layer F.Cu) (tedit 0)
    (at 98.92 116.95)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module badgelife_dev_board:wrench-silk-neg (layer B.Cu) (tedit 0)
    (at 98.82 115.15)
    (fp_text reference G*** (at 0 0) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer B.SilkS) hide)
  )
  (gr_text "DC26\nBHV" (at 100.02 100.75) (layer F.Mask))
  (gr_text "DC26\nBHV" (at 100.02 100.75) (layer F.Cu))
  (gr_line (start 105.37 87.3) (end 105.37 87.4) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 102.47 84.4) (end 105.37 87.3) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 97.42 84.4) (end 102.47 84.4) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 94.12 87.7) (end 97.42 84.4) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 110.72 115.95) (end 110.62 115.95) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 110.72 117.6) (end 110.72 115.95) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 111.92 118.8) (end 110.72 117.6) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 115.37 118.8) (end 111.92 118.8) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 115.36 118.74) (end 115.36 118.84) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 110.77 113.11) (end 110.77 117) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 111.89 111.99) (end 110.77 113.11) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 116.18 111.99) (end 111.89 111.99) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 121.9 106.27) (end 116.18 111.99) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 121.9 103.42) (end 121.9 106.27) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 118.01 99.53) (end 121.9 103.42) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 118.01 91.45) (end 118.01 99.53) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 113.93 87.37) (end 118.01 91.45) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 105.35 87.37) (end 113.93 87.37) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 86.91 87.67) (end 94.32 87.67) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 84.15 90.43) (end 86.91 87.67) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 84.15 99.86) (end 84.15 90.43) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 78.9 105.11) (end 84.15 99.86) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 78.9 109.8) (end 78.9 105.11) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 82.2 113.1) (end 78.9 109.8) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 89.19 113.1) (end 82.2 113.1) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 90.53 114.44) (end 89.19 113.1) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 90.53 119.25) (end 90.53 114.44) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 89.61 120.17) (end 90.53 119.25) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 86.34 120.17) (end 89.61 120.17) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 81.03 125.48) (end 86.34 120.17) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 81.03 133.14) (end 81.03 125.48) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 81.44 133.55) (end 81.03 133.14) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 81.95 134.06) (end 81.44 133.55) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 84.2 136.31) (end 81.95 134.06) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 91.77 136.31) (end 84.2 136.31) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 95.85 132.23) (end 91.77 136.31) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 95.85 130.08) (end 95.85 132.23) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 95.85 126.91) (end 95.85 130.08) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 103.61 126.91) (end 95.85 126.91) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 103.61 132.42) (end 103.61 126.91) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 108.32 137.13) (end 103.61 132.42) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 120.99 124.46) (end 108.32 137.13) (angle 90) (layer Edge.Cuts) (width 0.254))
  (gr_line (start 115.47 118.94) (end 120.99 124.46) (angle 90) (layer Edge.Cuts) (width 0.254))
  (dimension 33.909 (width 0.3) (layer Dwgs.User)
    (gr_text "33.909 mm" (at 119.968 100.0125 90) (layer Dwgs.User))
    (feature1 (pts (xy 99.949 83.058) (xy 121.318 83.058)))
    (feature2 (pts (xy 99.949 116.967) (xy 121.318 116.967)))
    (crossbar (pts (xy 118.618 116.967) (xy 118.618 83.058)))
    (arrow1a (pts (xy 118.618 83.058) (xy 119.204421 84.184504)))
    (arrow1b (pts (xy 118.618 83.058) (xy 118.031579 84.184504)))
    (arrow2a (pts (xy 118.618 116.967) (xy 119.204421 115.840496)))
    (arrow2b (pts (xy 118.618 116.967) (xy 118.031579 115.840496)))
  )
  (dimension 34.036 (width 0.3) (layer Dwgs.User)
    (gr_text "1.3400 in" (at 78.533 100.076 90) (layer Dwgs.User))
    (feature1 (pts (xy 99.949 83.058) (xy 77.183 83.058)))
    (feature2 (pts (xy 99.949 117.094) (xy 77.183 117.094)))
    (crossbar (pts (xy 79.883 117.094) (xy 79.883 83.058)))
    (arrow1a (pts (xy 79.883 83.058) (xy 80.469421 84.184504)))
    (arrow1b (pts (xy 79.883 83.058) (xy 79.296579 84.184504)))
    (arrow2a (pts (xy 79.883 117.094) (xy 80.469421 115.967496)))
    (arrow2b (pts (xy 79.883 117.094) (xy 79.296579 115.967496)))
  )
  (dimension 29.845 (width 0.3) (layer Dwgs.User)
    (gr_text "1.1750 in" (at 100.0125 124.54) (layer Dwgs.User))
    (feature1 (pts (xy 114.935 108.966) (xy 114.935 125.89)))
    (feature2 (pts (xy 85.09 108.966) (xy 85.09 125.89)))
    (crossbar (pts (xy 85.09 123.19) (xy 114.935 123.19)))
    (arrow1a (pts (xy 114.935 123.19) (xy 113.808496 123.776421)))
    (arrow1b (pts (xy 114.935 123.19) (xy 113.808496 122.603579)))
    (arrow2a (pts (xy 85.09 123.19) (xy 86.216504 123.776421)))
    (arrow2b (pts (xy 85.09 123.19) (xy 86.216504 122.603579)))
  )
  (dimension 29.845 (width 0.3) (layer Dwgs.User)
    (gr_text "29.845 mm" (at 100.0125 78.66) (layer Dwgs.User))
    (feature1 (pts (xy 114.935 92.075) (xy 114.935 77.31)))
    (feature2 (pts (xy 85.09 92.075) (xy 85.09 77.31)))
    (crossbar (pts (xy 85.09 80.01) (xy 114.935 80.01)))
    (arrow1a (pts (xy 114.935 80.01) (xy 113.808496 80.596421)))
    (arrow1b (pts (xy 114.935 80.01) (xy 113.808496 79.423579)))
    (arrow2a (pts (xy 85.09 80.01) (xy 86.216504 80.596421)))
    (arrow2b (pts (xy 85.09 80.01) (xy 86.216504 79.423579)))
  )
  (gr_text "Designed by \n\nwww.MakersBox.us" (at 104.775 93.218) (layer B.SilkS))
  (gr_text CR2032 (at 86.233 105.029 270) (layer B.SilkS))
  (gr_text "http://www.mathopenref.com/coordpolycalc.html\nx100 y100 6 sides 175 radius 30 deg starting angle" (at 97.82 143.25) (layer Dwgs.User))
)
