<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="50.47" y2="0" width="0" layer="20"/>
<wire x1="50.47" y1="0" x2="50.47" y2="80" width="0" layer="20"/>
<wire x1="50.47" y1="80" x2="0" y2="80" width="0" layer="20"/>
<wire x1="0" y1="80" x2="0" y2="0" width="0" layer="20"/>
<text>Arduboy</text>
<text>by Duncan Young</text>
<text>mk2 Slim</text>
<text>Power</text>
<text>Atmel 32u4 Powered</text>
<text>Design by</text>
<text>Duncan Young</text>
<text>dunkyoung25@gmail.com</text>
<text>Atmel Inside</text>
</plain>
<libraries>
<library name="switch-tact">
<description>&lt;b&gt;Diptronics THMD &amp; SMD tact switches&lt;/b&gt;
&lt;p&gt;&lt;ul&gt;
&lt;li&gt;DTS-3: 3.5x6mm THMD tact switch
&lt;li&gt;DTS-6, DTS-64: 6x6mm THMD tact switch
&lt;li&gt;DTSM-3: 3.5x6mm SMD tact switch
&lt;li&gt;DTSM-6, DTSM-64: 6x6mm SMD tact switch
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Doublecheck before using!&lt;/b&gt;&lt;/p&gt;</description>
<packages>
<package name="DTS-6">
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="P-LCC-4-3">
<description>&lt;h3&gt;Everlight Red/Green/Blue LED&lt;/h3&gt;
67-23/R6GHBHC-B01/2T &lt;b&gt;||&lt;/b&gt; 67-23/R6GHBH-B01</description>
</package>
</packages>
</library>
<library name="solpad">
<description>&lt;b&gt;Solder Pads/Test Points&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="LSP10">
<description>&lt;b&gt;SOLDER PAD&lt;/b&gt;&lt;p&gt;
drill 1.0 mm</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="AVRISP">
</package>
<package name="1X06">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SWITCH-SPDT-SMD">
</package>
</packages>
</library>
<library name="buzzer">
<description>&lt;b&gt;Speakers and Buzzers&lt;/b&gt;&lt;p&gt;
&lt;ul&gt;Distributors:
&lt;li&gt;Buerklin
&lt;li&gt;Spoerle
&lt;li&gt;Schukat
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="AL11P">
<description>&lt;b&gt;SPEAKER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Boards">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find boards and modules: Arduino footprints, breadboards, non-RF modules, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="ARDUINO_PRO_MICRO">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="A" library="switch-tact" package="DTS-6" value="DTS-6">
<attribute name="NAME"/>
</element>
<element name="B" library="switch-tact" package="DTS-6" value="DTS-6">
<attribute name="NAME"/>
</element>
<element name="D1" library="SparkFun-LED" package="P-LCC-4-3" value="">
<attribute name="PROD_ID" value="DIO-12986"/>
<attribute name="VALUE"/>
</element>
<element name="DOWN" library="switch-tact" package="DTS-6" value="DTS-6">
<attribute name="NAME"/>
</element>
<element name="GND" library="solpad" package="LSP10" value="LSP10">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="ISP1" library="adafruit" package="AVRISP" value="AVRISP-6"/>
<element name="JP1" library="adafruit" package="1X06" value="">
<attribute name="VALUE"/>
</element>
<element name="LEFT" library="switch-tact" package="DTS-6" value="DTS-6">
<attribute name="NAME"/>
</element>
<element name="RIGHT" library="switch-tact" package="DTS-6" value="DTS-6">
<attribute name="NAME"/>
</element>
<element name="S1" library="SparkFun-Electromechanical" package="SWITCH-SPDT-SMD" value="">
<attribute name="VALUE"/>
</element>
<element name="U$2" library="SparkFun-Boards" package="ARDUINO_PRO_MICRO" value="ARDUINO_PRO_MICRO"/>
<element name="UP" library="switch-tact" package="DTS-6" value="DTS-6">
<attribute name="NAME"/>
</element>
<element name="VCC" library="solpad" package="LSP10" value="LSP10">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SP1" library="buzzer" package="AL11P" value="AL11P"/>
</elements>
<signals>
<signal name="VCC">
<contactref element="D1" pad="4"/>
<contactref element="JP1" pad="1"/>
<contactref element="U$2" pad="21"/>
<contactref element="S1" pad="3"/>
<contactref element="ISP1" pad="2"/>
</signal>
<signal name="GND">
<contactref element="UP" pad="2"/>
<contactref element="JP1" pad="2"/>
<contactref element="B" pad="2"/>
<contactref element="A" pad="2"/>
<contactref element="LEFT" pad="2"/>
<contactref element="RIGHT" pad="2"/>
<contactref element="DOWN" pad="2"/>
<contactref element="GND" pad="MP"/>
<contactref element="U$2" pad="23"/>
<contactref element="U$2" pad="3"/>
<contactref element="U$2" pad="4"/>
<contactref element="ISP1" pad="6"/>
<contactref element="SP1" pad="+"/>
</signal>
<signal name="UP">
<contactref element="UP" pad="3"/>
<contactref element="U$2" pad="17"/>
</signal>
<signal name="B">
<contactref element="B" pad="3"/>
<contactref element="U$2" pad="11"/>
</signal>
<signal name="A">
<contactref element="A" pad="3"/>
<contactref element="U$2" pad="10"/>
</signal>
<signal name="DOWN">
<contactref element="DOWN" pad="3"/>
<contactref element="U$2" pad="20"/>
</signal>
<signal name="LEFT">
<contactref element="LEFT" pad="3"/>
<contactref element="U$2" pad="19"/>
</signal>
<signal name="RIGHT">
<contactref element="RIGHT" pad="3"/>
<contactref element="U$2" pad="18"/>
</signal>
<signal name="GREEN">
<contactref element="D1" pad="2"/>
<contactref element="U$2" pad="8"/>
</signal>
<signal name="CS">
<contactref element="JP1" pad="5"/>
<contactref element="U$2" pad="6"/>
</signal>
<signal name="DC">
<contactref element="JP1" pad="6"/>
<contactref element="U$2" pad="7"/>
</signal>
<signal name="MOSI">
<contactref element="JP1" pad="4"/>
<contactref element="ISP1" pad="4"/>
<contactref element="U$2" pad="14"/>
</signal>
<signal name="SOUND">
<contactref element="U$2" pad="5"/>
<contactref element="SP1" pad="-"/>
</signal>
<signal name="BLUE">
<contactref element="D1" pad="3"/>
<contactref element="U$2" pad="12"/>
</signal>
<signal name="N$11">
<contactref element="U$2" pad="9"/>
</signal>
<signal name="RED">
<contactref element="D1" pad="1"/>
<contactref element="U$2" pad="13"/>
</signal>
<signal name="BATTVCC">
<contactref element="VCC" pad="MP"/>
<contactref element="S1" pad="2"/>
</signal>
<signal name="RST">
<contactref element="ISP1" pad="5"/>
<contactref element="U$2" pad="22"/>
</signal>
<signal name="MISO">
<contactref element="ISP1" pad="1"/>
</signal>
<signal name="SCK">
<contactref element="ISP1" pad="3"/>
<contactref element="U$2" pad="16"/>
<contactref element="JP1" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
