(kicad_pcb (version 20171130) (host pcbnew "(5.1.0-0)")
  (general
    (thickness 1.6)
    (drawings 40)
    (tracks 231)
    (zones 0)
    (modules 36)
    (nets 17)
  )
  (page USLetter)
  (title_block
    (title "AVR ATtiny412 with integrated boost regulator")
    (date 2019-04-06)
    (rev 1)
    (comment 1 creativecommons.org/licenses)
    (comment 2 "CC BY-SA 4.0")
    (comment 3 "(C) Vlad Belous")
  )
  (layers
    (0 F.Cu mixed)
    (31 B.Cu mixed)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.2032)
    (user_trace_width 0.3048)
    (user_trace_width 0.4064)
    (user_trace_width 0.508)
    (trace_clearance 0.2032)
    (zone_clearance 0)
    (zone_45_only no)
    (trace_min 0.2032)
    (via_size 0.6096)
    (via_drill 0.3048)
    (via_min_size 0.6096)
    (via_min_drill 0.3048)
    (user_via 0.6604 0.3556)
    (user_via 0.762 0.4064)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.0254)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.076200)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 4)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "plot"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 VBAT)
  (net 3 VPP)
  (net 4 VSW)
  (net 5 "Net-(F1-Pad2)")
  (net 6 PA1)
  (net 7 PA2)
  (net 8 PA3)
  (net 9 PA6)
  (net 10 PA7)
  (net 11 UPDI)
  (net 12 "Net-(J14-Pad1)")
  (net 13 "Net-(L1-Pad2)")
  (net 14 "Net-(R1-Pad2)")
  (net 15 "Net-(R3-Pad2)")
  (net 16 "Net-(R5-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2032)
    (trace_width 0.2032)
    (via_dia 0.6096)
    (via_drill 0.3048)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_width 0.2032)
    (diff_pair_gap 0.25)
    (add_net GND)
    (add_net "Net-(F1-Pad2)")
    (add_net "Net-(J14-Pad1)")
    (add_net "Net-(L1-Pad2)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R5-Pad2)")
    (add_net PA1)
    (add_net PA2)
    (add_net PA3)
    (add_net PA6)
    (add_net PA7)
    (add_net UPDI)
    (add_net VBAT)
    (add_net VPP)
    (add_net VSW)
  )
  (module local_footprints:1206_HS (layer F.Cu) (tedit 5C0C843B)
    (at 139.9 98.6)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C1 (at 0 0 -180) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.95) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.65 0) (size 1.3 1.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.65 0) (size 1.3 1.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 VBAT))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module local_footprints:1206_HS (layer F.Cu) (tedit 5C0C843B)
    (at 145.2 100.6 305)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C2 (at -0.278546 0.049115 35) (layer F.SilkS))
    (fp_text value 4.7uF (at 0 1.95 305) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 305) (layer F.Fab))
    (pad 1 smd roundrect (at -1.65 0 305) (size 1.3 1.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VPP))
    (pad 2 smd roundrect (at 1.65 0 305) (size 1.3 1.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module local_footprints:1210_HS (layer F.Cu) (tedit 5C934426)
    (at 147.8 99.8 305)
    (descr "Generic SMD 1210")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C3 (at -0.278546 0.049115 35) (layer F.SilkS))
    (fp_text value 10uF (at 0 2.286 305) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 35) (layer F.Fab))
    (pad 2 smd roundrect (at 1.65 0 305) (size 1.3 2.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.65 0 305) (size 1.3 2.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VPP))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module local_footprints:0805_HS (layer F.Cu) (tedit 5C0C83D5)
    (at 154 104.14 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference C4 (at 0 0) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.75 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 1.15 0 270) (size 1.1 1.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.15 0 270) (size 1.1 1.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VPP))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module local_footprints:1210_HS (layer B.Cu) (tedit 5C934426)
    (at 163.83 102.87 270)
    (descr "Generic SMD 1210")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference C5 (at 0 0 180) (layer B.SilkS))
    (fp_text value 10uF (at 0 -2.286 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd roundrect (at -1.65 0 270) (size 1.3 2.5) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 4 VSW))
    (pad 2 smd roundrect (at 1.65 0 270) (size 1.3 2.5) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module local_footprints:1206_HS (layer F.Cu) (tedit 5C0C843B)
    (at 134.8 98 180)
    (descr "Resistor SMD 1206, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 1206")
    (attr smd)
    (fp_text reference F1 (at 0 0) (layer F.SilkS))
    (fp_text value Polyfuse (at 0 1.95 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd roundrect (at 1.65 0 180) (size 1.3 1.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(F1-Pad2)"))
    (pad 1 smd roundrect (at -1.65 0 180) (size 1.3 1.7) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 VBAT))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module local_footprints:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 5CA97A76)
    (at 162.56 96.52)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference J2 (at 0 -1.6) (layer F.SilkS) hide)
    (fp_text value Conn_01x01 (at 0 2.54) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.6 180) (layer F.Fab) hide)
    (pad 1 thru_hole roundrect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 6 PA1))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x07_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module local_footprints:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 5CA97A76)
    (at 160.02 96.52)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference J3 (at 0 -1.6) (layer F.SilkS) hide)
    (fp_text value Conn_01x01 (at 0 2.54) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.6 180) (layer F.Fab) hide)
    (pad 1 thru_hole roundrect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 7 PA2))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x07_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module local_footprints:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 5CA97A76)
    (at 157.48 96.52)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference J4 (at 0 -1.6) (layer F.SilkS) hide)
    (fp_text value Conn_01x01 (at 0 2.54) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.6 180) (layer F.Fab) hide)
    (pad 1 thru_hole roundrect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 8 PA3))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x07_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module local_footprints:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 5CA97A76)
    (at 165.1 96.52)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference J5 (at 0 -1.6) (layer F.SilkS) hide)
    (fp_text value Conn_01x01 (at 0 2.54) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.6 180) (layer F.Fab) hide)
    (pad 1 thru_hole roundrect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x07_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module local_footprints:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 5CA97A76)
    (at 157.48 109.22)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference J6 (at 0 -1.6) (layer F.SilkS) hide)
    (fp_text value Conn_01x01 (at 0 2.54) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.6 180) (layer F.Fab) hide)
    (pad 1 thru_hole roundrect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 3 VPP))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x07_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module local_footprints:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 5CA97A76)
    (at 160.02 109.22)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference J7 (at 0 -1.6) (layer F.SilkS) hide)
    (fp_text value Conn_01x01 (at 0 2.54) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.6 180) (layer F.Fab) hide)
    (pad 1 thru_hole roundrect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 9 PA6))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x07_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module local_footprints:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 5CA97A76)
    (at 162.56 109.22)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference J8 (at 0 -1.6) (layer F.SilkS) hide)
    (fp_text value Conn_01x01 (at 0 2.54) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.6 180) (layer F.Fab) hide)
    (pad 1 thru_hole roundrect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 10 PA7))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x07_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module local_footprints:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 5CA97A76)
    (at 165.1 109.22)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference J9 (at 0 -1.6) (layer F.SilkS) hide)
    (fp_text value Conn_01x01 (at 0 2.54) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.6 180) (layer F.Fab) hide)
    (pad 1 thru_hole roundrect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x07_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module local_footprints:Conn_1-wire (layer F.Cu) (tedit 5CA97B28)
    (at 149.86 96.52 90)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference J10 (at 0 -1.6 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x01 (at 0 2.54 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.6 270) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 90) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 VPP))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x07_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module local_footprints:Conn_1-wire (layer F.Cu) (tedit 5CA97B28)
    (at 152.4 96.52 90)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference J11 (at 0 -1.6 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x01 (at 0 2.54 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.6 270) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 90) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 11 UPDI))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x07_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module local_footprints:Conn_1-wire (layer F.Cu) (tedit 5CA97B28)
    (at 154.94 96.52 90)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference J12 (at 0 -1.6 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x01 (at 0 2.54 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.6 270) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 90) (size 1.5 1.5) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x07_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module local_footprints:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 5CA97A76)
    (at 166.37 100.33)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference J13 (at 0 -1.6) (layer F.SilkS) hide)
    (fp_text value Conn_01x01 (at 0 2.54) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.6 180) (layer F.Fab) hide)
    (pad 1 thru_hole roundrect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 4 VSW))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x07_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module local_footprints:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 5CA97A76)
    (at 166.37 102.87)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference J14 (at 0 -1.6) (layer F.SilkS) hide)
    (fp_text value Conn_01x01 (at 0 2.54) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.6 180) (layer F.Fab) hide)
    (pad 1 thru_hole roundrect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(J14-Pad1)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x07_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module local_footprints:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 5CA97A76)
    (at 166.37 105.41)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference J15 (at 0 -1.6) (layer F.SilkS) hide)
    (fp_text value Conn_01x01 (at 0 2.54) (layer F.Fab) hide)
    (fp_text user %R (at 0 -1.6 180) (layer F.Fab) hide)
    (pad 1 thru_hole roundrect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x07_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module local_footprints:JST_PH_S2B-PH-K_02x2.00mm_Angled_WiderHole (layer F.Cu) (tedit 5CA9552A)
    (at 133.6 101.6 270)
    (descr "JST PH series connector, S2B-PH-K, side entry type, through hole, Datasheet: http://www.jst-mfg.com/product/pdf/eng/ePH.pdf")
    (tags "connector jst ph")
    (fp_text reference JST_PH_BAT1 (at 1.5 -2.45 270) (layer F.SilkS) hide)
    (fp_text value JST_PH_BAT (at 1 7.25 270) (layer F.Fab))
    (fp_text user %R (at 1 2.5 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 2 0 270) (size 1.397 1.778) (drill 0.8382) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 1 thru_hole roundrect (at 0 0 270) (size 1.397 1.778) (drill 0.8382) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(F1-Pad2)"))
    (model ${KISYS3DMOD}/Connectors_JST.3dshapes/JST_PH_S2B-PH-K_02x2.00mm_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module local_footprints:L_Taiyo-Yuden_NR-S-40xx_HS (layer F.Cu) (tedit 5CA95432)
    (at 138 102.8 270)
    (descr "Inductor, Taiyo Yuden, NR series, Taiyo-Yuden_NR-40xx, 4.0mmx4.0mm")
    (tags "inductor taiyo-yuden nr smd")
    (attr smd)
    (fp_text reference L1 (at 0 0) (layer F.SilkS))
    (fp_text value 4.7uH (at 0 3.5 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 1.8 0 270) (size 2 3.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(L1-Pad2)"))
    (pad 1 smd roundrect (at -1.8 0 270) (size 2 3.9) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 VBAT))
    (model ${KISYS3DMOD}/Inductors_SMD.3dshapes/L_Taiyo-Yuden_NR-40xx.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module local_footprints:0805_HS (layer F.Cu) (tedit 5C0C83D5)
    (at 143.4 107.5)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 0 90) (layer F.SilkS))
    (fp_text value 100k (at 0 1.75) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.15 0) (size 1.1 1.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 VBAT))
    (pad 2 smd roundrect (at 1.15 0) (size 1.1 1.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module local_footprints:0805_HS (layer F.Cu) (tedit 5C0C83D5)
    (at 143.4 109.3)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0 0 90) (layer F.SilkS))
    (fp_text value 100k (at 0 1.75) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.15 0) (size 1.1 1.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.15 0) (size 1.1 1.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module local_footprints:0805_HS (layer F.Cu) (tedit 5C0C83D5)
    (at 149.2 104.8 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 0 0) (layer F.SilkS))
    (fp_text value R (at 0 1.75 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 1.15 0 270) (size 1.1 1.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 "Net-(R3-Pad2)"))
    (pad 1 smd roundrect (at -1.15 0 270) (size 1.1 1.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VPP))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module local_footprints:0805_HS (layer F.Cu) (tedit 5C0C83D5)
    (at 147.4 104.8 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 0 0 180) (layer F.SilkS))
    (fp_text value R (at 0 1.75 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 smd roundrect (at -1.15 0 90) (size 1.1 1.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 "Net-(R3-Pad2)"))
    (pad 2 smd roundrect (at 1.15 0 90) (size 1.1 1.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module local_footprints:0805_HS (layer F.Cu) (tedit 5C0C83D5)
    (at 154 100.2 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at 0 0) (layer F.SilkS))
    (fp_text value 3.3k (at 0 1.75 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -1.15 0 270) (size 1.1 1.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 11 UPDI))
    (pad 2 smd roundrect (at 1.15 0 270) (size 1.1 1.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 "Net-(R5-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module local_footprints:0805_HS (layer F.Cu) (tedit 5C0C83D5)
    (at 161.8 105 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at 0 0 180) (layer F.SilkS))
    (fp_text value 100k (at 0 1.75 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.15 0 90) (size 1.1 1.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.15 0 90) (size 1.1 1.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 PA6))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module local_footprints:0805_HS (layer F.Cu) (tedit 5C0C83D5)
    (at 163.8 105 270)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at 0 0) (layer F.SilkS))
    (fp_text value 1k (at 0 1.75 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -1.15 0 270) (size 1.1 1.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 12 "Net-(J14-Pad1)"))
    (pad 2 smd roundrect (at 1.15 0 270) (size 1.1 1.3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 PA7))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module local_footprints:0805_HS (layer B.Cu) (tedit 5C0C83D5)
    (at 159.5 100.1 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R8 (at 0 0) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.75 90) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd roundrect (at -1.15 0 90) (size 1.1 1.3) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 VPP))
    (pad 2 smd roundrect (at 1.15 0 90) (size 1.1 1.3) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 6 PA1))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module local_footprints:0805_HS (layer B.Cu) (tedit 5C0C83D5)
    (at 157.7 100.1 90)
    (descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R9 (at 0 0) (layer B.SilkS))
    (fp_text value 10k (at 0 -1.75 90) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd roundrect (at 1.15 0 90) (size 1.1 1.3) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 7 PA2))
    (pad 1 smd roundrect (at -1.15 0 90) (size 1.1 1.3) (layers B.Cu B.Paste B.Mask) (roundrect_rratio 0.25)
      (net 3 VPP))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module local_footprints:SW_SPST_PUSH_6mm_3mm (layer F.Cu) (tedit 5C735BCC)
    (at 150.8 108.6 180)
    (descr http://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=1437566-3&DocType=Customer+Drawing&DocLang=English)
    (tags "SPST button tactile switch")
    (attr smd)
    (fp_text reference SW1 (at 0 0 180) (layer F.SilkS))
    (fp_text value SW_Push (at 0 3 180) (layer F.Fab))
    (fp_text user %R (at 0 -2.6 180) (layer F.Fab))
    (pad 2 smd roundrect (at 3.9 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -3.9 0 180) (size 2 1.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 "Net-(R5-Pad2)"))
    (model ${KISYS3DMOD}/Buttons_Switches_SMD.3dshapes/SW_SPST_FSMSM.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module local_footprints:SOT-23-6_HS (layer F.Cu) (tedit 5C04944B)
    (at 142.4 103.2 90)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference U1 (at -2.8 -1.5) (layer F.SilkS))
    (fp_text value MCP1640 (at 0 2.9 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 5 smd roundrect (at 1.3 0 90) (size 1.46 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VPP))
    (pad 6 smd roundrect (at 1.3 -0.95 90) (size 1.46 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 VBAT))
    (pad 4 smd roundrect (at 1.3 0.95 90) (size 1.46 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 "Net-(R3-Pad2)"))
    (pad 3 smd roundrect (at -1.3 0.95 90) (size 1.46 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(R1-Pad2)"))
    (pad 2 smd roundrect (at -1.3 0 90) (size 1.46 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 1 smd roundrect (at -1.3 -0.95 90) (size 1.46 0.65) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 "Net-(L1-Pad2)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module local_footprints:SOT-23_HS (layer F.Cu) (tedit 5C0C84E5)
    (at 136.6 108.2 90)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference U2 (at 1.5 -1.6 180) (layer F.SilkS))
    (fp_text value MIC809 (at 0 2.5 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 3 smd roundrect (at 1.2 0 90) (size 1.3 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 VBAT))
    (pad 2 smd roundrect (at -1.2 0.95 90) (size 1.3 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 14 "Net-(R1-Pad2)"))
    (pad 1 smd roundrect (at -1.2 -0.95 90) (size 1.3 0.8) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module local_footprints:SOIC-8_3.9x4.9mm_Pitch1.27mm_HS (layer F.Cu) (tedit 5C735721)
    (at 157.8 102.87 90)
    (descr "8-Lead Plastic Small Outline (SN) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U3 (at -0.83 0.2) (layer F.SilkS) hide)
    (fp_text value attiny412 (at 0 3.5 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 8 smd roundrect (at 2.9 -1.905 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 7 smd roundrect (at 2.9 -0.635 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 PA3))
    (pad 6 smd roundrect (at 2.9 0.635 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 "Net-(R5-Pad2)"))
    (pad 5 smd roundrect (at 2.9 1.905 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 PA2))
    (pad 4 smd roundrect (at -2.9 1.905 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 PA1))
    (pad 3 smd roundrect (at -2.9 0.635 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 10 PA7))
    (pad 2 smd roundrect (at -2.9 -0.635 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 PA6))
    (pad 1 smd roundrect (at -2.9 -1.905 90) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VPP))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SOIC-8_3.9x4.9mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module local_footprints:SOT-363_SC-70-6_HS (layer F.Cu) (tedit 5CA953DE)
    (at 162.8 100.8 270)
    (descr "SOT-363, SC-70-6")
    (tags "SOT-363 SC-70-6")
    (attr smd)
    (fp_text reference U4 (at -1.1 -1.9 180) (layer F.SilkS))
    (fp_text value MIC9409x (at 0.05 1.95 270) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 6 smd roundrect (at 1.05 -0.7 270) (size 0.85 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 9 PA6))
    (pad 4 smd roundrect (at 1.05 0.7 270) (size 0.85 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 VPP))
    (pad 2 smd roundrect (at -1.05 0 270) (size 0.85 0.32) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 5 smd roundrect (at 1.05 0 270) (size 0.85 0.32) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 GND))
    (pad 3 smd roundrect (at -1.05 0.7 270) (size 0.85 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
    (pad 1 smd roundrect (at -1.05 -0.7 270) (size 0.85 0.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 VSW))
    (model ${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-363_SC-70-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (dimension 15.24 (width 0.15) (layer Cmts.User)
    (gr_text "15.240 mm" (at 176.56 102.87 270) (layer Cmts.User))
    (feature1 (pts (xy 173.99 110.49) (xy 175.846421 110.49)))
    (feature2 (pts (xy 173.99 95.25) (xy 175.846421 95.25)))
    (crossbar (pts (xy 175.26 95.25) (xy 175.26 110.49)))
    (arrow1a (pts (xy 175.26 110.49) (xy 174.673579 109.363496)))
    (arrow1b (pts (xy 175.26 110.49) (xy 175.846421 109.363496)))
    (arrow2a (pts (xy 175.26 95.25) (xy 174.673579 96.376504)))
    (arrow2b (pts (xy 175.26 95.25) (xy 175.846421 96.376504)))
  )
  (dimension 35.56 (width 0.15) (layer Cmts.User)
    (gr_text "35.560 mm" (at 149.86 119.41) (layer Cmts.User))
    (feature1 (pts (xy 167.64 116.84) (xy 167.64 118.696421)))
    (feature2 (pts (xy 132.08 116.84) (xy 132.08 118.696421)))
    (crossbar (pts (xy 132.08 118.11) (xy 167.64 118.11)))
    (arrow1a (pts (xy 167.64 118.11) (xy 166.513496 118.696421)))
    (arrow1b (pts (xy 167.64 118.11) (xy 166.513496 117.523579)))
    (arrow2a (pts (xy 132.08 118.11) (xy 133.206504 118.696421)))
    (arrow2b (pts (xy 132.08 118.11) (xy 133.206504 117.523579)))
  )
  (gr_text DO (at 164.8 102.6 90) (layer F.SilkS))
  (gr_text "I2C\npull-ups" (at 156.7 99.9) (layer B.SilkS))
  (gr_text "CC BY-SA 4.0" (at 154.2 109.1) (layer B.SilkS))
  (gr_text "(C) Vlad Belous" (at 154.2 107.4) (layer B.SilkS))
  (gr_text tiny412 (at 157.9 104) (layer F.SilkS))
  (gr_text "AVR ATtiny412\nwith onboard boost reg\nMCP1640, MCP16251,\n              or TPS6107x" (at 148.2 98.2) (layer B.SilkS))
  (gr_text GND (at 136 103.6) (layer B.SilkS))
  (gr_text VBAT (at 136 101.6) (layer B.SilkS))
  (gr_text VPP (at 157.5 107.7) (layer F.SilkS))
  (gr_text PA6 (at 160 107.7) (layer F.SilkS))
  (gr_text PA7 (at 162.8 107.7) (layer F.SilkS))
  (gr_text GND (at 165.1 107.7) (layer F.SilkS))
  (gr_text GND (at 166.9 107.7 90) (layer F.SilkS))
  (gr_text VSW (at 166.9 98.1 90) (layer F.SilkS))
  (gr_text GND (at 165 98.2) (layer F.SilkS))
  (gr_text PA1 (at 162.6 98.2) (layer F.SilkS))
  (gr_text PA2 (at 160 98.2) (layer F.SilkS))
  (gr_text PA3 (at 157.5 98.2) (layer F.SilkS))
  (gr_text GND (at 154.94 98) (layer F.SilkS))
  (gr_text UPDI (at 152.4 98) (layer F.SilkS))
  (gr_text VPP (at 149.86 98) (layer F.SilkS))
  (gr_text 750mA (at 134.8 96.4) (layer F.SilkS))
  (gr_text "VBAT -> VPP" (at 143.3 96.5) (layer F.SilkS))
  (gr_text R-LO (at 145.8 105 90) (layer F.SilkS))
  (gr_text R-HI (at 150.7 105 90) (layer F.SilkS))
  (gr_text detect (at 140 109.3) (layer F.SilkS))
  (gr_text always (at 140 107.5) (layer F.SilkS))
  (gr_text "Vth\n2.9V" (at 133.6 108.7) (layer F.SilkS))
  (gr_arc (start 133.35 96.52) (end 133.35 95.25) (angle -90) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 133.35 109.22) (end 132.08 109.22) (angle -90) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 166.37 109.22) (end 166.37 110.49) (angle -90) (layer Edge.Cuts) (width 0.0254))
  (gr_arc (start 166.37 96.52) (end 167.64 96.52) (angle -90) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 167.64 96.52) (end 167.64 109.22) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 132.08 96.52) (end 132.08 109.22) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 166.37 95.25) (end 133.35 95.25) (layer Edge.Cuts) (width 0.0254))
  (gr_line (start 166.37 110.49) (end 133.35 110.49) (layer Edge.Cuts) (width 0.0254))
  (dimension 35.56 (width 0.15) (layer Cmts.User)
    (gr_text "1.4000 in" (at 149.86 115.6) (layer Cmts.User))
    (feature1 (pts (xy 132.08 113.03) (xy 132.08 114.886421)))
    (feature2 (pts (xy 167.64 113.03) (xy 167.64 114.886421)))
    (crossbar (pts (xy 167.64 114.3) (xy 132.08 114.3)))
    (arrow1a (pts (xy 132.08 114.3) (xy 133.206504 113.713579)))
    (arrow1b (pts (xy 132.08 114.3) (xy 133.206504 114.886421)))
    (arrow2a (pts (xy 167.64 114.3) (xy 166.513496 113.713579)))
    (arrow2b (pts (xy 167.64 114.3) (xy 166.513496 114.886421)))
  )
  (dimension 15.24 (width 0.15) (layer Cmts.User)
    (gr_text "0.6000 in" (at 172.75 102.87 270) (layer Cmts.User))
    (feature1 (pts (xy 170.18 110.49) (xy 172.036421 110.49)))
    (feature2 (pts (xy 170.18 95.25) (xy 172.036421 95.25)))
    (crossbar (pts (xy 171.45 95.25) (xy 171.45 110.49)))
    (arrow1a (pts (xy 171.45 110.49) (xy 170.863579 109.363496)))
    (arrow1b (pts (xy 171.45 110.49) (xy 172.036421 109.363496)))
    (arrow2a (pts (xy 171.45 95.25) (xy 170.863579 96.376504)))
    (arrow2b (pts (xy 171.45 95.25) (xy 172.036421 96.376504)))
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.3048))
    (min_thickness 0.2032)
    (fill yes (arc_segments 32) (thermal_gap 0.3048) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 130.81 93.98) (xy 168.91 93.98) (xy 168.91 111.76) (xy 130.81 111.76)
      )
    )
  )
  (zone (net 3) (net_name VPP) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254)
    (fill yes (arc_segments 32) (thermal_gap 0.0254) (thermal_bridge_width 0.0508) (smoothing chamfer) (radius 0.0254))
    (polygon
      (pts
        (xy 142.7 101.3) (xy 142.7 101) (xy 142.9 100.6) (xy 143.2 100.3) (xy 144 100.1)
        (xy 143.4 99.2) (xy 142.9 99.7) (xy 142.5 100.1) (xy 142.2 100.6) (xy 142.1 101.1)
        (xy 142.1 101.3)
      )
    )
  )
  (zone (net 13) (net_name "Net-(L1-Pad2)") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254)
    (fill yes (arc_segments 32) (thermal_gap 0.0254) (thermal_bridge_width 0.0508) (smoothing chamfer) (radius 0.0508))
    (polygon
      (pts
        (xy 139.5 103.6) (xy 140.5 103.9) (xy 141.2 103.9) (xy 141.2 104.9) (xy 140.5 104.9)
        (xy 139.5 105.5)
      )
    )
  )
  (zone (net 3) (net_name VPP) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254)
    (fill yes (arc_segments 32) (thermal_gap 0.0254) (thermal_bridge_width 0.0508) (smoothing chamfer) (radius 0.0508))
    (polygon
      (pts
        (xy 144.7 98.660276) (xy 146.155655 98.560276) (xy 146.155655 99.260276) (xy 144.7 99.360276) (xy 144.7 98.960276)
      )
    )
  )
  (zone (net 0) (net_name "") (layers F&B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0))
    (min_thickness 0.0254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.0254) (thermal_bridge_width 0.0508))
    (polygon
      (pts
        (xy 167.6 103.8) (xy 165.3 103.8) (xy 165.3 104.9) (xy 167.6 104.9)
      )
    )
  )
)
