(kicad_pcb (version 20171130) (host pcbnew "(5.1.5)-3")
  (general
    (thickness 1.6)
    (drawings 34)
    (tracks 238)
    (zones 0)
    (modules 32)
    (nets 24)
  )
  (page A4)
  (layers
    (0 Top signal)
    (31 Bottom signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.1524)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 N$4)
  (net 2 N$5)
  (net 3 N$6)
  (net 4 N$7)
  (net 5 N$9)
  (net 6 CLKOUT)
  (net 7 CLKIN)
  (net 8 AGND)
  (net 9 5V)
  (net 10 N$1)
  (net 11 N$2)
  (net 12 V2N)
  (net 13 V2P)
  (net 14 MOSI)
  (net 15 CS)
  (net 16 SCLK)
  (net 17 MISO)
  (net 18 V1P)
  (net 19 V1N)
  (net 20 N$3)
  (net 21 N$8)
  (net 22 N$10)
  (net 23 N$11)
  (net_class Default "This is the default net class."
    (clearance 0.1524)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net 5V)
    (add_net AGND)
    (add_net CLKIN)
    (add_net CLKOUT)
    (add_net CS)
    (add_net MISO)
    (add_net MOSI)
    (add_net N$1)
    (add_net N$10)
    (add_net N$11)
    (add_net N$2)
    (add_net N$3)
    (add_net N$4)
    (add_net N$5)
    (add_net N$6)
    (add_net N$7)
    (add_net N$8)
    (add_net N$9)
    (add_net SCLK)
    (add_net V1N)
    (add_net V1P)
    (add_net V2N)
    (add_net V2P)
  )
  (module "" (layer Top) (tedit 0)
    (at 134.4421 93.6956)
    (fp_text reference @HOLE0 (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS))
    (pad "" np_thru_hole circle (at 0 0) (size 1.6 1.6) (drill 1.6) (layers *.Cu *.Mask))
  )
  (module "" (layer Top) (tedit 0)
    (at 162.6361 93.6956)
    (fp_text reference @HOLE1 (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS))
    (pad "" np_thru_hole circle (at 0 0) (size 1.6 1.6) (drill 1.6) (layers *.Cu *.Mask))
  )
  (module "" (layer Top) (tedit 0)
    (at 134.4421 116.0476)
    (fp_text reference @HOLE2 (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS))
    (pad "" np_thru_hole circle (at 0 0) (size 1.6 1.6) (drill 1.6) (layers *.Cu *.Mask))
  )
  (module "" (layer Top) (tedit 0)
    (at 162.6361 116.0476)
    (fp_text reference @HOLE3 (at 0 0) (layer F.SilkS) hide)
    (fp_text value "" (at 0 0) (layer F.SilkS))
    (pad "" np_thru_hole circle (at 0 0) (size 1.6 1.6) (drill 1.6) (layers *.Cu *.Mask))
  )
  (module C0603 (layer Top) (tedit 0)
    (at 156.2861 95.4736 270)
    (descr <b>0603<b><p>)
    (fp_text reference C1 (at -1.4936 -0.4319 90) (layer F.SilkS))
    (fp_text value 27p (at -1.27 0.1905 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.762 0 270) (size 0.889 0.889) (layers Top F.Paste F.Mask) (roundrect_rratio 0.125)
      (net 8 AGND) (solder_mask_margin 0.0762))
    (pad 1 smd roundrect (at -0.762 0 270) (size 0.889 0.889) (layers Top F.Paste F.Mask) (roundrect_rratio 0.125)
      (net 7 CLKIN) (solder_mask_margin 0.0762))
  )
  (module C0603 (layer Top) (tedit 0)
    (at 162.7885 110.358 270)
    (descr <b>0603<b><p>)
    (fp_text reference C10 (at -1.646 -0.2795 90) (layer F.SilkS))
    (fp_text value 33n (at -1.27 0.1905 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.762 0 270) (size 0.889 0.889) (layers Top F.Paste F.Mask) (roundrect_rratio 0.125)
      (net 3 N$6) (solder_mask_margin 0.0762))
    (pad 1 smd roundrect (at -0.762 0 270) (size 0.889 0.889) (layers Top F.Paste F.Mask) (roundrect_rratio 0.125)
      (net 8 AGND) (solder_mask_margin 0.0762))
  )
  (module AVX-A (layer Top) (tedit 0)
    (at 153.7461 103.0936 90)
    (fp_text reference C11 (at -3.9368 0.1934 90) (layer F.SilkS))
    (fp_text value 10u (at -2.362 2 90) (layer F.Fab))
    (pad - smd rect (at 1.27 0 270) (size 1.27 1.27) (layers Top F.Paste F.Mask)
      (net 8 AGND) (solder_mask_margin 0.0762))
    (pad + smd rect (at -1.27 0 90) (size 1.27 1.27) (layers Top F.Paste F.Mask)
      (net 5 N$9) (solder_mask_margin 0.0762))
  )
  (module C0603 (layer Top) (tedit 0)
    (at 156.2861 103.0936 270)
    (descr <b>0603<b><p>)
    (fp_text reference C12 (at -1.4936 -0.4319 90) (layer F.SilkS))
    (fp_text value 100n (at -1.27 0.1905 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.762 0 270) (size 0.889 0.889) (layers Top F.Paste F.Mask) (roundrect_rratio 0.125)
      (net 5 N$9) (solder_mask_margin 0.0762))
    (pad 1 smd roundrect (at -0.762 0 270) (size 0.889 0.889) (layers Top F.Paste F.Mask) (roundrect_rratio 0.125)
      (net 8 AGND) (solder_mask_margin 0.0762))
  )
  (module C0603 (layer Top) (tedit 0)
    (at 138.5061 95.4736 90)
    (descr <b>0603<b><p>)
    (fp_text reference C2 (at 1.4936 0.4319 90) (layer F.SilkS))
    (fp_text value 27p (at -1.27 0.1905 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.762 0 90) (size 0.889 0.889) (layers Top F.Paste F.Mask) (roundrect_rratio 0.125)
      (net 8 AGND) (solder_mask_margin 0.0762))
    (pad 1 smd roundrect (at -0.762 0 90) (size 0.889 0.889) (layers Top F.Paste F.Mask) (roundrect_rratio 0.125)
      (net 6 CLKOUT) (solder_mask_margin 0.0762))
  )
  (module AVX-A (layer Top) (tedit 0)
    (at 139.7761 103.0936 90)
    (fp_text reference C3 (at 2.4386 0.2696 90) (layer F.SilkS))
    (fp_text value 10u (at -2.362 2 90) (layer F.Fab))
    (pad - smd rect (at 1.27 0 270) (size 1.27 1.27) (layers Top F.Paste F.Mask)
      (net 8 AGND) (solder_mask_margin 0.0762))
    (pad + smd rect (at -1.27 0 90) (size 1.27 1.27) (layers Top F.Paste F.Mask)
      (net 9 5V) (solder_mask_margin 0.0762))
  )
  (module C0603 (layer Top) (tedit 0)
    (at 134.6961 103.0936 270)
    (descr <b>0603<b><p>)
    (fp_text reference C4 (at -1.7476 -0.4319 90) (layer F.SilkS))
    (fp_text value 100n (at -1.27 0.1905 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.762 0 270) (size 0.889 0.889) (layers Top F.Paste F.Mask) (roundrect_rratio 0.125)
      (net 9 5V) (solder_mask_margin 0.0762))
    (pad 1 smd roundrect (at -0.762 0 270) (size 0.889 0.889) (layers Top F.Paste F.Mask) (roundrect_rratio 0.125)
      (net 8 AGND) (solder_mask_margin 0.0762))
  )
  (module AVX-A (layer Top) (tedit 0)
    (at 142.3161 103.0936 90)
    (fp_text reference C5 (at 2.4132 0.295 90) (layer F.SilkS))
    (fp_text value 10u (at -2.362 2 90) (layer F.Fab))
    (pad - smd rect (at 1.27 0 270) (size 1.27 1.27) (layers Top F.Paste F.Mask)
      (net 8 AGND) (solder_mask_margin 0.0762))
    (pad + smd rect (at -1.27 0 90) (size 1.27 1.27) (layers Top F.Paste F.Mask)
      (net 9 5V) (solder_mask_margin 0.0762))
  )
  (module C0603 (layer Top) (tedit 0)
    (at 137.2361 103.0936 270)
    (descr <b>0603<b><p>)
    (fp_text reference C6 (at -1.7476 -0.4319 90) (layer F.SilkS))
    (fp_text value 100n (at -1.27 0.1905 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.762 0 270) (size 0.889 0.889) (layers Top F.Paste F.Mask) (roundrect_rratio 0.125)
      (net 9 5V) (solder_mask_margin 0.0762))
    (pad 1 smd roundrect (at -0.762 0 270) (size 0.889 0.889) (layers Top F.Paste F.Mask) (roundrect_rratio 0.125)
      (net 8 AGND) (solder_mask_margin 0.0762))
  )
  (module C0603 (layer Top) (tedit 0)
    (at 152.6285 110.358 90)
    (descr <b>0603<b><p>)
    (fp_text reference C7 (at -1.27 0.254 90) (layer F.Mask))
    (fp_text value 33n (at -1.27 0.1905 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.762 0 90) (size 0.889 0.889) (layers Top F.Paste F.Mask) (roundrect_rratio 0.125)
      (net 1 N$4) (solder_mask_margin 0.0762))
    (pad 1 smd roundrect (at -0.762 0 90) (size 0.889 0.889) (layers Top F.Paste F.Mask) (roundrect_rratio 0.125)
      (net 8 AGND) (solder_mask_margin 0.0762))
  )
  (module C0603 (layer Top) (tedit 0)
    (at 147.5485 110.358 90)
    (descr <b>0603<b><p>)
    (fp_text reference C8 (at -1.651 -0.889 90) (layer F.SilkS))
    (fp_text value 33n (at -1.27 0.1905 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.762 0 90) (size 0.889 0.889) (layers Top F.Paste F.Mask) (roundrect_rratio 0.125)
      (net 2 N$5) (solder_mask_margin 0.0762))
    (pad 1 smd roundrect (at -0.762 0 90) (size 0.889 0.889) (layers Top F.Paste F.Mask) (roundrect_rratio 0.125)
      (net 8 AGND) (solder_mask_margin 0.0762))
  )
  (module C0603 (layer Top) (tedit 0)
    (at 142.4685 110.358 270)
    (descr <b>0603<b><p>)
    (fp_text reference C9 (at -1.646 -0.2795 90) (layer F.SilkS))
    (fp_text value 33n (at -1.27 0.1905 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.762 0 270) (size 0.889 0.889) (layers Top F.Paste F.Mask) (roundrect_rratio 0.125)
      (net 4 N$7) (solder_mask_margin 0.0762))
    (pad 1 smd roundrect (at -0.762 0 270) (size 0.889 0.889) (layers Top F.Paste F.Mask) (roundrect_rratio 0.125)
      (net 8 AGND) (solder_mask_margin 0.0762))
  )
  (module HC49UP (layer Top) (tedit 0)
    (at 147.3961 95.4736 180)
    (descr <b>CRYSTAL</b>)
    (fp_text reference Q1 (at 8.4581 -2.8244) (layer F.SilkS))
    (fp_text value 3.58MHz (at -5.715 4.191) (layer F.Fab))
    (pad 2 smd rect (at 4.826 0 180) (size 5.334 1.9304) (layers Top F.Paste F.Mask)
      (net 6 CLKOUT) (solder_mask_margin 0.0762))
    (pad 1 smd rect (at -4.826 0 180) (size 5.334 1.9304) (layers Top F.Paste F.Mask)
      (net 7 CLKIN) (solder_mask_margin 0.0762))
  )
  (module RS_20-M (layer Top) (tedit 0)
    (at 148.1327 103.3984 90)
    (fp_text reference U1 (at -3.2816 -5.6387) (layer F.SilkS))
    (fp_text value ADE7763ARSZSSOP20 (at 14.2444 -14.7827 180) (layer F.Fab))
    (fp_text user * (at -4.318 -3.2766 90) (layer F.SilkS))
    (fp_text user * (at -4.318 -3.2766 90) (layer F.Fab))
    (pad 20 smd rect (at 3.4798 -2.921 90) (size 2.3622 0.4826) (layers Top F.Paste F.Mask)
      (net 14 MOSI) (solder_mask_margin 0.0762))
    (pad 19 smd rect (at 3.4798 -2.286 90) (size 2.3622 0.4826) (layers Top F.Paste F.Mask)
      (net 17 MISO) (solder_mask_margin 0.0762))
    (pad 18 smd rect (at 3.4798 -1.6256 90) (size 2.3622 0.4826) (layers Top F.Paste F.Mask)
      (net 16 SCLK) (solder_mask_margin 0.0762))
    (pad 17 smd rect (at 3.4798 -0.9652 90) (size 2.3622 0.4826) (layers Top F.Paste F.Mask)
      (net 15 CS) (solder_mask_margin 0.0762))
    (pad 16 smd rect (at 3.4798 -0.3302 90) (size 2.3622 0.4826) (layers Top F.Paste F.Mask)
      (net 6 CLKOUT) (solder_mask_margin 0.0762))
    (pad 15 smd rect (at 3.4798 0.3302 90) (size 2.3622 0.4826) (layers Top F.Paste F.Mask)
      (net 7 CLKIN) (solder_mask_margin 0.0762))
    (pad 14 smd rect (at 3.4798 0.9652 90) (size 2.3622 0.4826) (layers Top F.Paste F.Mask)
      (net 20 N$3) (solder_mask_margin 0.0762))
    (pad 13 smd rect (at 3.4798 1.6256 90) (size 2.3622 0.4826) (layers Top F.Paste F.Mask)
      (net 21 N$8) (solder_mask_margin 0.0762))
    (pad 12 smd rect (at 3.4798 2.286 90) (size 2.3622 0.4826) (layers Top F.Paste F.Mask)
      (net 22 N$10) (solder_mask_margin 0.0762))
    (pad 11 smd rect (at 3.4798 2.921 90) (size 2.3622 0.4826) (layers Top F.Paste F.Mask)
      (net 23 N$11) (solder_mask_margin 0.0762))
    (pad 10 smd rect (at -3.4798 2.921 90) (size 2.3622 0.4826) (layers Top F.Paste F.Mask)
      (net 8 AGND) (solder_mask_margin 0.0762))
    (pad 9 smd rect (at -3.4798 2.286 90) (size 2.3622 0.4826) (layers Top F.Paste F.Mask)
      (net 5 N$9) (solder_mask_margin 0.0762))
    (pad 8 smd rect (at -3.4798 1.6256 90) (size 2.3622 0.4826) (layers Top F.Paste F.Mask)
      (net 8 AGND) (solder_mask_margin 0.0762))
    (pad 7 smd rect (at -3.4798 0.9652 90) (size 2.3622 0.4826) (layers Top F.Paste F.Mask)
      (net 3 N$6) (solder_mask_margin 0.0762))
    (pad 6 smd rect (at -3.4798 0.3302 90) (size 2.3622 0.4826) (layers Top F.Paste F.Mask)
      (net 1 N$4) (solder_mask_margin 0.0762))
    (pad 5 smd rect (at -3.4798 -0.3302 90) (size 2.3622 0.4826) (layers Top F.Paste F.Mask)
      (net 2 N$5) (solder_mask_margin 0.0762))
    (pad 4 smd rect (at -3.4798 -0.9652 90) (size 2.3622 0.4826) (layers Top F.Paste F.Mask)
      (net 4 N$7) (solder_mask_margin 0.0762))
    (pad 3 smd rect (at -3.4798 -1.6256 90) (size 2.3622 0.4826) (layers Top F.Paste F.Mask)
      (net 9 5V) (solder_mask_margin 0.0762))
    (pad 2 smd rect (at -3.4798 -2.286 90) (size 2.3622 0.4826) (layers Top F.Paste F.Mask)
      (net 9 5V) (solder_mask_margin 0.0762))
    (pad 1 smd rect (at -3.4798 -2.921 90) (size 2.3622 0.4826) (layers Top F.Paste F.Mask)
      (net 9 5V) (solder_mask_margin 0.0762))
  )
  (module R0603 (layer Top) (tedit 0)
    (at 139.9285 110.358 90)
    (fp_text reference R1 (at -1.6256 -0.8636 90) (layer F.SilkS))
    (fp_text value 1K (at -1.651 1.4605 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.762 0 90) (size 0.889 0.889) (layers Top F.Paste F.Mask) (roundrect_rratio 0.125)
      (net 4 N$7) (solder_mask_margin 0.0762))
    (pad 1 smd roundrect (at -0.762 0 90) (size 0.889 0.889) (layers Top F.Paste F.Mask) (roundrect_rratio 0.125)
      (net 11 N$2) (solder_mask_margin 0.0762))
  )
  (module R0603 (layer Top) (tedit 0)
    (at 150.0885 110.358 90)
    (fp_text reference R2 (at -1.5494 -0.9652 90) (layer F.SilkS))
    (fp_text value 1K (at -1.651 1.4605 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.762 0 90) (size 0.889 0.889) (layers Top F.Paste F.Mask) (roundrect_rratio 0.125)
      (net 1 N$4) (solder_mask_margin 0.0762))
    (pad 1 smd roundrect (at -0.762 0 90) (size 0.889 0.889) (layers Top F.Paste F.Mask) (roundrect_rratio 0.125)
      (net 12 V2N) (solder_mask_margin 0.0762))
  )
  (module R0603 (layer Top) (tedit 0)
    (at 160.2485 110.358 90)
    (fp_text reference R3 (at -1.651 -0.9398 90) (layer F.SilkS))
    (fp_text value 1K (at -1.651 1.4605 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.762 0 90) (size 0.889 0.889) (layers Top F.Paste F.Mask) (roundrect_rratio 0.125)
      (net 3 N$6) (solder_mask_margin 0.0762))
    (pad 1 smd roundrect (at -0.762 0 90) (size 0.889 0.889) (layers Top F.Paste F.Mask) (roundrect_rratio 0.125)
      (net 13 V2P) (solder_mask_margin 0.0762))
  )
  (module R0603 (layer Top) (tedit 0)
    (at 145.0085 110.358 90)
    (fp_text reference R4 (at -1.5748 -1.016 90) (layer F.SilkS))
    (fp_text value 1K (at -1.651 1.4605 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.762 0 90) (size 0.889 0.889) (layers Top F.Paste F.Mask) (roundrect_rratio 0.125)
      (net 2 N$5) (solder_mask_margin 0.0762))
    (pad 1 smd roundrect (at -0.762 0 90) (size 0.889 0.889) (layers Top F.Paste F.Mask) (roundrect_rratio 0.125)
      (net 10 N$1) (solder_mask_margin 0.0762))
  )
  (module C0603 (layer Top) (tedit 0)
    (at 155.2955 110.358 270)
    (descr <b>0603<b><p>)
    (fp_text reference C13 (at -1.9 -0.4065 90) (layer F.SilkS))
    (fp_text value 33n (at -1.27 0.1905 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.762 0 270) (size 0.889 0.889) (layers Top F.Paste F.Mask) (roundrect_rratio 0.125)
      (net 10 N$1) (solder_mask_margin 0.0762))
    (pad 1 smd roundrect (at -0.762 0 270) (size 0.889 0.889) (layers Top F.Paste F.Mask) (roundrect_rratio 0.125)
      (net 8 AGND) (solder_mask_margin 0.0762))
  )
  (module C0603 (layer Top) (tedit 0)
    (at 137.3885 110.358 270)
    (descr <b>0603<b><p>)
    (fp_text reference C14 (at -1.646 -0.2795 90) (layer F.SilkS))
    (fp_text value 33n (at -1.27 0.1905 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.762 0 270) (size 0.889 0.889) (layers Top F.Paste F.Mask) (roundrect_rratio 0.125)
      (net 11 N$2) (solder_mask_margin 0.0762))
    (pad 1 smd roundrect (at -0.762 0 270) (size 0.889 0.889) (layers Top F.Paste F.Mask) (roundrect_rratio 0.125)
      (net 8 AGND) (solder_mask_margin 0.0762))
  )
  (module R0603 (layer Top) (tedit 0)
    (at 157.8355 110.358 90)
    (fp_text reference R5 (at -1.7018 -0.9652 90) (layer F.SilkS))
    (fp_text value 100 (at -1.651 1.4605 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.762 0 90) (size 0.889 0.889) (layers Top F.Paste F.Mask) (roundrect_rratio 0.125)
      (net 19 V1N) (solder_mask_margin 0.0762))
    (pad 1 smd roundrect (at -0.762 0 90) (size 0.889 0.889) (layers Top F.Paste F.Mask) (roundrect_rratio 0.125)
      (net 10 N$1) (solder_mask_margin 0.0762))
  )
  (module R0603 (layer Top) (tedit 0)
    (at 134.8485 110.358 90)
    (fp_text reference R6 (at -1.6002 -0.9652 90) (layer F.SilkS))
    (fp_text value 100 (at -1.651 1.4605 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.762 0 90) (size 0.889 0.889) (layers Top F.Paste F.Mask) (roundrect_rratio 0.125)
      (net 18 V1P) (solder_mask_margin 0.0762))
    (pad 1 smd roundrect (at -0.762 0 90) (size 0.889 0.889) (layers Top F.Paste F.Mask) (roundrect_rratio 0.125)
      (net 11 N$2) (solder_mask_margin 0.0762))
  )
  (module H10-2.54 (layer Top) (tedit 0)
    (at 148.4121 116.5556 270)
    (fp_text reference J1 (at 0.635 -2.54) (layer F.Mask))
    (fp_text value 10p-2.54 (at 2.54 1.27) (layer F.Fab))
    (pad 10 thru_hole circle (at 0 11.43 270) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask)
      (net 8 AGND) (solder_mask_margin 0.0762))
    (pad 9 thru_hole circle (at 0 8.89 270) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask)
      (net 15 CS) (solder_mask_margin 0.0762))
    (pad 8 thru_hole circle (at 0 6.35 270) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask)
      (net 16 SCLK) (solder_mask_margin 0.0762))
    (pad 7 thru_hole circle (at 0 3.81 270) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask)
      (net 14 MOSI) (solder_mask_margin 0.0762))
    (pad 6 thru_hole circle (at 0 1.27 270) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask)
      (net 17 MISO) (solder_mask_margin 0.0762))
    (pad 5 thru_hole circle (at 0 -1.27 270) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask)
      (net 12 V2N) (solder_mask_margin 0.0762))
    (pad 4 thru_hole circle (at 0 -3.81 270) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask)
      (net 13 V2P) (solder_mask_margin 0.0762))
    (pad 3 thru_hole circle (at 0 -6.35 270) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask)
      (net 19 V1N) (solder_mask_margin 0.0762))
    (pad 2 thru_hole circle (at 0 -8.89 270) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask)
      (net 18 V1P) (solder_mask_margin 0.0762))
    (pad 1 thru_hole rect (at 0 -11.43 270) (size 1.651 1.651) (drill 0.889) (layers *.Cu *.Mask)
      (net 9 5V) (solder_mask_margin 0.0762))
  )
  (module OSHW-LOGO-M (layer Bottom) (tedit 0)
    (at 148.7169 107.2592 180)
    (fp_text reference LOGO1 (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value OSHW-LOGOM (at 0 0 180) (layer B.SilkS) hide)
  )
  (module SMD1,27-2,54 (layer Bottom) (tedit 0)
    (at 162.0011 98.0136 90)
    (descr "<b>SMD PAD</b>")
    (fp_text reference INT (at -1.0538 -2.629 90) (layer B.SilkS))
    (fp_text value WIREPADSMD1,27-254 (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at 0 0 90) (size 1.27 2.54) (layers Bottom B.Paste B.Mask)
      (net 20 N$3) (solder_mask_margin 0.0762))
  )
  (module SMD1,27-2,54 (layer Bottom) (tedit 0)
    (at 162.0011 103.0936 90)
    (descr "<b>SMD PAD</b>")
    (fp_text reference ZX (at -0.8252 -2.6798 90) (layer B.SilkS))
    (fp_text value WIREPADSMD1,27-254 (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at 0 0 90) (size 1.27 2.54) (layers Bottom B.Paste B.Mask)
      (net 22 N$10) (solder_mask_margin 0.0762))
  )
  (module SMD1,27-2,54 (layer Bottom) (tedit 0)
    (at 162.0011 100.5536 90)
    (descr "<b>SMD PAD</b>")
    (fp_text reference SAG (at -1.4856 -2.6798 90) (layer B.SilkS))
    (fp_text value WIREPADSMD1,27-254 (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at 0 0 90) (size 1.27 2.54) (layers Bottom B.Paste B.Mask)
      (net 21 N$8) (solder_mask_margin 0.0762))
  )
  (module SMD1,27-2,54 (layer Bottom) (tedit 0)
    (at 162.0011 105.6336 90)
    (descr "<b>SMD PAD</b>")
    (fp_text reference CF (at -0.9776 -2.6544 90) (layer B.SilkS))
    (fp_text value WIREPADSMD1,27-254 (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at 0 0 90) (size 1.27 2.54) (layers Bottom B.Paste B.Mask)
      (net 23 N$11) (solder_mask_margin 0.0762))
  )
  (gr_line (start 132.1561 94.2136) (end 132.1561 115.7936) (layer Edge.Cuts) (width 0.4064))
  (gr_arc (start 134.6961 115.7936) (end 132.1561 115.7936) (angle -90) (layer Edge.Cuts) (width 0.4064))
  (gr_line (start 134.6961 118.3336) (end 162.3061 118.3336) (layer Edge.Cuts) (width 0.4064))
  (gr_arc (start 162.3061 115.7936) (end 162.3061 118.3336) (angle -90) (layer Edge.Cuts) (width 0.4064))
  (gr_line (start 164.8461 115.7936) (end 164.8461 94.2136) (layer Edge.Cuts) (width 0.4064))
  (gr_arc (start 162.3061 94.2136) (end 164.8461 94.2136) (angle -90) (layer Edge.Cuts) (width 0.4064))
  (gr_line (start 162.3061 91.6736) (end 134.6961 91.6736) (layer Edge.Cuts) (width 0.4064))
  (gr_arc (start 134.6961 94.2136) (end 134.6961 91.6736) (angle -90) (layer Edge.Cuts) (width 0.4064))
  (gr_text 5V (at 160.0961 114.7776 90) (layer F.SilkS))
  (gr_text V2P (at 152.5269 114.9554 90) (layer F.SilkS))
  (gr_text V2N (at 149.9615 114.9554 90) (layer F.SilkS))
  (gr_text MISO (at 147.4977 114.9808 90) (layer F.SilkS))
  (gr_text MOSI (at 144.9069 114.8284 90) (layer F.SilkS))
  (gr_text SCLK (at 142.3669 114.93 90) (layer F.SilkS))
  (gr_text CS (at 139.9285 114.6506 90) (layer F.SilkS))
  (gr_text "ADE7763\nBreakout" (at 157.4037 104.008) (layer F.SilkS))
  (gr_text "by Tisham Dhar" (at 152.2983 94.0258) (layer B.SilkS))
  (gr_text http://whatnicklife.blogspot.com (at 156.3623 95.7784) (layer B.SilkS))
  (gr_text "v4.0 11/02/2020" (at 152.5777 97.785) (layer B.SilkS))
  (gr_text "MAX Vp-p = 1V" (at 154.3303 98.5724) (layer F.SilkS))
  (gr_text C:/Users/tisham/Pictures/Artwork/whatnick_elec_logo.bmp (at 129.6161 118.4606) (layer F.SilkS))
  (gr_text V1N (at 154.9399 114.93 90) (layer F.SilkS))
  (gr_text V1P (at 157.4291 114.93 90) (layer F.SilkS))
  (gr_text GND (at 137.2361 114.7776 90) (layer F.SilkS))
  (gr_text GND (at 136.3979 114.7776 -90) (layer B.SilkS))
  (gr_text CS (at 139.1411 114.6506 -90) (layer B.SilkS))
  (gr_text SCLK (at 141.5287 114.93 -90) (layer B.SilkS))
  (gr_text MOSI (at 144.0687 114.8284 -90) (layer B.SilkS))
  (gr_text MISO (at 146.6849 114.9554 -90) (layer B.SilkS))
  (gr_text V2N (at 149.1995 114.9046 -90) (layer B.SilkS))
  (gr_text V2P (at 151.7649 114.8792 -90) (layer B.SilkS))
  (gr_text V1N (at 154.1779 114.9554 -90) (layer B.SilkS))
  (gr_text V1P (at 156.6417 114.9554 -90) (layer B.SilkS))
  (gr_text 5V (at 159.2325 114.7776 -90) (layer B.SilkS))
  (zone (net 8) (net_name AGND) (layer Top) (hatch edge 0.508)
    (priority 6)
    (connect_pads (clearance 0.000001))
    (min_thickness 0.2032)
    (fill yes (arc_segments 32) (thermal_gap 0.4564) (thermal_bridge_width 0.4564))
    (polygon
      (pts
        (xy 165.3793 118.5368) (xy 131.9529 118.5368) (xy 131.9529 91.4604) (xy 165.3793 91.4604)
      )
    )
  )
  (zone (net 8) (net_name AGND) (layer Bottom) (hatch edge 0.508)
    (priority 6)
    (connect_pads (clearance 0.000001))
    (min_thickness 0.2032)
    (fill yes (arc_segments 32) (thermal_gap 0.4564) (thermal_bridge_width 0.4564))
    (polygon
      (pts
        (xy 165.3793 118.5368) (xy 131.9529 118.5368) (xy 131.9529 91.4604) (xy 165.3793 91.4604)
      )
    )
  )
)
