(kicad_pcb (version 4) (host pcbnew 4.0.2-stable)
  (general
    (links 39)
    (no_connects 0)
    (area 196.02152 51.078 266.288523 97.636001)
    (thickness 1.6)
    (drawings 20)
    (tracks 92)
    (zones 0)
    (modules 15)
    (nets 18)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user hide)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.254)
    (trace_clearance 0.254)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x310fc_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory gerbers))
  )
  (net 0 "")
  (net 1 +12V)
  (net 2 GND)
  (net 3 "Net-(C2-Pad1)")
  (net 4 +5V)
  (net 5 "Net-(CON1-Pad1)")
  (net 6 /D15)
  (net 7 /D2)
  (net 8 /D3)
  (net 9 /D4)
  (net 10 /D9)
  (net 11 /D8)
  (net 12 /D7)
  (net 13 "Net-(D2-Pad1)")
  (net 14 "Net-(J2-Pad1)")
  (net 15 "Net-(J2-Pad2)")
  (net 16 "Net-(J4-Pad1)")
  (net 17 "Net-(J4-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net /D15)
    (add_net /D2)
    (add_net /D3)
    (add_net /D4)
    (add_net /D7)
    (add_net /D8)
    (add_net /D9)
    (add_net GND)
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(CON1-Pad1)")
    (add_net "Net-(D2-Pad1)")
  )
  (net_class Power ""
    (clearance 0.254)
    (trace_width 0.508)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +12V)
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad2)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(J4-Pad2)")
  )
  (module Wickerlib:DIP-16-W7.62MM-LONGPADS (layer F.Cu) (tedit 579044C0)
    (at 247.904 80.518 180)
    (descr "16-lead dip package, row spacing 7.62 mm (300 mils), longer pads")
    (tags "dil dip 2.54 300")
    (fp_text reference U2 (at 4.064 8.128 180) (layer F.Fab))
    (fp_text value SN754410PDIP (at 4.064 9.144 270) (layer F.Fab) hide)
    (fp_text user %R (at 3.81 21.336 180) (layer F.SilkS))
    (pad 1 thru_hole oval (at 0 0 180) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 /D2))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 8 /D3))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(J2-Pad1)"))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(J2-Pad2)"))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 9 /D4))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 +12V))
    (pad 9 thru_hole oval (at 7.62 17.78 180) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 10 /D9))
    (pad 10 thru_hole oval (at 7.62 15.24 180) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 11 /D8))
    (pad 11 thru_hole oval (at 7.62 12.7 180) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(J4-Pad1)"))
    (pad 12 thru_hole oval (at 7.62 10.16 180) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 13 thru_hole oval (at 7.62 7.62 180) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 14 thru_hole oval (at 7.62 5.08 180) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(J4-Pad2)"))
    (pad 15 thru_hole oval (at 7.62 2.54 180) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 12 /D7))
    (pad 16 thru_hole oval (at 7.62 0 180) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 4 +5V))
    (model Housings_DIP.3dshapes/DIP-16-W7.62MM-LONGPADS.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wickerlib:TEENSY-3.2-NOSILK (layer F.Cu) (tedit 5737ABAB)
    (at 225.552 84.328 180)
    (fp_text reference J1 (at -10.16 25.4 360) (layer F.SilkS))
    (fp_text value TEENSY3.2-72MHz (at -2.54 20.32 180) (layer F.Fab))
    (fp_text user "TEENSY 3.2" (at 2.54 25.4 180) (layer F.SilkS))
    (pad G1 thru_hole circle (at -10.16 -10.16 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 0 thru_hole circle (at -10.16 -7.62 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 1 thru_hole circle (at -10.16 -5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole circle (at -10.16 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 /D2))
    (pad 3 thru_hole circle (at -10.16 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 /D3))
    (pad 4 thru_hole circle (at -10.16 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 9 /D4))
    (pad 5 thru_hole circle (at -10.16 5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 6 thru_hole circle (at -10.16 7.62 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 7 thru_hole circle (at -10.16 10.16 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 /D7))
    (pad 8 thru_hole circle (at -10.16 12.7 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 /D8))
    (pad 9 thru_hole circle (at -10.16 15.24 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 /D9))
    (pad 10 thru_hole circle (at -10.16 17.78 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 11 thru_hole circle (at -10.16 20.32 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 12 thru_hole circle (at -10.16 22.86 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad VBAT thru_hole circle (at -7.62 22.86 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 3V1 thru_hole circle (at -5.08 22.86 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad G2 thru_hole circle (at -2.54 22.86 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad PGM thru_hole circle (at 0 22.86 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad DAC thru_hole circle (at 2.54 22.86 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 13 thru_hole circle (at 5.08 22.86 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 16 thru_hole circle (at 5.08 15.24 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 3V2 thru_hole circle (at 5.08 -5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 18 thru_hole circle (at 5.08 10.16 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 17 thru_hole circle (at 5.08 12.7 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad AG thru_hole circle (at 5.08 -7.62 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 22 thru_hole circle (at 5.08 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad VIN thru_hole circle (at 5.08 -10.16 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 +5V))
    (pad 21 thru_hole circle (at 5.08 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 20 thru_hole circle (at 5.08 5.08 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 19 thru_hole circle (at 5.08 7.62 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 23 thru_hole circle (at 5.08 -2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 14 thru_hole circle (at 5.08 20.32 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS))
    (pad 15 thru_hole circle (at 5.08 17.78 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 /D15))
  )
  (module Wickerlib:CONN-ONSHORE-SCREW-GREEN-2PIN-TH (layer F.Cu) (tedit 57902EA8)
    (at 246.38 90.17 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J2 (at 0 1.27 90) (layer F.Fab))
    (fp_text value CONN-TERM-SCREW-GREEN-2.54MM-2POS-TH (at -2.286 1.27 180) (layer F.Fab) hide)
    (fp_text user %R (at 4.318 0.254 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(J2-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(J2-Pad2)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:CONN-ONSHORE-SCREW-GREEN-3PIN-TH (layer F.Cu) (tedit 5790402C)
    (at 211.582 89.662 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J3 (at 0 2.54 90) (layer F.Fab))
    (fp_text value CONN-TERM-SCREW-GREEN-2.54MM-3POS-TH (at 2.286 3.302 180) (layer F.Fab) hide)
    (fp_text user %R (at 4.318 -0.508 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 /D15))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 4 +5V))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:CONN-ONSHORE-SCREW-GREEN-2PIN-TH (layer F.Cu) (tedit 57902EA8)
    (at 240.03 90.17 90)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference J4 (at 0 1.27 90) (layer F.Fab))
    (fp_text value CONN-TERM-SCREW-GREEN-2.54MM-2POS-TH (at -2.286 1.27 180) (layer F.Fab) hide)
    (fp_text user %R (at 4.318 0.254 180) (layer F.SilkS))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(J4-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 "Net-(J4-Pad2)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Wickerlib:RLC-0603-SMD (layer F.Cu) (tedit 579029AB)
    (at 211.062 73.914)
    (descr "Capacitor SMD RLC-0603-SMD, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor RLC-0603-SMD")
    (attr smd)
    (fp_text reference C1 (at 0.09 0.04) (layer F.Fab))
    (fp_text value "10uF 25V" (at 0 1.9) (layer F.Fab) hide)
    (fp_text user %R (at 0.07 -1.51) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +12V))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_RLC-0603-SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wickerlib:RLC-0603-SMD (layer F.Cu) (tedit 579029AB)
    (at 214.364 84.836)
    (descr "Capacitor SMD RLC-0603-SMD, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor RLC-0603-SMD")
    (attr smd)
    (fp_text reference C2 (at 0.09 0.04) (layer F.Fab))
    (fp_text value "10uF 25V" (at 0 1.9) (layer F.Fab) hide)
    (fp_text user %R (at 2.806 0) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_RLC-0603-SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wickerlib:RLC-0603-SMD (layer F.Cu) (tedit 579029AB)
    (at 212.852 59.944)
    (descr "Capacitor SMD RLC-0603-SMD, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor RLC-0603-SMD")
    (attr smd)
    (fp_text reference C3 (at 0.09 0.04) (layer F.Fab))
    (fp_text value 1uF (at 0 1.9) (layer F.Fab) hide)
    (fp_text user %R (at 0.07 -1.51) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +12V))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_RLC-0603-SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wickerlib:RLC-0603-SMD (layer F.Cu) (tedit 579029AB)
    (at 215.634 73.914 180)
    (descr "Capacitor SMD RLC-0603-SMD, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor RLC-0603-SMD")
    (attr smd)
    (fp_text reference C4 (at 0.09 0.04 180) (layer F.Fab))
    (fp_text value 0.1uF (at 0 1.9 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 1.524 180) (layer F.SilkS))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_RLC-0603-SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wickerlib:CONN-BARREL-JACK-2.5x5.5MM-TH (layer F.Cu) (tedit 5743C0C2)
    (at 203.2 87.93734 90)
    (descr "DC Barrel Jack")
    (tags "Power Jack")
    (fp_text reference CON1 (at -5.08 -3.302 270) (layer F.SilkS))
    (fp_text value BARREL_JACK (at 0 -5.99948 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 6.20014 0 90) (size 3.81 3.81) (drill 2.99974) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(CON1-Pad1)"))
    (pad 2 thru_hole circle (at 0.20066 0 90) (size 3.81 3.81) (drill 2.99974) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
    (pad 3 thru_hole circle (at 3.2004 4.699 90) (size 3.81 3.81) (drill 2.99974) (layers *.Cu *.Mask F.SilkS)
      (net 2 GND))
  )
  (module Wickerlib:DIODE-SMA (layer F.Cu) (tedit 579032A9)
    (at 203.708 75.438 270)
    (descr "Diode SMA")
    (tags "Diode SMA")
    (attr smd)
    (fp_text reference D1 (at 0 0 450) (layer F.Fab))
    (fp_text value 14V (at 0 0 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 2.54 450) (layer F.SilkS))
    (pad 1 smd rect (at -1.99898 0 270) (size 2.49936 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(CON1-Pad1)"))
    (pad 2 smd rect (at 1.99898 0 270) (size 2.49936 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Diodes_SMD.3dshapes/SMA_Standard.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 180))
    )
  )
  (module Wickerlib:DIODE-SMA (layer F.Cu) (tedit 579032A9)
    (at 203.708 67.056 270)
    (descr "Diode SMA")
    (tags "Diode SMA")
    (attr smd)
    (fp_text reference D2 (at 0 0 450) (layer F.Fab))
    (fp_text value "20V 1A" (at 0 0 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 2.794 450) (layer F.SilkS))
    (pad 1 smd rect (at -1.99898 0 270) (size 2.49936 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 1.99898 0 270) (size 2.49936 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(CON1-Pad1)"))
    (model Diodes_SMD.3dshapes/SMA_Standard.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 180))
    )
  )
  (module Wickerlib:DIODE-SMA (layer F.Cu) (tedit 579032A9)
    (at 213.36 79.46898 270)
    (descr "Diode SMA")
    (tags "Diode SMA")
    (attr smd)
    (fp_text reference D3 (at 0 0 450) (layer F.Fab))
    (fp_text value "20V 1A" (at 0 0 270) (layer F.Fab) hide)
    (fp_text user %R (at -2.032 2.794 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.99898 0 270) (size 2.49936 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 4 +5V))
    (pad 2 smd rect (at 1.99898 0 270) (size 2.49936 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (model Diodes_SMD.3dshapes/SMA_Standard.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3937 0.3937 0.3937))
      (rotate (xyz 0 0 180))
    )
  )
  (module Wickerlib:RLC-1812-SMD (layer F.Cu) (tedit 579037B4)
    (at 203.708 58.942 90)
    (descr "Capacitor SMD RLC-1812-SMD, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor RLC-1812-SMD")
    (attr smd)
    (fp_text reference F1 (at 0 0 90) (layer F.Fab))
    (fp_text value "1.1A 25V" (at 0 0 90) (layer F.Fab) hide)
    (fp_text user %R (at 0.014 -2.794 270) (layer F.SilkS))
    (pad 1 smd rect (at -2.3 0 90) (size 1 3) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(D2-Pad1)"))
    (pad 2 smd rect (at 2.3 0 90) (size 1 3) (layers F.Cu F.Paste F.Mask)
      (net 1 +12V))
    (model Capacitors_SMD.3dshapes/C_RLC-1812-SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Wickerlib:SOT-223 (layer F.Cu) (tedit 0)
    (at 212.852 66.548 180)
    (descr "module CMS SOT223 4 pins")
    (tags "CMS SOT")
    (attr smd)
    (fp_text reference U1 (at 5.08 3.81 360) (layer F.SilkS))
    (fp_text value NCP1117ST50T3G (at 0 0.762 180) (layer F.Fab))
    (pad 4 smd rect (at 0 -3.302 180) (size 3.6576 2.032) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0 3.302 180) (size 1.016 2.032) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 3 smd rect (at 2.286 3.302 180) (size 1.016 2.032) (layers F.Cu F.Paste F.Mask)
      (net 1 +12V))
    (pad 1 smd rect (at -2.286 3.302 180) (size 1.016 2.032) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model TO_SOT_Packages_SMD.3dshapes/SOT-223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text 8/11/2016 (at 204.978 52.578) (layer F.Fab))
  (gr_text "MyoRaptor Controller v1.0" (at 237.236 52.578) (layer F.Fab))
  (gr_text +5V (at 216.662 94.996 90) (layer F.SilkS))
  (gr_text GND (at 214.122 94.996 90) (layer F.SilkS))
  (gr_text SIG (at 211.582 94.742 90) (layer F.SilkS))
  (gr_text M- (at 248.92 95.25 90) (layer F.SilkS))
  (gr_text M+ (at 246.38 95.25 90) (layer F.SilkS))
  (gr_text M- (at 242.824 95.25 90) (layer F.SilkS))
  (gr_text M+ (at 240.284 95.25 90) (layer F.SilkS))
  (gr_text "Chloe Fleming\n8/11/2016" (at 207.772 58.928) (layer B.SilkS))
  (gr_text "MyoRaptor Controller v1.0" (at 235.712 57.658) (layer B.SilkS))
  (gr_line (start 198.12 54.864) (end 198.12 97.536) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 251.968 54.864) (end 198.12 54.864) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 251.968 57.912) (end 251.968 54.864) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 251.968 97.536) (end 251.968 57.912) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 198.12 97.536) (end 251.968 97.536) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 251.968 97.536) (xy 198.12 97.536) (xy 198.12 54.864) (xy 251.968 54.864) (xy 251.968 97.536)
      )
    )
  )
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 251.968 97.536) (xy 198.12 97.536) (xy 198.12 54.864) (xy 251.968 54.864) (xy 251.968 97.536)
      )
    )
  )
)
