(kicad_pcb (version 20171130) (host pcbnew "(5.1.5-0-10_14)")
  (general
    (thickness 1.6)
    (drawings 17)
    (tracks 74)
    (zones 0)
    (modules 16)
    (nets 43)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.05)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.12)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad2)")
  (net 2 "Net-(C1-Pad1)")
  (net 3 +3V3)
  (net 4 "Net-(C3-Pad2)")
  (net 5 "Net-(C3-Pad1)")
  (net 6 GND)
  (net 7 "Net-(C4-Pad1)")
  (net 8 "Net-(C5-Pad2)")
  (net 9 "Net-(J1-Pad16)")
  (net 10 "Net-(J1-Pad14)")
  (net 11 "Net-(J1-Pad12)")
  (net 12 "Net-(J1-Pad11)")
  (net 13 "Net-(J1-Pad10)")
  (net 14 "Net-(J1-Pad9)")
  (net 15 "Net-(J1-Pad8)")
  (net 16 "Net-(J1-Pad7)")
  (net 17 "Net-(J1-Pad6)")
  (net 18 "Net-(J1-Pad5)")
  (net 19 "Net-(J1-Pad4)")
  (net 20 /RX)
  (net 21 /TX)
  (net 22 "Net-(J1-Pad1)")
  (net 23 /T1)
  (net 24 "Net-(J2-PadTN)")
  (net 25 /R1)
  (net 26 "Net-(J2-PadRN)")
  (net 27 /T2)
  (net 28 "Net-(J3-PadTN)")
  (net 29 /R2)
  (net 30 "Net-(J3-PadRN)")
  (net 31 "Net-(J4-Pad12)")
  (net 32 "Net-(J4-Pad11)")
  (net 33 "Net-(J4-Pad10)")
  (net 34 "Net-(J4-Pad9)")
  (net 35 /D12)
  (net 36 "Net-(J4-Pad7)")
  (net 37 "Net-(J4-Pad6)")
  (net 38 "Net-(J4-Pad5)")
  (net 39 "Net-(J4-Pad4)")
  (net 40 /D5)
  (net 41 "Net-(J4-Pad2)")
  (net 42 "Net-(J4-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +3V3)
    (add_net /D12)
    (add_net /D5)
    (add_net /R1)
    (add_net /R2)
    (add_net /RX)
    (add_net /T1)
    (add_net /T2)
    (add_net /TX)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C4-Pad1)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(J1-Pad1)")
    (add_net "Net-(J1-Pad10)")
    (add_net "Net-(J1-Pad11)")
    (add_net "Net-(J1-Pad12)")
    (add_net "Net-(J1-Pad14)")
    (add_net "Net-(J1-Pad16)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(J1-Pad7)")
    (add_net "Net-(J1-Pad8)")
    (add_net "Net-(J1-Pad9)")
    (add_net "Net-(J2-PadRN)")
    (add_net "Net-(J2-PadTN)")
    (add_net "Net-(J3-PadRN)")
    (add_net "Net-(J3-PadTN)")
    (add_net "Net-(J4-Pad1)")
    (add_net "Net-(J4-Pad10)")
    (add_net "Net-(J4-Pad11)")
    (add_net "Net-(J4-Pad12)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(J4-Pad4)")
    (add_net "Net-(J4-Pad5)")
    (add_net "Net-(J4-Pad6)")
    (add_net "Net-(J4-Pad7)")
    (add_net "Net-(J4-Pad9)")
  )
  (module chickadee:chickadee_3mm_fcu (layer B.Cu) (tedit 0)
    (at 132.715 113.665 180)
    (fp_text reference G*** (at 0 0) (layer B.SilkS) hide)
    (fp_text value "Chickadee 3mm" (at 0.75 0) (layer B.SilkS) hide)
  )
  (module chickadee:chickadee_3mm_fcu (layer F.Cu) (tedit 0)
    (at 117.475 102.87)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value "Chickadee 3mm" (at 0.75 0) (layer F.SilkS) hide)
  )
  (module MountingHole:MountingHole_2.5mm (layer F.Cu) (tedit 56D1B4CB)
    (at 110.49 120.65)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.5mm (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.5mm (layer F.Cu) (tedit 56D1B4CB)
    (at 110.49 102.87)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.5mm (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.5mm (layer F.Cu) (tedit 56D1B4CB)
    (at 156.21 120.65)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.5mm (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module MountingHole:MountingHole_2.5mm (layer F.Cu) (tedit 56D1B4CB)
    (at 156.21 102.87)
    (descr "Mounting Hole 2.5mm, no annular")
    (tags "mounting hole 2.5mm no annular")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.5) (layer F.SilkS) hide)
    (fp_text value MountingHole_2.5mm (at 0 3.5) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 np_thru_hole circle (at 0 0) (size 2.5 2.5) (drill 2.5) (layers *.Cu *.Mask))
  )
  (module Package_SO:TSSOP-16_4.4x5mm_P0.65mm (layer F.Cu) (tedit 5A02F25C)
    (at 133.35 110.49 90)
    (descr "16-Lead Plastic Thin Shrink Small Outline (ST)-4.4 mm Body [TSSOP] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SSOP 0.65")
    (attr smd)
    (fp_text reference U1 (at 0 -3.55 90) (layer F.SilkS) hide)
    (fp_text value MAX232 (at 0 3.55 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 16 smd rect (at 2.95 -2.275 90) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 3 +3V3))
    (pad 15 smd rect (at 2.95 -1.625 90) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (pad 14 smd rect (at 2.95 -0.975 90) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 23 /T1))
    (pad 13 smd rect (at 2.95 -0.325 90) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 25 /R1))
    (pad 12 smd rect (at 2.95 0.325 90) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 20 /RX))
    (pad 11 smd rect (at 2.95 0.975 90) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 21 /TX))
    (pad 10 smd rect (at 2.95 1.625 90) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 35 /D12))
    (pad 9 smd rect (at 2.95 2.275 90) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 40 /D5))
    (pad 8 smd rect (at -2.95 2.275 90) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 29 /R2))
    (pad 7 smd rect (at -2.95 1.625 90) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 27 /T2))
    (pad 6 smd rect (at -2.95 0.975 90) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C5-Pad2)"))
    (pad 5 smd rect (at -2.95 0.325 90) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C3-Pad2)"))
    (pad 4 smd rect (at -2.95 -0.325 90) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C3-Pad1)"))
    (pad 3 smd rect (at -2.95 -0.975 90) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(C1-Pad2)"))
    (pad 2 smd rect (at -2.95 -1.625 90) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C4-Pad1)"))
    (pad 1 smd rect (at -2.95 -2.275 90) (size 1.5 0.45) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSSOP-16_4.4x5mm_P0.65mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x12_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A41D)
    (at 152.4 101.6 270)
    (descr "Through hole straight socket strip, 1x12, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x12 2.54mm single row")
    (fp_text reference J4 (at 0 -2.77 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x12_Female (at 0 30.71 90) (layer F.Fab))
    (fp_text user %R (at 0 13.97) (layer F.Fab))
    (pad 12 thru_hole oval (at 0 27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 31 "Net-(J4-Pad12)"))
    (pad 11 thru_hole oval (at 0 25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "Net-(J4-Pad11)"))
    (pad 10 thru_hole oval (at 0 22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 33 "Net-(J4-Pad10)"))
    (pad 9 thru_hole oval (at 0 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 34 "Net-(J4-Pad9)"))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 35 /D12))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 36 "Net-(J4-Pad7)"))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 37 "Net-(J4-Pad6)"))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 38 "Net-(J4-Pad5)"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "Net-(J4-Pad4)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 40 /D5))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 41 "Net-(J4-Pad2)"))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 42 "Net-(J4-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x12_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module adafruit:4UCONN_19269_TRS (layer F.Cu) (tedit 5C84372C)
    (at 156.21 111.76 180)
    (descr "<br>\n4UCONN: 19269\n<br>\n4UCONN: 19268\n<br>\n4UCONN: 19267\n<br>\nhttp://www.4uconnector.com/online/Itemadrawing.asp?fldseries=19267&seriesno_a=18")
    (fp_text reference J3 (at 1.9 -0.4) (layer F.SilkS) hide)
    (fp_text value AudioJack3_SwitchTR (at 4.445 4.445) (layer F.Fab))
    (pad S smd rect (at 2.5 3.5 180) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 6 GND) (solder_mask_margin 0.0508))
    (pad T smd rect (at 11.7 3.5 180) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 27 /T2) (solder_mask_margin 0.0508))
    (pad TN smd rect (at 15.8 -0.75 270) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(J3-PadTN)") (solder_mask_margin 0.0508))
    (pad R smd rect (at 4.3 -3.5 180) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 29 /R2) (solder_mask_margin 0.0508))
    (pad RN smd rect (at 1.5 -3.5 180) (size 1.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(J3-PadRN)") (solder_mask_margin 0.0508))
    (pad "" np_thru_hole circle (at 3.5 0 180) (size 2 2) (drill 2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 10.5 0 180) (size 2 2) (drill 2) (layers *.Cu *.Mask))
  )
  (module adafruit:4UCONN_19269_TRS (layer F.Cu) (tedit 5C84372C)
    (at 110.49 111.76)
    (descr "<br>\n4UCONN: 19269\n<br>\n4UCONN: 19268\n<br>\n4UCONN: 19267\n<br>\nhttp://www.4uconnector.com/online/Itemadrawing.asp?fldseries=19267&seriesno_a=18")
    (fp_text reference J2 (at 1.9 -0.4) (layer F.SilkS) hide)
    (fp_text value AudioJack3_SwitchTR (at 4.445 4.445) (layer F.Fab))
    (pad S smd rect (at 2.5 3.5) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 6 GND) (solder_mask_margin 0.0508))
    (pad T smd rect (at 11.7 3.5) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 23 /T1) (solder_mask_margin 0.0508))
    (pad TN smd rect (at 15.8 -0.75 90) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(J2-PadTN)") (solder_mask_margin 0.0508))
    (pad R smd rect (at 4.3 -3.5) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 25 /R1) (solder_mask_margin 0.0508))
    (pad RN smd rect (at 1.5 -3.5) (size 1.2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(J2-PadRN)") (solder_mask_margin 0.0508))
    (pad "" np_thru_hole circle (at 3.5 0) (size 2 2) (drill 2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 10.5 0) (size 2 2) (drill 2) (layers *.Cu *.Mask))
  )
  (module Connector_PinSocket_2.54mm:PinSocket_1x16_P2.54mm_Vertical (layer F.Cu) (tedit 5A19A41E)
    (at 152.4 121.92 270)
    (descr "Through hole straight socket strip, 1x16, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x16 2.54mm single row")
    (fp_text reference J1 (at 0 -2.77 90) (layer F.SilkS) hide)
    (fp_text value Conn_01x16_Female (at 0 40.87 90) (layer F.Fab))
    (fp_text user %R (at 0 19.05) (layer F.Fab))
    (pad 16 thru_hole oval (at 0 38.1 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 "Net-(J1-Pad16)"))
    (pad 15 thru_hole oval (at 0 35.56 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 +3V3))
    (pad 14 thru_hole oval (at 0 33.02 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(J1-Pad14)"))
    (pad 13 thru_hole oval (at 0 30.48 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 12 thru_hole oval (at 0 27.94 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(J1-Pad12)"))
    (pad 11 thru_hole oval (at 0 25.4 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 "Net-(J1-Pad11)"))
    (pad 10 thru_hole oval (at 0 22.86 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 "Net-(J1-Pad10)"))
    (pad 9 thru_hole oval (at 0 20.32 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 "Net-(J1-Pad9)"))
    (pad 8 thru_hole oval (at 0 17.78 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 15 "Net-(J1-Pad8)"))
    (pad 7 thru_hole oval (at 0 15.24 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad7)"))
    (pad 6 thru_hole oval (at 0 12.7 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J1-Pad6)"))
    (pad 5 thru_hole oval (at 0 10.16 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J1-Pad5)"))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J1-Pad4)"))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /RX))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /TX))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 "Net-(J1-Pad1)"))
    (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x16_P2.54mm_Vertical.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 135.89 116.84 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C5 (at 0 -1.43 90) (layer F.SilkS) hide)
    (fp_text value 0.1uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 8 "Net-(C5-Pad2)"))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 GND))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 130.81 116.84 270)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C4 (at 0 -1.43 90) (layer F.SilkS) hide)
    (fp_text value 0.1uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 GND))
    (pad 1 smd roundrect (at -0.875 0 270) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 7 "Net-(C4-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 133.35 116.84)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C3 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 0.1uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 4 "Net-(C3-Pad2)"))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 5 "Net-(C3-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 130.81 105.41)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C2 (at 0 -1.43) (layer F.SilkS) hide)
    (fp_text value 0.1uF (at 0 1.43) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 6 GND))
    (pad 1 smd roundrect (at -0.875 0) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 3 +3V3))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_0603_1608Metric_Pad1.05x0.95mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 128.905 113.03 90)
    (descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C1 (at 0 -1.43 90) (layer F.SilkS) hide)
    (fp_text value 0.1uF (at 0 1.43 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 1 "Net-(C1-Pad2)"))
    (pad 1 smd roundrect (at -0.875 0 90) (size 1.05 0.95) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text GND (at 121.92 119.38) (layer F.SilkS))
  (gr_text 3.3V (at 116.84 119.38) (layer F.SilkS))
  (gr_text D5 (at 147.32 104.14) (layer F.SilkS))
  (gr_text D12 (at 134.62 104.14) (layer F.SilkS))
  (gr_text RX (at 147.32 119.38) (layer F.SilkS))
  (gr_text TX (at 149.86 119.38) (layer F.SilkS))
  (gr_text ckd.tech/rs232wing/v1 (at 132.715 116.84) (layer B.SilkS))
  (gr_text "TIP D12\nRING D5" (at 137.795 118.11) (layer F.SilkS))
  (gr_text "TIP TX\nRING RX" (at 118.11 106.68) (layer F.SilkS))
  (gr_arc (start 110.49 120.65) (end 107.95 120.65) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 110.49 102.87) (end 110.49 100.33) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 156.21 120.65) (end 156.21 123.19) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 156.21 102.87) (end 158.75 102.87) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 107.95 120.65) (end 107.95 102.87) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 156.21 123.19) (end 110.49 123.19) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 158.75 102.87) (end 158.75 120.65) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 110.49 100.33) (end 156.21 100.33) (layer Edge.Cuts) (width 0.05))
  (zone (net 6) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 158.75 123.19) (xy 107.95 123.19) (xy 107.95 100.33) (xy 158.75 100.33)
      )
    )
  )
)
