(kicad_pcb (version 4) (host pcbnew 0.201601221446+6507~42~ubuntu14.04.1-product)
  (general
    (links 119)
    (no_connects 0)
    (area 32.411999 87.122 177.5968 116.345)
    (thickness 1.6)
    (drawings 39)
    (tracks 585)
    (zones 0)
    (modules 120)
    (nets 21)
  )
  (page A4)
  (title_block
    (title "Stima - I2C Hub module")
    (date 2015-07-27)
    (company http://rmap.cc/)
    (comment 2 "Released under MIT License(MIT)")
    (comment 3 "Author: Daniele Castellari dcast78@gmail.com")
    (comment 4 "This module is part of rmap project")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.254)
    (trace_clearance 0.254)
    (zone_clearance 0.064)
    (zone_45_only no)
    (trace_min 0.254)
    (segment_width 0.16)
    (edge_width 0.2)
    (via_size 1.035)
    (via_drill 0.635)
    (via_min_size 0.889)
    (via_min_drill 0.508)
    (uvia_size 0.6)
    (uvia_drill 0.254)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.16)
    (mod_text_size 1 1)
    (mod_text_width 0.16)
    (pad_size 1.4 1.4)
    (pad_drill 1)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 0 0)
    (visible_elements 7FFEF67D)
    (pcbplotparams
      (layerselection 0x010f0_ffffffff)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 "Net-(P2-Pad1)")
  (net 3 "Net-(P10-Pad1)")
  (net 4 "Net-(P12-Pad1)")
  (net 5 "Net-(P16-Pad1)")
  (net 6 "Net-(P20-Pad1)")
  (net 7 "Net-(P43-Pad1)")
  (net 8 "Net-(P47-Pad1)")
  (net 9 "Net-(P51-Pad1)")
  (net 10 "Net-(P56-Pad1)")
  (net 11 "Net-(P61-Pad1)")
  (net 12 "Net-(J5-Pad5)")
  (net 13 /+5V)
  (net 14 /+3.3V)
  (net 15 /SCL)
  (net 16 /SDA)
  (net 17 "Net-(J1-Pad5)")
  (net 18 "Net-(J2-Pad5)")
  (net 19 "Net-(J3-Pad5)")
  (net 20 "Net-(J4-Pad5)")
  (net_class Default "Questo è il gruppo di collegamenti predefinito"
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 1.035)
    (via_drill 0.635)
    (uvia_dia 0.6)
    (uvia_drill 0.254)
    (add_net /+3.3V)
    (add_net /+5V)
    (add_net /SCL)
    (add_net /SDA)
    (add_net GND)
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J2-Pad5)")
    (add_net "Net-(J3-Pad5)")
    (add_net "Net-(J4-Pad5)")
    (add_net "Net-(J5-Pad5)")
    (add_net "Net-(P10-Pad1)")
    (add_net "Net-(P12-Pad1)")
    (add_net "Net-(P16-Pad1)")
    (add_net "Net-(P2-Pad1)")
    (add_net "Net-(P20-Pad1)")
    (add_net "Net-(P43-Pad1)")
    (add_net "Net-(P47-Pad1)")
    (add_net "Net-(P51-Pad1)")
    (add_net "Net-(P56-Pad1)")
    (add_net "Net-(P61-Pad1)")
  )
  (module Connect:RJ45_8 (layer B.Cu) (tedit 56A7A6CF)
    (at 104.14 104.775 180)
    (tags RJ45)
    (fp_text reference J3 (at 0 -3.81 180) (layer B.SilkS))
    (fp_text value RJ45 (at 0.14224 0.1016 180) (layer B.Fab) hide)
    (pad Hole np_thru_hole circle (at 5.93852 0 180) (size 3.64998 3.64998) (drill 3.2512) (layers *.Cu *.SilkS *.Mask))
    (pad Hole np_thru_hole circle (at -5.9309 0 180) (size 3.64998 3.64998) (drill 3.2512) (layers *.Cu *.SilkS *.Mask))
    (pad 1 thru_hole rect (at -4.445 6.35 180) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask B.SilkS))
    (pad 2 thru_hole circle (at -3.175 8.89 180) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask B.SilkS))
    (pad 3 thru_hole circle (at -1.905 6.35 180) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask B.SilkS)
      (net 16 /SDA))
    (pad 4 thru_hole circle (at -0.635 8.89 180) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask B.SilkS)
      (net 1 GND))
    (pad 5 thru_hole circle (at 0.635 6.35 180) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask B.SilkS)
      (net 19 "Net-(J3-Pad5)"))
    (pad 6 thru_hole circle (at 1.905 8.89 180) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask B.SilkS)
      (net 15 /SCL))
    (pad 7 thru_hole circle (at 3.175 6.35 180) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask B.SilkS))
    (pad 8 thru_hole circle (at 4.445 8.89 180) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask B.SilkS))
    (model Connect.3dshapes/RJ45_8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:RJ45_8 (layer B.Cu) (tedit 56A7A6F6)
    (at 86.36 104.775 180)
    (tags RJ45)
    (fp_text reference J2 (at 0 -3.81 180) (layer B.SilkS))
    (fp_text value RJ45 (at -3.175 -5.715 180) (layer B.Fab) hide)
    (pad Hole np_thru_hole circle (at 5.93852 0 180) (size 3.64998 3.64998) (drill 3.2512) (layers *.Cu *.SilkS *.Mask))
    (pad Hole np_thru_hole circle (at -5.9309 0 180) (size 3.64998 3.64998) (drill 3.2512) (layers *.Cu *.SilkS *.Mask))
    (pad 1 thru_hole rect (at -4.445 6.35 180) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask B.SilkS))
    (pad 2 thru_hole circle (at -3.175 8.89 180) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask B.SilkS))
    (pad 3 thru_hole circle (at -1.905 6.35 180) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask B.SilkS)
      (net 16 /SDA))
    (pad 4 thru_hole circle (at -0.635 8.89 180) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask B.SilkS)
      (net 1 GND))
    (pad 5 thru_hole circle (at 0.635 6.35 180) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask B.SilkS)
      (net 18 "Net-(J2-Pad5)"))
    (pad 6 thru_hole circle (at 1.905 8.89 180) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask B.SilkS)
      (net 15 /SCL))
    (pad 7 thru_hole circle (at 3.175 6.35 180) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask B.SilkS))
    (pad 8 thru_hole circle (at 4.445 8.89 180) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask B.SilkS))
    (model Connect.3dshapes/RJ45_8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:RJ45_8 (layer B.Cu) (tedit 56A7A6B7)
    (at 139.7 104.775 180)
    (tags RJ45)
    (fp_text reference J5 (at 0 -3.81 180) (layer B.SilkS))
    (fp_text value RJ45 (at 0.14224 0.1016 180) (layer B.Fab) hide)
    (pad Hole np_thru_hole circle (at 5.93852 0 180) (size 3.64998 3.64998) (drill 3.2512) (layers *.Cu *.SilkS *.Mask))
    (pad Hole np_thru_hole circle (at -5.9309 0 180) (size 3.64998 3.64998) (drill 3.2512) (layers *.Cu *.SilkS *.Mask))
    (pad 1 thru_hole rect (at -4.445 6.35 180) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask B.SilkS))
    (pad 2 thru_hole circle (at -3.175 8.89 180) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask B.SilkS))
    (pad 3 thru_hole circle (at -1.905 6.35 180) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask B.SilkS)
      (net 16 /SDA))
    (pad 4 thru_hole circle (at -0.635 8.89 180) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask B.SilkS)
      (net 1 GND))
    (pad 5 thru_hole circle (at 0.635 6.35 180) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask B.SilkS)
      (net 12 "Net-(J5-Pad5)"))
    (pad 6 thru_hole circle (at 1.905 8.89 180) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask B.SilkS)
      (net 15 /SCL))
    (pad 7 thru_hole circle (at 3.175 6.35 180) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask B.SilkS))
    (pad 8 thru_hole circle (at 4.445 8.89 180) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask B.SilkS))
    (model Connect.3dshapes/RJ45_8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module i2c_hub:1pin (layer F.Cu) (tedit 554F30BE)
    (at 44.45 112.522)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF**11115 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask F.SilkS))
  )
  (module i2c_hub:1pin (layer F.Cu) (tedit 55F53FB4)
    (at 44.45 108.458)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF**11114 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 -1.016) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask F.SilkS))
  )
  (module i2c_hub:1pin (layer F.Cu) (tedit 55F53F64)
    (at 44.45 104.615)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF**11113 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 -1.745) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask F.SilkS))
  )
  (module i2c_hub:1pin (layer F.Cu) (tedit 55F53F20)
    (at 44.45 99.615)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF**11112 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 -1.571) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask F.SilkS))
  )
  (module i2c_hub:1pin (layer F.Cu) (tedit 55F53ECC)
    (at 44.45 94.615)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF**11111 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 -0.381) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask F.SilkS))
  )
  (module i2c_hub:1pin (layer F.Cu) (tedit 554F30BE)
    (at 163.83 112.522)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF**11116115 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask F.SilkS))
  )
  (module i2c_hub:1pin (layer F.Cu) (tedit 55F53F8D)
    (at 163.83 108.712)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF**11116114 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 -1.27) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask F.SilkS))
  )
  (module i2c_hub:1pin (layer F.Cu) (tedit 55F53F3A)
    (at 163.83 104.615)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF**11116113 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 -1.745) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask F.SilkS))
  )
  (module i2c_hub:1pin (layer F.Cu) (tedit 55F53EF9)
    (at 163.83 99.615)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF**11116112 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 -1.571) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask F.SilkS))
  )
  (module i2c_hub:1pin (layer F.Cu) (tedit 55F53EB4)
    (at 163.83 94.615)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF**11116111 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 -0.381) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask F.SilkS))
  )
  (module i2c_hub:1pin (layer F.Cu) (tedit 554F30BE)
    (at 158.75 112.522)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF**1111615 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask F.SilkS))
  )
  (module i2c_hub:1pin (layer F.Cu) (tedit 55F53F88)
    (at 158.75 108.712)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF**1111614 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 -1.27) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask F.SilkS))
  )
  (module i2c_hub:1pin (layer F.Cu) (tedit 55F53F35)
    (at 158.75 104.615)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF**1111613 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 -1.745) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask F.SilkS))
  )
  (module i2c_hub:1pin (layer F.Cu) (tedit 55F53EF4)
    (at 158.75 98.044)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF**1111612 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask F.SilkS))
  )
  (module i2c_hub:1pin (layer F.Cu) (tedit 554F30BE)
    (at 158.75 94.234)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF**1111611 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask F.SilkS))
  )
  (module i2c_hub:1pin (layer F.Cu) (tedit 55F53DC6)
    (at 148.59 112.268)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF**111165 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0.254) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask F.SilkS))
  )
  (module i2c_hub:1pin (layer F.Cu) (tedit 55F53DBC)
    (at 130.81 112.268)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF**111155 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0.254) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask F.SilkS))
  )
  (module i2c_hub:1pin (layer F.Cu) (tedit 55F53DB6)
    (at 113.03 112.268)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF**111145 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0.254) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask F.SilkS))
  )
  (module i2c_hub:1pin (layer F.Cu) (tedit 55F53DA1)
    (at 95.25 112.268)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF**111135 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0.254) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask F.SilkS))
  )
  (module i2c_hub:1pin (layer F.Cu) (tedit 554F30BE)
    (at 77.47 112.522)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF**111125 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask F.SilkS))
  )
  (module i2c_hub:1pin (layer F.Cu) (tedit 55F53D98)
    (at 59.69 112.522)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF**111115 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask F.SilkS))
  )
  (module i2c_hub:1pin (layer F.Cu) (tedit 554F30BE)
    (at 148.59 107.442)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF**111164 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask F.SilkS))
  )
  (module i2c_hub:1pin (layer F.Cu) (tedit 55F53F92)
    (at 130.81 108.712)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF**111154 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 -1.27) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask F.SilkS))
  )
  (module i2c_hub:1pin (layer F.Cu) (tedit 55F53F98)
    (at 113.03 108.458)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF**111144 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 -1.016) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask F.SilkS))
  )
  (module i2c_hub:1pin (layer F.Cu) (tedit 55F53F9D)
    (at 95.25 108.458)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF**111134 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 -1.016) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask F.SilkS))
  )
  (module i2c_hub:1pin (layer F.Cu) (tedit 55F53FA5)
    (at 77.47 108.458)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF**111124 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 -1.016) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask F.SilkS))
  )
  (module i2c_hub:1pin (layer F.Cu) (tedit 55F53FAA)
    (at 59.69 108.458)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF**111114 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 -1.016) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask F.SilkS))
  )
  (module i2c_hub:1pin (layer F.Cu) (tedit 554F30BE)
    (at 148.59 102.87)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF**111163 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask F.SilkS))
  )
  (module i2c_hub:1pin (layer F.Cu) (tedit 55F53F3F)
    (at 130.81 104.615)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF**111153 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 -1.745) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask F.SilkS))
  )
  (module i2c_hub:1pin (layer F.Cu) (tedit 55F53F46)
    (at 113.03 104.615)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF**111143 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 -1.745) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask F.SilkS))
  )
  (module i2c_hub:1pin (layer F.Cu) (tedit 55F53F4B)
    (at 95.25 104.615)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF**111133 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 -1.745) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask F.SilkS))
  )
  (module i2c_hub:1pin (layer F.Cu) (tedit 55F53F54)
    (at 77.47 104.615)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF**111123 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 -1.745) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask F.SilkS))
  )
  (module i2c_hub:1pin (layer F.Cu) (tedit 55F53F59)
    (at 59.69 104.615)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF**111113 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 -1.745) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask F.SilkS))
  )
  (module i2c_hub:1pin (layer F.Cu) (tedit 554F30BE)
    (at 148.59 98.044)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF**111162 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask F.SilkS))
  )
  (module i2c_hub:1pin (layer F.Cu) (tedit 55F53EFF)
    (at 130.81 99.615)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF**111152 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 -1.571) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask F.SilkS))
  )
  (module i2c_hub:1pin (layer F.Cu) (tedit 55F53F07)
    (at 113.03 99.615)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF**111142 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 -1.571) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask F.SilkS))
  )
  (module i2c_hub:1pin (layer F.Cu) (tedit 55F53F0C)
    (at 95.25 99.615)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF**111132 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 -1.571) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask F.SilkS))
  )
  (module i2c_hub:1pin (layer F.Cu) (tedit 554F30BE)
    (at 77.47 99.615)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF**111122 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask F.SilkS))
  )
  (module i2c_hub:1pin (layer F.Cu) (tedit 55F53F17)
    (at 59.69 99.615)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF**111112 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 -1.571) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask F.SilkS))
  )
  (module i2c_hub:1pin (layer F.Cu) (tedit 554F30BE)
    (at 148.59 94.234)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF**111161 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask F.SilkS))
  )
  (module i2c_hub:1pin (layer F.Cu) (tedit 55F53EB9)
    (at 130.81 94.615)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF**111151 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 -0.381) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask F.SilkS))
  )
  (module i2c_hub:1pin (layer F.Cu) (tedit 55F53EE8)
    (at 113.03 94.615)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF**111141 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 -0.381) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask F.SilkS))
  )
  (module i2c_hub:1pin (layer F.Cu) (tedit 55F53EC0)
    (at 95.25 94.615)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF**111131 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 -0.381) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask F.SilkS))
  )
  (module i2c_hub:1pin (layer F.Cu) (tedit 55F53EDD)
    (at 77.47 94.615)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF**111121 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 -0.381) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask F.SilkS))
  )
  (module i2c_hub:1pin (layer F.Cu) (tedit 55F53ED7)
    (at 59.69 94.615)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF**111111 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 -0.381) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask F.SilkS))
  )
  (module i2c_hub:1pin (layer F.Cu) (tedit 55F53D91)
    (at 49.53 112.522)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF**1115 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask F.SilkS))
  )
  (module i2c_hub:1pin (layer F.Cu) (tedit 55F53FAF)
    (at 49.53 108.458)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF**1114 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 -1.016) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask F.SilkS))
  )
  (module i2c_hub:1pin (layer F.Cu) (tedit 55F53F5E)
    (at 49.53 104.615)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF**1113 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 -1.745) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask F.SilkS))
  )
  (module i2c_hub:1pin (layer F.Cu) (tedit 55F53F1B)
    (at 49.53 99.615)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF**1112 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 -1.571) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask F.SilkS))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 554E7239)
    (at 151.13 111.125)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (fp_text reference P1 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value 5V (at 1.27 2.54) (layer F.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.524 1.524) (layers F.Cu F.Paste F.Mask)
      (net 13 /+5V))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 554E7232)
    (at 172.974 109.22)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (fp_text reference P2 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value SEL (at 1.27 2.54) (layer F.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.524 1.524) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(P2-Pad1)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 554E723D)
    (at 156.21 107.315)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (fp_text reference P3 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value 3V3 (at 1.27 2.54) (layer F.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.524 1.524) (layers F.Cu F.Paste F.Mask)
      (net 14 /+3.3V))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 554E71C1)
    (at 133.35 101.6)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (fp_text reference P6 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value 5V (at 1.27 2.54) (layer F.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.524 1.524) (layers F.Cu F.Paste F.Mask)
      (net 13 /+5V))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 554E7241)
    (at 166.37 109.22)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (fp_text reference P7 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value SEL (at 1.27 2.54) (layer F.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.524 1.524) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(P10-Pad1)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 554E724A)
    (at 161.29 107.315)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (fp_text reference P8 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value 3V3 (at 1.27 2.54) (layer F.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.524 1.524) (layers F.Cu F.Paste F.Mask)
      (net 14 /+3.3V))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 554E7296)
    (at 115.57 101.6)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (fp_text reference P11 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value 5V (at 1.27 2.54) (layer F.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.524 1.524) (layers F.Cu F.Paste F.Mask)
      (net 13 /+5V))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 554E724E)
    (at 161.29 109.22)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (fp_text reference P12 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value SEL (at 1.27 2.54) (layer F.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.524 1.524) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(P12-Pad1)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 554E1B78)
    (at 166.37 107.315)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (fp_text reference P13 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value 3V3 (at 1.27 2.54) (layer F.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.524 1.524) (layers F.Cu F.Paste F.Mask)
      (net 14 /+3.3V))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 554E72A5)
    (at 97.79 101.6)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (fp_text reference P15 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value 5V (at 1.27 2.54) (layer F.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.524 1.524) (layers F.Cu F.Paste F.Mask)
      (net 13 /+5V))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 554E1B7B)
    (at 156.21 109.22)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (fp_text reference P16 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value SEL (at 1.27 2.54) (layer F.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.524 1.524) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(P16-Pad1)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 554E1B6D)
    (at 172.974 107.315)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (fp_text reference P17 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value 3V3 (at 1.27 2.54) (layer F.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.524 1.524) (layers F.Cu F.Paste F.Mask)
      (net 14 /+3.3V))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 554E6DD8)
    (at 80.01 101.6)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (fp_text reference P19 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value 5V (at 1.27 2.54) (layer F.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.524 1.524) (layers F.Cu F.Paste F.Mask)
      (net 13 /+5V))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 554E1B71)
    (at 151.13 109.22)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (fp_text reference P20 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value SEL (at 1.27 2.54) (layer F.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.524 1.524) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(P20-Pad1)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 554E7527)
    (at 52.07 107.315)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (fp_text reference P21 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value 3V3 (at 1.27 2.54) (layer F.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.524 1.524) (layers F.Cu F.Paste F.Mask)
      (net 14 /+3.3V))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 554E6D38)
    (at 62.23 101.6)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (fp_text reference P24 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value 5V (at 1.27 2.54) (layer F.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.524 1.524) (layers F.Cu F.Paste F.Mask)
      (net 13 /+5V))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 554E6D33)
    (at 64.135 101.6)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (fp_text reference P25 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value SEL (at 1.27 2.54) (layer F.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.524 1.524) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(J1-Pad5)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 554E71CA)
    (at 137.16 101.6)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (fp_text reference P27 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value 3V3 (at 1.27 2.54) (layer F.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.524 1.524) (layers F.Cu F.Paste F.Mask)
      (net 14 /+3.3V))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 554E1B69)
    (at 172.974 111.125)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (fp_text reference P28 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value 5V (at 1.27 2.54) (layer F.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.524 1.524) (layers F.Cu F.Paste F.Mask)
      (net 13 /+5V))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 554E6DD4)
    (at 81.915 101.6)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (fp_text reference P29 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value SEL (at 1.27 2.54) (layer F.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.524 1.524) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(J2-Pad5)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 554E729A)
    (at 119.38 101.6)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (fp_text reference P30 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value 3V3 (at 1.27 2.54) (layer F.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.524 1.524) (layers F.Cu F.Paste F.Mask)
      (net 14 /+3.3V))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 554E1B7E)
    (at 166.37 111.125)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (fp_text reference P31 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value 5V (at 1.27 2.54) (layer F.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.524 1.524) (layers F.Cu F.Paste F.Mask)
      (net 13 /+5V))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 554E729D)
    (at 99.695 101.6)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (fp_text reference P32 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value SEL (at 1.27 2.54) (layer F.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.524 1.524) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(J3-Pad5)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 554E6DDB)
    (at 83.82 101.6)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (fp_text reference P33 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value 3V3 (at 1.27 2.54) (layer F.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.524 1.524) (layers F.Cu F.Paste F.Mask)
      (net 14 /+3.3V))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 554E7244)
    (at 156.21 111.125)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (fp_text reference P34 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value 5V (at 1.27 2.54) (layer F.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.524 1.524) (layers F.Cu F.Paste F.Mask)
      (net 13 /+5V))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 554E7292)
    (at 117.475 101.6)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (fp_text reference P35 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value SEL (at 1.27 2.54) (layer F.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.524 1.524) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(J4-Pad5)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 554E751E)
    (at 57.15 107.315)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (fp_text reference P36 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value 3V3 (at 1.27 2.54) (layer F.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.524 1.524) (layers F.Cu F.Paste F.Mask)
      (net 14 /+3.3V))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 554E7255)
    (at 161.29 111.125)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (fp_text reference P37 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value 5V (at 1.27 2.54) (layer F.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.524 1.524) (layers F.Cu F.Paste F.Mask)
      (net 13 /+5V))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 554E71C4)
    (at 135.255 101.6)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (fp_text reference P38 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value SEL (at 1.27 2.54) (layer F.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.524 1.524) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(J5-Pad5)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 554E72A8)
    (at 101.6 101.6)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (fp_text reference P39 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value 3V3 (at 1.27 2.54) (layer F.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.524 1.524) (layers F.Cu F.Paste F.Mask)
      (net 14 /+3.3V))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 554E7637)
    (at 52.07 111.125)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (fp_text reference P42 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value 5V (at 1.27 2.54) (layer F.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.524 1.524) (layers F.Cu F.Paste F.Mask)
      (net 13 /+5V))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 554E7520)
    (at 57.15 109.22)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (fp_text reference P43 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value SEL (at 1.27 2.54) (layer F.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.524 1.524) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(P43-Pad1)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 554E6D3C)
    (at 66.04 101.6)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (fp_text reference P44 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value 3V3 (at 1.27 2.54) (layer F.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.524 1.524) (layers F.Cu F.Paste F.Mask)
      (net 14 /+3.3V))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 554E7623)
    (at 41.91 111.125)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (fp_text reference P46 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value 5V (at 1.27 2.54) (layer F.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.524 1.524) (layers F.Cu F.Paste F.Mask)
      (net 13 /+5V))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 554E752C)
    (at 52.07 109.22)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (fp_text reference P47 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value SEL (at 1.27 2.54) (layer F.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.524 1.524) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(P47-Pad1)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 554E722E)
    (at 151.13 107.315)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (fp_text reference P48 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value 3V3 (at 1.27 2.54) (layer F.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.524 1.524) (layers F.Cu F.Paste F.Mask)
      (net 14 /+3.3V))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 554E7524)
    (at 57.15 111.125)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (fp_text reference P50 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value 5V (at 1.27 2.54) (layer F.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.524 1.524) (layers F.Cu F.Paste F.Mask)
      (net 13 /+5V))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 554E762E)
    (at 46.99 109.22)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (fp_text reference P51 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value SEL (at 1.27 2.54) (layer F.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.524 1.524) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(P51-Pad1)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 554E762A)
    (at 46.99 107.315)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (fp_text reference P52 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value 3V3 (at 1.27 2.54) (layer F.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.524 1.524) (layers F.Cu F.Paste F.Mask)
      (net 14 /+3.3V))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 554E7632)
    (at 46.99 111.125)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (fp_text reference P55 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value 5V (at 1.27 2.54) (layer F.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.524 1.524) (layers F.Cu F.Paste F.Mask)
      (net 13 /+5V))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 554E7620)
    (at 41.91 109.22)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (fp_text reference P56 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value SEL (at 1.27 2.54) (layer F.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.524 1.524) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(P56-Pad1)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 554E7616)
    (at 41.91 107.315)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (fp_text reference P57 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value 3V3 (at 1.27 2.54) (layer F.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.524 1.524) (layers F.Cu F.Paste F.Mask)
      (net 14 /+3.3V))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 554E760E)
    (at 34.798 111.125)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (fp_text reference P60 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value 5V (at 1.27 2.54) (layer F.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.524 1.524) (layers F.Cu F.Paste F.Mask)
      (net 13 /+5V))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 554E760A)
    (at 34.798 109.22)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (fp_text reference P61 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value SEL (at 1.27 2.54) (layer F.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.524 1.524) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(P61-Pad1)"))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 554E7605)
    (at 34.798 107.315)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (fp_text reference P62 (at 0 -2.54) (layer F.SilkS) hide)
    (fp_text value 3V3 (at 1.27 2.54) (layer F.SilkS) hide)
    (pad 1 smd circle (at 0 0) (size 1.524 1.524) (layers F.Cu F.Paste F.Mask)
      (net 14 /+3.3V))
  )
  (module w_smd_cap:c_1206 (layer F.Cu) (tedit 56A7A55C)
    (at 145.669 110.49 90)
    (descr "SMT capacitor, 1206")
    (fp_text reference C1 (at 3.048 0 180) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.27 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at 1.397 0 90) (size 1.6002 1.8034) (layers F.Cu F.Paste F.Mask)
      (net 13 /+5V))
    (pad 2 smd rect (at -1.397 0 90) (size 1.6002 1.8034) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model walter/smd_cap/c_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_cap:c_1206 (layer F.Cu) (tedit 55F53D42)
    (at 133.35 110.49 90)
    (descr "SMT capacitor, 1206")
    (fp_text reference C2 (at 3.048 0 180) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.27 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at 1.397 0 90) (size 1.6002 1.8034) (layers F.Cu F.Paste F.Mask)
      (net 14 /+3.3V))
    (pad 2 smd rect (at -1.397 0 90) (size 1.6002 1.8034) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model walter/smd_cap/c_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_cap:c_1206 (layer F.Cu) (tedit 56A7A54A)
    (at 75.057 110.49 90)
    (descr "SMT capacitor, 1206")
    (fp_text reference C3 (at 3.048 0 180) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.27 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at 1.397 0 90) (size 1.6002 1.8034) (layers F.Cu F.Paste F.Mask)
      (net 13 /+5V))
    (pad 2 smd rect (at -1.397 0 90) (size 1.6002 1.8034) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model walter/smd_cap/c_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_cap:c_1206 (layer F.Cu) (tedit 55F53D3E)
    (at 62.484 110.236 90)
    (descr "SMT capacitor, 1206")
    (fp_text reference C4 (at 2.921 0 180) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.27 90) (layer F.SilkS) hide)
    (pad 1 smd rect (at 1.397 0 90) (size 1.6002 1.8034) (layers F.Cu F.Paste F.Mask)
      (net 14 /+3.3V))
    (pad 2 smd rect (at -1.397 0 90) (size 1.6002 1.8034) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model walter/smd_cap/c_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_pin_strip:pin_strip_4 (layer B.Cu) (tedit 56A7A609)
    (at 172.974 100.33 90)
    (descr "Pin strip 4pin")
    (tags "CONN DEV")
    (fp_text reference P4 (at 6.35 0 180) (layer B.SilkS))
    (fp_text value CONN_01X04 (at 0.254 3.556 90) (layer B.SilkS) hide)
    (pad 1 thru_hole rect (at -3.81 0 90) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 2 "Net-(P2-Pad1)"))
    (pad 2 thru_hole oval (at -1.27 0 90) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 15 /SCL))
    (pad 3 thru_hole oval (at 1.27 0 90) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 16 /SDA))
    (pad 4 thru_hole oval (at 3.81 0 90) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 1 GND))
    (model walter/pin_strip/pin_strip_4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_pin_strip:pin_strip_4 (layer B.Cu) (tedit 56A7A5F6)
    (at 166.37 100.33 90)
    (descr "Pin strip 4pin")
    (tags "CONN DEV")
    (fp_text reference P10 (at 6.35 0 180) (layer B.SilkS))
    (fp_text value CONN_01X04 (at 0.254 3.556 90) (layer B.SilkS) hide)
    (pad 1 thru_hole rect (at -3.81 0 90) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 3 "Net-(P10-Pad1)"))
    (pad 2 thru_hole oval (at -1.27 0 90) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 15 /SCL))
    (pad 3 thru_hole oval (at 1.27 0 90) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 16 /SDA))
    (pad 4 thru_hole oval (at 3.81 0 90) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 1 GND))
    (model walter/pin_strip/pin_strip_4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_pin_strip:pin_strip_4 (layer B.Cu) (tedit 56A7A7EB)
    (at 161.29 100.33 90)
    (descr "Pin strip 4pin")
    (tags "CONN DEV")
    (fp_text reference P14 (at 6.35 0 180) (layer B.SilkS))
    (fp_text value CONN_01X04 (at 0.254 3.556 90) (layer B.SilkS) hide)
    (pad 1 thru_hole rect (at -3.81 0 90) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 4 "Net-(P12-Pad1)"))
    (pad 2 thru_hole oval (at -1.27 0 90) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 15 /SCL))
    (pad 3 thru_hole oval (at 1.27 0 90) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 16 /SDA))
    (pad 4 thru_hole oval (at 3.81 0 90) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 1 GND))
    (model walter/pin_strip/pin_strip_4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_pin_strip:pin_strip_4 (layer B.Cu) (tedit 56A7A5ED)
    (at 156.21 100.33 90)
    (descr "Pin strip 4pin")
    (tags "CONN DEV")
    (fp_text reference P18 (at 6.35 0 180) (layer B.SilkS))
    (fp_text value CONN_01X04 (at 0.254 3.556 90) (layer B.SilkS) hide)
    (pad 1 thru_hole rect (at -3.81 0 90) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 5 "Net-(P16-Pad1)"))
    (pad 2 thru_hole oval (at -1.27 0 90) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 15 /SCL))
    (pad 3 thru_hole oval (at 1.27 0 90) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 16 /SDA))
    (pad 4 thru_hole oval (at 3.81 0 90) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 1 GND))
    (model walter/pin_strip/pin_strip_4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_pin_strip:pin_strip_4 (layer B.Cu) (tedit 56A7A5DF)
    (at 151.13 100.33 90)
    (descr "Pin strip 4pin")
    (tags "CONN DEV")
    (fp_text reference P23 (at 6.35 -0.254 180) (layer B.SilkS))
    (fp_text value CONN_01X04 (at 0.254 3.556 90) (layer B.SilkS) hide)
    (pad 1 thru_hole rect (at -3.81 0 90) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 6 "Net-(P20-Pad1)"))
    (pad 2 thru_hole oval (at -1.27 0 90) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 15 /SCL))
    (pad 3 thru_hole oval (at 1.27 0 90) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 16 /SDA))
    (pad 4 thru_hole oval (at 3.81 0 90) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 1 GND))
    (model walter/pin_strip/pin_strip_4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_pin_strip:pin_strip_4 (layer B.Cu) (tedit 56A7A640)
    (at 57.15 100.33 90)
    (descr "Pin strip 4pin")
    (tags "CONN DEV")
    (fp_text reference P45 (at 6.35 0 180) (layer B.SilkS))
    (fp_text value CONN_01X04 (at 0.254 3.556 90) (layer B.SilkS) hide)
    (pad 1 thru_hole rect (at -3.81 0 90) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 7 "Net-(P43-Pad1)"))
    (pad 2 thru_hole oval (at -1.27 0 90) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 15 /SCL))
    (pad 3 thru_hole oval (at 1.27 0 90) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 16 /SDA))
    (pad 4 thru_hole oval (at 3.81 0 90) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 1 GND))
    (model walter/pin_strip/pin_strip_4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_pin_strip:pin_strip_4 (layer B.Cu) (tedit 56A7A636)
    (at 52.07 100.33 90)
    (descr "Pin strip 4pin")
    (tags "CONN DEV")
    (fp_text reference P49 (at 6.35 0 180) (layer B.SilkS))
    (fp_text value CONN_01X04 (at 0.254 3.556 90) (layer B.SilkS) hide)
    (pad 1 thru_hole rect (at -3.81 0 90) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 8 "Net-(P47-Pad1)"))
    (pad 2 thru_hole oval (at -1.27 0 90) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 15 /SCL))
    (pad 3 thru_hole oval (at 1.27 0 90) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 16 /SDA))
    (pad 4 thru_hole oval (at 3.81 0 90) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 1 GND))
    (model walter/pin_strip/pin_strip_4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_pin_strip:pin_strip_4 (layer B.Cu) (tedit 56A7A62E)
    (at 46.99 100.33 90)
    (descr "Pin strip 4pin")
    (tags "CONN DEV")
    (fp_text reference P53 (at 6.35 0 180) (layer B.SilkS))
    (fp_text value CONN_01X04 (at 0.254 3.556 90) (layer B.SilkS) hide)
    (pad 1 thru_hole rect (at -3.81 0 90) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 9 "Net-(P51-Pad1)"))
    (pad 2 thru_hole oval (at -1.27 0 90) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 15 /SCL))
    (pad 3 thru_hole oval (at 1.27 0 90) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 16 /SDA))
    (pad 4 thru_hole oval (at 3.81 0 90) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 1 GND))
    (model walter/pin_strip/pin_strip_4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_pin_strip:pin_strip_4 (layer B.Cu) (tedit 56A7A626)
    (at 41.91 100.33 90)
    (descr "Pin strip 4pin")
    (tags "CONN DEV")
    (fp_text reference P59 (at 6.35 0 180) (layer B.SilkS))
    (fp_text value CONN_01X04 (at 0.254 3.556 90) (layer B.SilkS) hide)
    (pad 1 thru_hole rect (at -3.81 0 90) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 10 "Net-(P56-Pad1)"))
    (pad 2 thru_hole oval (at -1.27 0 90) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 15 /SCL))
    (pad 3 thru_hole oval (at 1.27 0 90) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 16 /SDA))
    (pad 4 thru_hole oval (at 3.81 0 90) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 1 GND))
    (model walter/pin_strip/pin_strip_4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_pin_strip:pin_strip_4 (layer B.Cu) (tedit 56A7A61D)
    (at 34.798 100.33 90)
    (descr "Pin strip 4pin")
    (tags "CONN DEV")
    (fp_text reference P63 (at 6.35 0.127 180) (layer B.SilkS))
    (fp_text value CONN_01X04 (at 0.254 3.556 90) (layer B.SilkS) hide)
    (pad 1 thru_hole rect (at -3.81 0 90) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 11 "Net-(P61-Pad1)"))
    (pad 2 thru_hole oval (at -1.27 0 90) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 15 /SCL))
    (pad 3 thru_hole oval (at 1.27 0 90) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 16 /SDA))
    (pad 4 thru_hole oval (at 3.81 0 90) (size 1.524 2.19964) (drill 1.00076) (layers *.Cu *.Mask B.SilkS)
      (net 1 GND))
    (model walter/pin_strip/pin_strip_4.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_trans:sot223 (layer F.Cu) (tedit 56A7A67B)
    (at 139.7 107.95)
    (descr SOT223)
    (fp_text reference U1 (at 0 -5.08) (layer F.SilkS))
    (fp_text value LM317_SOT223 (at 0 1.0414) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.30124 2.99974) (size 1.30048 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0 2.99974) (size 1.30048 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 14 /+3.3V))
    (pad 3 smd rect (at 2.30124 2.99974) (size 1.30048 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 13 /+5V))
    (pad 4 smd rect (at 0 -2.99974) (size 3.79984 1.80086) (layers F.Cu F.Paste F.Mask))
    (model walter/smd_trans/sot223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_trans:sot223 (layer F.Cu) (tedit 56A7A4C0)
    (at 68.58 107.95)
    (descr SOT223)
    (fp_text reference U2 (at 0 -5.08) (layer F.SilkS))
    (fp_text value LM317_SOT223 (at 0 1.0414) (layer F.SilkS) hide)
    (pad 1 smd rect (at -2.30124 2.99974) (size 1.30048 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 0 2.99974) (size 1.30048 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 14 /+3.3V))
    (pad 3 smd rect (at 2.30124 2.99974) (size 1.30048 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 13 /+5V))
    (pad 4 smd rect (at 0 -2.99974) (size 3.79984 1.80086) (layers F.Cu F.Paste F.Mask))
    (model walter/smd_trans/sot223.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_trans:sot23-6 (layer F.Cu) (tedit 554E7BB7)
    (at 169.672 100.584)
    (descr SOT23-6)
    (fp_text reference U3 (at 0 -3.175) (layer F.SilkS))
    (fp_text value ESDA6V1-5SC6 (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 1.05664) (size 0.59944 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 14 /+3.3V))
    (pad 3 smd rect (at 0.9525 1.05664) (size 0.59944 1.00076) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0 1.05664) (size 0.59944 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0.9525 -1.05664) (size 0.59944 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 16 /SDA))
    (pad 6 smd rect (at -0.9525 -1.05664) (size 0.59944 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 13 /+5V))
    (pad 5 smd rect (at 0 -1.05664) (size 0.59944 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 15 /SCL))
    (model walter/smd_trans/sot23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_trans:sot23-6 (layer F.Cu) (tedit 554E7BEE)
    (at 121.92 106.045)
    (descr SOT23-6)
    (fp_text reference U4 (at 0 -3.175) (layer F.SilkS))
    (fp_text value ESDA6V1-5SC6 (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 1.05664) (size 0.59944 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 14 /+3.3V))
    (pad 3 smd rect (at 0.9525 1.05664) (size 0.59944 1.00076) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0 1.05664) (size 0.59944 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0.9525 -1.05664) (size 0.59944 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 16 /SDA))
    (pad 6 smd rect (at -0.9525 -1.05664) (size 0.59944 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 13 /+5V))
    (pad 5 smd rect (at 0 -1.05664) (size 0.59944 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 15 /SCL))
    (model walter/smd_trans/sot23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_trans:sot23-6 (layer F.Cu) (tedit 554E7B4D)
    (at 86.36 106.045)
    (descr SOT23-6)
    (fp_text reference U5 (at 0 -3.175) (layer F.SilkS))
    (fp_text value ESDA6V1-5SC6 (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 1.05664) (size 0.59944 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 14 /+3.3V))
    (pad 3 smd rect (at 0.9525 1.05664) (size 0.59944 1.00076) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0 1.05664) (size 0.59944 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0.9525 -1.05664) (size 0.59944 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 16 /SDA))
    (pad 6 smd rect (at -0.9525 -1.05664) (size 0.59944 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 13 /+5V))
    (pad 5 smd rect (at 0 -1.05664) (size 0.59944 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 15 /SCL))
    (model walter/smd_trans/sot23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module w_smd_trans:sot23-6 (layer F.Cu) (tedit 554E7AFF)
    (at 38.354 100.584)
    (descr SOT23-6)
    (fp_text reference U6 (at 0 -3.175) (layer F.SilkS))
    (fp_text value ESDA6V1-5SC6 (at 0 0) (layer F.SilkS) hide)
    (pad 1 smd rect (at -0.9525 1.05664) (size 0.59944 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 14 /+3.3V))
    (pad 3 smd rect (at 0.9525 1.05664) (size 0.59944 1.00076) (layers F.Cu F.Paste F.Mask))
    (pad 2 smd rect (at 0 1.05664) (size 0.59944 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 4 smd rect (at 0.9525 -1.05664) (size 0.59944 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 16 /SDA))
    (pad 6 smd rect (at -0.9525 -1.05664) (size 0.59944 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 13 /+5V))
    (pad 5 smd rect (at 0 -1.05664) (size 0.59944 1.00076) (layers F.Cu F.Paste F.Mask)
      (net 15 /SCL))
    (model walter/smd_trans/sot23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:RJ45_8 (layer B.Cu) (tedit 56A7A705)
    (at 68.58 104.775 180)
    (tags RJ45)
    (fp_text reference J1 (at 0 -3.175 180) (layer B.SilkS))
    (fp_text value RJ45 (at 0.14224 0.1016 180) (layer B.Fab) hide)
    (pad Hole np_thru_hole circle (at 5.93852 0 180) (size 3.64998 3.64998) (drill 3.2512) (layers *.Cu *.SilkS *.Mask))
    (pad Hole np_thru_hole circle (at -5.9309 0 180) (size 3.64998 3.64998) (drill 3.2512) (layers *.Cu *.SilkS *.Mask))
    (pad 1 thru_hole rect (at -4.445 6.35 180) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask B.SilkS))
    (pad 2 thru_hole circle (at -3.175 8.89 180) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask B.SilkS))
    (pad 3 thru_hole circle (at -1.905 6.35 180) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask B.SilkS)
      (net 16 /SDA))
    (pad 4 thru_hole circle (at -0.635 8.89 180) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask B.SilkS)
      (net 1 GND))
    (pad 5 thru_hole circle (at 0.635 6.35 180) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask B.SilkS)
      (net 17 "Net-(J1-Pad5)"))
    (pad 6 thru_hole circle (at 1.905 8.89 180) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask B.SilkS)
      (net 15 /SCL))
    (pad 7 thru_hole circle (at 3.175 6.35 180) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask B.SilkS))
    (pad 8 thru_hole circle (at 4.445 8.89 180) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask B.SilkS))
    (model Connect.3dshapes/RJ45_8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connect:RJ45_8 (layer B.Cu) (tedit 56A7A6C3)
    (at 121.92 104.775 180)
    (tags RJ45)
    (fp_text reference J4 (at 0 -3.81 180) (layer B.SilkS))
    (fp_text value RJ45 (at -2.54 1.905 180) (layer B.Fab) hide)
    (pad Hole np_thru_hole circle (at 5.93852 0 180) (size 3.64998 3.64998) (drill 3.2512) (layers *.Cu *.SilkS *.Mask))
    (pad Hole np_thru_hole circle (at -5.9309 0 180) (size 3.64998 3.64998) (drill 3.2512) (layers *.Cu *.SilkS *.Mask))
    (pad 1 thru_hole rect (at -4.445 6.35 180) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask B.SilkS))
    (pad 2 thru_hole circle (at -3.175 8.89 180) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask B.SilkS))
    (pad 3 thru_hole circle (at -1.905 6.35 180) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask B.SilkS)
      (net 16 /SDA))
    (pad 4 thru_hole circle (at -0.635 8.89 180) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask B.SilkS)
      (net 1 GND))
    (pad 5 thru_hole circle (at 0.635 6.35 180) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask B.SilkS)
      (net 20 "Net-(J4-Pad5)"))
    (pad 6 thru_hole circle (at 1.905 8.89 180) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask B.SilkS)
      (net 15 /SCL))
    (pad 7 thru_hole circle (at 3.175 6.35 180) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask B.SilkS))
    (pad 8 thru_hole circle (at 4.445 8.89 180) (size 1.50114 1.50114) (drill 0.89916) (layers *.Cu *.Mask B.SilkS))
    (model Connect.3dshapes/RJ45_8.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.4 0.4 0.4))
      (rotate (xyz 0 0 0))
    )
  )
  (module i2c_hub:1pin (layer F.Cu) (tedit 55F53ED2)
    (at 49.53 94.615)
    (descr "module 1 pin (ou trou mecanique de percage)")
    (tags DEV)
    (fp_text reference REF**1111 (at 0 -3.048) (layer F.SilkS) hide)
    (fp_text value 1pin (at 0 2.794) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 -0.381) (size 1.4 1.4) (drill 1) (layers *.Cu *.Mask F.SilkS))
  )
  (gr_text rmap.cc (at 104.14 109.855) (layer F.SilkS))
  (gr_line (start 32.512 114.046) (end 32.512 92.71) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 175.26 114.046) (end 32.512 114.046) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 175.26 113.792) (end 175.26 114.046) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 175.26 92.71) (end 175.26 113.792) (angle 90) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 32.512 92.71) (end 175.26 92.71) (angle 90) (layer Edge.Cuts) (width 0.2))
  (dimension 6.148689 (width 0.3) (layer F.Fab)
    (gr_text "6,149 mm" (at 164.424502 98.927765 51.70983681) (layer F.Fab))
    (feature1 (pts (xy 150.622 91.948) (xy 163.579094 102.177285)))
    (feature2 (pts (xy 154.432 87.122) (xy 167.389094 97.351285)))
    (crossbar (pts (xy 165.269911 95.678245) (xy 161.459911 100.504245)))
    (arrow1a (pts (xy 161.459911 100.504245) (xy 161.697671 99.256699)))
    (arrow1b (pts (xy 161.459911 100.504245) (xy 162.618214 99.983444)))
    (arrow2a (pts (xy 165.269911 95.678245) (xy 164.111608 96.199046)))
    (arrow2b (pts (xy 165.269911 95.678245) (xy 165.032151 96.925791)))
  )
  (dimension 3.818457 (width 0.3) (layer F.Fab)
    (gr_text "3,818 mm" (at 154.379762 96.516517 86.18592517) (layer F.Fab))
    (feature1 (pts (xy 148.59 98.044) (xy 155.599772 98.511318)))
    (feature2 (pts (xy 148.844 94.234) (xy 155.853772 94.701318)))
    (crossbar (pts (xy 153.159752 94.521717) (xy 152.905752 98.331717)))
    (arrow1a (pts (xy 152.905752 98.331717) (xy 152.395564 97.1687)))
    (arrow1b (pts (xy 152.905752 98.331717) (xy 153.565808 97.246716)))
    (arrow2a (pts (xy 153.159752 94.521717) (xy 152.499696 95.606718)))
    (arrow2b (pts (xy 153.159752 94.521717) (xy 153.66994 95.684734)))
  )
  (dimension 3.81 (width 0.3) (layer F.Fab)
    (gr_text "3,810 mm" (at 148.59 96.139 270) (layer F.Fab))
    (feature1 (pts (xy 148.59 98.044) (xy 148.59 98.044)))
    (feature2 (pts (xy 148.59 94.234) (xy 148.59 94.234)))
    (crossbar (pts (xy 148.59 94.234) (xy 148.59 98.044)))
    (arrow1a (pts (xy 148.59 98.044) (xy 148.003579 96.917496)))
    (arrow1b (pts (xy 148.59 98.044) (xy 149.176421 96.917496)))
    (arrow2a (pts (xy 148.59 94.234) (xy 148.003579 95.360504)))
    (arrow2b (pts (xy 148.59 94.234) (xy 149.176421 95.360504)))
  )
  (gr_text 5V (at 62.23 99.695) (layer F.SilkS))
  (gr_text 5V (at 79.756 99.568) (layer F.SilkS))
  (gr_text 3V3 (at 86.614 100.838) (layer F.SilkS))
  (gr_text 3V3 (at 68.834 101.346) (layer F.SilkS))
  (gr_text 5V (at 97.79 99.568) (layer F.SilkS))
  (gr_text 3V3 (at 104.14 101.092) (layer F.SilkS))
  (gr_text 5V (at 115.57 99.314) (layer F.SilkS))
  (gr_text 3V3 (at 122.555 100.965) (layer F.SilkS))
  (gr_text 5V (at 133.4008 99.6188) (layer F.SilkS))
  (gr_text 3V3 (at 139.7 101.6) (layer F.SilkS))
  (gr_text 5V (at 153.67 111.252) (layer F.SilkS))
  (gr_text VCC (at 153.67 109.474) (layer F.SilkS))
  (gr_text 3V3 (at 153.67 107.442) (layer F.SilkS))
  (gr_text VCC (at 54.61 109.22) (layer F.SilkS))
  (gr_text 5V (at 169.926 111.252) (layer F.SilkS))
  (gr_text 3V3 (at 169.926 107.188) (layer F.SilkS))
  (gr_text VCC (at 169.926 109.22) (layer F.SilkS))
  (gr_text VCC (at 38.354 109.22) (layer F.SilkS))
  (gr_text VCC (at 169.672 104.394) (layer B.SilkS))
  (gr_text 3V3 (at 54.61 107.442) (layer F.SilkS))
  (gr_text 5V (at 54.61 111.252) (layer F.SilkS))
  (gr_text VCC (at 38.354 104.14) (layer B.SilkS))
  (gr_text 5V (at 38.354 111.252) (layer F.SilkS))
  (gr_text SCL (at 38.354 101.6) (layer B.SilkS))
  (gr_text SCL (at 169.926 101.6) (layer B.SilkS))
  (gr_text SDA (at 169.672 98.806) (layer B.SilkS))
  (gr_text SDA (at 38.608 99.06) (layer B.SilkS))
  (gr_text GND (at 169.672 96.012) (layer B.SilkS))
  (gr_text GND (at 38.608 96.52) (layer B.SilkS))
  (gr_text 3V3 (at 38.354 107.188) (layer F.SilkS))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.508)
    (fill yes (arc_segments 16) (thermal_gap 0.509) (thermal_bridge_width 0.509))
    (polygon
      (pts
        (xy 174.752 113.792) (xy 32.766 113.792) (xy 32.766 92.964) (xy 174.752 92.964) (xy 174.752 113.792)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.064))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 174.752 113.792) (xy 32.766 113.792) (xy 32.766 92.964) (xy 174.752 92.964) (xy 174.752 113.792)
      )
    )
  )
)
