(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "VCC")
  (net 2 "GND")
  (net 3 "/XTAL1")
  (net 4 "/XTAL2")
  (net 5 "/RESET")
  (net 6 "/SCK")
  (net 7 "/MOSI")
  (net 8 "/MISO")
  (footprint "Button_Switch_THT:SW_PUSH_6mm" (layer "F.Cu")
    (at 122.301 96.901 180)
    (descr "https://www.omron.com/ecb/products/pdf/en-b3f.pdf")
    (tags "tact sw push 6mm")
    (property "Sheetfile" "my Micro.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Push button switch, generic, two pins")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr through_hole)
    (fp_text reference "SW1" (at 10.16 1.96) (layer "F.SilkS") hide)
    (fp_text value "SW_Push" (at 3.25 2.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.25 2.25) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 5 "/RESET") (pinfunction "1") (pintype "passive"))
    (pad "1" thru_hole circle (at 6.5 0 270) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 5 "/RESET") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 4.5 270) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "2") (pintype "passive"))
    (pad "2" thru_hole circle (at 6.5 4.5 270) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH_6mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (at 132.08 111.76 -90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "my Micro.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x02, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J2" (at 0 -2.33 90) (layer "F.SilkS") hide)
    (fp_text value "Conn_01x02_Pin" (at 0 4.87 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 1.27) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "VCC") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical" (layer "F.Cu")
    (at 133.604 93.091 -90)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (property "Sheetfile" "my Micro.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, double row, 02x03, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J1" (at 1.27 -2.33 90) (layer "F.SilkS") hide)
    (fp_text value "Conn_02x03_Odd_Even" (at 1.27 7.41 90) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 1.27 2.54) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 8 "/MISO") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 6 "/SCK") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 2.54 2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "/MOSI") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 5 "/RESET") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 2.54 5.08 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "VCC") (pinfunction "Pin_6") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DIP:DIP-8_W7.62mm" (layer "F.Cu")
    (at 126.3904 99.187)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Sheetfile" "my Micro.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "20MHz, 8kB Flash, 512B SRAM, 512B EEPROM, debugWIRE, DIP-8")
    (property "ki_keywords" "AVR 8bit Microcontroller tinyAVR")
    (attr through_hole)
    (fp_text reference "U1" (at 3.3596 3.623 90) (layer "F.SilkS"))
    (fp_text value "ATtiny85-20P" (at 4.064 3.834 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 3.81) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 5 "/RESET") (pinfunction "~{RESET}/PB5") (pintype "bidirectional"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "/XTAL1") (pinfunction "XTAL1/PB3") (pintype "bidirectional"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "/XTAL2") (pinfunction "XTAL2/PB4") (pintype "bidirectional"))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "5" thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "/MOSI") (pinfunction "AREF/PB0") (pintype "bidirectional"))
    (pad "6" thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 8 "/MISO") (pinfunction "PB1") (pintype "bidirectional"))
    (pad "7" thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 6 "/SCK") (pinfunction "PB2") (pintype "bidirectional"))
    (pad "8" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "VCC") (pinfunction "VCC") (pintype "power_in"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-8_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (at 115.2775 102.1842 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "my Micro.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C1" (at 0 0) (layer "F.SilkS"))
    (fp_text value "20PF" (at 0 1.85) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0 180) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 3 "/XTAL1") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0 180) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder" (layer "F.Cu")
    (at 115.2267 106.9848)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (property "Sheetfile" "my Micro.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor, small symbol")
    (property "ki_keywords" "capacitor cap")
    (attr smd)
    (fp_text reference "C2" (at 0 0) (layer "F.SilkS"))
    (fp_text value "20PF" (at 0 1.85) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.5625 0) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 1.5625 0) (size 1.325 1.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.188679)
      (net 4 "/XTAL2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Crystal:Crystal_HC49-U_Vertical" (layer "F.Cu")
    (at 121.8438 106.9964 90)
    (descr "Crystal THT HC-49/U http://5hertz.com/pdfs/04404_D.pdf")
    (tags "THT crystalHC-49/U")
    (property "Sheetfile" "my Micro.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Two pin crystal")
    (property "ki_keywords" "quartz ceramic resonator oscillator")
    (attr through_hole)
    (fp_text reference "Y1" (at 2.4364 -0.0338 90) (layer "F.SilkS"))
    (fp_text value "8MHZ" (at 2.44 3.525 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.44 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.5 1.5) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "/XTAL2") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 4.88 0 90) (size 1.5 1.5) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "/XTAL1") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Crystal.3dshapes/Crystal_HC49-U_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect (start 111.76 90.424) (end 137.287 114.3)
    (fill none) (layer "Edge.Cuts"))
  (gr_text "VCC" (at 134.01 112.57) (layer "F.SilkS"))
  (gr_text "GND" (at 124.38 112.54) (layer "F.SilkS"))
  (gr_text "Will's Toy" (at 112.16 113.72) (layer "F.SilkS"))
  (zone (net 1) (net_name "VCC") (layer "F.Cu") (hatch edge 0.5)
    (priority 1)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 111.76 90.424)
        (xy 137.287 90.424)
        (xy 137.287 114.173)
        (xy 111.76 114.173)
      )
    )
  )
  (zone (net 2) (net_name "GND") (layer "B.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 111.76 90.424)
        (xy 137.287 90.424)
        (xy 137.287 114.3)
        (xy 111.76 114.3)
      )
    )
  )
)
