(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 262)
    (no_connects 97)
    (area 109.228 95.047999 132.8116 113.232001)
    (thickness 1.6)
    (drawings 4)
    (tracks 531)
    (zones 0)
    (modules 31)
    (nets 57)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (1 In1.Cu signal hide)
    (2 In2.Cu signal hide)
    (31 B.Cu signal hide)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
    (47 F.CrtYd user)
  )
  (setup
    (last_trace_width 0.127)
    (trace_clearance 0.127)
    (zone_clearance 0.127)
    (zone_45_only yes)
    (trace_min 0.127)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.4572)
    (via_drill 0.254)
    (via_min_size 0.4)
    (via_min_drill 0.254)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 0 0)
    (mod_text_width 0)
    (pad_size 0.399999 0.2)
    (pad_drill 0)
    (pad_to_mask_clearance 0)
    (pad_to_paste_clearance_ratio -0.075)
    (aux_axis_origin 110.49 113.03)
    (grid_origin 110.49 113.03)
    (visible_elements 7FFFF79F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(ANT1-Pad2)")
  (net 2 "Net-(ANT1-Pad1)")
  (net 3 "Net-(BPF1-Pad2)")
  (net 4 GND)
  (net 5 "Net-(BPF1-Pad4)")
  (net 6 "Net-(C1-Pad1)")
  (net 7 +1V8)
  (net 8 "Net-(C5-Pad2)")
  (net 9 "Net-(C6-Pad2)")
  (net 10 "Net-(C11-Pad1)")
  (net 11 "Net-(C15-Pad1)")
  (net 12 +BATT)
  (net 13 "Net-(C19-Pad1)")
  (net 14 "Net-(C20-Pad1)")
  (net 15 "Net-(C21-Pad1)")
  (net 16 "Net-(C22-Pad1)")
  (net 17 "Net-(OSC1-Pad3)")
  (net 18 /~nSHUTD)
  (net 19 /HCL_RX)
  (net 20 /AUD_OUT)
  (net 21 /HCI_TX)
  (net 22 /AUD_IN)
  (net 23 /HCI_CTS)
  (net 24 /AUD_FSYNC)
  (net 25 /HCI_RTS)
  (net 26 /AUD_CLK)
  (net 27 "Net-(U1-PadA1)")
  (net 28 "Net-(U1-PadA13)")
  (net 29 "Net-(U1-PadA14)")
  (net 30 "Net-(U1-PadA15)")
  (net 31 "Net-(U1-PadA16)")
  (net 32 "Net-(U1-PadA18)")
  (net 33 "Net-(U1-PadA19)")
  (net 34 "Net-(U1-PadA20)")
  (net 35 "Net-(U1-PadA21)")
  (net 36 "Net-(U1-PadA22)")
  (net 37 "Net-(U1-PadA23)")
  (net 38 "Net-(U1-PadA27)")
  (net 39 "Net-(U1-PadA30)")
  (net 40 "Net-(U1-PadA31)")
  (net 41 "Net-(U1-PadA36)")
  (net 42 "Net-(U1-PadA37)")
  (net 43 "Net-(U1-PadA39)")
  (net 44 "Net-(U1-PadA40)")
  (net 45 "Net-(U1-PadB12)")
  (net 46 "Net-(U1-PadB13)")
  (net 47 "Net-(U1-PadB14)")
  (net 48 "Net-(U1-PadB16)")
  (net 49 "Net-(U1-PadB17)")
  (net 50 "Net-(U1-PadB20)")
  (net 51 "Net-(U1-PadB23)")
  (net 52 "Net-(U1-PadB28)")
  (net 53 "Net-(U1-PadB29)")
  (net 54 "Net-(U1-PadB30)")
  (net 55 "Net-(U1-PadB31)")
  (net 56 "Net-(TP1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.127)
    (trace_width 0.127)
    (via_dia 0.4572)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +1V8)
    (add_net /AUD_CLK)
    (add_net /AUD_FSYNC)
    (add_net /AUD_IN)
    (add_net /AUD_OUT)
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(C6-Pad2)")
    (add_net "Net-(OSC1-Pad3)")
    (add_net "Net-(TP1-Pad1)")
    (add_net "Net-(U1-PadA1)")
    (add_net "Net-(U1-PadA13)")
    (add_net "Net-(U1-PadA14)")
    (add_net "Net-(U1-PadA15)")
    (add_net "Net-(U1-PadA16)")
    (add_net "Net-(U1-PadA18)")
    (add_net "Net-(U1-PadA19)")
    (add_net "Net-(U1-PadA20)")
    (add_net "Net-(U1-PadA21)")
    (add_net "Net-(U1-PadA22)")
    (add_net "Net-(U1-PadA23)")
    (add_net "Net-(U1-PadA27)")
    (add_net "Net-(U1-PadA30)")
    (add_net "Net-(U1-PadA31)")
    (add_net "Net-(U1-PadA36)")
    (add_net "Net-(U1-PadA37)")
    (add_net "Net-(U1-PadA39)")
    (add_net "Net-(U1-PadA40)")
    (add_net "Net-(U1-PadB12)")
    (add_net "Net-(U1-PadB13)")
    (add_net "Net-(U1-PadB14)")
    (add_net "Net-(U1-PadB16)")
    (add_net "Net-(U1-PadB17)")
    (add_net "Net-(U1-PadB20)")
    (add_net "Net-(U1-PadB23)")
    (add_net "Net-(U1-PadB28)")
    (add_net "Net-(U1-PadB29)")
    (add_net "Net-(U1-PadB30)")
    (add_net "Net-(U1-PadB31)")
  )
  (net_class 10thou ""
    (clearance 0.1143)
    (trace_width 0.254)
    (via_dia 0.4572)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +BATT)
    (add_net /HCI_CTS)
    (add_net /HCI_RTS)
    (add_net /HCI_TX)
    (add_net /HCL_RX)
    (add_net /~nSHUTD)
    (add_net GND)
    (add_net "Net-(C15-Pad1)")
    (add_net "Net-(C19-Pad1)")
    (add_net "Net-(C20-Pad1)")
    (add_net "Net-(C21-Pad1)")
    (add_net "Net-(C22-Pad1)")
  )
  (net_class 50ohm ""
    (clearance 0.127)
    (trace_width 0.3345)
    (via_dia 0.4572)
    (via_drill 0.254)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net "Net-(ANT1-Pad1)")
    (add_net "Net-(ANT1-Pad2)")
    (add_net "Net-(BPF1-Pad2)")
    (add_net "Net-(BPF1-Pad4)")
    (add_net "Net-(C1-Pad1)")
  )
  (module CC2564 (layer F.Cu) (tedit 58DC6A67)
    (at 117.6782 104.013 180)
    (fp_text reference U1 (at 1.27 5.08 180) (layer F.SilkS))
    (fp_text value CC2564 (at 0 -5.08 180) (layer F.SilkS))
    (pad EPAD smd rect (at 0.9525 -0.6985 270) (size 1.25 1.4) (layers F.Paste)
      (net 4 GND) (solder_paste_margin_ratio -0.00000001))
    (pad EPAD smd rect (at 0.9525 0.762 270) (size 1.25 1.4) (layers F.Paste)
      (net 4 GND) (solder_paste_margin_ratio -0.00000001))
    (pad EPAD smd rect (at -0.635 -0.6985 270) (size 1.25 1.4) (layers F.Paste)
      (net 4 GND) (solder_paste_margin_ratio -0.00000001))
    (pad A1 smd oval (at -3.9 -2.7 180) (size 0.599999 0.2) (layers F.Cu F.Paste)
      (net 27 "Net-(U1-PadA1)"))
    (pad A1 smd oval (at -3.9 -2.7 180) (size 0.701599 0.3016) (layers F.Mask)
      (net 27 "Net-(U1-PadA1)"))
    (pad A1 smd oval (at -3.9 -2.7 180) (size 0.0254 0.0254) (layers F.Paste)
      (net 27 "Net-(U1-PadA1)"))
    (pad A2 smd oval (at -3.9 -2.100001 180) (size 0.599999 0.2) (layers F.Cu F.Paste)
      (net 10 "Net-(C11-Pad1)"))
    (pad A2 smd oval (at -3.9 -2.100001 180) (size 0.701599 0.3016) (layers F.Mask)
      (net 10 "Net-(C11-Pad1)"))
    (pad A2 smd oval (at -3.9 -2.100001 180) (size 0.0254 0.0254) (layers F.Paste)
      (net 10 "Net-(C11-Pad1)"))
    (pad A3 smd oval (at -3.9 -1.5 180) (size 0.599999 0.2) (layers F.Cu F.Paste)
      (net 10 "Net-(C11-Pad1)"))
    (pad A3 smd oval (at -3.9 -1.5 180) (size 0.701599 0.3016) (layers F.Mask)
      (net 10 "Net-(C11-Pad1)"))
    (pad A3 smd oval (at -3.9 -1.5 180) (size 0.0254 0.0254) (layers F.Paste)
      (net 10 "Net-(C11-Pad1)"))
    (pad A4 smd oval (at -3.9 -0.900001 180) (size 0.599999 0.2) (layers F.Cu F.Paste)
      (net 9 "Net-(C6-Pad2)"))
    (pad A4 smd oval (at -3.9 -0.900001 180) (size 0.701599 0.3016) (layers F.Mask)
      (net 9 "Net-(C6-Pad2)"))
    (pad A4 smd oval (at -3.9 -0.900001 180) (size 0.0254 0.0254) (layers F.Paste)
      (net 9 "Net-(C6-Pad2)"))
    (pad A5 smd oval (at -3.9 -0.299999 180) (size 0.599999 0.2) (layers F.Cu F.Paste)
      (net 11 "Net-(C15-Pad1)"))
    (pad A5 smd oval (at -3.9 -0.299999 180) (size 0.701599 0.3016) (layers F.Mask)
      (net 11 "Net-(C15-Pad1)"))
    (pad A5 smd oval (at -3.9 -0.299999 180) (size 0.0254 0.0254) (layers F.Paste)
      (net 11 "Net-(C15-Pad1)"))
    (pad A6 smd oval (at -3.9 0.299999 180) (size 0.599999 0.2) (layers F.Cu F.Paste)
      (net 18 /~nSHUTD))
    (pad A6 smd oval (at -3.9 0.299999 180) (size 0.701599 0.3016) (layers F.Mask)
      (net 18 /~nSHUTD))
    (pad A6 smd oval (at -3.9 0.299999 180) (size 0.0254 0.0254) (layers F.Paste)
      (net 18 /~nSHUTD))
    (pad A7 smd oval (at -3.9 0.900001 180) (size 0.599999 0.2) (layers F.Cu F.Paste)
      (net 16 "Net-(C22-Pad1)"))
    (pad A7 smd oval (at -3.9 0.900001 180) (size 0.701599 0.3016) (layers F.Mask)
      (net 16 "Net-(C22-Pad1)"))
    (pad A7 smd oval (at -3.9 0.900001 180) (size 0.0254 0.0254) (layers F.Paste)
      (net 16 "Net-(C22-Pad1)"))
    (pad A8 smd oval (at -3.9 1.5 180) (size 0.599999 0.2) (layers F.Cu F.Paste)
      (net 15 "Net-(C21-Pad1)"))
    (pad A8 smd oval (at -3.9 1.5 180) (size 0.701599 0.3016) (layers F.Mask)
      (net 15 "Net-(C21-Pad1)"))
    (pad A8 smd oval (at -3.9 1.5 180) (size 0.0254 0.0254) (layers F.Paste)
      (net 15 "Net-(C21-Pad1)"))
    (pad A9 smd oval (at -3.9 2.100001 180) (size 0.599999 0.2) (layers F.Cu F.Paste)
      (net 11 "Net-(C15-Pad1)"))
    (pad A9 smd oval (at -3.9 2.100001 180) (size 0.701599 0.3016) (layers F.Mask)
      (net 11 "Net-(C15-Pad1)"))
    (pad A9 smd oval (at -3.9 2.100001 180) (size 0.0254 0.0254) (layers F.Paste)
      (net 11 "Net-(C15-Pad1)"))
    (pad A10 smd oval (at -3.9 2.7 180) (size 0.599999 0.2) (layers F.Cu F.Paste)
      (net 4 GND))
    (pad A10 smd oval (at -3.9 2.7 180) (size 0.701599 0.3016) (layers F.Mask)
      (net 4 GND))
    (pad A10 smd oval (at -3.9 2.7 180) (size 0.0254 0.0254) (layers F.Paste)
      (net 4 GND))
    (pad A11 smd oval (at -2.700002 3.9 270) (size 0.599999 0.2) (layers F.Cu F.Paste)
      (net 4 GND))
    (pad A11 smd oval (at -2.700002 3.9 270) (size 0.701599 0.3016) (layers F.Mask)
      (net 4 GND))
    (pad A11 smd oval (at -2.700002 3.9 270) (size 0.0254 0.0254) (layers F.Paste)
      (net 4 GND))
    (pad A12 smd oval (at -2.100001 3.9 270) (size 0.599999 0.2) (layers F.Cu F.Paste)
      (net 13 "Net-(C19-Pad1)"))
    (pad A12 smd oval (at -2.100001 3.9 270) (size 0.701599 0.3016) (layers F.Mask)
      (net 13 "Net-(C19-Pad1)"))
    (pad A12 smd oval (at -2.100001 3.9 270) (size 0.0254 0.0254) (layers F.Paste)
      (net 13 "Net-(C19-Pad1)"))
    (pad A13 smd oval (at -1.500002 3.9 270) (size 0.599999 0.2) (layers F.Cu F.Paste)
      (net 28 "Net-(U1-PadA13)"))
    (pad A13 smd oval (at -1.500002 3.9 270) (size 0.701599 0.3016) (layers F.Mask)
      (net 28 "Net-(U1-PadA13)"))
    (pad A13 smd oval (at -1.500002 3.9 270) (size 0.0254 0.0254) (layers F.Paste)
      (net 28 "Net-(U1-PadA13)"))
    (pad A14 smd oval (at -0.900001 3.9 270) (size 0.599999 0.2) (layers F.Cu F.Paste)
      (net 29 "Net-(U1-PadA14)"))
    (pad A14 smd oval (at -0.900001 3.9 270) (size 0.701599 0.3016) (layers F.Mask)
      (net 29 "Net-(U1-PadA14)"))
    (pad A14 smd oval (at -0.900001 3.9 270) (size 0.0254 0.0254) (layers F.Paste)
      (net 29 "Net-(U1-PadA14)"))
    (pad A15 smd oval (at -0.300002 3.9 270) (size 0.599999 0.2) (layers F.Cu F.Paste)
      (net 30 "Net-(U1-PadA15)"))
    (pad A15 smd oval (at -0.300002 3.9 270) (size 0.701599 0.3016) (layers F.Mask)
      (net 30 "Net-(U1-PadA15)"))
    (pad A15 smd oval (at -0.300002 3.9 270) (size 0.0254 0.0254) (layers F.Paste)
      (net 30 "Net-(U1-PadA15)"))
    (pad A16 smd oval (at 0.299999 3.9 270) (size 0.599999 0.2) (layers F.Cu F.Paste)
      (net 31 "Net-(U1-PadA16)"))
    (pad A16 smd oval (at 0.299999 3.9 270) (size 0.701599 0.3016) (layers F.Mask)
      (net 31 "Net-(U1-PadA16)"))
    (pad A16 smd oval (at 0.299999 3.9 270) (size 0.0254 0.0254) (layers F.Paste)
      (net 31 "Net-(U1-PadA16)"))
    (pad A17 smd oval (at 0.899998 3.9 270) (size 0.599999 0.2) (layers F.Cu F.Paste)
      (net 7 +1V8))
    (pad A17 smd oval (at 0.899998 3.9 270) (size 0.701599 0.3016) (layers F.Mask)
      (net 7 +1V8))
    (pad A17 smd oval (at 0.899998 3.9 270) (size 0.0254 0.0254) (layers F.Paste)
      (net 7 +1V8))
    (pad A18 smd oval (at 1.5 3.9 270) (size 0.599999 0.2) (layers F.Cu F.Paste)
      (net 32 "Net-(U1-PadA18)"))
    (pad A18 smd oval (at 1.5 3.9 270) (size 0.701599 0.3016) (layers F.Mask)
      (net 32 "Net-(U1-PadA18)"))
    (pad A18 smd oval (at 1.5 3.9 270) (size 0.0254 0.0254) (layers F.Paste)
      (net 32 "Net-(U1-PadA18)"))
    (pad A19 smd oval (at 2.099998 3.9 270) (size 0.599999 0.2) (layers F.Cu F.Paste)
      (net 33 "Net-(U1-PadA19)"))
    (pad A19 smd oval (at 2.099998 3.9 270) (size 0.701599 0.3016) (layers F.Mask)
      (net 33 "Net-(U1-PadA19)"))
    (pad A19 smd oval (at 2.099998 3.9 270) (size 0.0254 0.0254) (layers F.Paste)
      (net 33 "Net-(U1-PadA19)"))
    (pad A20 smd oval (at 2.7 3.9 270) (size 0.599999 0.2) (layers F.Cu F.Paste)
      (net 34 "Net-(U1-PadA20)"))
    (pad A20 smd oval (at 2.7 3.9 270) (size 0.701599 0.3016) (layers F.Mask)
      (net 34 "Net-(U1-PadA20)"))
    (pad A20 smd oval (at 2.7 3.9 270) (size 0.0254 0.0254) (layers F.Paste)
      (net 34 "Net-(U1-PadA20)"))
    (pad A21 smd oval (at 3.9 2.7 180) (size 0.599999 0.2) (layers F.Cu F.Paste)
      (net 35 "Net-(U1-PadA21)"))
    (pad A21 smd oval (at 3.9 2.7 180) (size 0.701599 0.3016) (layers F.Mask)
      (net 35 "Net-(U1-PadA21)"))
    (pad A21 smd oval (at 3.9 2.7 180) (size 0.0254 0.0254) (layers F.Paste)
      (net 35 "Net-(U1-PadA21)"))
    (pad A22 smd oval (at 3.9 2.099998 180) (size 0.599999 0.2) (layers F.Cu F.Paste)
      (net 36 "Net-(U1-PadA22)"))
    (pad A22 smd oval (at 3.9 2.099998 180) (size 0.701599 0.3016) (layers F.Mask)
      (net 36 "Net-(U1-PadA22)"))
    (pad A22 smd oval (at 3.9 2.099998 180) (size 0.0254 0.0254) (layers F.Paste)
      (net 36 "Net-(U1-PadA22)"))
    (pad A23 smd oval (at 3.9 1.5 180) (size 0.599999 0.2) (layers F.Cu F.Paste)
      (net 37 "Net-(U1-PadA23)"))
    (pad A23 smd oval (at 3.9 1.5 180) (size 0.701599 0.3016) (layers F.Mask)
      (net 37 "Net-(U1-PadA23)"))
    (pad A23 smd oval (at 3.9 1.5 180) (size 0.0254 0.0254) (layers F.Paste)
      (net 37 "Net-(U1-PadA23)"))
    (pad A24 smd oval (at 3.9 0.899998 180) (size 0.599999 0.2) (layers F.Cu F.Paste)
      (net 4 GND))
    (pad A24 smd oval (at 3.9 0.899998 180) (size 0.701599 0.3016) (layers F.Mask)
      (net 4 GND))
    (pad A24 smd oval (at 3.9 0.899998 180) (size 0.0254 0.0254) (layers F.Paste)
      (net 4 GND))
    (pad A25 smd oval (at 3.9 0.299999 180) (size 0.599999 0.2) (layers F.Cu F.Paste)
      (net 17 "Net-(OSC1-Pad3)"))
    (pad A25 smd oval (at 3.9 0.299999 180) (size 0.701599 0.3016) (layers F.Mask)
      (net 17 "Net-(OSC1-Pad3)"))
    (pad A25 smd oval (at 3.9 0.299999 180) (size 0.0254 0.0254) (layers F.Paste)
      (net 17 "Net-(OSC1-Pad3)"))
    (pad A26 smd oval (at 3.9 -0.300002 180) (size 0.599999 0.2) (layers F.Cu F.Paste)
      (net 19 /HCL_RX))
    (pad A26 smd oval (at 3.9 -0.300002 180) (size 0.701599 0.3016) (layers F.Mask)
      (net 19 /HCL_RX))
    (pad A26 smd oval (at 3.9 -0.300002 180) (size 0.0254 0.0254) (layers F.Paste)
      (net 19 /HCL_RX))
    (pad A27 smd oval (at 3.9 -0.900001 180) (size 0.599999 0.2) (layers F.Cu F.Paste)
      (net 38 "Net-(U1-PadA27)"))
    (pad A27 smd oval (at 3.9 -0.900001 180) (size 0.701599 0.3016) (layers F.Mask)
      (net 38 "Net-(U1-PadA27)"))
    (pad A27 smd oval (at 3.9 -0.900001 180) (size 0.0254 0.0254) (layers F.Paste)
      (net 38 "Net-(U1-PadA27)"))
    (pad A28 smd oval (at 3.9 -1.500002 180) (size 0.599999 0.2) (layers F.Cu F.Paste)
      (net 4 GND))
    (pad A28 smd oval (at 3.9 -1.500002 180) (size 0.701599 0.3016) (layers F.Mask)
      (net 4 GND))
    (pad A28 smd oval (at 3.9 -1.500002 180) (size 0.0254 0.0254) (layers F.Paste)
      (net 4 GND))
    (pad A29 smd oval (at 3.9 -2.100001 180) (size 0.599999 0.2) (layers F.Cu F.Paste)
      (net 23 /HCI_CTS))
    (pad A29 smd oval (at 3.9 -2.100001 180) (size 0.701599 0.3016) (layers F.Mask)
      (net 23 /HCI_CTS))
    (pad A29 smd oval (at 3.9 -2.100001 180) (size 0.0254 0.0254) (layers F.Paste)
      (net 23 /HCI_CTS))
    (pad A30 smd oval (at 3.9 -2.700002 180) (size 0.599999 0.2) (layers F.Cu F.Paste)
      (net 39 "Net-(U1-PadA30)"))
    (pad A30 smd oval (at 3.9 -2.700002 180) (size 0.701599 0.3016) (layers F.Mask)
      (net 39 "Net-(U1-PadA30)"))
    (pad A30 smd oval (at 3.9 -2.700002 180) (size 0.0254 0.0254) (layers F.Paste)
      (net 39 "Net-(U1-PadA30)"))
    (pad A31 smd oval (at 2.7 -3.9 270) (size 0.599999 0.2) (layers F.Cu F.Paste)
      (net 40 "Net-(U1-PadA31)"))
    (pad A31 smd oval (at 2.7 -3.9 270) (size 0.701599 0.3016) (layers F.Mask)
      (net 40 "Net-(U1-PadA31)"))
    (pad A31 smd oval (at 2.7 -3.9 270) (size 0.0254 0.0254) (layers F.Paste)
      (net 40 "Net-(U1-PadA31)"))
    (pad A32 smd oval (at 2.099998 -3.9 270) (size 0.599999 0.2) (layers F.Cu F.Paste)
      (net 25 /HCI_RTS))
    (pad A32 smd oval (at 2.099998 -3.9 270) (size 0.701599 0.3016) (layers F.Mask)
      (net 25 /HCI_RTS))
    (pad A32 smd oval (at 2.099998 -3.9 270) (size 0.0254 0.0254) (layers F.Paste)
      (net 25 /HCI_RTS))
    (pad A33 smd oval (at 1.5 -3.9 270) (size 0.599999 0.2) (layers F.Cu F.Paste)
      (net 21 /HCI_TX))
    (pad A33 smd oval (at 1.5 -3.9 270) (size 0.701599 0.3016) (layers F.Mask)
      (net 21 /HCI_TX))
    (pad A33 smd oval (at 1.5 -3.9 270) (size 0.0254 0.0254) (layers F.Paste)
      (net 21 /HCI_TX))
    (pad A34 smd oval (at 0.899998 -3.9 270) (size 0.599999 0.2) (layers F.Cu F.Paste)
      (net 7 +1V8))
    (pad A34 smd oval (at 0.899998 -3.9 270) (size 0.701599 0.3016) (layers F.Mask)
      (net 7 +1V8))
    (pad A34 smd oval (at 0.899998 -3.9 270) (size 0.0254 0.0254) (layers F.Paste)
      (net 7 +1V8))
    (pad A35 smd oval (at 0.299999 -3.9 270) (size 0.599999 0.2) (layers F.Cu F.Paste)
      (net 24 /AUD_FSYNC))
    (pad A35 smd oval (at 0.299999 -3.9 270) (size 0.701599 0.3016) (layers F.Mask)
      (net 24 /AUD_FSYNC))
    (pad A35 smd oval (at 0.299999 -3.9 270) (size 0.0254 0.0254) (layers F.Paste)
      (net 24 /AUD_FSYNC))
    (pad A36 smd oval (at -0.300002 -3.9 270) (size 0.599999 0.2) (layers F.Cu F.Paste)
      (net 41 "Net-(U1-PadA36)"))
    (pad A36 smd oval (at -0.300002 -3.9 270) (size 0.701599 0.3016) (layers F.Mask)
      (net 41 "Net-(U1-PadA36)"))
    (pad A36 smd oval (at -0.300002 -3.9 270) (size 0.0254 0.0254) (layers F.Paste)
      (net 41 "Net-(U1-PadA36)"))
    (pad A37 smd oval (at -0.900001 -3.9 270) (size 0.599999 0.2) (layers F.Cu F.Paste)
      (net 42 "Net-(U1-PadA37)"))
    (pad A37 smd oval (at -0.900001 -3.9 270) (size 0.701599 0.3016) (layers F.Mask)
      (net 42 "Net-(U1-PadA37)"))
    (pad A37 smd oval (at -0.900001 -3.9 270) (size 0.0254 0.0254) (layers F.Paste)
      (net 42 "Net-(U1-PadA37)"))
    (pad A38 smd oval (at -1.500002 -3.9 270) (size 0.599999 0.2) (layers F.Cu F.Paste)
      (net 7 +1V8))
    (pad A38 smd oval (at -1.500002 -3.9 270) (size 0.701599 0.3016) (layers F.Mask)
      (net 7 +1V8))
    (pad A38 smd oval (at -1.500002 -3.9 270) (size 0.0254 0.0254) (layers F.Paste)
      (net 7 +1V8))
    (pad A39 smd oval (at -2.100001 -3.9 270) (size 0.599999 0.2) (layers F.Cu F.Paste)
      (net 43 "Net-(U1-PadA39)"))
    (pad A39 smd oval (at -2.100001 -3.9 270) (size 0.701599 0.3016) (layers F.Mask)
      (net 43 "Net-(U1-PadA39)"))
    (pad A39 smd oval (at -2.100001 -3.9 270) (size 0.0254 0.0254) (layers F.Paste)
      (net 43 "Net-(U1-PadA39)"))
    (pad A40 smd oval (at -2.700002 -3.9 270) (size 0.599999 0.2) (layers F.Cu F.Paste)
      (net 44 "Net-(U1-PadA40)"))
    (pad A40 smd oval (at -2.700002 -3.9 270) (size 0.701599 0.3016) (layers F.Mask)
      (net 44 "Net-(U1-PadA40)"))
    (pad A40 smd oval (at -2.700002 -3.9 270) (size 0.0254 0.0254) (layers F.Paste)
      (net 44 "Net-(U1-PadA40)"))
    (pad B1 smd rect (at -3.099999 -2.4 180) (size 0.399999 0.2) (layers F.Cu F.Paste)
      (net 14 "Net-(C20-Pad1)"))
    (pad B1 smd rect (at -3.099999 -2.4 180) (size 0.501599 0.3016) (layers F.Mask)
      (net 14 "Net-(C20-Pad1)"))
    (pad B1 smd rect (at -3.099999 -2.4 180) (size 0.0254 0.0254) (layers F.Paste)
      (net 14 "Net-(C20-Pad1)"))
    (pad B2 smd rect (at -3.099999 -1.800001 180) (size 0.399999 0.2) (layers F.Cu F.Paste)
      (net 11 "Net-(C15-Pad1)"))
    (pad B2 smd rect (at -3.099999 -1.800001 180) (size 0.501599 0.3016) (layers F.Mask)
      (net 11 "Net-(C15-Pad1)"))
    (pad B2 smd rect (at -3.099999 -1.800001 180) (size 0.0254 0.0254) (layers F.Paste)
      (net 11 "Net-(C15-Pad1)"))
    (pad B3 smd rect (at -3.099999 -1.2 180) (size 0.399999 0.2) (layers F.Cu F.Paste)
      (net 4 GND))
    (pad B3 smd rect (at -3.099999 -1.2 180) (size 0.501599 0.3016) (layers F.Mask)
      (net 4 GND))
    (pad B3 smd rect (at -3.099999 -1.2 180) (size 0.0254 0.0254) (layers F.Paste)
      (net 4 GND))
    (pad B4 smd rect (at -3.099999 -0.600001 180) (size 0.399999 0.2) (layers F.Cu F.Paste)
      (net 8 "Net-(C5-Pad2)"))
    (pad B4 smd rect (at -3.099999 -0.600001 180) (size 0.501599 0.3016) (layers F.Mask)
      (net 8 "Net-(C5-Pad2)"))
    (pad B4 smd rect (at -3.099999 -0.600001 180) (size 0.0254 0.0254) (layers F.Paste)
      (net 8 "Net-(C5-Pad2)"))
    (pad B5 smd rect (at -3.099999 0 180) (size 0.399999 0.2) (layers F.Cu F.Paste)
      (net 12 +BATT))
    (pad B5 smd rect (at -3.099999 0 180) (size 0.501599 0.3016) (layers F.Mask)
      (net 12 +BATT))
    (pad B5 smd rect (at -3.099999 0 180) (size 0.0254 0.0254) (layers F.Paste)
      (net 12 +BATT))
    (pad B6 smd rect (at -3.099999 0.599999 180) (size 0.399999 0.2) (layers F.Cu F.Paste)
      (net 12 +BATT))
    (pad B6 smd rect (at -3.099999 0.599999 180) (size 0.501599 0.3016) (layers F.Mask)
      (net 12 +BATT))
    (pad B6 smd rect (at -3.099999 0.599999 180) (size 0.0254 0.0254) (layers F.Paste)
      (net 12 +BATT))
    (pad B7 smd rect (at -3.099999 1.2 180) (size 0.399999 0.2) (layers F.Cu F.Paste)
      (net 11 "Net-(C15-Pad1)"))
    (pad B7 smd rect (at -3.099999 1.2 180) (size 0.501599 0.3016) (layers F.Mask)
      (net 11 "Net-(C15-Pad1)"))
    (pad B7 smd rect (at -3.099999 1.2 180) (size 0.0254 0.0254) (layers F.Paste)
      (net 11 "Net-(C15-Pad1)"))
    (pad B8 smd rect (at -3.099999 1.799999 180) (size 0.399999 0.2) (layers F.Cu F.Paste)
      (net 6 "Net-(C1-Pad1)"))
    (pad B8 smd rect (at -3.099999 1.799999 180) (size 0.501599 0.3016) (layers F.Mask)
      (net 6 "Net-(C1-Pad1)"))
    (pad B8 smd rect (at -3.099999 1.799999 180) (size 0.0254 0.0254) (layers F.Paste)
      (net 6 "Net-(C1-Pad1)"))
    (pad B9 smd rect (at -3.099999 2.4 180) (size 0.399999 0.2) (layers F.Cu F.Paste)
      (net 4 GND))
    (pad B9 smd rect (at -3.099999 2.4 180) (size 0.501599 0.3016) (layers F.Mask)
      (net 4 GND))
    (pad B9 smd rect (at -3.099999 2.4 180) (size 0.0254 0.0254) (layers F.Paste)
      (net 4 GND))
    (pad B10 smd rect (at -2.4 3.099999 270) (size 0.399999 0.2) (layers F.Cu F.Paste)
      (net 4 GND))
    (pad B10 smd rect (at -2.4 3.099999 270) (size 0.501599 0.3016) (layers F.Mask)
      (net 4 GND))
    (pad B10 smd rect (at -2.4 3.099999 270) (size 0.0254 0.0254) (layers F.Paste)
      (net 4 GND))
    (pad B11 smd rect (at -1.800001 3.099999 270) (size 0.399999 0.2) (layers F.Cu F.Paste)
      (net 4 GND))
    (pad B11 smd rect (at -1.800001 3.099999 270) (size 0.501599 0.3016) (layers F.Mask)
      (net 4 GND))
    (pad B11 smd rect (at -1.800001 3.099999 270) (size 0.0254 0.0254) (layers F.Paste)
      (net 4 GND))
    (pad B12 smd rect (at -1.2 3.099999 270) (size 0.399999 0.2) (layers F.Cu F.Paste)
      (net 45 "Net-(U1-PadB12)"))
    (pad B12 smd rect (at -1.2 3.099999 270) (size 0.501599 0.3016) (layers F.Mask)
      (net 45 "Net-(U1-PadB12)"))
    (pad B12 smd rect (at -1.2 3.099999 270) (size 0.0254 0.0254) (layers F.Paste)
      (net 45 "Net-(U1-PadB12)"))
    (pad B13 smd rect (at -0.600001 3.099999 270) (size 0.399999 0.2) (layers F.Cu F.Paste)
      (net 46 "Net-(U1-PadB13)"))
    (pad B13 smd rect (at -0.600001 3.099999 270) (size 0.501599 0.3016) (layers F.Mask)
      (net 46 "Net-(U1-PadB13)"))
    (pad B13 smd rect (at -0.600001 3.099999 270) (size 0.0254 0.0254) (layers F.Paste)
      (net 46 "Net-(U1-PadB13)"))
    (pad B14 smd rect (at 0 3.099999 270) (size 0.399999 0.2) (layers F.Cu F.Paste)
      (net 47 "Net-(U1-PadB14)"))
    (pad B14 smd rect (at 0 3.099999 270) (size 0.501599 0.3016) (layers F.Mask)
      (net 47 "Net-(U1-PadB14)"))
    (pad B14 smd rect (at 0 3.099999 270) (size 0.0254 0.0254) (layers F.Paste)
      (net 47 "Net-(U1-PadB14)"))
    (pad B15 smd rect (at 0.599999 3.099999 270) (size 0.399999 0.2) (layers F.Cu F.Paste)
      (net 10 "Net-(C11-Pad1)"))
    (pad B15 smd rect (at 0.599999 3.099999 270) (size 0.501599 0.3016) (layers F.Mask)
      (net 10 "Net-(C11-Pad1)"))
    (pad B15 smd rect (at 0.599999 3.099999 270) (size 0.0254 0.0254) (layers F.Paste)
      (net 10 "Net-(C11-Pad1)"))
    (pad B16 smd rect (at 1.2 3.099999 270) (size 0.399999 0.2) (layers F.Cu F.Paste)
      (net 48 "Net-(U1-PadB16)"))
    (pad B16 smd rect (at 1.2 3.099999 270) (size 0.501599 0.3016) (layers F.Mask)
      (net 48 "Net-(U1-PadB16)"))
    (pad B16 smd rect (at 1.2 3.099999 270) (size 0.0254 0.0254) (layers F.Paste)
      (net 48 "Net-(U1-PadB16)"))
    (pad B17 smd rect (at 1.799999 3.099999 270) (size 0.399999 0.2) (layers F.Cu F.Paste)
      (net 49 "Net-(U1-PadB17)"))
    (pad B17 smd rect (at 1.799999 3.099999 270) (size 0.501599 0.3016) (layers F.Mask)
      (net 49 "Net-(U1-PadB17)"))
    (pad B17 smd rect (at 1.799999 3.099999 270) (size 0.0254 0.0254) (layers F.Paste)
      (net 49 "Net-(U1-PadB17)"))
    (pad B18 smd rect (at 2.4 3.099999 270) (size 0.399999 0.2) (layers F.Cu F.Paste)
      (net 7 +1V8))
    (pad B18 smd rect (at 2.4 3.099999 270) (size 0.501599 0.3016) (layers F.Mask)
      (net 7 +1V8))
    (pad B18 smd rect (at 2.4 3.099999 270) (size 0.0254 0.0254) (layers F.Paste)
      (net 7 +1V8))
    (pad B19 smd rect (at 3.099999 2.4 180) (size 0.399999 0.2) (layers F.Cu F.Paste)
      (net 7 +1V8))
    (pad B19 smd rect (at 3.099999 2.4 180) (size 0.501599 0.3016) (layers F.Mask)
      (net 7 +1V8))
    (pad B19 smd rect (at 3.099999 2.4 180) (size 0.0254 0.0254) (layers F.Paste)
      (net 7 +1V8))
    (pad B20 smd rect (at 3.099999 1.800001 180) (size 0.399999 0.2) (layers F.Cu F.Paste)
      (net 50 "Net-(U1-PadB20)"))
    (pad B20 smd rect (at 3.099999 1.800001 180) (size 0.501599 0.3016) (layers F.Mask)
      (net 50 "Net-(U1-PadB20)"))
    (pad B20 smd rect (at 3.099999 1.800001 180) (size 0.0254 0.0254) (layers F.Paste)
      (net 50 "Net-(U1-PadB20)"))
    (pad B21 smd rect (at 3.099999 1.2 180) (size 0.399999 0.2) (layers F.Cu F.Paste)
      (net 7 +1V8))
    (pad B21 smd rect (at 3.099999 1.2 180) (size 0.501599 0.3016) (layers F.Mask)
      (net 7 +1V8))
    (pad B21 smd rect (at 3.099999 1.2 180) (size 0.0254 0.0254) (layers F.Paste)
      (net 7 +1V8))
    (pad B22 smd rect (at 3.099999 0.600001 180) (size 0.399999 0.2) (layers F.Cu F.Paste)
      (net 7 +1V8))
    (pad B22 smd rect (at 3.099999 0.600001 180) (size 0.501599 0.3016) (layers F.Mask)
      (net 7 +1V8))
    (pad B22 smd rect (at 3.099999 0.600001 180) (size 0.0254 0.0254) (layers F.Paste)
      (net 7 +1V8))
    (pad B23 smd rect (at 3.099999 0 180) (size 0.399999 0.2) (layers F.Cu F.Paste)
      (net 51 "Net-(U1-PadB23)"))
    (pad B23 smd rect (at 3.099999 0 180) (size 0.501599 0.3016) (layers F.Mask)
      (net 51 "Net-(U1-PadB23)"))
    (pad B23 smd rect (at 3.099999 0 180) (size 0.0254 0.0254) (layers F.Paste)
      (net 51 "Net-(U1-PadB23)"))
    (pad B24 smd rect (at 3.099999 -0.599999 180) (size 0.399999 0.2) (layers F.Cu F.Paste)
      (net 56 "Net-(TP1-Pad1)"))
    (pad B24 smd rect (at 3.099999 -0.599999 180) (size 0.501599 0.3016) (layers F.Mask)
      (net 56 "Net-(TP1-Pad1)"))
    (pad B24 smd rect (at 3.099999 -0.599999 180) (size 0.0254 0.0254) (layers F.Paste)
      (net 56 "Net-(TP1-Pad1)"))
    (pad B25 smd rect (at 3.099999 -1.2 180) (size 0.399999 0.2) (layers F.Cu F.Paste)
      (net 7 +1V8))
    (pad B25 smd rect (at 3.099999 -1.2 180) (size 0.501599 0.3016) (layers F.Mask)
      (net 7 +1V8))
    (pad B25 smd rect (at 3.099999 -1.2 180) (size 0.0254 0.0254) (layers F.Paste)
      (net 7 +1V8))
    (pad B26 smd rect (at 3.099999 -1.799999 180) (size 0.399999 0.2) (layers F.Cu F.Paste)
      (net 10 "Net-(C11-Pad1)"))
    (pad B26 smd rect (at 3.099999 -1.799999 180) (size 0.501599 0.3016) (layers F.Mask)
      (net 10 "Net-(C11-Pad1)"))
    (pad B26 smd rect (at 3.099999 -1.799999 180) (size 0.0254 0.0254) (layers F.Paste)
      (net 10 "Net-(C11-Pad1)"))
    (pad B27 smd rect (at 3.099999 -2.4 180) (size 0.399999 0.2) (layers F.Cu F.Paste)
      (net 10 "Net-(C11-Pad1)"))
    (pad B27 smd rect (at 3.099999 -2.4 180) (size 0.501599 0.3016) (layers F.Mask)
      (net 10 "Net-(C11-Pad1)"))
    (pad B27 smd rect (at 3.099999 -2.4 180) (size 0.0254 0.0254) (layers F.Paste)
      (net 10 "Net-(C11-Pad1)"))
    (pad B28 smd rect (at 2.4 -3.099999 270) (size 0.399999 0.2) (layers F.Cu F.Paste)
      (net 52 "Net-(U1-PadB28)"))
    (pad B28 smd rect (at 2.4 -3.099999 270) (size 0.501599 0.3016) (layers F.Mask)
      (net 52 "Net-(U1-PadB28)"))
    (pad B28 smd rect (at 2.4 -3.099999 270) (size 0.0254 0.0254) (layers F.Paste)
      (net 52 "Net-(U1-PadB28)"))
    (pad B29 smd rect (at 1.800001 -3.099999 270) (size 0.399999 0.2) (layers F.Cu F.Paste)
      (net 53 "Net-(U1-PadB29)"))
    (pad B29 smd rect (at 1.800001 -3.099999 270) (size 0.501599 0.3016) (layers F.Mask)
      (net 53 "Net-(U1-PadB29)"))
    (pad B29 smd rect (at 1.800001 -3.099999 270) (size 0.0254 0.0254) (layers F.Paste)
      (net 53 "Net-(U1-PadB29)"))
    (pad B30 smd rect (at 1.2 -3.099999 270) (size 0.399999 0.2) (layers F.Cu F.Paste)
      (net 54 "Net-(U1-PadB30)"))
    (pad B30 smd rect (at 1.2 -3.099999 270) (size 0.501599 0.3016) (layers F.Mask)
      (net 54 "Net-(U1-PadB30)"))
    (pad B30 smd rect (at 1.2 -3.099999 270) (size 0.0254 0.0254) (layers F.Paste)
      (net 54 "Net-(U1-PadB30)"))
    (pad B31 smd rect (at 0.600001 -3.099999 270) (size 0.399999 0.2) (layers F.Cu F.Paste)
      (net 55 "Net-(U1-PadB31)"))
    (pad B31 smd rect (at 0.600001 -3.099999 270) (size 0.501599 0.3016) (layers F.Mask)
      (net 55 "Net-(U1-PadB31)"))
    (pad B31 smd rect (at 0.600001 -3.099999 270) (size 0.0254 0.0254) (layers F.Paste)
      (net 55 "Net-(U1-PadB31)"))
    (pad B32 smd rect (at 0 -3.099999 270) (size 0.399999 0.2) (layers F.Cu F.Paste)
      (net 26 /AUD_CLK))
    (pad B32 smd rect (at 0 -3.099999 270) (size 0.501599 0.3016) (layers F.Mask)
      (net 26 /AUD_CLK))
    (pad B33 smd rect (at -0.599999 -3.099999 270) (size 0.399999 0.2) (layers F.Cu F.Paste)
      (net 20 /AUD_OUT))
    (pad B33 smd rect (at -0.599999 -3.099999 270) (size 0.501599 0.3016) (layers F.Mask)
      (net 20 /AUD_OUT))
    (pad B33 smd rect (at -0.599999 -3.099999 270) (size 0.0254 0.0254) (layers F.Paste)
      (net 20 /AUD_OUT))
    (pad B34 smd rect (at -1.2 -3.099999 270) (size 0.399999 0.2) (layers F.Cu F.Paste)
      (net 22 /AUD_IN))
    (pad B34 smd rect (at -1.2 -3.099999 270) (size 0.501599 0.3016) (layers F.Mask)
      (net 22 /AUD_IN))
    (pad B34 smd rect (at -1.2 -3.099999 270) (size 0.0254 0.0254) (layers F.Paste)
      (net 22 /AUD_IN))
    (pad B35 smd rect (at -1.799999 -3.099999 270) (size 0.399999 0.2) (layers F.Cu F.Paste)
      (net 10 "Net-(C11-Pad1)"))
    (pad B35 smd rect (at -1.799999 -3.099999 270) (size 0.501599 0.3016) (layers F.Mask)
      (net 10 "Net-(C11-Pad1)"))
    (pad B35 smd rect (at -1.799999 -3.099999 270) (size 0.0254 0.0254) (layers F.Paste)
      (net 10 "Net-(C11-Pad1)"))
    (pad B36 smd rect (at -2.4 -3.099999 270) (size 0.399999 0.2) (layers F.Cu F.Paste)
      (net 10 "Net-(C11-Pad1)"))
    (pad B36 smd rect (at -2.4 -3.099999 270) (size 0.501599 0.3016) (layers F.Mask)
      (net 10 "Net-(C11-Pad1)"))
    (pad B36 smd rect (at -2.4 -3.099999 270) (size 0.0254 0.0254) (layers F.Paste)
      (net 10 "Net-(C11-Pad1)"))
    (pad EPAD smd rect (at 0.17 0 270) (size 2.999999 3.300001) (layers F.Cu)
      (net 4 GND))
    (pad EPAD smd rect (at 0.17 0 270) (size 3.101599 3.401601) (layers F.Mask)
      (net 4 GND))
    (pad EPAD smd rect (at -0.635 0.762 270) (size 1.25 1.4) (layers F.Paste)
      (net 4 GND) (solder_paste_margin_ratio -0.00000001))
  )
  (module Measurement_Points:Measurement_Point_Round-SMD-Pad_Small (layer F.Cu) (tedit 58D5C5DB)
    (at 111.379 105.156)
    (descr "Mesurement Point, Round, SMD Pad, DM 1.5mm,")
    (tags "Mesurement Point Round SMD Pad 1.5mm")
    (attr virtual)
    (fp_text reference TP1 (at 0 -2) (layer F.SilkS))
    (fp_text value TEST_1P (at 0 2) (layer F.Fab))
    (pad 1 smd circle (at 0 0) (size 1 1) (layers F.Cu F.Mask)
      (net 56 "Net-(TP1-Pad1)"))
  )
  (module Capacitors_SMD:C_0201 (layer F.Cu) (tedit 58AA83DF)
    (at 126.7079 104.8512 180)
    (descr "Capacitor SMD 0201, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0201")
    (attr smd)
    (fp_text reference C2 (at 0 -1.27 180) (layer F.SilkS))
    (fp_text value TBD (at 0 1.27 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 180) (layer F.Fab))
    (pad 1 smd rect (at -0.28 0 180) (size 0.3 0.35) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(BPF1-Pad2)"))
    (pad 2 smd rect (at 0.28 0 180) (size 0.3 0.35) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0201.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58AA841A)
    (at 122.9868 99.314)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C1 (at 0 -1.27) (layer F.SilkS))
    (fp_text value 22pF (at 0 1.27) (layer F.Fab))
    (fp_text user %R (at 0 -1.27) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(BPF1-Pad4)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Footprints:2450AT18A100E (layer F.Cu) (tedit 58C9E4BC)
    (at 127 108.839 270)
    (fp_text reference ANT1 (at 2 3 270) (layer F.SilkS))
    (fp_text value Antenna_2.45GHz (at 1.6 -2.8 270) (layer F.Fab))
    (pad 2 smd rect (at 3.4 0 270) (size 0.8 1.6) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(ANT1-Pad2)"))
    (pad 1 smd rect (at 0 0 270) (size 0.8 1.6) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(ANT1-Pad1)"))
  )
  (module Footprints:LFB212G45SG8A192 (layer F.Cu) (tedit 58C9E61A)
    (at 127.6096 100.457 270)
    (fp_text reference BPF1 (at 0.05 5.3 270) (layer F.SilkS))
    (fp_text value BP_FIlter_2.45GHz (at 0 -5 270) (layer F.Fab))
    (pad 2 smd rect (at 1 0.625 270) (size 0.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(BPF1-Pad2)"))
    (pad 3 smd rect (at 0 1.25 270) (size 1.6 0.5) (drill (offset 0 -0.05)) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 1 smd rect (at 0 0 270) (size 1.6 0.5) (drill (offset 0 0.05)) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 4 smd rect (at -1 0.625 270) (size 0.6 0.3) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(BPF1-Pad4)"))
  )
  (module Capacitors_SMD:C_0201 (layer F.Cu) (tedit 58AA83DF)
    (at 126.7079 106.8832 180)
    (descr "Capacitor SMD 0201, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0201")
    (attr smd)
    (fp_text reference C3 (at 0 -1.27 180) (layer F.SilkS))
    (fp_text value TBD (at 0 1.27 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 180) (layer F.Fab))
    (pad 1 smd rect (at -0.28 0 180) (size 0.3 0.35) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(ANT1-Pad1)"))
    (pad 2 smd rect (at 0.28 0 180) (size 0.3 0.35) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0201.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58AA841A)
    (at 111.887 100.711)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C4 (at 0 -1.27) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27) (layer F.Fab))
    (fp_text user %R (at 0 -1.27) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 7 +1V8))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58AA841A)
    (at 123.9774 102.7557 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C5 (at 0 -1.27 180) (layer F.SilkS))
    (fp_text value 16pF (at 0 1.27 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C5-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58AA841A)
    (at 124.0028 106.8197)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C6 (at 0 -1.27) (layer F.SilkS))
    (fp_text value 16pF (at 0 1.27) (layer F.Fab))
    (fp_text user %R (at 0 -1.27) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C6-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58AA841A)
    (at 115.443 99.06 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C7 (at 0 -1.27 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 7 +1V8))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58AA841A)
    (at 113.03 99.06 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C8 (at 0 -1.27 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 7 +1V8))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer B.Cu) (tedit 58AA841A)
    (at 117.983 106.0196 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C9 (at 0 1.27 90) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.27 90) (layer B.Fab))
    (fp_text user %R (at 0 1.27 90) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 7 +1V8))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer B.Cu) (tedit 58AA841A)
    (at 115.7732 104.267)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C10 (at 0 1.27) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.27) (layer B.Fab))
    (fp_text user %R (at 0 1.27) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 7 +1V8))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58AA841A)
    (at 117.729 99.06)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C11 (at 0 -1.27) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27) (layer F.Fab))
    (fp_text user %R (at 0 -1.27) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C11-Pad1)"))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58AA841A)
    (at 113.792 108.966 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C12 (at 0 -1.27 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C11-Pad1)"))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58AA841A)
    (at 122.682 108.458 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C13 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value 0.47uF (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C11-Pad1)"))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58AA841A)
    (at 120.3325 108.966)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C14 (at 0 -1.27) (layer F.SilkS))
    (fp_text value 0.47uF (at 0 1.27) (layer F.Fab))
    (fp_text user %R (at 0 -1.27) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C11-Pad1)"))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer B.Cu) (tedit 58AA841A)
    (at 120.9548 104.8258 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C15 (at 0 1.27 270) (layer B.SilkS))
    (fp_text value 1uF (at 0 -1.27 270) (layer B.Fab))
    (fp_text user %R (at 0 1.27 270) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(C15-Pad1)"))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer B.Cu) (tedit 58AA841A)
    (at 120.142 101.1682 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C16 (at 0 1.27 180) (layer B.SilkS))
    (fp_text value 1uF (at 0 -1.27 180) (layer B.Fab))
    (fp_text user %R (at 0 1.27 180) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(C15-Pad1)"))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer B.Cu) (tedit 58AA841A)
    (at 119.5324 102.6922 90)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C17 (at 0 1.27 90) (layer B.SilkS))
    (fp_text value 1uF (at 0 -1.27 90) (layer B.Fab))
    (fp_text user %R (at 0 1.27 90) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 90) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 12 +BATT))
    (pad 2 smd rect (at 0.55 0 90) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer B.Cu) (tedit 58AA841A)
    (at 119.5324 104.8004 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C18 (at 0 1.27 270) (layer B.SilkS))
    (fp_text value 1uF (at 0 -1.27 270) (layer B.Fab))
    (fp_text user %R (at 0 1.27 270) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 12 +BATT))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58AA841A)
    (at 120.015 99.06 180)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C19 (at 0 -1.27 180) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 180) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C19-Pad1)"))
    (pad 2 smd rect (at 0.55 0 180) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer B.Cu) (tedit 58AA841A)
    (at 120.9548 106.934 270)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C20 (at 0 1.27 270) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.27 270) (layer B.Fab))
    (fp_text user %R (at 0 1.27 270) (layer B.Fab))
    (pad 1 smd rect (at -0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 14 "Net-(C20-Pad1)"))
    (pad 2 smd rect (at 0.55 0 270) (size 0.6 0.5) (layers B.Cu B.Paste B.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58AA841A)
    (at 123.9774 100.8761)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C21 (at 0 -1.27) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27) (layer F.Fab))
    (fp_text user %R (at 0 -1.27) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C21-Pad1)"))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0402 (layer F.Cu) (tedit 58AA841A)
    (at 123.9774 101.8159)
    (descr "Capacitor SMD 0402, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0402")
    (attr smd)
    (fp_text reference C22 (at 0 -1.27) (layer F.SilkS))
    (fp_text value 0.1uF (at 0 1.27) (layer F.Fab))
    (fp_text user %R (at 0 -1.27) (layer F.Fab))
    (pad 1 smd rect (at -0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(C22-Pad1)"))
    (pad 2 smd rect (at 0.55 0) (size 0.6 0.5) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (model Capacitors_SMD.3dshapes/C_0402.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Footprints:OYKTGLJANF-0.032768 (layer F.Cu) (tedit 58BF5644)
    (at 111.252 102.108 270)
    (fp_text reference OSC1 (at 1.4 1.6 270) (layer F.SilkS))
    (fp_text value Oscillator_32kHz (at 0.4 -2.6 270) (layer F.Fab))
    (pad 4 smd rect (at 0 -1.22 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 +1V8))
    (pad 3 smd rect (at 1.62 -1.22 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(OSC1-Pad3)"))
    (pad 2 smd rect (at 1.62 0 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 1 smd rect (at 0 0 270) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 +1V8))
  )
  (module Footprints:FH2600022 (layer F.Cu) (tedit 58BF57B2)
    (at 123.19 103.8225 270)
    (fp_text reference Y1 (at 1.45 1.3 270) (layer F.SilkS))
    (fp_text value 26MHz (at 1 -3.1 270) (layer F.Fab))
    (pad 4 smd rect (at 0 -1.55 270) (size 1 0.95) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 3 smd rect (at 1.85 -1.55 270) (size 1 0.95) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(C6-Pad2)"))
    (pad 2 smd rect (at 1.85 0 270) (size 1 0.95) (layers F.Cu F.Paste F.Mask)
      (net 4 GND))
    (pad 1 smd rect (at 0 0 270) (size 1 0.95) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(C5-Pad2)"))
  )
  (module Capacitors_SMD:C_0201 (layer F.Cu) (tedit 58AA83DF)
    (at 126.9873 105.8672 270)
    (descr "Capacitor SMD 0201, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0201")
    (attr smd)
    (fp_text reference L1 (at 0 -1.27 270) (layer F.SilkS))
    (fp_text value TBD (at 0 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.27 270) (layer F.Fab))
    (pad 1 smd rect (at -0.28 0 270) (size 0.3 0.35) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(BPF1-Pad2)"))
    (pad 2 smd rect (at 0.28 0 270) (size 0.3 0.35) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(ANT1-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0201.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Footprints:Pin_Header_Straight_1x05_Pitch2.54mm locked (layer F.Cu) (tedit 590E0435)
    (at 111.76 111.76 90)
    (descr "Through hole straight pin header, 1x05, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x05 2.54mm single row")
    (fp_text reference P2 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value CONN_01X05 (at 0 12.49 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 24 /AUD_FSYNC))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 26 /AUD_CLK))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /AUD_OUT))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 22 /AUD_IN))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 +BATT))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x05_Pitch2.54mm.wrl
      (at (xyz 0 -0.2 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Footprints:SIP7 locked (layer F.Cu) (tedit 590E03FB)
    (at 111.76 96.52 90)
    (descr "Through hole straight pin header, 1x07, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x07 2.54mm single row")
    (fp_text reference P1 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value CONN_01X07 (at 0 17.57 90) (layer F.Fab))
    (fp_text user %R (at 0 -2.33 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 +1V8))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /HCL_RX))
    (pad 3 thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 23 /HCI_CTS))
    (pad 4 thru_hole oval (at 0 7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 25 /HCI_RTS))
    (pad 5 thru_hole oval (at 0 10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 /HCI_TX))
    (pad 6 thru_hole oval (at 0 12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 /~nSHUTD))
    (pad 7 thru_hole oval (at 0 15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x07_Pitch2.54mm.wrl
      (at (xyz 0 -0.3 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (gr_line (start 110.49 113.03) (end 110.49 95.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 128.27 113.03) (end 110.49 113.03) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 128.27 95.25) (end 128.27 113.03) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 110.49 95.25) (end 128.27 95.25) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.127)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 128.27 107.442) (xy 123.19 107.442) (xy 123.19 113.03) (xy 128.27 113.03)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In1.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.127)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 128.27 107.442) (xy 123.19 107.442) (xy 123.19 113.03) (xy 128.27 113.03)
      )
    )
  )
  (zone (net 0) (net_name "") (layer In2.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.127)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 128.27 107.442) (xy 123.19 107.442) (xy 123.19 113.03) (xy 128.27 113.03)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.127)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 128.27 107.442) (xy 123.19 107.442) (xy 123.19 113.03) (xy 128.27 113.03)
      )
    )
  )
  (zone (net 4) (net_name GND) (layer In1.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.127)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 110.871 95.631) (xy 127.889 95.631) (xy 127.889 112.649) (xy 110.871 112.649)
      )
    )
  )
  (zone (net 4) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.127)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 110.871 95.631) (xy 127.889 95.631) (xy 127.889 112.649) (xy 110.871 112.649)
      )
    )
  )
  (zone (net 4) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.127)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 110.871 95.631) (xy 127.889 95.631) (xy 127.889 112.649) (xy 110.871 112.649)
      )
    )
  )
  (zone (net 4) (net_name GND) (layer In2.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.127)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 110.871 95.631) (xy 127.889 95.631) (xy 127.889 112.649) (xy 110.871 112.649)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.127)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 120.1547 99.2251) (xy 119.9261 99.2251) (xy 119.9261 101.9556) (xy 119.0244 101.9556) (xy 119.0244 98.6917)
        (xy 120.1547 98.6917)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.127))
    (min_thickness 0.127)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 119.888 104.14) (xy 119.888 105.283) (xy 120.523 105.283) (xy 120.523 104.14)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.127)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 120.5484 104.9528) (xy 122.6566 104.9528) (xy 122.6566 105.7402) (xy 120.5484 105.7402)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.127)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 120.1928 109.3216) (xy 121.3104 109.3216) (xy 121.3104 107.9754) (xy 120.1928 107.9754)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.127)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 116.205 100.584) (xy 117.221 100.584) (xy 117.221 99.695) (xy 118.999 99.695) (xy 118.999 101.219)
        (xy 114.935 101.219) (xy 114.935 106.807) (xy 114.173 106.807) (xy 114.173 106.934) (xy 113.411 106.934)
        (xy 113.411 105.918) (xy 114.173 105.918) (xy 114.173 102.616) (xy 113.411 102.616) (xy 113.411 101.219)
        (xy 114.681 101.219) (xy 114.935 100.584) (xy 114.681 100.584) (xy 114.681 99.695) (xy 116.205 99.695)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.127)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 117.094 106.807) (xy 118.237 106.807) (xy 118.237 107.569) (xy 117.094 107.569)
      )
    )
  )
  (zone (net 0) (net_name "") (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.127))
    (min_thickness 0.127)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 119.634 106.807) (xy 120.015 106.807) (xy 120.015 107.569) (xy 119.634 107.569)
      )
    )
  )
)
