(kicad_pcb (version 20171130) (host pcbnew "(5.0.0)")
  (general
    (thickness 1.6002)
    (drawings 19)
    (tracks 138)
    (zones 0)
    (modules 7)
    (nets 20)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (44 Edge.Cuts user)
  )
  (setup
    (last_trace_width 0.254)
    (user_trace_width 0.1524)
    (user_trace_width 0.2)
    (user_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.4)
    (user_trace_width 0.5)
    (user_trace_width 0.6)
    (user_trace_width 0.8)
    (trace_clearance 0.254)
    (zone_clearance 0.1524)
    (zone_45_only no)
    (trace_min 0.1524)
    (segment_width 0.127)
    (edge_width 0.127)
    (via_size 0.6858)
    (via_drill 0.3302)
    (via_min_size 0.6858)
    (via_min_drill 0.3302)
    (uvia_size 0.508)
    (uvia_drill 0.127)
    (uvias_allowed no)
    (uvia_min_size 0.508)
    (uvia_min_drill 0.127)
    (pcb_text_width 0.127)
    (pcb_text_size 0.6 0.6)
    (mod_edge_width 0.127)
    (mod_text_size 0.6 0.6)
    (mod_text_width 0.127)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.05)
    (pad_to_paste_clearance -0.04)
    (aux_axis_origin 0 0)
    (grid_origin 160.02 119.38)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x3ffff_80000001)
      (usegerberextensions true)
      (usegerberattributes true)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.127000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "CAM/"))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 GND)
  (net 3 /Anode)
  (net 4 /Din)
  (net 5 /HV6)
  (net 6 /HV5)
  (net 7 /HV10)
  (net 8 /HV4)
  (net 9 /HV9)
  (net 10 /HV3)
  (net 11 /HV8)
  (net 12 /HV2)
  (net 13 /HV7)
  (net 14 /HV1)
  (net 15 "Net-(NX1-PadP$3)")
  (net 16 "Net-(LED1-Pad1-DO)")
  (net 17 "Net-(J1-Pad4)")
  (net 18 "Net-(J1-Pad6)")
  (net 19 "Net-(J1-Pad16)")
  (net_class Default "Imperial - this is the standard class"
    (clearance 0.254)
    (trace_width 0.254)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
    (add_net +5V)
    (add_net /Anode)
    (add_net /Din)
    (add_net /HV1)
    (add_net /HV10)
    (add_net /HV2)
    (add_net /HV3)
    (add_net /HV4)
    (add_net /HV5)
    (add_net /HV6)
    (add_net /HV7)
    (add_net /HV8)
    (add_net /HV9)
    (add_net GND)
    (add_net "Net-(J1-Pad16)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(J1-Pad6)")
    (add_net "Net-(LED1-Pad1-DO)")
    (add_net "Net-(NX1-PadP$3)")
  )
  (net_class 0.2mm ""
    (clearance 0.2)
    (trace_width 0.2)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (net_class Minimal ""
    (clearance 0.1524)
    (trace_width 0.1524)
    (via_dia 0.6858)
    (via_drill 0.3302)
    (uvia_dia 0.508)
    (uvia_drill 0.127)
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 5A712598)
    (at 160.0835 116.6495)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C1 (at -2.4 0.05 90) (layer F.SilkS) hide)
    (fp_text value 0.1uF (at 4.0005 0.3175) (layer F.SilkS))
    (fp_text user %R (at 0 -1.25) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 0.95 0) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x09_Pitch2.54mm (layer B.Cu) (tedit 5A3B14FF)
    (at 170.18 101.6 90)
    (descr "Through hole straight pin header, 2x09, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x09 2.54mm double row")
    (fp_text reference J1 (at 1.27 2.33 90) (layer B.SilkS) hide)
    (fp_text value Nixie (at 1.27 -22.65 90) (layer B.Fab))
    (fp_text user %R (at 1.27 -10.16) (layer B.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /Anode))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 3 /Anode))
    (pad 3 thru_hole oval (at 0 -2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 5 /HV6))
    (pad 4 thru_hole oval (at 2.54 -2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 "Net-(J1-Pad4)"))
    (pad 5 thru_hole oval (at 0 -5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 6 /HV5))
    (pad 6 thru_hole oval (at 2.54 -5.08 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J1-Pad6)"))
    (pad 7 thru_hole oval (at 0 -7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 /HV4))
    (pad 8 thru_hole oval (at 2.54 -7.62 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 /HV10))
    (pad 9 thru_hole oval (at 0 -10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 /HV3))
    (pad 10 thru_hole oval (at 2.54 -10.16 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 /HV9))
    (pad 11 thru_hole oval (at 0 -12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 12 /HV2))
    (pad 12 thru_hole oval (at 2.54 -12.7 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 /HV8))
    (pad 13 thru_hole oval (at 0 -15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 /HV1))
    (pad 14 thru_hole oval (at 2.54 -15.24 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 /HV7))
    (pad 15 thru_hole oval (at 0 -17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 4 /Din))
    (pad 16 thru_hole oval (at 2.54 -17.78 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 "Net-(J1-Pad16)"))
    (pad 17 thru_hole oval (at 0 -20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 +5V))
    (pad 18 thru_hole oval (at 2.54 -20.32 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GND))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x09_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module adafruit:adafruit-LED3535 (layer F.Cu) (tedit 5A3B14EC)
    (at 159.98952 119.42826)
    (attr smd)
    (fp_text reference LED1 (at 0.15748 2.61874 180) (layer F.SilkS))
    (fp_text value WS2812BSK6812MINI (at 0.127 2.54) (layer F.SilkS) hide)
    (pad 1-DO smd rect (at 1.74752 0.87376 90) (size 0.84836 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(LED1-Pad1-DO)"))
    (pad 2-GN smd rect (at 1.74752 -0.87376 90) (size 0.84836 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 3-DI smd rect (at -1.74752 -0.87376 90) (size 0.84836 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 4 /Din))
    (pad 4-VD smd rect (at -1.74752 0.87376 90) (size 0.84836 0.99822) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
  )
  (module logos:mermaid_l (layer B.Cu) (tedit 0)
    (at 170.688 127.762 180)
    (fp_text reference G*** (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (module mynixies:mynixies-SK-116-1 (layer F.Cu) (tedit 5A7125C0)
    (at 160.12414 119.45366)
    (attr virtual)
    (fp_text reference NX1 (at -0.10414 -10.23366) (layer F.SilkS))
    (fp_text value XN-3 (at -11.53414 -3.88366) (layer F.SilkS) hide)
    (pad P$1 thru_hole circle (at 4.99872 0) (size 2.3241 2.3241) (drill 1.5494) (layers *.Cu *.Paste *.Mask)
      (net 9 /HV9))
    (pad P$3 thru_hole circle (at 2.49936 -4.32816) (size 2.3241 2.3241) (drill 1.5494) (layers *.Cu *.Paste *.Mask)
      (net 15 "Net-(NX1-PadP$3)"))
    (pad P$4 thru_hole circle (at 0 -4.99872) (size 2.3241 2.3241) (drill 1.5494) (layers *.Cu *.Paste *.Mask)
      (net 7 /HV10))
    (pad P$5 thru_hole circle (at -2.49936 -4.32816) (size 2.3241 2.3241) (drill 1.5494) (layers *.Cu *.Paste *.Mask)
      (net 14 /HV1))
    (pad P$6 thru_hole circle (at -4.32816 -2.49936) (size 2.3241 2.3241) (drill 1.5494) (layers *.Cu *.Paste *.Mask)
      (net 12 /HV2))
    (pad P$7 thru_hole circle (at -4.99872 0) (size 2.3241 2.3241) (drill 1.5494) (layers *.Cu *.Paste *.Mask)
      (net 10 /HV3))
    (pad P$8 thru_hole circle (at -4.32816 2.49936) (size 2.3241 2.3241) (drill 1.5494) (layers *.Cu *.Paste *.Mask)
      (net 8 /HV4))
    (pad P$9 thru_hole circle (at -2.49936 4.32816) (size 2.3241 2.3241) (drill 1.5494) (layers *.Cu *.Paste *.Mask)
      (net 6 /HV5))
    (pad P$10 thru_hole circle (at 0 4.99872) (size 2.3241 2.3241) (drill 1.5494) (layers *.Cu *.Paste *.Mask)
      (net 5 /HV6))
    (pad P$11 thru_hole circle (at 2.49936 4.32816) (size 2.3241 2.3241) (drill 1.5494) (layers *.Cu *.Paste *.Mask)
      (net 13 /HV7))
    (pad P$12 thru_hole circle (at 4.32816 2.49936) (size 2.3241 2.3241) (drill 1.5494) (layers *.Cu *.Paste *.Mask)
      (net 11 /HV8))
  )
  (module Resistors_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal (layer B.Cu) (tedit 5BEB6794)
    (at 170.18 115.38 90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (fp_text reference R1 (at 5.08 2.31 90) (layer B.SilkS) hide)
    (fp_text value 18k (at 5.08 -2.31 90) (layer B.SilkS))
    (pad 2 thru_hole oval (at 10.16 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 3 /Anode))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(NX1-PadP$3)"))
    (model ${KISYS3DMOD}/Resistors_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_ISO7380_Pad (layer F.Cu) (tedit 5BEB68B2)
    (at 160.02 133.35)
    (descr "Mounting Hole 3.2mm, M3, ISO7380")
    (tags "mounting hole 3.2mm m3 iso7380")
    (attr virtual)
    (fp_text reference REF** (at 0 -3.85) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_ISO7380_Pad (at 0 3.85) (layer F.Fab))
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.7 5.7) (drill 3.2) (layers *.Cu *.Mask))
  )
  (gr_text 9 (at 167.132 119.507) (layer F.SilkS))
  (gr_text 8 (at 166.116 123.063) (layer F.SilkS))
  (gr_text 7 (at 163.957 125.476) (layer F.SilkS))
  (gr_text 6 (at 160.02 126.492) (layer F.SilkS))
  (gr_text 5 (at 156.21 125.476) (layer F.SilkS))
  (gr_text 4 (at 153.924 122.936) (layer F.SilkS))
  (gr_text 3 (at 153.162 119.38) (layer F.SilkS))
  (gr_text 2 (at 154.051 116.078) (layer F.SilkS))
  (gr_text 1 (at 156.464 113.538) (layer F.SilkS))
  (gr_text 0 (at 160.147 112.522) (layer F.SilkS))
  (gr_text A (at 163.703 113.284) (layer F.SilkS))
  (gr_line (start 152.02 137.38) (end 168.02 137.38) (layer Edge.Cuts) (width 0.127))
  (gr_arc (start 152.02 132.38) (end 147.02 132.38) (angle -90) (layer Edge.Cuts) (width 0.127))
  (gr_arc (start 168.02 132.38) (end 168.02 137.38) (angle -90) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 147.02 96.38) (end 147.02 132.38) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 173.02 96.38) (end 173.02 132.38) (layer Edge.Cuts) (width 0.127))
  (gr_line (start 147.02 96.38) (end 173.02 96.38) (layer Edge.Cuts) (width 0.127))
  (gr_text "Mill-Max\n0665-0-15-15-30-27-10-0" (at 160.02 106.299) (layer B.SilkS))
  (gr_text "nixies.us\nXN-3,XN-13,GN-13A,GN-6A" (at 169.672 128.143) (layer B.Mask))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.1524))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing chamfer))
    (polygon
      (pts
        (xy 174.02 95.38) (xy 146.02 95.38) (xy 146.02 138.38) (xy 174.02 138.38)
      )
    )
  )
)
