<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.6.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="42.926" x2="26.9748" y2="42.926" width="0.1016" layer="20"/>
<wire x1="6.6294" y1="0" x2="20.32" y2="0" width="0.1016" layer="20"/>
<wire x1="0" y1="42.926" x2="0" y2="19.05" width="0.1016" layer="20"/>
<wire x1="0" y1="16.6624" x2="0" y2="6.6294" width="0.1016" layer="20"/>
<wire x1="26.9748" y1="42.926" x2="26.9748" y2="19.05" width="0.1016" layer="20"/>
<wire x1="26.9748" y1="16.6624" x2="26.9748" y2="6.6294" width="0.1016" layer="20"/>
<wire x1="0" y1="6.6294" x2="6.6294" y2="0" width="0.1016" layer="20"/>
<wire x1="26.9748" y1="6.6294" x2="20.32" y2="0" width="0.1016" layer="20"/>
<wire x1="26.9748" y1="16.6624" x2="26.9748" y2="19.05" width="0.1016" layer="20" curve="-180"/>
<wire x1="0" y1="19.05" x2="0" y2="16.6624" width="0.1016" layer="20" curve="-180"/>
<text>GND</text>
<text>GND</text>
<text>RX</text>
<text>TX</text>
<text>TX</text>
<text>RX</text>
<text>Vcc</text>
<text>Vcc</text>
<text>RA1</text>
<text>RA0</text>
<text>RA4</text>
<text>RA5</text>
<text>RA2</text>
<text>RC0</text>
</plain>
<libraries>
<library name="rtotte">
<packages>
<package name="BATTERY_2032_CLIP">
</package>
<package name="BUTTON_PCB">
</package>
<package name="0402">
</package>
<package name="0603">
<description>0603 (1608 Metric)</description>
</package>
<package name="LED_0805">
<description>Wurth 0805 LED

Recommended land pattern</description>
</package>
<package name="CRYSTAL_ABM8G">
</package>
<package name="SOP65P640X120-20N">
<description>&lt;b&gt;(ST)20-Lead(TSSOP)&lt;/b&gt;&lt;br&gt;
</description>
</package>
<package name="TC2030-MCP-NL">
<description>&lt;B&gt;TAG-CONNECT ICSP Connector&lt;/B&gt;&lt;BR&gt;&lt;I&gt;Manufacturer:&lt;/I&gt; &lt;a href="www.tag-connect.com"&gt;Tag-Connect&lt;/a&gt;&lt;BR&gt;
&lt;BR&gt;Cable for easy In-Circuit Serial Programming. Designed for Microchip ICD2, suitable for many others.&lt;BR&gt;

&lt;TABLE cellspacing=0 cellpadding=0 border=0&gt;
&lt;TR&gt;&lt;TD width=20&gt;&lt;/TD&gt;&lt;TD&gt;
&lt;TABLE cellspacing=0 cellpadding=1 border=1&gt;
&lt;TR bgcolor=silver&gt;&lt;TD align=center&gt;PAD&lt;/TD&gt;&lt;TD align=center&gt;Description&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;1&lt;/TD&gt;&lt;TD&gt;MCLR/Vpp&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;2&lt;/TD&gt;&lt;TD&gt;Vdd&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;3&lt;/TD&gt;&lt;TD&gt;GND&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;4&lt;/TD&gt;&lt;TD&gt;PGD (ISPDAT)&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;5&lt;/TD&gt;&lt;TD&gt;PGC (ISPCLK)&lt;/TD&gt;&lt;/TR&gt;
&lt;TR&gt;&lt;TD align=center&gt;6&lt;/TD&gt;&lt;TD&gt;nc (used for LVP)&lt;/TD&gt;&lt;/TR&gt;
&lt;/TABLE&gt;
&lt;/TD&gt;&lt;/TR&gt;&lt;/TABLE&gt;&lt;BR&gt;&lt;BR&gt;

©2009 ROFA.cz - modified and updated by Robert Darlington &amp;#8249;rdarlington@gmail.com&amp;#8250;</description>
</package>
<package name="ANTENNA_915MHZ_OPEN">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X04_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole - 4 Pin No Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="BAT" library="rtotte" package="BATTERY_2032_CLIP" value=""/>
<element name="BDOWN" library="rtotte" package="BUTTON_PCB" value="BUTTON_PCB"/>
<element name="BCENTER" library="rtotte" package="BUTTON_PCB" value="BUTTON_PCB"/>
<element name="BUP" library="rtotte" package="BUTTON_PCB" value="BUTTON_PCB"/>
<element name="BRIGHT" library="rtotte" package="BUTTON_PCB" value="BUTTON_PCB"/>
<element name="BLEFT" library="rtotte" package="BUTTON_PCB" value="BUTTON_PCB"/>
<element name="L6" library="rtotte" package="0402" value=""/>
<element name="L7" library="rtotte" package="0402" value=""/>
<element name="C1" library="rtotte" package="0402" value=""/>
<element name="L8" library="rtotte" package="0402" value="120nH"/>
<element name="L9" library="rtotte" package="0402" value=""/>
<element name="L10" library="rtotte" package="0402" value=""/>
<element name="C8" library="rtotte" package="0402" value=""/>
<element name="C9" library="rtotte" package="0402" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="rtotte" package="0402" value="1000pF"/>
<element name="C11" library="rtotte" package="0603" value=""/>
<element name="C12" library="rtotte" package="0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="rtotte" package="0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$14" library="rtotte" package="LED_0805" value="LED_0805_WURTH"/>
<element name="U$15" library="rtotte" package="CRYSTAL_ABM8G" value="CRYSTAL_4PORT"/>
<element name="IC1" library="rtotte" package="SOP65P640X120-20N" value="PIC16LF1824T39A-I_ST">
<attribute name="3D_PACKAGE" value=""/>
<attribute name="ALLIED_NUMBER" value=""/>
<attribute name="DESCRIPTION" value="8-bit Microcontrollers - MCU PIC16LF1824 Microcontroller"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="MANUFACTURER_NAME" value="Microchip"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="PIC16LF1824T39A-I/ST"/>
<attribute name="OTHER_PART_NUMBER" value=""/>
<attribute name="RS_PART_NUMBER" value=""/>
<attribute name="SUPPLIER_NAME" value="RS"/>
</element>
<element name="U$20" library="rtotte" package="TC2030-MCP-NL" value="TC_PIC"/>
<element name="U$1" library="rtotte" package="ANTENNA_915MHZ_OPEN" value="ANTENNA_LOOP_915_O"/>
<element name="R1" library="rtotte" package="0402" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="1X04_NO_SILK" value="">
<attribute name="PROD_ID" value="CONN-09696"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="L9" pad="P$1"/>
<contactref element="L10" pad="P$1"/>
<contactref element="C10" pad="P$2"/>
<contactref element="C11" pad="2"/>
<contactref element="C12" pad="2"/>
<contactref element="U$15" pad="3"/>
<contactref element="U$15" pad="2"/>
<contactref element="U$15" pad="4"/>
<contactref element="IC1" pad="11"/>
<contactref element="IC1" pad="20"/>
<contactref element="U$20" pad="3"/>
<contactref element="U$1" pad="GND"/>
<contactref element="R1" pad="P$1"/>
<contactref element="U$14" pad="PAD_CATHODE(-)"/>
<contactref element="BAT" pad="NEG"/>
<contactref element="BDOWN" pad="P2"/>
<contactref element="BCENTER" pad="P2"/>
<contactref element="BUP" pad="P2"/>
<contactref element="BLEFT" pad="P2"/>
<contactref element="BRIGHT" pad="P2"/>
<contactref element="J3" pad="4"/>
</signal>
<signal name="N$7">
<contactref element="L6" pad="P$1"/>
<contactref element="U$1" pad="P$4"/>
<contactref element="U$1" pad="P$1"/>
<contactref element="U$1" pad="P$3"/>
<contactref element="U$1" pad="RF"/>
</signal>
<signal name="N$9">
<contactref element="L6" pad="P$2"/>
<contactref element="L7" pad="P$1"/>
<contactref element="C8" pad="P$1"/>
</signal>
<signal name="N$10">
<contactref element="L7" pad="P$2"/>
<contactref element="C1" pad="P$1"/>
<contactref element="C9" pad="P$1"/>
</signal>
<signal name="N$11">
<contactref element="C8" pad="P$2"/>
<contactref element="L9" pad="P$2"/>
</signal>
<signal name="N$12">
<contactref element="C9" pad="P$2"/>
<contactref element="L10" pad="P$2"/>
</signal>
<signal name="RFOUT">
<contactref element="L8" pad="P$1"/>
<contactref element="C1" pad="P$2"/>
<contactref element="IC1" pad="10"/>
</signal>
<signal name="VCC">
<contactref element="C10" pad="P$1"/>
<contactref element="L8" pad="P$2"/>
<contactref element="C12" pad="1"/>
<contactref element="C11" pad="1"/>
<contactref element="IC1" pad="1"/>
<contactref element="IC1" pad="8"/>
<contactref element="U$20" pad="2"/>
<contactref element="BAT" pad="P1"/>
<contactref element="BAT" pad="P0"/>
<contactref element="J3" pad="1"/>
</signal>
<signal name="RESET">
<contactref element="IC1" pad="4"/>
<contactref element="U$20" pad="1"/>
</signal>
<signal name="RA0">
<contactref element="IC1" pad="19"/>
<contactref element="U$20" pad="4"/>
<contactref element="BCENTER" pad="P1"/>
</signal>
<signal name="RA1">
<contactref element="IC1" pad="18"/>
<contactref element="U$20" pad="5"/>
<contactref element="BRIGHT" pad="P1"/>
</signal>
<signal name="RA4">
<contactref element="IC1" pad="3"/>
<contactref element="BDOWN" pad="P1"/>
</signal>
<signal name="N$17">
<contactref element="IC1" pad="13"/>
<contactref element="U$15" pad="1"/>
</signal>
<signal name="RC5_RX">
<contactref element="IC1" pad="5"/>
<contactref element="J3" pad="2"/>
</signal>
<signal name="RC4_TX">
<contactref element="IC1" pad="6"/>
<contactref element="J3" pad="3"/>
</signal>
<signal name="RC3_DATA">
<contactref element="IC1" pad="7"/>
<contactref element="IC1" pad="12"/>
</signal>
<signal name="LED">
<contactref element="IC1" pad="16"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="RC2_CTRL">
<contactref element="IC1" pad="14"/>
<contactref element="IC1" pad="9"/>
<contactref element="R1" pad="P$2"/>
</signal>
<signal name="RA5">
<contactref element="IC1" pad="2"/>
<contactref element="BLEFT" pad="P1"/>
</signal>
<signal name="RA2">
<contactref element="IC1" pad="17"/>
<contactref element="BUP" pad="P1"/>
</signal>
<signal name="N$2">
<contactref element="R2" pad="2"/>
<contactref element="U$14" pad="PAD_ANODE(+)"/>
</signal>
<signal name="RC1">
<contactref element="IC1" pad="15"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
