(kicad_pcb (version 4) (host pcbnew 4.0.2+dfsg1-stable)
  (general
    (links 66)
    (no_connects 2)
    (area 100.047667 75.89 163.956 132.216002)
    (thickness 1.6)
    (drawings 9)
    (tracks 214)
    (zones 0)
    (modules 37)
    (nets 27)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user hide)
    (33 F.Adhes user hide)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user hide)
    (39 F.Mask user hide)
    (40 Dwgs.User user hide)
    (41 Cmts.User user hide)
    (42 Eco1.User user hide)
    (43 Eco2.User user hide)
    (44 Edge.Cuts user)
    (45 Margin user hide)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.75)
    (user_trace_width 0.5)
    (user_trace_width 0.75)
    (user_trace_width 1)
    (user_trace_width 1.5)
    (user_trace_width 2)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.1)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 0.8 0.5)
    (user_via 1 0.8)
    (user_via 1.2 1)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 2 1.8)
    (pad_drill 1)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 101.6 131.064)
    (grid_origin 101.6 131.064)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x0c030_00000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.150000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 5)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ../../../../../wewwe/))
  )
  (net 0 "")
  (net 1 "Net-(C1-Pad1)")
  (net 2 "Net-(C1-Pad2)")
  (net 3 "Net-(C2-Pad1)")
  (net 4 "Net-(C2-Pad2)")
  (net 5 GND)
  (net 6 "Net-(C3-Pad2)")
  (net 7 "Net-(C4-Pad2)")
  (net 8 "Net-(C5-Pad1)")
  (net 9 "Net-(C5-Pad2)")
  (net 10 "Net-(C6-Pad2)")
  (net 11 "Net-(C7-Pad1)")
  (net 12 "Net-(C10-Pad1)")
  (net 13 "Net-(C10-Pad2)")
  (net 14 "Net-(C11-Pad1)")
  (net 15 "Net-(C11-Pad2)")
  (net 16 "Net-(C12-Pad2)")
  (net 17 VCC)
  (net 18 "Net-(P2-Pad1)")
  (net 19 "Net-(P3-Pad1)")
  (net 20 "Net-(P4-Pad1)")
  (net 21 "Net-(R5-Pad2)")
  (net 22 SF_OUT)
  (net 23 "Net-(R10-Pad1)")
  (net 24 /ECG_PLL_pll/PC1)
  (net 25 "Net-(R16-Pad1)")
  (net 26 /ECG_PLL_pll/COMP_IN)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /ECG_PLL_pll/COMP_IN)
    (add_net /ECG_PLL_pll/PC1)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C10-Pad1)")
    (add_net "Net-(C10-Pad2)")
    (add_net "Net-(C11-Pad1)")
    (add_net "Net-(C11-Pad2)")
    (add_net "Net-(C12-Pad2)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C3-Pad2)")
    (add_net "Net-(C4-Pad2)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(C6-Pad2)")
    (add_net "Net-(C7-Pad1)")
    (add_net "Net-(P2-Pad1)")
    (add_net "Net-(P3-Pad1)")
    (add_net "Net-(P4-Pad1)")
    (add_net "Net-(R10-Pad1)")
    (add_net "Net-(R16-Pad1)")
    (add_net "Net-(R5-Pad2)")
    (add_net SF_OUT)
    (add_net VCC)
  )
  (module Potentiometers:Potentiometer_VishaySpectrol-Econtrim-Type36X (layer F.Cu) (tedit 5446FD75)
    (at 148.85 95.814 90)
    (descr "Potentiometer, Trimmer, Spectrol Type 36X, Econtrim, Rev A, 02 Aug 2010,")
    (tags "Potentiometer, Trimmer, Spectrol Type 36X, Econtrim, Rev A, 02 Aug 2010,")
    (fp_text reference RV1 (at -2.5 -0.05 180) (layer F.SilkS))
    (fp_text value 5k (at 5.03936 3.32994 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 2.5 -2.5 90) (size 2.49936 2.49936) (drill 1.19888) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(R5-Pad2)"))
    (pad 3 thru_hole circle (at 4.99872 0 90) (size 2.49936 2.49936) (drill 1.19888) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(R5-Pad2)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.49936 2.49936) (drill 1.19888) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(P2-Pad1)"))
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 569FCF07)
    (at 112.268 96.52 180)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R9 (at 0 10.033 360) (layer F.SilkS))
    (fp_text value 47k (at 3.81 3.81 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 11 "Net-(C7-Pad1)"))
    (pad 2 thru_hole circle (at 7.62 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 22 SF_OUT))
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 569FCF07)
    (at 138.684 113.284 90)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R2 (at -0.381 -2.286 270) (layer F.SilkS))
    (fp_text value 150k (at 3.81 3.81 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 2 thru_hole circle (at 7.62 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 6 "Net-(C3-Pad2)"))
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 5D141F27)
    (at 134.62 88.432 270)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C4 (at -1.564 0 360) (layer F.SilkS))
    (fp_text value 33n (at 1.25 2.5 270) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 270) (size 1.8 2) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 5 GND))
    (pad 2 thru_hole oval (at 2.5 0 270) (size 1.8 2) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(C4-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 5D1418C2)
    (at 130.556 111.252)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C1 (at 4.294 -0.188 90) (layer F.SilkS))
    (fp_text value 100n (at 1.25 2.5) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 1.8 2) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole oval (at 2.5 0) (size 1.8 2) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 2 "Net-(C1-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 5D141F53)
    (at 138.684 88.392 270)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C2 (at -1.524 0 360) (layer F.SilkS))
    (fp_text value 330n (at 1.25 2.5 270) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 270) (size 1.8 2) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 thru_hole oval (at 2.5 0 270) (size 1.8 2) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 4 "Net-(C2-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 0)
    (at 135.128 107.696 90)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C3 (at -0.368 -2.528 180) (layer F.SilkS))
    (fp_text value 10n (at 1.25 2.5 90) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.8 2) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 5 GND))
    (pad 2 thru_hole oval (at 2.5 0 90) (size 1.8 2) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(C3-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 0)
    (at 125.476 84.328 180)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C5 (at 4.572 0 270) (layer F.SilkS))
    (fp_text value 470n (at 1.25 2.5 180) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 180) (size 1.8 2) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(C5-Pad1)"))
    (pad 2 thru_hole oval (at 2.5 0 180) (size 1.8 2) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(C5-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 5D141EF3)
    (at 115.824 88.9)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C6 (at 2.54 -2.54) (layer F.SilkS))
    (fp_text value 22n (at 1.25 2.5) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 1.8 2) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 5 GND))
    (pad 2 thru_hole oval (at 2.5 0) (size 1.8 2) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(C6-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 5D14202A)
    (at 116.332 100.584 90)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C7 (at 0.127 2.54 90) (layer F.SilkS))
    (fp_text value 10n (at 1.25 2.5 90) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.8 2) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(C7-Pad1)"))
    (pad 2 thru_hole oval (at 2.5 0 90) (size 1.8 2) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 5 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 5D141F0B)
    (at 118.324 93.472 180)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C8 (at -0.04 -2.54 180) (layer F.SilkS))
    (fp_text value 100n (at 1.25 2.5 180) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 180) (size 1.8 2) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 17 VCC))
    (pad 2 thru_hole oval (at 2.5 0 180) (size 1.8 2) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 5 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 5D141D9C)
    (at 106.68 112.268 180)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C10 (at -1.778 0 270) (layer F.SilkS))
    (fp_text value 100n (at 1.25 2.5 180) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 180) (size 1.8 2) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(C10-Pad1)"))
    (pad 2 thru_hole oval (at 2.5 0 180) (size 1.8 2) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(C10-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 5D154EFE)
    (at 121.412 111.252)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C11 (at 4.532 0 90) (layer F.SilkS))
    (fp_text value 10n (at 1.25 2.5) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 1.8 2) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(C11-Pad1)"))
    (pad 2 thru_hole oval (at 2.5 0) (size 1.8 2) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(C11-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 0)
    (at 123.952 125.476 180)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C12 (at -2.032 0 270) (layer F.SilkS))
    (fp_text value 10n (at 1.25 2.5 180) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 180) (size 1.8 2) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 5 GND))
    (pad 2 thru_hole oval (at 2.5 0 180) (size 1.8 2) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(C12-Pad2)"))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Disc_D3_P2.5 (layer F.Cu) (tedit 0)
    (at 104.18 123.444)
    (descr "Capacitor 3mm Disc, Pitch 2.5mm")
    (tags Capacitor)
    (fp_text reference C13 (at 4.278 0 90) (layer F.SilkS))
    (fp_text value 100n (at 1.25 2.5) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 1.8 2) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 5 GND))
    (pad 2 thru_hole oval (at 2.5 0) (size 1.8 2) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 17 VCC))
    (model Capacitors_ThroughHole.3dshapes/C_Disc_D3_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 54EA08DC)
    (at 130.556 84.328)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value OCR (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(C2-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 54EA08DC)
    (at 148.336 102.616)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at -0.762 2.667 180) (layer F.SilkS))
    (fp_text value V (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(P2-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 54EA08DC)
    (at 148.336 109.22)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P3 (at -0.762 2.667 180) (layer F.SilkS))
    (fp_text value LL (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(P3-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 54EA08DC)
    (at 148.336 115.316)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P4 (at -0.762 2.667 180) (layer F.SilkS))
    (fp_text value LA (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 20 "Net-(P4-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x01 (layer F.Cu) (tedit 54EA08DC)
    (at 148.336 121.412)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P5 (at -0.762 2.667 180) (layer F.SilkS))
    (fp_text value RA/RL (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.2352 2.2352) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x01.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 5D154F5C)
    (at 105.156 116.332)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P6 (at 3.048 -0.889) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 2 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(C10-Pad2)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 569FCF07)
    (at 124.968 116.332)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R1 (at -2.54 0) (layer F.SilkS))
    (fp_text value 10k (at 3.81 3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 8 "Net-(C5-Pad1)"))
    (pad 2 thru_hole circle (at 7.62 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 2 "Net-(C1-Pad2)"))
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 569FCF07)
    (at 134.62 101.6 90)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R3 (at -2.032 -0.635 180) (layer F.SilkS))
    (fp_text value 2k2 (at 3.81 3.81 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 1 "Net-(C1-Pad1)"))
    (pad 2 thru_hole circle (at 7.62 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 4 "Net-(C2-Pad2)"))
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 569FCF07)
    (at 138.684 93.98 270)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R4 (at 9.652 0.635 360) (layer F.SilkS))
    (fp_text value 68k (at 3.81 3.81 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 4 "Net-(C2-Pad2)"))
    (pad 2 thru_hole circle (at 7.62 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 7 "Net-(C4-Pad2)"))
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 569FCF07)
    (at 135.636 84.328)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R5 (at -2.032 0 90) (layer F.SilkS))
    (fp_text value 22k (at 3.81 3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 3 "Net-(C2-Pad1)"))
    (pad 2 thru_hole circle (at 7.62 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 21 "Net-(R5-Pad2)"))
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 569FCF07)
    (at 143.1 88.9 270)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R7 (at 8.001 2.286 270) (layer F.SilkS))
    (fp_text value 560 (at 3.81 3.81 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 18 "Net-(P2-Pad1)"))
    (pad 2 thru_hole circle (at 7.62 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 19 "Net-(P3-Pad1)"))
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 569FCF07)
    (at 143.764 101.6 270)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R8 (at 8.001 2.286 270) (layer F.SilkS))
    (fp_text value 270 (at 3.81 3.81 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 19 "Net-(P3-Pad1)"))
    (pad 2 thru_hole circle (at 7.62 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 20 "Net-(P4-Pad1)"))
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 569FCF07)
    (at 112.268 92.79265 180)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R10 (at -0.508 7.70265 360) (layer F.SilkS))
    (fp_text value 10k (at 3.81 3.81 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 23 "Net-(R10-Pad1)"))
    (pad 2 thru_hole circle (at 7.62 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 9 "Net-(C5-Pad2)"))
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 569FCF07)
    (at 104.648 88.9)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R11 (at 8.128 -5.207 180) (layer F.SilkS))
    (fp_text value 10k (at 3.81 3.81) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 9 "Net-(C5-Pad2)"))
    (pad 2 thru_hole circle (at 7.62 0) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 10 "Net-(C6-Pad2)"))
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 569FCF07)
    (at 143.764 114.3 270)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R13 (at 5.588 2.54 270) (layer F.SilkS))
    (fp_text value 100 (at 3.81 3.81 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 20 "Net-(P4-Pad1)"))
    (pad 2 thru_hole circle (at 7.62 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 5 GND))
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 569FCF07)
    (at 132.588 120.396 180)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R14 (at 10.541 0.127 180) (layer F.SilkS))
    (fp_text value 10k (at 3.81 3.81 180) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 16 "Net-(C12-Pad2)"))
    (pad 2 thru_hole circle (at 7.62 0 180) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 24 /ECG_PLL_pll/PC1))
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 569FCF07)
    (at 107.188 100.076 270)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R15 (at 0 -4.191 270) (layer F.SilkS))
    (fp_text value 10k (at 3.81 3.81 270) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 5 GND))
    (pad 2 thru_hole circle (at 7.62 0 270) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 22 SF_OUT))
  )
  (module Resistors_ThroughHole:Resistor_Horizontal_RM7mm (layer F.Cu) (tedit 569FCF07)
    (at 104.14 107.696 90)
    (descr "Resistor, Axial,  RM 7.62mm, 1/3W,")
    (tags "Resistor Axial RM 7.62mm 1/3W R3")
    (fp_text reference R16 (at 7.62 5.588 90) (layer F.SilkS))
    (fp_text value 7k5 (at 3.81 3.81 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 25 "Net-(R16-Pad1)"))
    (pad 2 thru_hole circle (at 7.62 0 90) (size 1.99898 1.99898) (drill 1.00076) (layers *.Cu *.SilkS *.Mask)
      (net 5 GND))
  )
  (module Housings_DIP:DIP-14_W7.62mm_LongPads (layer F.Cu) (tedit 5D1421D1)
    (at 122.428 90.932)
    (descr "14-lead dip package, row spacing 7.62 mm (300 mils), longer pads")
    (tags "dil dip 2.54 300")
    (fp_text reference U1 (at 1.016 -3.556) (layer F.SilkS))
    (fp_text value LM324 (at 0 -3.72) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(C5-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(C5-Pad1)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 10 "Net-(C6-Pad2)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 17 VCC))
    (pad 5 thru_hole oval (at 0 10.16) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(C7-Pad1)"))
    (pad 6 thru_hole oval (at 0 12.7) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(R10-Pad1)"))
    (pad 7 thru_hole oval (at 0 15.24) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(R10-Pad1)"))
    (pad 8 thru_hole oval (at 7.62 15.24) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(C1-Pad1)"))
    (pad 9 thru_hole oval (at 7.62 12.7) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 1 "Net-(C1-Pad1)"))
    (pad 10 thru_hole oval (at 7.62 10.16) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(C3-Pad2)"))
    (pad 11 thru_hole oval (at 7.62 7.62) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 5 GND))
    (pad 12 thru_hole oval (at 7.62 5.08) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(C4-Pad2)"))
    (pad 13 thru_hole oval (at 7.62 2.54) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(C2-Pad1)"))
    (pad 14 thru_hole oval (at 7.62 0) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 3 "Net-(C2-Pad1)"))
    (model Housings_DIP.3dshapes/DIP-14_W7.62mm_LongPads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-16_W7.62mm_LongPads (layer F.Cu) (tedit 54130A77)
    (at 118.364 122.428 180)
    (descr "16-lead dip package, row spacing 7.62 mm (300 mils), longer pads")
    (tags "dil dip 2.54 300")
    (fp_text reference U2 (at -0.508 -4.064 180) (layer F.SilkS))
    (fp_text value HEF4046 (at 0 -3.72 180) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 180) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 24 /ECG_PLL_pll/PC1))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 26 /ECG_PLL_pll/COMP_IN))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 26 /ECG_PLL_pll/COMP_IN))
    (pad 5 thru_hole oval (at 0 10.16 180) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 5 GND))
    (pad 6 thru_hole oval (at 0 12.7 180) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(C11-Pad1)"))
    (pad 7 thru_hole oval (at 0 15.24 180) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(C11-Pad2)"))
    (pad 8 thru_hole oval (at 0 17.78 180) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 5 GND))
    (pad 9 thru_hole oval (at 7.62 17.78 180) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(C12-Pad2)"))
    (pad 10 thru_hole oval (at 7.62 15.24 180) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 22 SF_OUT))
    (pad 11 thru_hole oval (at 7.62 12.7 180) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 25 "Net-(R16-Pad1)"))
    (pad 12 thru_hole oval (at 7.62 10.16 180) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
    (pad 13 thru_hole oval (at 7.62 7.62 180) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
    (pad 14 thru_hole oval (at 7.62 5.08 180) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(C10-Pad1)"))
    (pad 15 thru_hole oval (at 7.62 2.54 180) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
    (pad 16 thru_hole oval (at 7.62 0 180) (size 2.3 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 17 VCC))
    (model Housings_DIP.3dshapes/DIP-16_W7.62mm_LongPads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 5D1420B7)
    (at 133.096 128.016 270)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P7 (at -2.794 -1.016 360) (layer F.SilkS))
    (fp_text value 9VDC (at 0 -3.1 270) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 270) (size 2 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 17 VCC))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2 1.8) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_ThroughHole:C_Radial_D5_L6_P2.5 (layer F.Cu) (tedit 5D154FBA)
    (at 141.732 128.016 90)
    (descr "Radial Electrolytic Capacitor Diameter 5mm x Length 6mm, Pitch 2.5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C9 (at -1.016 3.048 180) (layer F.SilkS))
    (fp_text value 100u/16v (at 1.25 3.8 90) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 90) (size 1.8 2) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 17 VCC))
    (pad 2 thru_hole oval (at 2.5 0 90) (size 1.8 2) (drill 1) (layers *.Cu *.Mask F.SilkS)
      (net 5 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D5_L6_P2.5.wrl
      (at (xyz 0.0492126 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (gr_text "SimECG\nr1.5\n" (at 137.668 115.824 90) (layer F.SilkS))
  (gr_text "UADER FCYT\n" (at 121.92 128.524) (layer F.SilkS))
  (gr_line (start 101.6 81.28) (end 101.6 131.064) (layer Edge.Cuts) (width 0.1))
  (gr_text "SimECG\nr1.5\n" (at 137.668 123.444 90) (layer B.Cu))
  (gr_line (start 151.384 131.064) (end 101.6 131.064) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 151.384 81.28) (end 151.384 131.064) (layer Edge.Cuts) (width 0.1))
  (dimension 49.784 (width 0.3) (layer F.Fab)
    (gr_text "49,784 mm" (at 157.306 106.172 270) (layer F.Fab))
    (feature1 (pts (xy 151.892 131.064) (xy 158.656 131.064)))
    (feature2 (pts (xy 151.892 81.28) (xy 158.656 81.28)))
    (crossbar (pts (xy 155.956 81.28) (xy 155.956 131.064)))
    (arrow1a (pts (xy 155.956 131.064) (xy 155.369579 129.937496)))
    (arrow1b (pts (xy 155.956 131.064) (xy 156.542421 129.937496)))
    (arrow2a (pts (xy 155.956 81.28) (xy 155.369579 82.406504)))
    (arrow2b (pts (xy 155.956 81.28) (xy 156.542421 82.406504)))
  )
  (gr_line (start 101.6 81.28) (end 151.384 81.28) (layer Edge.Cuts) (width 0.1))
  (dimension 49.784 (width 0.3) (layer F.Fab)
    (gr_text "49,784 mm" (at 126.492 77.39) (layer F.Fab))
    (feature1 (pts (xy 151.384 80.772) (xy 151.384 76.04)))
    (feature2 (pts (xy 101.6 80.772) (xy 101.6 76.04)))
    (crossbar (pts (xy 101.6 78.74) (xy 151.384 78.74)))
    (arrow1a (pts (xy 151.384 78.74) (xy 150.257496 79.326421)))
    (arrow1b (pts (xy 151.384 78.74) (xy 150.257496 78.153579)))
    (arrow2a (pts (xy 101.6 78.74) (xy 102.726504 79.326421)))
    (arrow2b (pts (xy 101.6 78.74) (xy 102.726504 78.153579)))
  )
)
