(kicad_pcb (version 4) (host pcbnew 4.0.5)
  (general
    (links 45)
    (no_connects 0)
    (area 103.165 72.93 193.587858 106.875)
    (thickness 1.6)
    (drawings 16)
    (tracks 110)
    (zones 0)
    (modules 27)
    (nets 20)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user)
    (48 B.Fab user hide)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.3)
    (user_trace_width 0.6)
    (user_trace_width 0.9)
    (user_trace_width 1.2)
    (user_trace_width 1.4)
    (user_trace_width 1.6)
    (user_trace_width 1.8)
    (user_trace_width 2)
    (trace_clearance 0.2)
    (zone_clearance 0.381)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 0.000001 0.000001)
    (mod_text_width 0.15)
    (pad_size 6.4 6.4)
    (pad_drill 3.2)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x010f0_80000001)
      (usegerberextensions true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 GNDPWR)
  (net 3 "Net-(AT1-Pad3)")
  (net 4 "Net-(AT1-Pad4)")
  (net 5 "Net-(AT1-Pad5)")
  (net 6 "Net-(AT1-Pad6)")
  (net 7 PB2)
  (net 8 PB1)
  (net 9 PB0)
  (net 10 "Net-(BU1-Pad1)")
  (net 11 "Net-(D1-Pad1)")
  (net 12 VIN)
  (net 13 RESET)
  (net 14 "Net-(IC1-Pad2)")
  (net 15 "Net-(IC1-Pad3)")
  (net 16 "Net-(J1-Pad2)")
  (net 17 "Net-(J1-Pad3)")
  (net 18 "Net-(J1-Pad4)")
  (net 19 "Net-(SW1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GNDPWR)
    (add_net "Net-(AT1-Pad3)")
    (add_net "Net-(AT1-Pad4)")
    (add_net "Net-(AT1-Pad5)")
    (add_net "Net-(AT1-Pad6)")
    (add_net "Net-(BU1-Pad1)")
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(IC1-Pad2)")
    (add_net "Net-(IC1-Pad3)")
    (add_net "Net-(J1-Pad2)")
    (add_net "Net-(J1-Pad3)")
    (add_net "Net-(J1-Pad4)")
    (add_net "Net-(SW1-Pad1)")
    (add_net PB0)
    (add_net PB1)
    (add_net PB2)
    (add_net RESET)
    (add_net VCC)
    (add_net VIN)
  )
  (module Buzzers_Beepers:Buzzer_12x9.5RM7.6 (layer F.Cu) (tedit 5927FCA4)
    (at 175.26 87.376)
    (descr "Generic Buzzer, D12mm height 9.5mm with RM7.6mm")
    (tags buzzer)
    (fp_text reference BU1 (at 3.81 3.175) (layer F.SilkS))
    (fp_text value BUZZER (at 3.8 7.4) (layer F.Fab) hide)
    (fp_text user + (at -0.01 -2.54) (layer F.Fab))
    (fp_text user + (at -0.01 -2.54) (layer F.SilkS))
    (fp_text user %R (at 3.8 -4) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(BU1-Pad1)"))
    (pad 2 thru_hole circle (at 7.6 0) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 GNDPWR))
    (model Buzzers_Beepers.3dshapes/Buzzer_12x9.5RM7.6.wrl
      (at (xyz 0.15 0 0))
      (scale (xyz 4 4 4))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D6.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5927FC0C)
    (at 135.89 93.98 90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=6*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 6mm width 2.5mm Capacitor")
    (fp_text reference C3 (at 2.54 0 90) (layer F.SilkS))
    (fp_text value 100n (at 2.5 2.31 90) (layer F.Fab) hide)
    (fp_text user %R (at 2.5 0 90) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GNDPWR))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 VCC))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D6.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_D3.0mm (layer F.Cu) (tedit 59281F0E)
    (at 181.356 95.504)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (fp_text reference D1 (at 3.048 -3.048) (layer F.SilkS))
    (fp_text value LED (at 1.27 2.96) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 11 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers *.Cu *.Mask)
      (net 2 GNDPWR))
    (model LEDs.3dshapes/LED_D3.0mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module G0TDJ:1N4001_Diode_Case_59-10_Axial (layer F.Cu) (tedit 5927FC0F)
    (at 132.715 91.44 270)
    (fp_text reference D2 (at 0 0 270) (layer F.SilkS))
    (fp_text value DIODE (at 0 -2.54 270) (layer F.Fab) hide)
    (fp_text user K (at 2.794 -0.508 270) (layer F.SilkS))
    (fp_text user A (at -2.54 -0.508 270) (layer F.SilkS))
    (pad 2 thru_hole circle (at 5.08 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 1 thru_hole circle (at -5.08 0 270) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 12 VIN))
  )
  (module Housings_DIP:DIP-8_W7.62mm_LongPads (layer F.Cu) (tedit 5927FBDA)
    (at 152.4 77.47 270)
    (descr "8-lead dip package, row spacing 7.62 mm (300 mils), LongPads")
    (tags "DIL DIP PDIP 2.54mm 7.62mm 300mil LongPads")
    (fp_text reference IC1 (at 3.81 3.81 270) (layer F.SilkS))
    (fp_text value ATTINY85-P (at 3.81 10.01 270) (layer F.Fab) hide)
    (fp_text user %R (at 3.81 3.81 270) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 13 RESET))
    (pad 5 thru_hole oval (at 7.62 7.62 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 9 PB0))
    (pad 2 thru_hole oval (at 0 2.54 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 14 "Net-(IC1-Pad2)"))
    (pad 6 thru_hole oval (at 7.62 5.08 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 8 PB1))
    (pad 3 thru_hole oval (at 0 5.08 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 15 "Net-(IC1-Pad3)"))
    (pad 7 thru_hole oval (at 7.62 2.54 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 PB2))
    (pad 4 thru_hole oval (at 0 7.62 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 GNDPWR))
    (pad 8 thru_hole oval (at 7.62 0 270) (size 2.4 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 VCC))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-8_W7.62mm_LongPads.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module G0TDJ:USB_A_MALE_RA_TH (layer B.Cu) (tedit 591C57AC)
    (at 122 90.5 90)
    (fp_text reference J1 (at -3.51 -17.86 90) (layer B.SilkS))
    (fp_text value USB_2 (at -6.35 -9.59 180) (layer B.Fab))
    (fp_text user "Board Edge" (at 0.5 -2.6 90) (layer B.SilkS))
    (pad 2 thru_hole circle (at -0.5 3 90) (size 1.524 1.524) (drill 0.92) (layers *.Cu *.Mask)
      (net 16 "Net-(J1-Pad2)"))
    (pad 3 thru_hole circle (at 1.5 3 90) (size 1.524 1.524) (drill 0.92) (layers *.Cu *.Mask)
      (net 17 "Net-(J1-Pad3)"))
    (pad 1 thru_hole circle (at -3 3 90) (size 1.524 1.524) (drill 0.92) (layers *.Cu *.Mask)
      (net 2 GNDPWR))
    (pad 4 thru_hole circle (at 4 3 90) (size 1.524 1.524) (drill 0.92) (layers *.Cu *.Mask)
      (net 18 "Net-(J1-Pad4)"))
    (pad 6 thru_hole circle (at -1.75 0.5 90) (size 1.4 1.4) (drill 1.4) (layers *.Cu *.Mask))
    (pad 7 thru_hole circle (at 2.75 0.5 90) (size 1.4 1.4) (drill 1.4) (layers *.Cu *.Mask))
    (pad GND thru_hole oval (at 6.35 0.5 90) (size 1.4 3.8) (drill oval 1 2.5) (layers *.Cu *.Mask))
    (pad GND thru_hole oval (at -5.35 0.5 90) (size 1.4 3.8) (drill oval 1 2.5) (layers *.Cu *.Mask))
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5927FCB8)
    (at 176.53 100.33 180)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference P1 (at 0 5.08 180) (layer F.SilkS))
    (fp_text value CONN_2 (at 0 4.87 180) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.33 180) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 PB2))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 11 "Net-(D1-Pad1)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 5927FD0E)
    (at 128.25 88.75)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference P2 (at 2.56 -0.485 90) (layer F.SilkS))
    (fp_text value CONN_2 (at 0 4.87) (layer F.Fab) hide)
    (fp_text user %R (at 0.02 5.865) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J1-Pad4)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GNDPWR))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_2x03_Pitch2.54mm (layer F.Cu) (tedit 5927FB8A)
    (at 151.13 90.17 270)
    (descr "Through hole straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x03 2.54mm double row")
    (fp_text reference P3 (at 1.27 -2.33 270) (layer F.SilkS))
    (fp_text value CONN_3X2 (at 1.27 7.41 270) (layer F.Fab) hide)
    (fp_text user %R (at 1.27 -2.33 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 8 PB1))
    (pad 2 thru_hole oval (at 2.54 0 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 3 thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 7 PB2))
    (pad 4 thru_hole oval (at 2.54 2.54 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 PB0))
    (pad 5 thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 13 RESET))
    (pad 6 thru_hole oval (at 2.54 5.08 270) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 2 GNDPWR))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_2x03_Pitch2.54mm.wrl
      (at (xyz 0.05 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm (layer F.Cu) (tedit 59283C58)
    (at 162.56 81.28 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (fp_text reference P4 (at 0 -2.33 90) (layer F.SilkS))
    (fp_text value CONN_2 (at 0 4.87 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 -2.33 90) (layer F.Fab) hide)
    (pad 1 thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 9 PB0))
    (pad 2 thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(BU1-Pad1)"))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch2.54mm.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Discret:R3-LARGE_PADS (layer F.Cu) (tedit 5927FD66)
    (at 163.83 77.47 180)
    (descr "Resitance 3 pas")
    (tags R)
    (fp_text reference R1 (at 0 0 180) (layer F.SilkS))
    (fp_text value 51r (at 0 0 180) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -3.81 0 180) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.Mask)
      (net 10 "Net-(BU1-Pad1)"))
    (pad 2 thru_hole circle (at 3.81 0 180) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.Mask)
      (net 9 PB0))
    (model Discret.3dshapes/R3-LARGE_PADS.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Discret:R3-LARGE_PADS (layer F.Cu) (tedit 5927FB6D)
    (at 163.83 99.695 180)
    (descr "Resitance 3 pas")
    (tags R)
    (fp_text reference R2 (at 0 0 180) (layer F.SilkS))
    (fp_text value 10k (at 0 0 180) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -3.81 0 180) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.Mask)
      (net 2 GNDPWR))
    (pad 2 thru_hole circle (at 3.81 0 180) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.Mask)
      (net 8 PB1))
    (model Discret.3dshapes/R3-LARGE_PADS.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Discret:R3-LARGE_PADS (layer F.Cu) (tedit 5927FB68)
    (at 173.355 99.06 270)
    (descr "Resitance 3 pas")
    (tags R)
    (fp_text reference R3 (at 0 0 270) (layer F.SilkS))
    (fp_text value 330r (at 0 0 270) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -3.81 0 270) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.Mask)
      (net 11 "Net-(D1-Pad1)"))
    (pad 2 thru_hole circle (at 3.81 0 270) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.Mask)
      (net 7 PB2))
    (model Discret.3dshapes/R3-LARGE_PADS.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module Discret:R3-LARGE_PADS (layer F.Cu) (tedit 5927FB71)
    (at 163.83 102.87)
    (descr "Resitance 3 pas")
    (tags R)
    (fp_text reference R4 (at 0 0) (layer F.SilkS))
    (fp_text value 10K (at 0 0) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -3.81 0) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.Mask)
      (net 4 "Net-(AT1-Pad4)"))
    (pad 2 thru_hole circle (at 3.81 0) (size 1.651 1.651) (drill 0.8128) (layers *.Cu *.Mask)
      (net 1 VCC))
    (model Discret.3dshapes/R3-LARGE_PADS.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.3 0.3 0.3))
      (rotate (xyz 0 0 0))
    )
  )
  (module G0TDJ:Omron_B3F_Tact_Switch (layer F.Cu) (tedit 5927FCC7)
    (at 163.83 90.17 180)
    (fp_text reference S1 (at -1.27 0 180) (layer F.SilkS))
    (fp_text value TAC_SWITCH (at -1.27 -7.366 180) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at -7.62 -2.54 180) (size 2 2) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 PB1))
    (pad 2 thru_hole circle (at 5.08 -2.54 180) (size 2 2) (drill 1.016) (layers *.Cu *.Mask)
      (net 8 PB1))
    (pad 3 thru_hole circle (at 5.08 2.54 180) (size 2 2) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 4 thru_hole circle (at -7.62 2.54 180) (size 2 2) (drill 1.016) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 5 thru_hole circle (at -1.25 -4.55 180) (size 2 2) (drill 2) (layers *.Cu *.Mask))
    (pad 6 thru_hole circle (at -1.25 4.45 180) (size 2 2) (drill 2) (layers *.Cu *.Mask))
  )
  (module G0TDJ:TACTILE-PTH (layer F.Cu) (tedit 5927FCD2)
    (at 165.1 90.17 180)
    (descr "<b>OMRON SWITCH</b>")
    (solder_mask_margin 0.1)
    (fp_text reference S2 (at 3.175 -5.08 180) (layer F.SilkS))
    (fp_text value TAC_SWITCH (at 0.254 4.064 180) (layer F.SilkS) hide)
    (pad 1 thru_hole circle (at -3.2512 -2.2606 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 PB1) (solder_mask_margin 0.2))
    (pad 2 thru_hole circle (at 3.2512 -2.2606 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 8 PB1) (solder_mask_margin 0.2))
    (pad 3 thru_hole circle (at -3.2512 2.2606 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC) (solder_mask_margin 0.2))
    (pad 4 thru_hole circle (at 3.2512 2.2606 180) (size 1.8796 1.8796) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 1 VCC) (solder_mask_margin 0.2))
  )
  (module G0TDJ:SPDT_SWITCH_PCB (layer F.Cu) (tedit 5927FC20)
    (at 132.08 77.47)
    (solder_mask_margin 0.1)
    (fp_text reference SW1 (at 0 -3.556) (layer F.SilkS) hide)
    (fp_text value SPDT_SWITCH (at -3.302 3.81) (layer F.SilkS) hide)
    (pad 1 thru_hole oval (at -3 0 90) (size 2.616 1.308) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(SW1-Pad1)") (solder_mask_margin 0.2))
    (pad COM thru_hole oval (at 0 0 90) (size 2.616 1.308) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 18 "Net-(J1-Pad4)") (solder_mask_margin 0.2))
    (pad 2 thru_hole oval (at 3 0 90) (size 2.616 1.308) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 12 VIN) (solder_mask_margin 0.2))
  )
  (module G0TDJ:Digispark_ATTiny85 (layer F.Cu) (tedit 59281CC9)
    (at 147.32 88.9 270)
    (fp_text reference AT1 (at -6.89 10.19 270) (layer F.SilkS) hide)
    (fp_text value Digispark_ATTiny85 (at 15.24 0.635 360) (layer F.SilkS) hide)
    (fp_text user PB0 (at 10.16 5.08 270) (layer F.SilkS))
    (fp_text user PB1 (at 10.16 2.54 270) (layer F.SilkS))
    (fp_text user PB2 (at 10.16 0 270) (layer F.SilkS))
    (fp_text user PB3 (at 10.16 -2.54 270) (layer F.SilkS))
    (fp_text user PB4 (at 10.16 -5.08 270) (layer F.SilkS))
    (fp_text user PB5 (at 10.16 -7.62 270) (layer F.SilkS))
    (fp_text user Vin (at 5.08 5.08 360) (layer F.SilkS))
    (fp_text user GND (at 2.54 5.08 360) (layer F.SilkS))
    (fp_text user VCC (at 0 5.08 360) (layer F.SilkS))
    (fp_text user ATTiny85 (at 10.9 10.2 270) (layer Eco2.User) hide)
    (pad 1 thru_hole circle (at 0 7.62 270) (size 2 2) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 2 thru_hole circle (at 2.54 7.62 270) (size 2 2) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 GNDPWR))
    (pad 3 thru_hole circle (at 5.08 7.62 270) (size 2 2) (drill 0.762) (layers *.Cu *.Mask)
      (net 3 "Net-(AT1-Pad3)"))
    (pad 4 thru_hole circle (at 12.7 -7.62 270) (size 2 2) (drill 0.762) (layers *.Cu *.Mask)
      (net 4 "Net-(AT1-Pad4)"))
    (pad 5 thru_hole circle (at 12.7 -5.08 270) (size 2 2) (drill 0.762) (layers *.Cu *.Mask)
      (net 5 "Net-(AT1-Pad5)"))
    (pad 6 thru_hole circle (at 12.7 -2.54 270) (size 2 2) (drill 0.762) (layers *.Cu *.Mask)
      (net 6 "Net-(AT1-Pad6)"))
    (pad 7 thru_hole circle (at 12.7 0 270) (size 2 2) (drill 0.762) (layers *.Cu *.Mask)
      (net 7 PB2))
    (pad 8 thru_hole circle (at 12.7 2.54 270) (size 2 2) (drill 0.762) (layers *.Cu *.Mask)
      (net 8 PB1))
    (pad 9 thru_hole circle (at 12.7 5.08 270) (size 2 2) (drill 0.762) (layers *.Cu *.Mask)
      (net 9 PB0))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_Pad (layer F.Cu) (tedit 59282086)
    (at 123.825 78.105)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_Pad (at 0 4.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 2 GNDPWR))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_Pad (layer F.Cu) (tedit 59282094)
    (at 123.825 101.6)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_Pad (at 0 4.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 2 GNDPWR))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_Pad (layer F.Cu) (tedit 5928209E)
    (at 182.245 101.6)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_Pad (at 0 4.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 2 GNDPWR))
  )
  (module Mounting_Holes:MountingHole_3.2mm_M3_Pad (layer F.Cu) (tedit 59282099)
    (at 182.245 78.105)
    (descr "Mounting Hole 3.2mm, M3")
    (tags "mounting hole 3.2mm m3")
    (fp_text reference REF** (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value MountingHole_3.2mm_M3_Pad (at 0 4.2) (layer F.Fab) hide)
    (pad 1 thru_hole circle (at 0 0) (size 6.4 6.4) (drill 3.2) (layers *.Cu *.Mask)
      (net 2 GNDPWR))
  )
  (module G0TDJ:OSHW_Logo_6.4mm_F.CU (layer F.Cu) (tedit 0)
    (at 172.72 78.74)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module G0TDJ:OSHW_Logo_6.4mm_F.MASK (layer F.Cu) (tedit 0)
    (at 172.72 78.74)
    (fp_text reference G*** (at 0 0) (layer F.SilkS) hide)
    (fp_text value LOGO (at 0.75 0) (layer F.SilkS) hide)
  )
  (module G0TDJ:projectavr_logo_F_Copper_11.5mm (layer F.Cu) (tedit 58ECE162)
    (at 133.985 99.695)
    (fp_text reference G*** (at 0 -2.54) (layer F.Cu) hide)
    (fp_text value LOGO (at 1.27 2.54) (layer F.Cu) hide)
  )
  (module G0TDJ:projectavr_logo_MASK_11.5mm (layer F.Cu) (tedit 58ECE162)
    (at 133.985 99.695)
    (fp_text reference G*** (at 0 -2.54) (layer F.Mask) hide)
    (fp_text value LOGO (at 1.27 2.54) (layer F.Mask) hide)
  )
  (module G0TDJ:KiCad-Logo_Copper_11mmx5mm (layer B.Cu) (tedit 56780A65)
    (at 134.112 101.092 180)
    (fp_text reference G*** (at -0.8 1.6 180) (layer Cmts.User))
    (fp_text value "KiCad Logo" (at 2.8 1 180) (layer B.SilkS) hide)
    (fp_text user "DESIGNED WITH" (at 0 -2.6 180) (layer B.SilkS))
    (pad 1 smd circle (at -2.17 1.49 180) (size 0.9 0.9) (layers B.Cu B.Mask)
      (solder_mask_margin -0.01))
  )
  (gr_text DIGISPARK (at 155.448 89.916 90) (layer F.SilkS))
  (gr_text ICSP (at 148.59 87.884) (layer F.SilkS))
  (gr_text 4 (at 123.19 86.106) (layer F.SilkS))
  (gr_text 1 (at 123.19 93.98) (layer F.SilkS))
  (gr_text "Electronic Film Clapper\nby Steve Smith - G0TDJ" (at 128.27 101.6) (layer F.SilkS))
  (gr_text GND (at 128.27 93.98) (layer F.SilkS))
  (gr_text +Vin (at 128.27 86.36) (layer F.SilkS))
  (gr_text ON (at 139.192 77.216) (layer F.SilkS))
  (gr_line (start 120.015 76.2) (end 120.015 103.505) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 184.15 74.295) (end 121.92 74.295) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 186.055 103.505) (end 186.055 76.2) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 121.92 105.41) (end 184.15 105.41) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 121.92 76.2) (end 120.015 76.2) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 184.15 76.2) (end 184.15 74.295) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 184.15 103.505) (end 186.055 103.505) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_arc (start 121.92 103.505) (end 121.92 105.41) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GNDPWR) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.381))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 120.015 74.295) (xy 120.015 105.41) (xy 186.055 105.41) (xy 186.055 74.295)
      )
    )
  )
  (zone (net 2) (net_name GNDPWR) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.381))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 120.015 74.295) (xy 120.015 105.41) (xy 186.055 105.41) (xy 186.055 74.295)
      )
    )
  )
)
